======================================================================
                  BAT GRB EVENT DATA PROCESSING REPORT
    Process Script Ver: batgrbproduct v2.48
    Process Start Time: Tue Nov 11 11:57:54 GMT 2025
             Host Name: fireball.star.le.ac.uk
   Current Working Dir: /fbdata/autoproc/tmp/batxrtlc_3gA4x
======================================================================

  Trigger: 00321376      Segment: 000

  BAT Trigger Time: 241131776   [s; MET]
      Trigger Stop: 241131840   [s; MET]
               UTC: 2008-08-22T21:02:52.960620    [includes UTCF correction] 
       Where From?: TDRSS position message

  BAT 
    RA: 63.4950367894906   Dec: 25.7428354460579  [deg; J2000]

     Catalogged Source?: NO
     Point Source?:      YES
     GRB Indicated?:     YES    [ by BAT flight software ]
     Image S/N Ratio:    7.15
     Image Trigger?:     YES
     Rate S/N Ratio:     0  [ if not an image trigger ]
     Image S/N Ratio:    7.15

  Analysis Position:   [ source = BAT ]
    RA: 63.4950367894906   Dec: 25.7428354460579  [deg; J2000]

  Refined Position:   [ source = BAT pre-slew burst ]
    RA: 63.5602949699223   Dec: 25.7598699175685  [deg; J2000]  
        { 04h 14m 14.5s , +25d 45' 35.5" }
         +/- 3.60767737732545 [arcmin] (estimated 90% radius based on SNR)
         +/- 1.94827496599252 [arcmin] (formal 1-sigma fit error)
    SNR: 4.8649548987709



  Partial Coding Fraction: 0.8203125    [ including projection effects ]

  Duration
     T90: 64 +/- 
        Measured from: 0
                   to: 64     [s; relative to TRIGTIME]
     T50: 64 +/- 
        Measured from: 0
                   to: 64     [s; relative to TRIGTIME]

    WARNING: battblocks failed.  Used TDRSS fore/background intervals

  Fluence
     Peak Flux  (peak 64 second)
        Measured from: 0     
                   to: 64     [s; relative to TRIGTIME]
     Total Fluence        
        Measured from: 0     
                   to: 64     [s; relative to TRIGTIME]
     
             Band 1     Band 2     Band 3     Band 4
              15-25      25-50     50-100    100-350     keV
 Total     0.216379   0.195504  -0.011686  -0.017961
           0.042473   0.042265   0.036346   0.030853 [error]
 Peak      0.216379   0.195504  -0.011686  -0.017961
           0.042473   0.042265   0.036346   0.030853 [error]

     [ fluence units of on-axis counts / fully illuminated detector ] 

======================================================================
