======================================================================
                  BAT GRB EVENT DATA PROCESSING REPORT
    Process Script Ver: batgrbproduct v2.48
    Process Start Time: Tue Nov 11 12:00:27 GMT 2025
             Host Name: fireball.star.le.ac.uk
   Current Working Dir: /fbdata/autoproc/tmp/batxrtlc_umxvx
======================================================================

  Trigger: 00331964      Segment: 000

  BAT Trigger Time: 245979496   [s; MET]
      Trigger Stop: 245979816   [s; MET]
               UTC: 2008-10-17T23:38:12.816960    [includes UTCF correction] 
       Where From?: TDRSS position message

  BAT 
    RA: 230.179956090345   Dec: -32.815165184944  [deg; J2000]

     Catalogged Source?: NO
     Point Source?:      YES
     GRB Indicated?:     NO    [ by BAT flight software ]
     Image S/N Ratio:    8.34
     Image Trigger?:     YES
     Rate S/N Ratio:     0  [ if not an image trigger ]
     Image S/N Ratio:    8.34

  Analysis Position:   [ source = BAT ]
    RA: 230.179956090345   Dec: -32.815165184944  [deg; J2000]

  Refined Position:   [ source = BAT pre-slew burst ]
    RA: 230.211672777236   Dec: -32.7919482688296  [deg; J2000]  
        { 15h 20m 50.8s , -32d 47' 31.0" }
         +/- 2.28906135637761 [arcmin] (estimated 90% radius based on SNR)
         +/- 1.38824215737663 [arcmin] (formal 1-sigma fit error)
    SNR: 9.31798583879837



  Partial Coding Fraction: 0.8046875    [ including projection effects ]

  Duration
     T90: 320 +/- 
        Measured from: 0
                   to: 320     [s; relative to TRIGTIME]
     T50: 320 +/- 
        Measured from: 0
                   to: 320     [s; relative to TRIGTIME]

    WARNING: battblocks failed.  Used TDRSS fore/background intervals

  Fluence
     Peak Flux  (peak 320 second)
        Measured from: 0     
                   to: 320     [s; relative to TRIGTIME]
     Total Fluence        
        Measured from: 0     
                   to: 320     [s; relative to TRIGTIME]
     
             Band 1     Band 2     Band 3     Band 4
              15-25      25-50     50-100    100-350     keV
 Total     0.847028   0.762145   0.628830   0.110292
           0.108942   0.098841   0.087157   0.082510 [error]
 Peak      0.847028   0.762145   0.628830   0.110292
           0.108942   0.098841   0.087157   0.082510 [error]

     [ fluence units of on-axis counts / fully illuminated detector ] 

======================================================================
