======================================================================
                  BAT GRB EVENT DATA PROCESSING REPORT
    Process Script Ver: batgrbproduct v2.48
    Process Start Time: Tue Nov 11 14:20:46 GMT 2025
             Host Name: fireball.star.le.ac.uk
   Current Working Dir: /fbdata/autoproc/tmp/batxrtlc_mmaxf
======================================================================

  Trigger: 00932058      Segment: 000

  BAT Trigger Time: 594040544   [s; MET]
      Trigger Stop: 594040608   [s; MET]
               UTC: 2019-10-29T11:15:20.169860    [includes UTCF correction] 
       Where From?: TDRSS position message

  BAT 
    RA: 352.139953073243   Dec: -40.4638223155307  [deg; J2000]

     Catalogged Source?: NO
     Point Source?:      YES
     GRB Indicated?:     YES    [ by BAT flight software ]
     Image S/N Ratio:    9.55
     Image Trigger?:     YES
     Rate S/N Ratio:     0  [ if not an image trigger ]
     Image S/N Ratio:    9.55

  Analysis Position:   [ source = BAT ]
    RA: 352.139953073243   Dec: -40.4638223155307  [deg; J2000]

  Refined Position:   [ source = BAT pre-slew burst ]
    RA: 352.171888347978   Dec: -40.4478845827337  [deg; J2000]  
        { 23h 28m 41.3s , -40d 26' 52.4" }
         +/- 2.72075647405484 [arcmin] (estimated 90% radius based on SNR)
         +/- 1.15220815293668 [arcmin] (formal 1-sigma fit error)
    SNR: 7.280029436049



  Partial Coding Fraction: 0.4335938    [ including projection effects ]

  Duration
     T90: 20 +/- 4.24264068711928
        Measured from: -4
                   to: 16     [s; relative to TRIGTIME]
     T50: 9 +/- 2.23606797749979
        Measured from: 1
                   to: 10     [s; relative to TRIGTIME]



  Fluence
     Peak Flux  (peak 1 second)
        Measured from: 2     
                   to: 3     [s; relative to TRIGTIME]
     Total Fluence        
        Measured from: -4     
                   to: 18     [s; relative to TRIGTIME]
     
             Band 1     Band 2     Band 3     Band 4
              15-25      25-50     50-100    100-350     keV
 Total     0.374079   0.603298   0.369699   0.047278
           0.045704   0.048621   0.043378   0.039477 [error]
 Peak      0.013645   0.077714   0.020792   0.008422
           0.010273   0.010613   0.009525   0.008637 [error]

     [ fluence units of on-axis counts / fully illuminated detector ] 

======================================================================
