++lUtils/createLog.cpp::      createLog:  line   51  INFO   >>  Created FileAppender: 'genlc.log', level info
++/genlc_cpp/genlc.cpp::           main:  line  151  INFO   >>  Starting to run genlc.cpp, mode=0
++/genlc_cpp/genlc.cpp::           main:  line  152  INFO   >>  Argparsing reported: Selected GRB binning.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: WT, with files: wtsourcetotal.evt, wtbacktotal.evt, and wtcorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 2796.34 - 3000
++/SourceEventList.cpp::SourceEventList:  line   67  FATAL  >>  Can't open file wtsourcetotal.evt
++/genlc_cpp/genlc.cpp::           main:  line  388  WARN   >>  Unable to open the files for this mode, skipping
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: WT, with files: wtsourcetotal_incbad.evt, wtbacktotal_incbad.evt, and wtcorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 2796.34 - 3000
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	2796.34 - 2798.32
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - WT mode, suffix = _incbad
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 30 ct/bin at rateFact=10 and binFact= 1.5 with minT 0.5 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file WTCURVE_incbad.qdp, reading from wtsourcetotal_incbad.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2796.34 - 2798.32), exposure 1.97484
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0 bg counts (0), with cf=1.08821 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.17642 +/- 1.53896
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2796.34 - 2798.32), exposure 1.97484, 1 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.551039, 0.551039 and 1. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2796.34 and stop= 2798.32 so gap is 1.97484, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x19d4fe0
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2796.34 - 2798.32), exposure 1.97484
++taStructures/bin.cpp::   bayesian_bin:  line  273  INFO   >>  Making a Bayesian bin - I have 2 counts and 0 bg counts, with cf=1.08821
++taStructures/bin.cpp::   bayesian_bin:  line  274  INFO   >>    Therefore net =2.17642 + 2.02081 -1.23621 and sigma=1000
++tructures/grbBin.cpp::        binData:  line  929  INFO   >>  Not saving this bin as it is an incomplete WT one
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2796.34 - 2798.32), exposure 1.97484, 1 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.551039, 0.551039 and 1. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for WT mode.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: PC, with files: pcsourcetotal.evt, pcbacktotal.evt, and pccorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 2799.65 - 762051
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	2799.65 - 5400.97
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	8618.07 - 11179.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	14396.2 - 16953.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	20188.4 - 22741.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	25965.5 - 28521.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	31768.6 - 33580.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	37590.1 - 40100.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	43348.8 - 45875.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	49101.2 - 51664
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	54886.2 - 57230.5
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - PC mode, suffix = 
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 20 ct/bin at rateFact=10 and binFact= 1.5 with minT 2.51 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file PCCURVE.qdp, reading from pcsourcetotal.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2799.65 - 2914.99), exposure 115.337
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.20848 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9571 +/- 5.405
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2799.65 and stop= 2914.99 so gap is 115.337, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2799.65 - 2914.99), with lastBin= 0 and workMinC was 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2914.99 - 3010.26), exposure 95.2782
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.109878 bg counts (5), with cf=1.20201 and errBG= 0.049139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9082 +/- 5.37588
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2914.99 and stop= 3010.26 so gap is 95.2782, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2914.99 - 3010.26), with lastBin= 0x19d4fe0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2799.65 - 2914.99), exposure 115.337
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.20848 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9571 +/- 5.405
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3010.26 - 3193.3), exposure 183.034
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.263708 bg counts (12), with cf=1.19802 and errBG= 0.0761259
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6446 +/- 5.35851
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3010.26 and stop= 3193.3 so gap is 183.034, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (3010.26 - 3193.3), with lastBin= 0x19967a0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2914.99 - 3010.26), exposure 95.2782
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.109878 bg counts (5), with cf=1.20201 and errBG= 0.049139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9082 +/- 5.37588
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 1, last was 0 so increasing dead to 0.00464842
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3193.3 - 3411.44), exposure 218.132
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.151243 bg counts (7), with cf=2.24801 and errBG= 0.0571647
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6202 +/- 10.0542
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3193.3 and stop= 3411.44 so gap is 218.137, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (3193.3 - 3411.44), with lastBin= 0x19d4fe0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3010.26 - 3193.3), exposure 183.034
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.263708 bg counts (12), with cf=1.19802 and errBG= 0.0761259
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6446 +/- 5.35851
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 2, last was 1 so increasing dead to 0.00138
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3411.44 - 3742.4), exposure 330.964
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.243019 bg counts (12), with cf=2.25461 and errBG= 0.0701537
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.5443 +/- 10.0842
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3411.44 and stop= 3742.4 so gap is 330.966, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (3411.44 - 3742.4), with lastBin= 0x19967a0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3193.3 - 3411.44), exposure 218.132
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.151243 bg counts (7), with cf=2.24801 and errBG= 0.0571647
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6202 +/- 10.0542
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3742.4 - 3870.27), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0879026 bg counts (4), with cf=1.21107 and errBG= 0.0439513
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.115 +/- 5.41634
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3742.4 and stop= 3870.27 so gap is 127.873, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (3742.4 - 3870.27), with lastBin= 0x19d4fe0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3411.44 - 3742.4), exposure 330.964
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.243019 bg counts (12), with cf=2.25461 and errBG= 0.0701537
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.5443 +/- 10.0842
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2799.65 - 3917.91), exposure 1118.26, 15 soft counts and 108 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0202052, 0.148351 and 7.34224. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3870.27 and stop= 3917.91 so gap is 47.6389, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (2799.65 - 3917.91) = 2799.65- 3917.91
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3870.27 - 4070.86), exposure 200.585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.197781 bg counts (9), with cf=1.22588 and errBG= 0.0659269
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.1457 +/- 4.74849
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3870.27 and stop= 4070.86 so gap is 200.585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (3870.27 - 4070.86), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3742.4 - 3870.27), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0879026 bg counts (4), with cf=1.21107 and errBG= 0.0439513
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.115 +/- 5.41634
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4070.86 - 4221.3), exposure 150.439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.109878 bg counts (5), with cf=1.21302 and errBG= 0.049139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1272 +/- 5.42513
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4070.86 and stop= 4221.3 so gap is 150.439, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4070.86 - 4221.3), with lastBin= 0x19d4fe0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3870.27 - 4070.86), exposure 200.585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.197781 bg counts (9), with cf=1.22588 and errBG= 0.0659269
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.1457 +/- 4.74849
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4221.3 - 4401.82), exposure 180.526
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.21118 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.0106 +/- 5.41708
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4221.3 and stop= 4401.82 so gap is 180.526, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4221.3 - 4401.82), with lastBin= 0x19967a0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4070.86 - 4221.3), exposure 150.439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.109878 bg counts (5), with cf=1.21302 and errBG= 0.049139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1272 +/- 5.42513
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (3917.91 - 4451.97), exposure 534.057, 15 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0337142, 0.0900872 and 2.67208. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4401.82 and stop= 4451.97 so gap is 50.1462, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (3917.91 - 4451.97) = 3917.91- 4451.97
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4401.82 - 4584.86), exposure 183.034
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.329635 bg counts (15), with cf=1.20353 and errBG= 0.0851113
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6739 +/- 5.38333
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4401.82 and stop= 4584.86 so gap is 183.034, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4401.82 - 4584.86), with lastBin= 0x19d4fe0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4221.3 - 4401.82), exposure 180.526
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.21118 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.0106 +/- 5.41708
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4584.86 - 4795.47), exposure 210.614
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.20549 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8979 +/- 5.39163
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4584.86 and stop= 4795.47 so gap is 210.614, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4584.86 - 4795.47), with lastBin= 0x19967a0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4401.82 - 4584.86), exposure 183.034
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.329635 bg counts (15), with cf=1.20353 and errBG= 0.0851113
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6739 +/- 5.38333
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4795.47 - 4998.56), exposure 203.092
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.219756 bg counts (10), with cf=1.1979 and errBG= 0.0694931
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6947 +/- 5.35781
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4795.47 and stop= 4998.56 so gap is 203.092, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4795.47 - 4998.56), with lastBin= 0x19d4fe0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4584.86 - 4795.47), exposure 210.614
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.20549 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8979 +/- 5.39163
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 7.92245
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 15.8485
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 24.8555
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 33.8463
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 39.6359
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 46.5101
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 52.2985
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 59.2684
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 67.1924
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4998.56 - 5313.97), exposure 248.216
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.373586 bg counts (17), with cf=1.19794 and errBG= 0.0906079
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.5216 +/- 4.64088
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4998.56 and stop= 5313.97 so gap is 315.409, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4998.56 - 5313.97), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4795.47 - 4998.56), exposure 203.092
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.219756 bg counts (10), with cf=1.1979 and errBG= 0.0694931
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6947 +/- 5.35781
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 12
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 11
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 12, last was 11 so increasing dead to 8.99798
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 14, last was 12 so increasing dead to 15.8545
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 14, last was 12 so increasing dead to 24.8653
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5313.97 - 5400.97), exposure 22.5657
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.109878 bg counts (5), with cf=1.20044 and errBG= 0.049139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.26898 +/- 1.6987
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (4451.97 - 5400.97), exposure 817.376, 13 soft counts and 61 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0181196, 0.0890159 and 4.9127. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5313.97 and stop= 5400.97 so gap is 86.9942, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (5400.97) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=86.9942 whereas forward=3217.11
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4998.56 - 5400.97), exposure 270.782
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.483464 bg counts (22), with cf=1.19824 and errBG= 0.103075
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7907 +/- 4.942
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (5400.97) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (3917.91 - 5400.97), exposure 1351.43, 28 soft counts and 101 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0242787, 0.0894392 and 3.68386. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4998.56 - 5400.97), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 8618.07
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (3917.91 - 5400.97) = 3917.91- 5400.97
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 8618.07 - 11179.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8618.07 - 8811.14), exposure 193.063
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.105564 bg counts (7), with cf=1.25124 and errBG= 0.0398995
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6365 +/- 4.84628
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=8618.07 and stop= 8811.14 so gap is 193.063, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (8618.07 - 8811.14), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4998.56 - 5400.97), exposure 270.782
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.483464 bg counts (22), with cf=1.19824 and errBG= 0.103075
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7907 +/- 4.942
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 13
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8811.14 - 9086.94), exposure 275.805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.271451 bg counts (18), with cf=1.26085 and errBG= 0.0639815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.5704 +/- 4.8839
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=8811.14 and stop= 9086.94 so gap is 275.805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (8811.14 - 9086.94), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8618.07 - 8811.14), exposure 193.063
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.105564 bg counts (7), with cf=1.25124 and errBG= 0.0398995
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6365 +/- 4.84628
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 14
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9086.94 - 9297.56), exposure 210.615
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.120645 bg counts (8), with cf=1.27128 and errBG= 0.0426543
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9158 +/- 4.92395
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=9086.94 and stop= 9297.56 so gap is 210.615, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (9086.94 - 9297.56), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8811.14 - 9086.94), exposure 275.805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.271451 bg counts (18), with cf=1.26085 and errBG= 0.0639815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.5704 +/- 4.8839
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 15
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9297.56 - 9648.58), exposure 351.024
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.180967 bg counts (12), with cf=1.27094 and errBG= 0.0522407
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8342 +/- 4.92279
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=9297.56 and stop= 9648.58 so gap is 351.024, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (9297.56 - 9648.58), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9086.94 - 9297.56), exposure 210.615
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.120645 bg counts (8), with cf=1.27128 and errBG= 0.0426543
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9158 +/- 4.92395
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 16
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9648.58 - 9879.25), exposure 230.673
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.120645 bg counts (8), with cf=1.26356 and errBG= 0.0426543
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.801 +/- 4.89406
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=9648.58 and stop= 9879.25 so gap is 230.673, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (9648.58 - 9879.25), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9297.56 - 9648.58), exposure 351.024
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.180967 bg counts (12), with cf=1.27094 and errBG= 0.0522407
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8342 +/- 4.92279
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 17
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (8618.07 - 10109.9), exposure 1491.85, 15 soft counts and 72 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0124896, 0.0604464 and 4.83972. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=9879.25 and stop= 10109.9 so gap is 230.672, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (8618.07 - 10109.9) = 8618.07- 10109.9
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9879.25 - 10155.1), exposure 275.804
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0754029 bg counts (5), with cf=1.26282 and errBG= 0.0337212
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8471 +/- 4.89106
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=9879.25 and stop= 10155.1 so gap is 275.804, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (9879.25 - 10155.1), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9648.58 - 9879.25), exposure 230.673
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.120645 bg counts (8), with cf=1.26356 and errBG= 0.0426543
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.801 +/- 4.89406
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 18
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10155.1 - 10415.8), exposure 260.76
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.150806 bg counts (10), with cf=1.27095 and errBG= 0.047689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8726 +/- 4.92274
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=10155.1 and stop= 10415.8 so gap is 260.76, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10155.1 - 10415.8), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9879.25 - 10155.1), exposure 275.804
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0754029 bg counts (5), with cf=1.26282 and errBG= 0.0337212
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8471 +/- 4.89106
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 19
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10415.8 - 10734.2), exposure 318.428
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.211128 bg counts (14), with cf=1.26771 and errBG= 0.0564264
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.748 +/- 4.91035
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=10415.8 and stop= 10734.2 so gap is 318.428, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10415.8 - 10734.2), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10155.1 - 10415.8), exposure 260.76
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.150806 bg counts (10), with cf=1.27095 and errBG= 0.047689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8726 +/- 4.92274
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 6.84587
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 12.642
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 18.4545
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 24.2473
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 30.0301
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 35.8341
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 41.6269
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 48.5021
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 54.2959
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 60.0889
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 66.9821
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 75.9774
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 83.9086
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 91.8428
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 97.6641
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 103.479
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 110.344
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 123.616
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 41, last was 39 so increasing dead to 133.698
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 41, last was 39 so increasing dead to 139.614
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 146.633
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 157.829
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 165.913
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 172.198
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 180.991
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 188.032
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10734.2 - 11179.8), exposure 228.154
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 1.07072 bg counts (71), with cf=1.26402 and errBG= 0.127071
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =13.8149 +/- 4.38166
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (10109.9 - 11179.8), exposure 852.474, 10 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0132234, 0.0515675 and 3.89971. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=10734.2 and stop= 11179.8 so gap is 445.557, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 1 (11179.8) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=445.557 whereas forward=3216.43
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10415.8 - 11179.8), exposure 546.583
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 1.28185 bg counts (85), with cf=1.26607 and errBG= 0.139036
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.5611 +/- 6.58106
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 1 (11179.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (8618.07 - 11179.8), exposure 2344.33, 25 soft counts and 107 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0127562, 0.0572179 and 4.48551. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10415.8 - 11179.8), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 14396.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 50
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (8618.07 - 11179.8) = 8618.07- 11179.8
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 14396.2 - 16953.4


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 52, last was 50 so increasing dead to 5.85102
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 52, last was 50 so increasing dead to 11.6711
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 56, last was 52 so increasing dead to 17.5212
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 56, last was 52 so increasing dead to 23.3526
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 56, last was 52 so increasing dead to 29.2063
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 56, last was 52 so increasing dead to 35.0603
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 58, last was 56 so increasing dead to 41.9168
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 58, last was 56 so increasing dead to 49.8424
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 61, last was 58 so increasing dead to 58.8462
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 61, last was 58 so increasing dead to 64.6571
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 61, last was 58 so increasing dead to 74.7154
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 64, last was 61 so increasing dead to 86.9153
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 64, last was 61 so increasing dead to 92.7521
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 64, last was 61 so increasing dead to 104.945
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 110.755
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 116.637
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 126.729
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 133.587
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 139.416
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 145.232
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 151.059
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 156.878
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 162.717
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 168.533
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 79, last was 74 so increasing dead to 175.392
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 79, last was 74 so increasing dead to 182.248
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 79, last was 74 so increasing dead to 189.124
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 79, last was 74 so increasing dead to 197.064
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 79, last was 74 so increasing dead to 202.887
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 82, last was 79 so increasing dead to 211.878
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 82, last was 79 so increasing dead to 219.8
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 82, last was 79 so increasing dead to 230.927
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 83, last was 82 so increasing dead to 236.746
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 86, last was 83 so increasing dead to 245.756
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 86, last was 83 so increasing dead to 256.897
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 86, last was 83 so increasing dead to 262.708
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 89, last was 86 so increasing dead to 269.56
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 89, last was 86 so increasing dead to 281.757
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 89, last was 86 so increasing dead to 287.561
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 92, last was 89 so increasing dead to 294.429
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 92, last was 89 so increasing dead to 305.553
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 92, last was 89 so increasing dead to 312.406
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 96, last was 92 so increasing dead to 319.272
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 96, last was 92 so increasing dead to 330.396
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 96, last was 92 so increasing dead to 336.21
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 96, last was 92 so increasing dead to 342.032
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (14396.2 - 14979), exposure 240.701
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121047 bg counts (14), with cf=1.27785 and errBG= 0.0323512
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0131 +/- 4.94928
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=14396.2 and stop= 14979 so gap is 582.733, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (14396.2 - 14979), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10415.8 - 11179.8), exposure 546.583
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 1.28185 bg counts (85), with cf=1.26607 and errBG= 0.139036
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.5611 +/- 6.58106
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 21
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 96
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 98, last was 96 so increasing dead to 7.93407
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 98, last was 96 so increasing dead to 13.757
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 101, last was 98 so increasing dead to 20.6222
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 101, last was 98 so increasing dead to 26.443
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 101, last was 98 so increasing dead to 33.3118
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 104, last was 101 so increasing dead to 40.178
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 104, last was 101 so increasing dead to 47.0431
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 104, last was 101 so increasing dead to 54.9783
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 107, last was 104 so increasing dead to 60.792
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 107, last was 104 so increasing dead to 66.5917
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 107, last was 104 so increasing dead to 80.9325
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 92.0699
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 97.8713
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 105.822
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 112.689
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 125.978
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 132.847
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 138.644
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 148.716
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 157.718
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 166.733
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 118, last was 117 so increasing dead to 172.535
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 121, last was 118 so increasing dead to 181.542
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 121, last was 118 so increasing dead to 188.41
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 121, last was 118 so increasing dead to 205.951
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 123, last was 121 so increasing dead to 214.953
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 123, last was 121 so increasing dead to 222.884
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 128, last was 123 so increasing dead to 232.955
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 128, last was 123 so increasing dead to 239.82
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 128, last was 123 so increasing dead to 249.888
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 128, last was 123 so increasing dead to 258.89
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 128, last was 123 so increasing dead to 270.036
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 130, last was 128 so increasing dead to 276.975
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 130, last was 128 so increasing dead to 284.903
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 131, last was 130 so increasing dead to 292.828
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 133, last was 131 so increasing dead to 298.619
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 133, last was 131 so increasing dead to 308.679
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 134, last was 133 so increasing dead to 315.539
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (14979 - 15605.4), exposure 310.905
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.103755 bg counts (12), with cf=1.27782 and errBG= 0.0299514
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0348 +/- 4.94914
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=14979 and stop= 15605.4 so gap is 626.444, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (14979 - 15605.4), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (14396.2 - 14979), exposure 240.701
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121047 bg counts (14), with cf=1.27785 and errBG= 0.0323512
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0131 +/- 4.94928
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 22
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 134
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 135, last was 134 so increasing dead to 5.7781
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 138, last was 135 so increasing dead to 14.7838
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 138, last was 135 so increasing dead to 29.0949
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 138, last was 135 so increasing dead to 35.9523
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 139, last was 138 so increasing dead to 42.7895
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (15605.4 - 15883.9), exposure 235.687
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.0345849 bg counts (4), with cf=1.27809 and errBG= 0.0172924
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.4053 +/- 5.11242
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=15605.4 and stop= 15883.9 so gap is 278.476, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (15605.4 - 15883.9), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (14979 - 15605.4), exposure 310.905
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.103755 bg counts (12), with cf=1.27782 and errBG= 0.0299514
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0348 +/- 4.94914
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 23
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 139
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (14396.2 - 16164.7), exposure 1068.11, 15 soft counts and 39 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0177931, 0.0464506 and 2.61059. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=15883.9 and stop= 16164.7 so gap is 280.818, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (14396.2 - 16164.7) = 14396.2- 16164.7
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (15883.9 - 16307.6), exposure 423.735
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121047 bg counts (14), with cf=1.28061 and errBG= 0.0323512
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0542 +/- 4.95996
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=15883.9 and stop= 16307.6 so gap is 423.735, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (15883.9 - 16307.6), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (15605.4 - 15883.9), exposure 235.687
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.0345849 bg counts (4), with cf=1.27809 and errBG= 0.0172924
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.4053 +/- 5.11242
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 24
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 139
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16307.6 - 16953.4), exposure 493.937
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.181571 bg counts (21), with cf=1.28342 and errBG= 0.039622
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0182 +/- 4.97091
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16164.7 - 16953.4), exposure 636.853, 4 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.007696, 0.0361241 and 4.69388. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16307.6 and stop= 16953.4 so gap is 645.734, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 2 (16953.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (14396.2 - 16953.4), exposure 1704.96, 19 soft counts and 57 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0140215, 0.0425933 and 3.03771. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16307.6 - 16953.4), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (15883.9 - 16307.6), exposure 423.735
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121047 bg counts (14), with cf=1.28061 and errBG= 0.0323512
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0542 +/- 4.95996
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 25
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 20188.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 157
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (14396.2 - 16953.4) = 14396.2- 16953.4
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 20188.4 - 22741.9


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 161, last was 157 so increasing dead to 5.92152
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 161, last was 157 so increasing dead to 11.8298
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 161, last was 157 so increasing dead to 17.7278
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 161, last was 157 so increasing dead to 24.7055
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 35.8548
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 41.7812
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 47.6952
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 55.6579
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 61.5931
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 67.5256
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 77.6355
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 86.7298
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 92.6352
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 98.5478
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 105.547
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 111.457
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 117.383
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 124.34
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 130.251
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 137.216
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 145.161
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 153.109
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 162.129
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 172.23
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 179.164
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 185.088
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 191.003
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 196.915
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 202.848
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 189, last was 186 so increasing dead to 209.761
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 189, last was 186 so increasing dead to 218.775
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 189, last was 186 so increasing dead to 225.693
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 193, last was 189 so increasing dead to 235.773
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 193, last was 189 so increasing dead to 243.715
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 193, last was 189 so increasing dead to 250.608
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 193, last was 189 so increasing dead to 256.517
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 197, last was 193 so increasing dead to 263.41
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 197, last was 193 so increasing dead to 273.5
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 197, last was 193 so increasing dead to 280.387
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 197, last was 193 so increasing dead to 289.388
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 295.294
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 305.364
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 315.439
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 322.336
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 328.218
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 337.215
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 343.077
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 353.141
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 359.032
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 374.463
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 384.522
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 392.457
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 399.334
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 406.197
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 214, last was 211 so increasing dead to 418.417
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 214, last was 211 so increasing dead to 426.358
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 214, last was 211 so increasing dead to 442.83
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 217, last was 214 so increasing dead to 448.679
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 217, last was 214 so increasing dead to 457.689
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 217, last was 214 so increasing dead to 465.624
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 473.547
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 479.393
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 485.223
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 493.146
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 500.01
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 514.371
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 522.301
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 528.14
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 541.399
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 227, last was 226 so increasing dead to 552.525
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 230, last was 227 so increasing dead to 561.515
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 230, last was 227 so increasing dead to 571.595
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 230, last was 227 so increasing dead to 577.404
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 234, last was 230 so increasing dead to 585.331
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 234, last was 230 so increasing dead to 592.187
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 234, last was 230 so increasing dead to 598.026
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 234, last was 230 so increasing dead to 603.848
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 610.703
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 616.539
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 622.365
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 631.354
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 637.179
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 643.008
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 649.859
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 658.846
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 677.445
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 686.455
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 694.425
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 702.348
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 708.138
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 716.084
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 724.022
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 729.845
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 735.653
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 750.014
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 756.883
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 764.822
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 797.307
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 810.583
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 822.788
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 834.994
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 848.267
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 856.222
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 878.141
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (20188.4 - 21507.8), exposure 441.285
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.752119 bg counts (87), with cf=1.28113 and errBG= 0.0806356
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5345 +/- 5.12555
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=20188.4 and stop= 21507.8 so gap is 1319.43, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (20188.4 - 21507.8), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16307.6 - 16953.4), exposure 493.937
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.181571 bg counts (21), with cf=1.28342 and errBG= 0.039622
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0182 +/- 4.97091
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 26
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 261
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 266, last was 261 so increasing dead to 5.81726
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 266, last was 261 so increasing dead to 14.8307
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 266, last was 261 so increasing dead to 21.7205
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 266, last was 261 so increasing dead to 29.6562
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 266, last was 261 so increasing dead to 47.1972
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 55.1511
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 66.2883
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 79.5588
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 89.6259
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 99.6927
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 106.557
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 273, last was 272 so increasing dead to 127.3
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 278, last was 273 so increasing dead to 141.637
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 278, last was 273 so increasing dead to 171.986
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 278, last was 273 so increasing dead to 179.917
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 278, last was 273 so increasing dead to 185.715
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 278, last was 273 so increasing dead to 201.119
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 280, last was 278 so increasing dead to 210.132
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 280, last was 278 so increasing dead to 239.419
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 281, last was 280 so increasing dead to 249.496
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 284, last was 281 so increasing dead to 255.287
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 284, last was 281 so increasing dead to 268.55
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 284, last was 281 so increasing dead to 274.34
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 286, last was 284 so increasing dead to 284.4
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 286, last was 284 so increasing dead to 299.809
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 287, last was 286 so increasing dead to 305.579
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 288, last was 287 so increasing dead to 312.438
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 289, last was 288 so increasing dead to 318.23
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (21507.8 - 22184.6), exposure 358.544
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.155611 bg counts (18), with cf=1.28144 and errBG= 0.0366778
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0222 +/- 4.96322
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=21507.8 and stop= 22184.6 so gap is 676.774, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (21507.8 - 22184.6), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (20188.4 - 21507.8), exposure 441.285
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.752119 bg counts (87), with cf=1.28113 and errBG= 0.0806356
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5345 +/- 5.12555
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 27
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 289
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22184.6 - 22741.9), exposure 478.894
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.475477 bg counts (55), with cf=1.28116 and errBG= 0.0641133
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.07777 +/- 3.13925
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20188.4 - 22741.9), exposure 1278.72, 4 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00304575, 0.0326419 and 10.7172. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22184.6 and stop= 22741.9 so gap is 557.332, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 3 (22741.9) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=557.332 whereas forward=3223.55
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (21507.8 - 22741.9), exposure 837.438
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.631088 bg counts (73), with cf=1.28136 and errBG= 0.0738633
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.0999 +/- 5.87269
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 3 (22741.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (21507.8 - 22741.9), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 25965.5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 299
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 25965.5 - 28521.4


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 7.00258
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 13.9983
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 19.9748
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 26.9455
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 41.2942
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 49.3478
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 55.2599
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 61.1666
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 68.1516
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 74.0773
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 79.9958
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 85.9168
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 93.9401
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 102.971
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 109.968
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 115.877
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 122.894
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 135.117
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 321, last was 317 so increasing dead to 142.113
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 321, last was 317 so increasing dead to 148.007
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 321, last was 317 so increasing dead to 153.937
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 321, last was 317 so increasing dead to 159.851
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 323, last was 321 so increasing dead to 167.835
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 323, last was 321 so increasing dead to 176.852
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 325, last was 323 so increasing dead to 183.834
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 325, last was 323 so increasing dead to 190.807
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 328, last was 325 so increasing dead to 198.789
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 328, last was 325 so increasing dead to 204.707
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 328, last was 325 so increasing dead to 212.695
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 218.608
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 224.516
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 230.45
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 236.36
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 245.373
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 254.403
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 263.412
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 272.442
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 283.607
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 292.616
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 300.559
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 307.5
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 315.439
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 321.344
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 327.252
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 339.463
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 352.752
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 358.668
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 366.606
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 373.507
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 379.418
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 388.42
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 396.359
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 408.563
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 414.447
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 421.346
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 429.293
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 435.205
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 441.112
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 447.004
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 452.865
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 460.795
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 466.663
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 472.537
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 479.415
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 488.414
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 495.272
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 501.147
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 509.075
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 514.949
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 522.875
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 538.272
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 544.134
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 552.066
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 561.057
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 377, last was 373 so increasing dead to 569.002
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 377, last was 373 so increasing dead to 579.074
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 377, last was 373 so increasing dead to 584.922
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 377, last was 373 so increasing dead to 590.763
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 600.822
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 606.654
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 614.598
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 621.455
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 628.316
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 634.129
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 641
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 652.154
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 657.98
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 663.819
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 669.643
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 675.452
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 682.309
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 688.12
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 696.062
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 708.252
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 717.243
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 726.234
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 735.223
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 741.032
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 750.043
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 756.898
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 763.771
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 769.595
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 784.987
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 797.179
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 809.373
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 815.189
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 821.009
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 826.844
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 832.686
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 839.56
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 847.494
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 853.305
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 413, last was 411 so increasing dead to 868.716
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 413, last was 411 so increasing dead to 885.197
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 414, last was 413 so increasing dead to 891.032
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 901.104
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 909.035
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 921.242
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 928.107
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 942.445
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 948.245
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 955.112
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 961.975
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 972.043
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 978.907
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 987.906
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 995.846
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1004.84
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1018.12
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1027.12
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1036.11
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1063.28
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1073.35
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1098.38
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1108.45
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 436, last was 434 so increasing dead to 1119.59
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 436, last was 434 so increasing dead to 1131.79
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 437, last was 436 so increasing dead to 1141.86
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1147.66
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1154.53
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1167.8
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1174.66
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1191.15
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1200.15
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1208.07
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1214.94
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (25965.5 - 27882.5), exposure 702.044
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0870268 bg counts (120), with cf=3.77285 and errBG= 0.00794443
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =75.1287 +/- 16.8727
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25965.5 and stop= 27882.5 so gap is 1916.98, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (25965.5 - 27882.5), with lastBin= 0x19967a0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (21507.8 - 22741.9), exposure 837.438
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.631088 bg counts (73), with cf=1.28136 and errBG= 0.0738633
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.0999 +/- 5.87269
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 28
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 445
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 6.8595
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 21.191
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 28.0705
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 34.9269
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 40.7462
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 52.9426
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 61.9346
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 76.264
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 83.1198
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 94.253
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 102.177
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 116.505
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 124.431
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 133.424
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 141.351
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 147.151
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 152.939
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 162.982
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 169.836
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 175.649
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 188.893
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 196.815
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 203.674
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 210.54
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 217.397
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 225.308
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 231.118
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 236.989
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 251.317
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 259.26
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 267.19
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 273.09
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 281.024
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (27882.5 - 28521.4), exposure 330.964
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.0415542 bg counts (38), with cf=1.9983 and errBG= 0.00674098
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =3.91357 +/- 2.82606
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20188.4 - 28521.4), exposure 2311.73, 11 soft counts and 48 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0173555, 0.0353378 and 2.03612. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=27882.5 and stop= 28521.4 so gap is 638.924, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 4 (28521.4) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=638.924 whereas forward=3247.23
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (25965.5 - 28521.4), exposure 1033.01
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.128581 bg counts (158), with cf=3.61153 and errBG= 0.0102294
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =78.9893 +/- 16.9396
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 4 (28521.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (25965.5 - 28521.4), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 31768.6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 483
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 31768.6 - 33580.4


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 11.1456
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 21.2015
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 29.1476
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 36.0345
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 41.9016
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 47.7565
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 54.6118
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 60.4934
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 66.3446
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 72.1859
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 78.054
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 87.0649
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 92.9142
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 99.7721
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 105.598
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 113.542
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 119.386
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 125.237
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 132.102
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 137.954
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 145.878
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 151.702
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 167.099
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 173.954
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 179.786
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 185.625
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 196.749
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 202.591
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 208.403
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 216.346
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 223.202
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 230.06
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 237.985
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 244.838
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 250.652
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 256.491
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 262.302
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 269.173
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 275.016
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 281.868
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 289.787
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 295.592
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 302.446
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 309.325
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 316.213
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 327.336
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 334.204
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 340.022
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 346.892
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 359.084
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 364.908
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 372.839
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 382.91
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 388.753
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 398.823
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 539, last was 538 so increasing dead to 405.691
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 540, last was 539 so increasing dead to 416.824
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 422.647
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 428.446
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 435.317
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 445.382
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 452.264
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 462.338
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 469.219
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 484.625
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 491.49
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 497.29
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 506.287
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 512.085
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 518.961
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 525.825
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 536.961
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 550.233
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 556.032
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 566.098
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 574.033
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 586.248
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 593.114
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 599.984
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 606.865
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 613.733
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 621.657
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 632.792
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 638.587
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 570, last was 567 so increasing dead to 644.378
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 570, last was 567 so increasing dead to 651.234
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 570, last was 567 so increasing dead to 658.112
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 574, last was 570 so increasing dead to 666.057
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 574, last was 570 so increasing dead to 671.865
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 574, last was 570 so increasing dead to 678.72
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 574, last was 570 so increasing dead to 694.119
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 577, last was 574 so increasing dead to 700.957
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 577, last was 574 so increasing dead to 706.747
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 577, last was 574 so increasing dead to 713.582
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (31768.6 - 33580.4), exposure 1098.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.52243 bg counts (61), with cf=1.2858 and errBG= 0.0668904
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6153 +/- 4.98063
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20188.4 - 33580.4), exposure 3409.93, 11 soft counts and 63 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0115734, 0.0294564 and 2.54518. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=31768.6 and stop= 33580.4 so gap is 1811.78, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 5 (33580.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (31768.6 - 33580.4), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (25965.5 - 28521.4), exposure 1033.01
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.128581 bg counts (158), with cf=3.61153 and errBG= 0.0102294
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =78.9893 +/- 16.9396
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 29
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 37590.1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 578
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 37590.1 - 40100.8


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 580, last was 578 so increasing dead to 12.2028
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 580, last was 578 so increasing dead to 24.4059
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 581, last was 580 so increasing dead to 33.4049
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20188.4 - 38300.5), exposure 4086.9, 15 soft counts and 72 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0111281, 0.027392 and 2.46151. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=37590.1 and stop= 38300.5 so gap is 710.379, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (20188.4 - 38300.5) = 20188.4- 38300.5
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (37590.1 - 38473.5), exposure 849.978
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.316088 bg counts (37), with cf=1.30309 and errBG= 0.0519646
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1345 +/- 5.04731
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=37590.1 and stop= 38473.5 so gap is 883.383, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (37590.1 - 38473.5), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (31768.6 - 33580.4), exposure 1098.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.52243 bg counts (61), with cf=1.2858 and errBG= 0.0668904
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6153 +/- 4.98063
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 30
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 581
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (38473.5 - 39438.8), exposure 965.313
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.418603 bg counts (49), with cf=1.29453 and errBG= 0.0598004
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8761 +/- 5.01429
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=38473.5 and stop= 39438.8 so gap is 965.313, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (38473.5 - 39438.8), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (37590.1 - 38473.5), exposure 849.978
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.316088 bg counts (37), with cf=1.30309 and errBG= 0.0519646
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1345 +/- 5.04731
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 31
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 581
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (39438.8 - 40100.8), exposure 473.874
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.153773 bg counts (18), with cf=1.31044 and errBG= 0.0362445
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.41937 +/- 1.85385
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (38300.5 - 40100.8), exposure 1612.19, 2 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0014103, 0.0133 and 9.43063. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=39438.8 and stop= 40100.8 so gap is 662.037, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 6 (40100.8) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=662.037 whereas forward=3248
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (38473.5 - 40100.8), exposure 1439.19
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.572376 bg counts (67), with cf=1.2964 and errBG= 0.0699268
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.2968 +/- 5.34597
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 6 (40100.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20188.4 - 40100.8), exposure 5699.09, 17 soft counts and 89 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0083489, 0.0233977 and 2.80249. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (38473.5 - 40100.8), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 43348.8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 602
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (20188.4 - 40100.8) = 20188.4- 40100.8
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 43348.8 - 45875.7


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (43348.8 - 44271.5), exposure 922.69
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.265729 bg counts (31), with cf=1.30372 and errBG= 0.0477264
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.2094 +/- 5.04969
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=43348.8 and stop= 44271.5 so gap is 922.69, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (43348.8 - 44271.5), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (38473.5 - 40100.8), exposure 1439.19
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.572376 bg counts (67), with cf=1.2964 and errBG= 0.0699268
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.2968 +/- 5.34597
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 32
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 602
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (44271.5 - 45061.3), exposure 789.801
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.317161 bg counts (37), with cf=1.29902 and errBG= 0.0521409
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0733 +/- 5.03153
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=44271.5 and stop= 45061.3 so gap is 789.801, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (44271.5 - 45061.3), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (43348.8 - 44271.5), exposure 922.69
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.265729 bg counts (31), with cf=1.30372 and errBG= 0.0477264
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.2094 +/- 5.04969
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 33
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 602
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (45061.3 - 45875.7), exposure 769.736
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.274301 bg counts (32), with cf=1.298 and errBG= 0.0484901
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.2199 +/- 4.49683
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (43348.8 - 45875.7), exposure 2482.23, 10 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00508895, 0.0164652 and 3.23547. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=45061.3 and stop= 45875.7 so gap is 814.355, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 7 (45875.7) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=814.355 whereas forward=3225.57
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (44271.5 - 45875.7), exposure 1559.54
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.591462 bg counts (69), with cf=1.29856 and errBG= 0.0712037
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.2932 +/- 6.74817
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 7 (45875.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (44271.5 - 45875.7), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 49101.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 609
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 49101.2 - 51664


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (49101.2 - 50502.8), exposure 1401.58
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.245829 bg counts (45), with cf=1.55887 and errBG= 0.0366461
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.9999 +/- 6.03776
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=49101.2 and stop= 50502.8 so gap is 1401.58, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (49101.2 - 50502.8), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (44271.5 - 45875.7), exposure 1559.54
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.591462 bg counts (69), with cf=1.29856 and errBG= 0.0712037
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.2932 +/- 6.74817
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 34
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 609
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (50502.8 - 51664), exposure 1148.34
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.404252 bg counts (74), with cf=1.53618 and errBG= 0.0469934
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.59608 +/- 3.76355
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (43348.8 - 51664), exposure 5032.15, 11 soft counts and 52 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00276098, 0.0141601 and 5.12864. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=50502.8 and stop= 51664 so gap is 1161.18, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 8 (51664) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=1161.18 whereas forward=3222.22
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (49101.2 - 51664), exposure 2549.92
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.650082 bg counts (119), with cf=1.55239 and errBG= 0.0595929
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.591 +/- 7.11454
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 8 (51664) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (49101.2 - 51664), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 54886.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 612
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 54886.2 - 57230.5


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (54886.2 - 56385.6), exposure 1499.37
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.524526 bg counts (61), with cf=1.28603 and errBG= 0.0671587
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6159 +/- 4.98153
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=54886.2 and stop= 56385.6 so gap is 1499.37, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (54886.2 - 56385.6), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (49101.2 - 51664), exposure 2549.92
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.650082 bg counts (119), with cf=1.55239 and errBG= 0.0595929
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.591 +/- 7.11454
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 35
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 612
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (43348.8 - 57137.8), exposure 7283.71, 15 soft counts and 72 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00256318, 0.0132232 and 5.15888. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=56385.6 and stop= 57137.8 so gap is 752.191, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (43348.8 - 57137.8) = 43348.8- 57137.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (56385.6 - 57230.5), exposure 844.956
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.292359 bg counts (34), with cf=1.28599 and errBG= 0.0501392
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.4839 +/- 4.06716
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (57137.8 - 57230.5), exposure 92.7648, 0 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -0.000185389, 0.0137421 and -74.1258. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=56385.6 and stop= 57230.5 so gap is 844.956, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 9 (57230.5) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=844.956 whereas forward=1.8287e+08
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (54886.2 - 57230.5), exposure 2344.33
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.816886 bg counts (95), with cf=1.28601 and errBG= 0.0838107
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.0998 +/- 6.43097
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 9 (57230.5) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (43348.8 - 57230.5), exposure 7376.48, 15 soft counts and 73 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00252788, 0.0132298 and 5.23356. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x19967a0
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (54886.2 - 57230.5), exposure 2344.33
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.816886 bg counts (95), with cf=1.28601 and errBG= 0.0838107
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.0998 +/- 6.43097
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 36
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (43348.8 - 57230.5), exposure 7376.48, 15 soft counts and 73 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00252788, 0.0132298 and 5.23356. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  941  INFO   >>  Saving a final HR bin.
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for PC mode.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: PC, with files: pcsourcetotal_incbad.evt, pcbacktotal_incbad.evt, and pccorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 2799.65 - 762051
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	2799.65 - 5400.97
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	8618.07 - 11179.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	14396.2 - 16953.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	20188.4 - 22741.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	25965.5 - 28521.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	31768.6 - 33580.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	37590.1 - 40100.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	43348.8 - 45875.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	49101.2 - 51664
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	54886.2 - 57230.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	73584.4 - 74630
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	79349.8 - 80390.3
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	85166.8 - 86209.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	90862.8 - 91910.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	96688.4 - 97728.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	102443 - 103489
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	119785 - 120831
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	125544 - 126590
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	131304 - 132350
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	137006 - 138049
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	142885 - 143931
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	148763 - 149809
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	154404 - 155570
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	166104 - 167270
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	170964 - 172610
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	176725 - 178370
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	182549 - 184189
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	188305 - 189950
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	194063 - 195710
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	199883 - 201530
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	205644 - 207289
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	211464 - 213111
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	217223 - 217644
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	223102 - 223430
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	257723 - 258144
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	263545 - 263929
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	269303 - 269714
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	275064 - 275498
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	280888 - 281284
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	286652 - 287070
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	292462 - 292855
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	298222 - 298641
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	304042 - 304425
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	309983 - 310211
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	315982 - 315997
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	344542 - 344923
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	350302 - 350706
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	356129 - 356493
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	357568 - 357769
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	361885 - 363109
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	367642 - 369289
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	373465 - 375110
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	379225 - 380870
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	385042 - 385416
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	390805 - 391199
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	396682 - 396985
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	402742 - 402767
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	409953 - 410151
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	414624 - 415970
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	419462 - 420831
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	425542 - 426771
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	431302 - 432531
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	437127 - 438351
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	442882 - 444111
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	448706 - 449930
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	454462 - 455691
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	460290 - 461511
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	466042 - 467271
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	471871 - 473089
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	477622 - 478851
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	483502 - 484730
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	489509 - 490730
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	495563 - 496431
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	501446 - 502670
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	512183 - 513530
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	517942 - 519291
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	523771 - 525110
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	529524 - 530871
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	535342 - 536689
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	541102 - 542330
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	546924 - 548150
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	553295 - 553909
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	559078 - 559730
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	564262 - 565491
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	570083 - 571311
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	576090 - 577311
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	582084 - 583310
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	588086 - 589249
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	593006 - 594530
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	598779 - 600291
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	604562 - 606111
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	610347 - 611871
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	616129 - 617631
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	621912 - 623449
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	627693 - 629210
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	633476 - 635031
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	639259 - 640789
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	645044 - 646551
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	650826 - 652371
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	656606 - 658131
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	662391 - 663950
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	668176 - 669710
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	673955 - 675469
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	675840 - 675916
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	675966 - 676249
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	679745 - 681289
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	685427 - 687049
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	691247 - 692870
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	698146 - 699349
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	703967 - 705170
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	709727 - 710390
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	715555 - 716270
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	720168 - 721790
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	725926 - 727551
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	731688 - 733310
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	737508 - 739130
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	743269 - 744891
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	749089 - 750711
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	754848 - 756470
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	760606 - 762051
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - PC mode, suffix = _incbad
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 20 ct/bin at rateFact=10 and binFact= 1.5 with minT 2.51 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file PCCURVE_incbad.qdp, reading from pcsourcetotal_incbad.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2799.65 - 2914.99), exposure 115.337
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.20848 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9571 +/- 5.405
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2799.65 and stop= 2914.99 so gap is 115.337, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2799.65 - 2914.99), with lastBin= 0 and workMinC was 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2914.99 - 3010.26), exposure 95.2782
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.109878 bg counts (5), with cf=1.20201 and errBG= 0.049139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9082 +/- 5.37588
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2914.99 and stop= 3010.26 so gap is 95.2782, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2914.99 - 3010.26), with lastBin= 0x19967a0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2799.65 - 2914.99), exposure 115.337
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.20848 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9571 +/- 5.405
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3010.26 - 3193.3), exposure 183.034
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.263708 bg counts (12), with cf=1.19802 and errBG= 0.0761259
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6446 +/- 5.35851
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3010.26 and stop= 3193.3 so gap is 183.034, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (3010.26 - 3193.3), with lastBin= 0x19d4fe0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2914.99 - 3010.26), exposure 95.2782
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.109878 bg counts (5), with cf=1.20201 and errBG= 0.049139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9082 +/- 5.37588
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 1, last was 0 so increasing dead to 0.00464842
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3193.3 - 3411.44), exposure 218.132
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.151243 bg counts (7), with cf=2.24801 and errBG= 0.0571647
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6202 +/- 10.0542
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3193.3 and stop= 3411.44 so gap is 218.137, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (3193.3 - 3411.44), with lastBin= 0x19967a0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3010.26 - 3193.3), exposure 183.034
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.263708 bg counts (12), with cf=1.19802 and errBG= 0.0761259
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6446 +/- 5.35851
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 2, last was 1 so increasing dead to 0.00138
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3411.44 - 3742.4), exposure 330.964
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.243019 bg counts (12), with cf=2.25461 and errBG= 0.0701537
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.5443 +/- 10.0842
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3411.44 and stop= 3742.4 so gap is 330.966, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (3411.44 - 3742.4), with lastBin= 0x19d4fe0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3193.3 - 3411.44), exposure 218.132
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.151243 bg counts (7), with cf=2.24801 and errBG= 0.0571647
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6202 +/- 10.0542
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3742.4 - 3870.27), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0879026 bg counts (4), with cf=1.21107 and errBG= 0.0439513
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.115 +/- 5.41634
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3742.4 and stop= 3870.27 so gap is 127.873, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (3742.4 - 3870.27), with lastBin= 0x19967a0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3411.44 - 3742.4), exposure 330.964
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.243019 bg counts (12), with cf=2.25461 and errBG= 0.0701537
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.5443 +/- 10.0842
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2799.65 - 3917.91), exposure 1118.26, 15 soft counts and 108 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0202052, 0.148351 and 7.34224. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3870.27 and stop= 3917.91 so gap is 47.6389, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (2799.65 - 3917.91) = 2799.65- 3917.91
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3870.27 - 4070.86), exposure 200.585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.197781 bg counts (9), with cf=1.22588 and errBG= 0.0659269
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.1457 +/- 4.74849
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=3870.27 and stop= 4070.86 so gap is 200.585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (3870.27 - 4070.86), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3742.4 - 3870.27), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0879026 bg counts (4), with cf=1.21107 and errBG= 0.0439513
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.115 +/- 5.41634
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4070.86 - 4221.3), exposure 150.439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.109878 bg counts (5), with cf=1.21302 and errBG= 0.049139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1272 +/- 5.42513
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4070.86 and stop= 4221.3 so gap is 150.439, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4070.86 - 4221.3), with lastBin= 0x19967a0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (3870.27 - 4070.86), exposure 200.585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.197781 bg counts (9), with cf=1.22588 and errBG= 0.0659269
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.1457 +/- 4.74849
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4221.3 - 4401.82), exposure 180.526
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.21118 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.0106 +/- 5.41708
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4221.3 and stop= 4401.82 so gap is 180.526, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4221.3 - 4401.82), with lastBin= 0x19d4fe0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4070.86 - 4221.3), exposure 150.439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.109878 bg counts (5), with cf=1.21302 and errBG= 0.049139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1272 +/- 5.42513
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (3917.91 - 4451.97), exposure 534.057, 15 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0337142, 0.0900872 and 2.67208. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4401.82 and stop= 4451.97 so gap is 50.1462, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (3917.91 - 4451.97) = 3917.91- 4451.97
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4401.82 - 4584.86), exposure 183.034
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.329635 bg counts (15), with cf=1.20353 and errBG= 0.0851113
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6739 +/- 5.38333
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4401.82 and stop= 4584.86 so gap is 183.034, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4401.82 - 4584.86), with lastBin= 0x19967a0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4221.3 - 4401.82), exposure 180.526
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.21118 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.0106 +/- 5.41708
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4584.86 - 4795.47), exposure 210.614
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.20549 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8979 +/- 5.39163
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4584.86 and stop= 4795.47 so gap is 210.614, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4584.86 - 4795.47), with lastBin= 0x19d4fe0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4401.82 - 4584.86), exposure 183.034
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.329635 bg counts (15), with cf=1.20353 and errBG= 0.0851113
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6739 +/- 5.38333
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4795.47 - 4998.56), exposure 203.092
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.219756 bg counts (10), with cf=1.1979 and errBG= 0.0694931
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6947 +/- 5.35781
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4795.47 and stop= 4998.56 so gap is 203.092, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4795.47 - 4998.56), with lastBin= 0x19967a0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4584.86 - 4795.47), exposure 210.614
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.175805 bg counts (8), with cf=1.20549 and errBG= 0.0621565
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8979 +/- 5.39163
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 7.92245
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 15.8485
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 24.8555
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 33.8463
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 39.6359
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 46.5101
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 52.2985
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 59.2684
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 2 so increasing dead to 67.1924
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4998.56 - 5313.97), exposure 248.216
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.373586 bg counts (17), with cf=1.19794 and errBG= 0.0906079
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.5216 +/- 4.64088
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4998.56 and stop= 5313.97 so gap is 315.409, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4998.56 - 5313.97), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4795.47 - 4998.56), exposure 203.092
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.219756 bg counts (10), with cf=1.1979 and errBG= 0.0694931
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.6947 +/- 5.35781
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 12
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 11
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 12, last was 11 so increasing dead to 8.99798
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 14, last was 12 so increasing dead to 15.8545
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 14, last was 12 so increasing dead to 24.8653
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5313.97 - 5400.97), exposure 22.5657
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.109878 bg counts (5), with cf=1.20044 and errBG= 0.049139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.26898 +/- 1.6987
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (4451.97 - 5400.97), exposure 817.376, 13 soft counts and 61 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0181196, 0.0890159 and 4.9127. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5313.97 and stop= 5400.97 so gap is 86.9942, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (5400.97) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=86.9942 whereas forward=3217.11
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4998.56 - 5400.97), exposure 270.782
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.483464 bg counts (22), with cf=1.19824 and errBG= 0.103075
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7907 +/- 4.942
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (5400.97) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (3917.91 - 5400.97), exposure 1351.43, 28 soft counts and 101 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0242787, 0.0894392 and 3.68386. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4998.56 - 5400.97), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 8618.07
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (3917.91 - 5400.97) = 3917.91- 5400.97
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 8618.07 - 11179.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8618.07 - 8811.14), exposure 193.063
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.105564 bg counts (7), with cf=1.25124 and errBG= 0.0398995
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6365 +/- 4.84628
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=8618.07 and stop= 8811.14 so gap is 193.063, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (8618.07 - 8811.14), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4998.56 - 5400.97), exposure 270.782
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.483464 bg counts (22), with cf=1.19824 and errBG= 0.103075
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7907 +/- 4.942
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 13
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8811.14 - 9086.94), exposure 275.805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.271451 bg counts (18), with cf=1.26085 and errBG= 0.0639815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.5704 +/- 4.8839
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=8811.14 and stop= 9086.94 so gap is 275.805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (8811.14 - 9086.94), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8618.07 - 8811.14), exposure 193.063
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.105564 bg counts (7), with cf=1.25124 and errBG= 0.0398995
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6365 +/- 4.84628
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 14
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9086.94 - 9297.56), exposure 210.615
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.120645 bg counts (8), with cf=1.27128 and errBG= 0.0426543
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9158 +/- 4.92395
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=9086.94 and stop= 9297.56 so gap is 210.615, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (9086.94 - 9297.56), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8811.14 - 9086.94), exposure 275.805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.271451 bg counts (18), with cf=1.26085 and errBG= 0.0639815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.5704 +/- 4.8839
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 15
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9297.56 - 9648.58), exposure 351.024
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.180967 bg counts (12), with cf=1.27094 and errBG= 0.0522407
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8342 +/- 4.92279
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=9297.56 and stop= 9648.58 so gap is 351.024, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (9297.56 - 9648.58), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9086.94 - 9297.56), exposure 210.615
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.120645 bg counts (8), with cf=1.27128 and errBG= 0.0426543
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9158 +/- 4.92395
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 16
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9648.58 - 9879.25), exposure 230.673
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.120645 bg counts (8), with cf=1.26356 and errBG= 0.0426543
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.801 +/- 4.89406
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=9648.58 and stop= 9879.25 so gap is 230.673, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (9648.58 - 9879.25), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9297.56 - 9648.58), exposure 351.024
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.180967 bg counts (12), with cf=1.27094 and errBG= 0.0522407
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8342 +/- 4.92279
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 17
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (8618.07 - 10109.9), exposure 1491.85, 15 soft counts and 72 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0124896, 0.0604464 and 4.83972. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=9879.25 and stop= 10109.9 so gap is 230.672, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (8618.07 - 10109.9) = 8618.07- 10109.9
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9879.25 - 10155.1), exposure 275.804
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0754029 bg counts (5), with cf=1.26282 and errBG= 0.0337212
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8471 +/- 4.89106
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=9879.25 and stop= 10155.1 so gap is 275.804, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (9879.25 - 10155.1), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9648.58 - 9879.25), exposure 230.673
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.120645 bg counts (8), with cf=1.26356 and errBG= 0.0426543
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.801 +/- 4.89406
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 18
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10155.1 - 10415.8), exposure 260.76
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.150806 bg counts (10), with cf=1.27095 and errBG= 0.047689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8726 +/- 4.92274
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=10155.1 and stop= 10415.8 so gap is 260.76, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10155.1 - 10415.8), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (9879.25 - 10155.1), exposure 275.804
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0754029 bg counts (5), with cf=1.26282 and errBG= 0.0337212
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8471 +/- 4.89106
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 19
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10415.8 - 10734.2), exposure 318.428
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.211128 bg counts (14), with cf=1.26771 and errBG= 0.0564264
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.748 +/- 4.91035
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=10415.8 and stop= 10734.2 so gap is 318.428, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10415.8 - 10734.2), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10155.1 - 10415.8), exposure 260.76
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.150806 bg counts (10), with cf=1.27095 and errBG= 0.047689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8726 +/- 4.92274
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 6.84587
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 12.642
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 18.4545
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 24.2473
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 30.0301
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 35.8341
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 41.6269
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 48.5021
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 54.2959
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 60.0889
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 66.9821
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 75.9774
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 83.9086
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 91.8428
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 97.6641
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 103.479
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 110.344
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 39, last was 21 so increasing dead to 123.616
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 41, last was 39 so increasing dead to 133.698
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 41, last was 39 so increasing dead to 139.614
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 146.633
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 157.829
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 165.913
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 172.198
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 180.991
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 47, last was 41 so increasing dead to 188.032
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10734.2 - 11179.8), exposure 228.154
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 1.07072 bg counts (71), with cf=1.26402 and errBG= 0.127071
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =13.8149 +/- 4.38166
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (10109.9 - 11179.8), exposure 852.474, 10 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0132234, 0.0515675 and 3.89971. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=10734.2 and stop= 11179.8 so gap is 445.557, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 1 (11179.8) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=445.557 whereas forward=3216.43
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10415.8 - 11179.8), exposure 546.583
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 1.28185 bg counts (85), with cf=1.26607 and errBG= 0.139036
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.5611 +/- 6.58106
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 1 (11179.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (8618.07 - 11179.8), exposure 2344.33, 25 soft counts and 107 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0127562, 0.0572179 and 4.48551. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10415.8 - 11179.8), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 14396.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 50
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (8618.07 - 11179.8) = 8618.07- 11179.8
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 14396.2 - 16953.4


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 52, last was 50 so increasing dead to 5.85102
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 52, last was 50 so increasing dead to 11.6711
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 56, last was 52 so increasing dead to 17.5212
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 56, last was 52 so increasing dead to 23.3526
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 56, last was 52 so increasing dead to 29.2063
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 56, last was 52 so increasing dead to 35.0603
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 58, last was 56 so increasing dead to 41.9168
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 58, last was 56 so increasing dead to 49.8424
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 61, last was 58 so increasing dead to 58.8462
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 61, last was 58 so increasing dead to 64.6571
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 61, last was 58 so increasing dead to 74.7154
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 64, last was 61 so increasing dead to 86.9153
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 64, last was 61 so increasing dead to 92.7521
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 64, last was 61 so increasing dead to 104.945
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 110.755
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 116.637
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 126.729
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 133.587
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 139.416
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 145.232
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 151.059
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 156.878
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 162.717
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 74, last was 64 so increasing dead to 168.533
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 79, last was 74 so increasing dead to 175.392
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 79, last was 74 so increasing dead to 182.248
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 79, last was 74 so increasing dead to 189.124
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 79, last was 74 so increasing dead to 197.064
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 79, last was 74 so increasing dead to 202.887
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 82, last was 79 so increasing dead to 211.878
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 82, last was 79 so increasing dead to 219.8
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 82, last was 79 so increasing dead to 230.927
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 83, last was 82 so increasing dead to 236.746
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 86, last was 83 so increasing dead to 245.756
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 86, last was 83 so increasing dead to 256.897
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 86, last was 83 so increasing dead to 262.708
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 89, last was 86 so increasing dead to 269.56
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 89, last was 86 so increasing dead to 281.757
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 89, last was 86 so increasing dead to 287.561
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 92, last was 89 so increasing dead to 294.429
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 92, last was 89 so increasing dead to 305.553
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 92, last was 89 so increasing dead to 312.406
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 96, last was 92 so increasing dead to 319.272
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 96, last was 92 so increasing dead to 330.396
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 96, last was 92 so increasing dead to 336.21
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 96, last was 92 so increasing dead to 342.032
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (14396.2 - 14979), exposure 240.701
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121047 bg counts (14), with cf=1.27785 and errBG= 0.0323512
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0131 +/- 4.94928
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=14396.2 and stop= 14979 so gap is 582.733, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (14396.2 - 14979), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10415.8 - 11179.8), exposure 546.583
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 1.28185 bg counts (85), with cf=1.26607 and errBG= 0.139036
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.5611 +/- 6.58106
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 21
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 96
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 98, last was 96 so increasing dead to 7.93407
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 98, last was 96 so increasing dead to 13.757
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 101, last was 98 so increasing dead to 20.6222
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 101, last was 98 so increasing dead to 26.443
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 101, last was 98 so increasing dead to 33.3118
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 104, last was 101 so increasing dead to 40.178
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 104, last was 101 so increasing dead to 47.0431
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 104, last was 101 so increasing dead to 54.9783
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 107, last was 104 so increasing dead to 60.792
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 107, last was 104 so increasing dead to 66.5917
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 107, last was 104 so increasing dead to 80.9325
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 92.0699
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 97.8713
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 105.822
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 112.689
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 125.978
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 132.847
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 138.644
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 148.716
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 157.718
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 117, last was 107 so increasing dead to 166.733
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 118, last was 117 so increasing dead to 172.535
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 121, last was 118 so increasing dead to 181.542
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 121, last was 118 so increasing dead to 188.41
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 121, last was 118 so increasing dead to 205.951
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 123, last was 121 so increasing dead to 214.953
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 123, last was 121 so increasing dead to 222.884
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 128, last was 123 so increasing dead to 232.955
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 128, last was 123 so increasing dead to 239.82
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 128, last was 123 so increasing dead to 249.888
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 128, last was 123 so increasing dead to 258.89
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 128, last was 123 so increasing dead to 270.036
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 130, last was 128 so increasing dead to 276.975
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 130, last was 128 so increasing dead to 284.903
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 131, last was 130 so increasing dead to 292.828
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 133, last was 131 so increasing dead to 298.619
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 133, last was 131 so increasing dead to 308.679
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 134, last was 133 so increasing dead to 315.539
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (14979 - 15605.4), exposure 310.905
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.103755 bg counts (12), with cf=1.27782 and errBG= 0.0299514
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0348 +/- 4.94914
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=14979 and stop= 15605.4 so gap is 626.444, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (14979 - 15605.4), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (14396.2 - 14979), exposure 240.701
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121047 bg counts (14), with cf=1.27785 and errBG= 0.0323512
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0131 +/- 4.94928
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 22
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 134
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 135, last was 134 so increasing dead to 5.7781
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 138, last was 135 so increasing dead to 14.7838
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 138, last was 135 so increasing dead to 29.0949
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 138, last was 135 so increasing dead to 35.9523
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 139, last was 138 so increasing dead to 42.7895
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (15605.4 - 15883.9), exposure 235.687
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.0345849 bg counts (4), with cf=1.27809 and errBG= 0.0172924
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.4053 +/- 5.11242
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=15605.4 and stop= 15883.9 so gap is 278.476, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (15605.4 - 15883.9), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (14979 - 15605.4), exposure 310.905
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.103755 bg counts (12), with cf=1.27782 and errBG= 0.0299514
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0348 +/- 4.94914
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 23
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 139
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (14396.2 - 16164.7), exposure 1068.11, 15 soft counts and 39 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0177931, 0.0464506 and 2.61059. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=15883.9 and stop= 16164.7 so gap is 280.818, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (14396.2 - 16164.7) = 14396.2- 16164.7
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (15883.9 - 16307.6), exposure 423.735
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121047 bg counts (14), with cf=1.28061 and errBG= 0.0323512
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0542 +/- 4.95996
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=15883.9 and stop= 16307.6 so gap is 423.735, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (15883.9 - 16307.6), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (15605.4 - 15883.9), exposure 235.687
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.0345849 bg counts (4), with cf=1.27809 and errBG= 0.0172924
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.4053 +/- 5.11242
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 24
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 139
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16307.6 - 16953.4), exposure 493.937
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.181571 bg counts (21), with cf=1.28342 and errBG= 0.039622
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0182 +/- 4.97091
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16164.7 - 16953.4), exposure 636.853, 4 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.007696, 0.0361241 and 4.69388. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16307.6 and stop= 16953.4 so gap is 645.734, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 2 (16953.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (14396.2 - 16953.4), exposure 1704.96, 19 soft counts and 57 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0140215, 0.0425933 and 3.03771. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16307.6 - 16953.4), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (15883.9 - 16307.6), exposure 423.735
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121047 bg counts (14), with cf=1.28061 and errBG= 0.0323512
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0542 +/- 4.95996
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 25
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 20188.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 157
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (14396.2 - 16953.4) = 14396.2- 16953.4
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 20188.4 - 22741.9


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 161, last was 157 so increasing dead to 5.92152
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 161, last was 157 so increasing dead to 11.8298
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 161, last was 157 so increasing dead to 17.7278
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 161, last was 157 so increasing dead to 24.7055
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 35.8548
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 41.7812
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 47.6952
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 55.6579
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 61.5931
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 67.5256
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 77.6355
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 86.7298
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 92.6352
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 98.5478
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 105.547
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 111.457
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 117.383
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 124.34
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 130.251
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 137.216
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 145.161
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 153.109
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 162.129
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 172.23
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 179.164
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 185.088
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 191.003
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 196.915
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 186, last was 161 so increasing dead to 202.848
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 189, last was 186 so increasing dead to 209.761
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 189, last was 186 so increasing dead to 218.775
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 189, last was 186 so increasing dead to 225.693
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 193, last was 189 so increasing dead to 235.773
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 193, last was 189 so increasing dead to 243.715
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 193, last was 189 so increasing dead to 250.608
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 193, last was 189 so increasing dead to 256.517
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 197, last was 193 so increasing dead to 263.41
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 197, last was 193 so increasing dead to 273.5
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 197, last was 193 so increasing dead to 280.387
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 197, last was 193 so increasing dead to 289.388
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 295.294
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 305.364
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 315.439
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 322.336
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 328.218
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 337.215
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 343.077
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 353.141
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 359.032
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 374.463
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 384.522
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 392.457
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 399.334
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 211, last was 197 so increasing dead to 406.197
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 214, last was 211 so increasing dead to 418.417
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 214, last was 211 so increasing dead to 426.358
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 214, last was 211 so increasing dead to 442.83
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 217, last was 214 so increasing dead to 448.679
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 217, last was 214 so increasing dead to 457.689
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 217, last was 214 so increasing dead to 465.624
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 473.547
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 479.393
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 485.223
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 493.146
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 500.01
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 514.371
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 522.301
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 528.14
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 226, last was 217 so increasing dead to 541.399
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 227, last was 226 so increasing dead to 552.525
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 230, last was 227 so increasing dead to 561.515
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 230, last was 227 so increasing dead to 571.595
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 230, last was 227 so increasing dead to 577.404
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 234, last was 230 so increasing dead to 585.331
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 234, last was 230 so increasing dead to 592.187
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 234, last was 230 so increasing dead to 598.026
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 234, last was 230 so increasing dead to 603.848
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 610.703
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 616.539
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 622.365
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 631.354
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 637.179
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 643.008
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 649.859
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 658.846
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 677.445
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 686.455
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 694.425
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 702.348
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 708.138
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 716.084
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 724.022
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 729.845
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 735.653
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 750.014
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 756.883
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 764.822
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 797.307
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 810.583
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 822.788
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 834.994
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 848.267
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 856.222
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 261, last was 234 so increasing dead to 878.141
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (20188.4 - 21507.8), exposure 441.285
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.752119 bg counts (87), with cf=1.28113 and errBG= 0.0806356
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5345 +/- 5.12555
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=20188.4 and stop= 21507.8 so gap is 1319.43, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (20188.4 - 21507.8), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16307.6 - 16953.4), exposure 493.937
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.181571 bg counts (21), with cf=1.28342 and errBG= 0.039622
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0182 +/- 4.97091
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 26
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 261
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 266, last was 261 so increasing dead to 5.81726
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 266, last was 261 so increasing dead to 14.8307
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 266, last was 261 so increasing dead to 21.7205
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 266, last was 261 so increasing dead to 29.6562
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 266, last was 261 so increasing dead to 47.1972
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 55.1511
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 66.2883
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 79.5588
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 89.6259
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 99.6927
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 272, last was 266 so increasing dead to 106.557
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 273, last was 272 so increasing dead to 127.3
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 278, last was 273 so increasing dead to 141.637
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 278, last was 273 so increasing dead to 171.986
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 278, last was 273 so increasing dead to 179.917
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 278, last was 273 so increasing dead to 185.715
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 278, last was 273 so increasing dead to 201.119
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 280, last was 278 so increasing dead to 210.132
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 280, last was 278 so increasing dead to 239.419
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 281, last was 280 so increasing dead to 249.496
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 284, last was 281 so increasing dead to 255.287
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 284, last was 281 so increasing dead to 268.55
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 284, last was 281 so increasing dead to 274.34
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 286, last was 284 so increasing dead to 284.4
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 286, last was 284 so increasing dead to 299.809
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 287, last was 286 so increasing dead to 305.579
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 288, last was 287 so increasing dead to 312.438
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 289, last was 288 so increasing dead to 318.23
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (21507.8 - 22184.6), exposure 358.544
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.155611 bg counts (18), with cf=1.28144 and errBG= 0.0366778
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0222 +/- 4.96322
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=21507.8 and stop= 22184.6 so gap is 676.774, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (21507.8 - 22184.6), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (20188.4 - 21507.8), exposure 441.285
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.752119 bg counts (87), with cf=1.28113 and errBG= 0.0806356
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5345 +/- 5.12555
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 27
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 289
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22184.6 - 22741.9), exposure 478.894
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.475477 bg counts (55), with cf=1.28116 and errBG= 0.0641133
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.07777 +/- 3.13925
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20188.4 - 22741.9), exposure 1278.72, 4 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00304575, 0.0326419 and 10.7172. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22184.6 and stop= 22741.9 so gap is 557.332, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 3 (22741.9) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=557.332 whereas forward=3223.55
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (21507.8 - 22741.9), exposure 837.438
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.631088 bg counts (73), with cf=1.28136 and errBG= 0.0738633
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.0999 +/- 5.87269
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 3 (22741.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (21507.8 - 22741.9), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 25965.5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 299
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 25965.5 - 28521.4


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 7.00258
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 13.9983
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 19.9748
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 26.9455
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 41.2942
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 305, last was 299 so increasing dead to 49.3478
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 55.2599
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 61.1666
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 68.1516
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 74.0773
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 79.9958
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 311, last was 305 so increasing dead to 85.9168
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 93.9401
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 102.971
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 109.968
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 115.877
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 122.894
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 317, last was 311 so increasing dead to 135.117
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 321, last was 317 so increasing dead to 142.113
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 321, last was 317 so increasing dead to 148.007
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 321, last was 317 so increasing dead to 153.937
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 321, last was 317 so increasing dead to 159.851
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 323, last was 321 so increasing dead to 167.835
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 323, last was 321 so increasing dead to 176.852
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 325, last was 323 so increasing dead to 183.834
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 325, last was 323 so increasing dead to 190.807
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 328, last was 325 so increasing dead to 198.789
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 328, last was 325 so increasing dead to 204.707
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 328, last was 325 so increasing dead to 212.695
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 218.608
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 224.516
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 230.45
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 236.36
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 245.373
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 254.403
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 263.412
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 272.442
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 283.607
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 292.616
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 300.559
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 307.5
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 315.439
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 321.344
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 327.252
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 339.463
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 352.752
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 358.668
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 366.606
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 373.507
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 379.418
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 388.42
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 396.359
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 408.563
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 414.447
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 421.346
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 429.293
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 435.205
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 441.112
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 447.004
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 452.865
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 460.795
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 466.663
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 472.537
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 479.415
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 488.414
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 495.272
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 501.147
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 367, last was 328 so increasing dead to 509.075
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 514.949
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 522.875
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 538.272
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 544.134
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 552.066
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 373, last was 367 so increasing dead to 561.057
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 377, last was 373 so increasing dead to 569.002
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 377, last was 373 so increasing dead to 579.074
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 377, last was 373 so increasing dead to 584.922
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 377, last was 373 so increasing dead to 590.763
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 600.822
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 606.654
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 614.598
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 621.455
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 628.316
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 634.129
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 641
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 652.154
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 657.98
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 663.819
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 669.643
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 675.452
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 682.309
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 391, last was 377 so increasing dead to 688.12
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 696.062
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 708.252
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 717.243
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 726.234
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 735.223
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 741.032
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 750.043
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 756.898
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 763.771
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 401, last was 391 so increasing dead to 769.595
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 784.987
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 797.179
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 809.373
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 815.189
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 821.009
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 826.844
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 832.686
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 839.56
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 847.494
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 411, last was 401 so increasing dead to 853.305
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 413, last was 411 so increasing dead to 868.716
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 413, last was 411 so increasing dead to 885.197
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 414, last was 413 so increasing dead to 891.032
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 901.104
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 909.035
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 921.242
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 928.107
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 942.445
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 420, last was 414 so increasing dead to 948.245
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 955.112
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 961.975
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 972.043
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 978.907
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 987.906
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 995.846
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1004.84
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1018.12
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1027.12
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1036.11
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1063.28
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1073.35
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1098.38
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 434, last was 420 so increasing dead to 1108.45
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 436, last was 434 so increasing dead to 1119.59
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 436, last was 434 so increasing dead to 1131.79
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 437, last was 436 so increasing dead to 1141.86
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1147.66
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1154.53
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1167.8
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1174.66
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1191.15
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1200.15
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1208.07
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 445, last was 437 so increasing dead to 1214.94
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (25965.5 - 27882.5), exposure 702.044
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0870268 bg counts (120), with cf=3.77285 and errBG= 0.00794443
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =75.1287 +/- 16.8727
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25965.5 and stop= 27882.5 so gap is 1916.98, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (25965.5 - 27882.5), with lastBin= 0x19d4fe0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (21507.8 - 22741.9), exposure 837.438
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.631088 bg counts (73), with cf=1.28136 and errBG= 0.0738633
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.0999 +/- 5.87269
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 28
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 445
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 6.8595
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 21.191
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 28.0705
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 34.9269
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 40.7462
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 52.9426
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 61.9346
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 76.264
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 83.1198
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 94.253
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 102.177
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 116.505
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 124.431
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 133.424
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 141.351
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 461, last was 445 so increasing dead to 147.151
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 152.939
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 162.982
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 169.836
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 175.649
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 188.893
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 196.815
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 203.674
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 210.54
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 217.397
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 225.308
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 231.118
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 236.989
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 251.317
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 259.26
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 267.19
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 273.09
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 478, last was 461 so increasing dead to 281.024
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (27882.5 - 28521.4), exposure 330.964
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.0415542 bg counts (38), with cf=1.9983 and errBG= 0.00674098
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =3.91357 +/- 2.82606
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20188.4 - 28521.4), exposure 2311.73, 11 soft counts and 48 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0173555, 0.0353378 and 2.03612. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=27882.5 and stop= 28521.4 so gap is 638.924, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 4 (28521.4) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=638.924 whereas forward=3247.23
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (25965.5 - 28521.4), exposure 1033.01
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.128581 bg counts (158), with cf=3.61153 and errBG= 0.0102294
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =78.9893 +/- 16.9396
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 4 (28521.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (25965.5 - 28521.4), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 31768.6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 483
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 31768.6 - 33580.4


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 11.1456
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 21.2015
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 29.1476
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 36.0345
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 41.9016
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 47.7565
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 54.6118
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 60.4934
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 66.3446
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 493, last was 483 so increasing dead to 72.1859
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 78.054
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 87.0649
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 92.9142
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 99.7721
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 105.598
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 113.542
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 119.386
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 125.237
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 132.102
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 137.954
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 145.878
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 151.702
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 167.099
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 173.954
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 508, last was 493 so increasing dead to 179.786
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 185.625
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 196.749
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 202.591
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 208.403
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 216.346
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 223.202
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 230.06
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 237.985
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 244.838
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 250.652
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 256.491
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 262.302
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 269.173
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 275.016
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 281.868
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 289.787
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 295.592
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 302.446
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 309.325
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 316.213
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 327.336
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 334.204
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 531, last was 508 so increasing dead to 340.022
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 346.892
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 359.084
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 364.908
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 372.839
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 382.91
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 388.753
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 538, last was 531 so increasing dead to 398.823
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 539, last was 538 so increasing dead to 405.691
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 540, last was 539 so increasing dead to 416.824
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 422.647
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 428.446
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 435.317
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 445.382
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 452.264
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 462.338
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 469.219
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 484.625
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 491.49
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 497.29
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 506.287
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 512.085
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 518.961
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 525.825
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 536.961
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 550.233
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 556.032
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 566.098
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 574.033
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 586.248
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 593.114
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 599.984
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 606.865
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 613.733
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 621.657
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 632.792
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 567, last was 540 so increasing dead to 638.587
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 570, last was 567 so increasing dead to 644.378
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 570, last was 567 so increasing dead to 651.234
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 570, last was 567 so increasing dead to 658.112
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 574, last was 570 so increasing dead to 666.057
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 574, last was 570 so increasing dead to 671.865
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 574, last was 570 so increasing dead to 678.72
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 574, last was 570 so increasing dead to 694.119
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 577, last was 574 so increasing dead to 700.957
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 577, last was 574 so increasing dead to 706.747
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 577, last was 574 so increasing dead to 713.582
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (31768.6 - 33580.4), exposure 1098.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.52243 bg counts (61), with cf=1.2858 and errBG= 0.0668904
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6153 +/- 4.98063
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20188.4 - 33580.4), exposure 3409.93, 11 soft counts and 63 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0115734, 0.0294564 and 2.54518. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=31768.6 and stop= 33580.4 so gap is 1811.78, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 5 (33580.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (31768.6 - 33580.4), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (25965.5 - 28521.4), exposure 1033.01
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.128581 bg counts (158), with cf=3.61153 and errBG= 0.0102294
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =78.9893 +/- 16.9396
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 29
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 37590.1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 578
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 37590.1 - 40100.8


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 580, last was 578 so increasing dead to 12.2028
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 580, last was 578 so increasing dead to 24.4059
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 581, last was 580 so increasing dead to 33.4049
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20188.4 - 38300.5), exposure 4086.9, 15 soft counts and 72 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0111281, 0.027392 and 2.46151. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=37590.1 and stop= 38300.5 so gap is 710.379, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (20188.4 - 38300.5) = 20188.4- 38300.5
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (37590.1 - 38473.5), exposure 849.978
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.316088 bg counts (37), with cf=1.30309 and errBG= 0.0519646
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1345 +/- 5.04731
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=37590.1 and stop= 38473.5 so gap is 883.383, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (37590.1 - 38473.5), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (31768.6 - 33580.4), exposure 1098.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.52243 bg counts (61), with cf=1.2858 and errBG= 0.0668904
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6153 +/- 4.98063
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 30
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 581
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (38473.5 - 39438.8), exposure 965.313
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.418603 bg counts (49), with cf=1.29453 and errBG= 0.0598004
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8761 +/- 5.01429
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=38473.5 and stop= 39438.8 so gap is 965.313, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (38473.5 - 39438.8), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (37590.1 - 38473.5), exposure 849.978
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.316088 bg counts (37), with cf=1.30309 and errBG= 0.0519646
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1345 +/- 5.04731
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 31
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 581
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (39438.8 - 40100.8), exposure 473.874
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.153773 bg counts (18), with cf=1.31044 and errBG= 0.0362445
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.41937 +/- 1.85385
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (38300.5 - 40100.8), exposure 1612.19, 2 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0014103, 0.0133 and 9.43063. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=39438.8 and stop= 40100.8 so gap is 662.037, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 6 (40100.8) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=662.037 whereas forward=3248
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (38473.5 - 40100.8), exposure 1439.19
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.572376 bg counts (67), with cf=1.2964 and errBG= 0.0699268
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.2968 +/- 5.34597
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 6 (40100.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20188.4 - 40100.8), exposure 5699.09, 17 soft counts and 89 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0083489, 0.0233977 and 2.80249. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (38473.5 - 40100.8), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 43348.8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 602
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (20188.4 - 40100.8) = 20188.4- 40100.8
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 43348.8 - 45875.7


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (43348.8 - 44271.5), exposure 922.69
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.265729 bg counts (31), with cf=1.30372 and errBG= 0.0477264
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.2094 +/- 5.04969
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=43348.8 and stop= 44271.5 so gap is 922.69, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (43348.8 - 44271.5), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (38473.5 - 40100.8), exposure 1439.19
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.572376 bg counts (67), with cf=1.2964 and errBG= 0.0699268
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.2968 +/- 5.34597
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 32
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 602
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (44271.5 - 45061.3), exposure 789.801
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.317161 bg counts (37), with cf=1.29902 and errBG= 0.0521409
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0733 +/- 5.03153
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=44271.5 and stop= 45061.3 so gap is 789.801, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (44271.5 - 45061.3), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (43348.8 - 44271.5), exposure 922.69
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.265729 bg counts (31), with cf=1.30372 and errBG= 0.0477264
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.2094 +/- 5.04969
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 33
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 602
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (45061.3 - 45875.7), exposure 769.736
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.274301 bg counts (32), with cf=1.298 and errBG= 0.0484901
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.2199 +/- 4.49683
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (43348.8 - 45875.7), exposure 2482.23, 10 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00508895, 0.0164652 and 3.23547. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=45061.3 and stop= 45875.7 so gap is 814.355, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 7 (45875.7) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=814.355 whereas forward=3225.57
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (44271.5 - 45875.7), exposure 1559.54
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.591462 bg counts (69), with cf=1.29856 and errBG= 0.0712037
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.2932 +/- 6.74817
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 7 (45875.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (44271.5 - 45875.7), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 49101.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 609
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 49101.2 - 51664


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (49101.2 - 50502.8), exposure 1401.58
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.245829 bg counts (45), with cf=1.55887 and errBG= 0.0366461
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.9999 +/- 6.03776
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=49101.2 and stop= 50502.8 so gap is 1401.58, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (49101.2 - 50502.8), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (44271.5 - 45875.7), exposure 1559.54
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.591462 bg counts (69), with cf=1.29856 and errBG= 0.0712037
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.2932 +/- 6.74817
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 34
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 609
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (50502.8 - 51664), exposure 1148.34
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.404252 bg counts (74), with cf=1.53618 and errBG= 0.0469934
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.59608 +/- 3.76355
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (43348.8 - 51664), exposure 5032.15, 11 soft counts and 52 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00276098, 0.0141601 and 5.12864. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=50502.8 and stop= 51664 so gap is 1161.18, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 8 (51664) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=1161.18 whereas forward=3222.22
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (49101.2 - 51664), exposure 2549.92
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.650082 bg counts (119), with cf=1.55239 and errBG= 0.0595929
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.591 +/- 7.11454
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 8 (51664) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (49101.2 - 51664), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 54886.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 612
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 54886.2 - 57230.5


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (54886.2 - 56385.6), exposure 1499.37
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.524526 bg counts (61), with cf=1.28603 and errBG= 0.0671587
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6159 +/- 4.98153
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=54886.2 and stop= 56385.6 so gap is 1499.37, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (54886.2 - 56385.6), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (49101.2 - 51664), exposure 2549.92
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.650082 bg counts (119), with cf=1.55239 and errBG= 0.0595929
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.591 +/- 7.11454
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 35
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 612
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (43348.8 - 57137.8), exposure 7283.71, 15 soft counts and 72 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00256318, 0.0132232 and 5.15888. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=56385.6 and stop= 57137.8 so gap is 752.191, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (43348.8 - 57137.8) = 43348.8- 57137.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (56385.6 - 57230.5), exposure 844.956
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.292359 bg counts (34), with cf=1.28599 and errBG= 0.0501392
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.4839 +/- 4.06716
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (57137.8 - 57230.5), exposure 92.7648, 0 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -0.000185389, 0.0137421 and -74.1258. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=56385.6 and stop= 57230.5 so gap is 844.956, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 9 (57230.5) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=844.956 whereas forward=16353.9
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (54886.2 - 57230.5), exposure 2344.33
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.816886 bg counts (95), with cf=1.28601 and errBG= 0.0838107
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.0998 +/- 6.43097
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 9 (57230.5) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (43348.8 - 57230.5), exposure 7376.48, 15 soft counts and 73 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00252788, 0.0132298 and 5.23356. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (54886.2 - 57230.5), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 73584.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 613
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (43348.8 - 57230.5) = 43348.8- 57230.5
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 73584.4 - 74630


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (73584.4 - 74630), exposure 1045.54
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.410387 bg counts (48), with cf=1.31425 and errBG= 0.0592343
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.2317 +/- 4.55337
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 74630), exposure 1045.54, 2 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00232112, 0.0122436 and 5.27488. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73584.4 and stop= 74630 so gap is 1045.54, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 10 (74630) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=17399.4 whereas forward=4719.83
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 10 (74630) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 79349.8 - 80390.3


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (73584.4 - 79530.3), exposure 1226.07
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.482068 bg counts (61), with cf=1.3256 and errBG= 0.0617225
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.245 +/- 5.13469
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73584.4 and stop= 79530.3 so gap is 5945.9, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (73584.4 - 79530.3), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (54886.2 - 57230.5), exposure 2344.33
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.816886 bg counts (95), with cf=1.28601 and errBG= 0.0838107
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.0998 +/- 6.43097
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 36
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 614
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (79530.3 - 80390.3), exposure 860.004
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 3 counts and 0.237098 bg counts (43), with cf=1.37091 and errBG= 0.0361571
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =3.7877 +/- 2.37501
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 80390.3), exposure 2086.07, 3 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00175155, 0.00928983 and 5.30379. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79530.3 and stop= 80390.3 so gap is 860.004, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 11 (80390.3) and the bin is not full 3 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=860.004 whereas forward=4776.51
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (73584.4 - 80390.3), exposure 2086.07
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 18 counts and 0.719166 bg counts (104), with cf=1.33315 and errBG= 0.07052
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.038 +/- 5.65687
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 11 (80390.3) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (73584.4 - 80390.3), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 85166.8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 615
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 85166.8 - 86209.9


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85166.8 - 86209.9), exposure 1043.04
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.289495 bg counts (34), with cf=1.33327 and errBG= 0.0496479
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.9467 +/- 4.21668
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 86209.9), exposure 3129.11, 5 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00200355, 0.00949456 and 4.73887. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=85166.8 and stop= 86209.9 so gap is 1043.04, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 12 (86209.9) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5819.55 whereas forward=4652.96
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 12 (86209.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 90862.8 - 91910.9


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85166.8 - 91737.9), exposure 1918.09
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.5297 bg counts (78), with cf=1.36227 and errBG= 0.0599767
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7124 +/- 5.27667
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=85166.8 and stop= 91737.9 so gap is 6571.04, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (85166.8 - 91737.9), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (73584.4 - 80390.3), exposure 2086.07
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 18 counts and 0.719166 bg counts (104), with cf=1.33315 and errBG= 0.07052
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.038 +/- 5.65687
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 37
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 616
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (91737.9 - 91910.9), exposure 173.002
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0655106 bg counts (12), with cf=1.43688 and errBG= 0.0189113
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.34275 +/- 1.43714
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 91910.9), exposure 4177.16, 8 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00247516, 0.00807948 and 3.26423. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91737.9 and stop= 91910.9 so gap is 173.002, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 13 (91910.9) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=173.002 whereas forward=4777.49
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85166.8 - 91910.9), exposure 2091.09
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.595211 bg counts (90), with cf=1.36693 and errBG= 0.0627407
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.0573 +/- 5.4684
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 13 (91910.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (85166.8 - 91910.9), with lastBin= 0 and workMinC was 8
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 96688.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 617
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 96688.4 - 97728.9


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (96688.4 - 97728.9), exposure 1040.53
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.284802 bg counts (52), with cf=1.48201 and errBG= 0.0394949
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.46996 +/- 3.63063
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 97728.9), exposure 5217.69, 8 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00195123, 0.00812375 and 4.1634. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=96688.4 and stop= 97728.9 so gap is 1040.53, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 14 (97728.9) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5818.02 whereas forward=4713.92
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 14 (97728.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 102443 - 103489


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 623, last was 618 so increasing dead to 7.92644
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 623, last was 618 so increasing dead to 16.9171
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 623, last was 618 so increasing dead to 23.776
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 623, last was 618 so increasing dead to 39.1545
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 623, last was 618 so increasing dead to 46.0255
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (96688.4 - 103489), exposure 2040.94
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.454475 bg counts (105), with cf=1.63023 and errBG= 0.0443522
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.5614 +/- 5.15576
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 103489), exposure 6218.1, 8 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00161889, 0.00798004 and 4.92934. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=96688.4 and stop= 103489 so gap is 6800.88, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 15 (103489) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 16 counts, because gotBinThisOrb=0 and gapBack=11578.4 whereas forward=16296.1
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85166.8 - 103489), exposure 4132.03
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 1.04969 bg counts (195), with cf=1.4682 and errBG= 0.0751696
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.6321 +/- 7.4872
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 15 (103489) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (85166.8 - 103489), with lastBin= 0 and workMinC was 8
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 119785
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 624
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 119785 - 120831


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (119785 - 120831), exposure 1045.54
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.182098 bg counts (57), with cf=1.47348 and errBG= 0.0241195
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.09907 +/- 3.29499
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 120831), exposure 7263.65, 9 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00157362, 0.00762075 and 4.84283. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=119785 and stop= 120831 so gap is 1045.54, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 16 (120831) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=17341.7 whereas forward=4713.19
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 16 (120831) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 125544 - 126590


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (119785 - 126590), exposure 2066.02
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 0.361233 bg counts (113), with cf=1.48199 and errBG= 0.0339819
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.8025 +/- 4.44625
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 126590), exposure 8284.12, 10 soft counts and 43 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0015461, 0.00720412 and 4.65955. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=119785 and stop= 126590 so gap is 6804.28, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 17 (126590) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=23100.4 whereas forward=4714.55
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 17 (126590) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 131304 - 132350


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (119785 - 132350), exposure 3111.56
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.527565 bg counts (165), with cf=1.51657 and errBG= 0.0410708
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.3988 +/- 5.25393
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 132350), exposure 9329.66, 10 soft counts and 46 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00136181, 0.00690173 and 5.06804. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=119785 and stop= 132350 so gap is 12564.4, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 18 (132350) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=28860.5 whereas forward=4656.44
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 18 (132350) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 137006 - 138049


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (119785 - 138049), exposure 4154.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.6972 bg counts (218), with cf=1.51476 and errBG= 0.0472203
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.6653 +/- 5.86707
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 138049), exposure 10372.7, 11 soft counts and 48 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00135725, 0.00648685 and 4.7794. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=119785 and stop= 138049 so gap is 18263.9, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 19 (138049) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (119785 - 138049), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85166.8 - 103489), exposure 4132.03
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 1.04969 bg counts (195), with cf=1.4682 and errBG= 0.0751696
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.6321 +/- 7.4872
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 38
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 142885
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 629
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 142885 - 143931


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (142885 - 143931), exposure 1045.54
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.241272 bg counts (45), with cf=1.45612 and errBG= 0.0359667
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.2976 +/- 4.11885
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 143931), exposure 11418.2, 14 soft counts and 53 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00160346, 0.00651122 and 4.06073. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=142885 and stop= 143931 so gap is 1045.54, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 20 (143931) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5881.59 whereas forward=4832.34
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 20 (143931) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 148763 - 149809


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 148851), exposure 11506, 15 soft counts and 53 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00170577, 0.00646017 and 3.78724. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=142885 and stop= 148851 so gap is 5965.64, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (73584.4 - 148851) = 73584.4- 148851
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (142885 - 149809), exposure 2091.09
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.572084 bg counts (105), with cf=1.41015 and errBG= 0.0558297
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.5252 +/- 5.08497
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (148851 - 149809), exposure 957.789, 2 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00263714, 0.00252268 and 0.956596. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=142885 and stop= 149809 so gap is 6923.43, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 21 (149809) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=11759.5 whereas forward=4595.4
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 21 (149809) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (73584.4 - 149809), exposure 12463.8, 17 soft counts and 55 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00177752, 0.00615648 and 3.46352. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (73584.4 - 149809) = 73584.4- 149809
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 154404 - 155570


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (142885 - 155570), exposure 3256.98
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 0.758098 bg counts (163), with cf=1.42321 and errBG= 0.0593788
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.846 +/- 5.32584
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 155570), exposure 1165.89, 0 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -5.77666e-05, 0.00120421 and -20.8461. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=142885 and stop= 155570 so gap is 12684.7, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 22 (155570) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=17520.8 whereas forward=10534.5
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 22 (155570) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 166104 - 167270


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (142885 - 167270), exposure 4422.88
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.961891 bg counts (226), with cf=1.42476 and errBG= 0.063984
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.0009 +/- 5.51883
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 167270), exposure 2331.79, 0 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -6.35649e-05, 0.00114604 and -18.0295. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=142885 and stop= 167270 so gap is 24385.1, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 23 (167270) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (142885 - 167270), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (119785 - 138049), exposure 4154.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.6972 bg counts (218), with cf=1.51476 and errBG= 0.0472203
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.6653 +/- 5.86707
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 39
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 170964
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 633
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 170964 - 172610


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 640, last was 633 so increasing dead to 7.92233
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 640, last was 633 so increasing dead to 13.7192
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 640, last was 633 so increasing dead to 20.5796
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 640, last was 633 so increasing dead to 26.3676
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 640, last was 633 so increasing dead to 37.4729
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 640, last was 633 so increasing dead to 44.3341
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 640, last was 633 so increasing dead to 54.375
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (170964 - 172610), exposure 1592.14
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.407463 bg counts (76), with cf=1.44992 and errBG= 0.0467392
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.0085 +/- 4.10154
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 172610), exposure 3923.92, 4 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00136588, 0.00206725 and 1.51349. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=170964 and stop= 172610 so gap is 1646.51, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 24 (172610) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5339.68 whereas forward=4114.77
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 24 (172610) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 176725 - 178370


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (170964 - 177991), exposure 2858.33
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.663708 bg counts (123), with cf=1.42259 and errBG= 0.0598445
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.3947 +/- 5.51033
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=170964 and stop= 177991 so gap is 7027.47, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (170964 - 177991), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (142885 - 167270), exposure 4422.88
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.961891 bg counts (226), with cf=1.42476 and errBG= 0.063984
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.0009 +/- 5.51883
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 40
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 641
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (177991 - 178370), exposure 378.599
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.0981364 bg counts (18), with cf=1.39507 and errBG= 0.023131
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.65323 +/- 1.97319
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 178370), exposure 5568.71, 6 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00142945, 0.00315357 and 2.20615. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=177991 and stop= 178370 so gap is 378.599, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 25 (178370) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=378.599 whereas forward=4179.48
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (170964 - 178370), exposure 3236.92
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.761844 bg counts (141), with cf=1.41935 and errBG= 0.0641589
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.0477 +/- 5.85285
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 25 (178370) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (170964 - 178370), with lastBin= 0 and workMinC was 8
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 182549
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 642
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 182549 - 184189


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (182549 - 184189), exposure 1639.77
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 3 counts and 0.26537 bg counts (83), with cf=1.48285 and errBG= 0.0291282
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =4.05505 +/- 2.56874
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 184189), exposure 7208.49, 6 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00108904, 0.00301467 and 2.7682. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=182549 and stop= 184189 so gap is 1639.77, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 26 (184189) and the bin is not full 3 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5819.25 whereas forward=4115.96
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 26 (184189) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 188305 - 189950


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (182549 - 189950), exposure 3284.56
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.425058 bg counts (168), with cf=1.73178 and errBG= 0.0327939
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.92277 +/- 3.87278
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 189950), exposure 8853.28, 6 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000877296, 0.0029053 and 3.31165. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=182549 and stop= 189950 so gap is 7400.52, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 27 (189950) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=11580 whereas forward=4113.09
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 27 (189950) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 194063 - 195710


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (182549 - 195710), exposure 4931.86
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.674836 bg counts (248), with cf=1.65904 and errBG= 0.0428521
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.4937 +/- 4.38998
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 195710), exposure 10500.6, 7 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000867734, 0.00256732 and 2.95864. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=182549 and stop= 195710 so gap is 13160.9, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 28 (195710) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=17340.4 whereas forward=4172.7
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 28 (195710) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 199883 - 201530


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (182549 - 201530), exposure 6579.16
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 0.970948 bg counts (341), with cf=1.60439 and errBG= 0.0525798
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.0906 +/- 5.32184
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 201530), exposure 12147.9, 9 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000985474, 0.00244338 and 2.4794. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=182549 and stop= 201530 so gap is 18980.9, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 29 (201530) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=23160.4 whereas forward=4113.91
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 29 (201530) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 205644 - 207289


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (182549 - 207203), exposure 8138.7
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.18861 bg counts (409), with cf=1.57149 and errBG= 0.0587728
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.7044 +/- 6.08704
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=182549 and stop= 207203 so gap is 24654.4, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (182549 - 207203), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (170964 - 178370), exposure 3236.92
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.761844 bg counts (141), with cf=1.41935 and errBG= 0.0641589
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.0477 +/- 5.85285
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 41
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 646
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (207203 - 207289), exposure 85.2466
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0288077 bg counts (9), with cf=1.4815 and errBG= 0.00960255
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.43882 +/- 1.48157
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 207289), exposure 13792.7, 10 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000965548, 0.00256506 and 2.65658. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=207203 and stop= 207289 so gap is 85.2466, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 30 (207289) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=85.2466 whereas forward=4174.85
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (182549 - 207289), exposure 8223.94
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 1.21741 bg counts (418), with cf=1.56586 and errBG= 0.0595456
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.1475 +/- 6.26415
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 30 (207289) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (182549 - 207289), with lastBin= 0 and workMinC was 7
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 211464
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 647
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 211464 - 213111


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (211464 - 213111), exposure 1647.3
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.27925 bg counts (87), with cf=1.47315 and errBG= 0.0299387
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =5.48123 +/- 2.94663
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 213111), exposure 15440, 11 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000949442, 0.00255947 and 2.69577. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=211464 and stop= 213111 so gap is 1647.3, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 31 (213111) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5822.14 whereas forward=4111.83
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 31 (213111) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 217223 - 217644


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (211464 - 217644), exposure 2068.52
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.407745 bg counts (113), with cf=1.46036 and errBG= 0.0383574
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.16671 +/- 3.57758
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 217644), exposure 15861.2, 12 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00101243, 0.00257251 and 2.54093. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=211464 and stop= 217644 so gap is 6180.35, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 32 (217644) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=10355.2 whereas forward=5457.87
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 32 (217644) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 223102 - 223430


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (211464 - 223430), exposure 2396.98
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.439691 bg counts (123), with cf=1.46365 and errBG= 0.0396456
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =9.60196 +/- 3.87288
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 223430), exposure 16189.6, 12 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00099045, 0.00261053 and 2.6357. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=211464 and stop= 223430 so gap is 11966.7, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 33 (223430) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 16 counts, because gotBinThisOrb=0 and gapBack=16141.5 whereas forward=34292.4
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (182549 - 223430), exposure 10620.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 1.6571 bg counts (541), with cf=1.53475 and errBG= 0.0712445
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.7561 +/- 7.36123
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 33 (223430) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (182549 - 223430), with lastBin= 0 and workMinC was 7
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 257723
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 650
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 257723 - 258144


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 257723 - 258144
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 257723 - 258144 the cf is 2.10501
++tructures/grbBin.cpp::        binData:  line  405  INFO   >>  This bin is empty, so found a emptyBin CF of 2.10501
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 258144), exposure 421.226
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 0 counts and 0.0205881 bg counts (19), with cf=2.10501 and errBG= 0.00472323
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =-0.043338 +/- 0.00994242
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 258144), exposure 16610.9, 12 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000965048, 0.00254276 and 2.63486. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 258144 so gap is 421.226, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 34 (258144) and the bin is not full 0 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=34713.6 whereas forward=5401.54
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 34 (258144) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 263545 - 263929


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 257723 - 263929
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 257723 - 263929 the cf is 2.0833
++tructures/grbBin.cpp::        binData:  line  405  INFO   >>  This bin is empty, so found a emptyBin CF of 2.0833
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 263929), exposure 804.843
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 0 counts and 0.034675 bg counts (32), with cf=2.0833 and errBG= 0.00612973
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =-0.0722384 +/- 0.0127701
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 263929), exposure 16994.5, 12 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000943078, 0.00248431 and 2.63426. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 263929 so gap is 6206.38, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 35 (263929) and the bin is not full 0 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=40498.8 whereas forward=5373.82
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 35 (263929) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 269303 - 269714


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 275064 - 275498 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 275498), exposure 1649.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.139741 bg counts (80), with cf=1.46767 and errBG= 0.0156236
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.73024 +/- 2.07572
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 275498), exposure 17839.4, 13 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000977096, 0.00244384 and 2.50112. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 275498 so gap is 17775.5, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 37 (275498) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=52067.9 whereas forward=5390.09
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 37 (275498) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 280888 - 281284


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 286652 - 287070 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 287070), exposure 2464.68
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.17446 bg counts (112), with cf=1.46767 and errBG= 0.0164849
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.67928 +/- 2.07573
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 287070), exposure 18654.3, 13 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000933565, 0.00233517 and 2.50134. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 287070 so gap is 29347.8, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 39 (287070) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=63640.2 whereas forward=5391.4
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 39 (287070) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 292462 - 292855


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 298222 - 298641 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 298641), exposure 3277.04
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.209156 bg counts (144), with cf=1.46767 and errBG= 0.0174296
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.62836 +/- 2.07575
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 298641), exposure 19466.7, 13 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000893631, 0.00223605 and 2.50221. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 298641 so gap is 40918.3, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 41 (298641) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=75210.7 whereas forward=5400.67
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 41 (298641) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 304042 - 304425


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 309983 - 310211 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 315982 - 315997 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 315997), exposure 3903.87
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 3 counts and 0.267982 bg counts (172), with cf=1.46754 and errBG= 0.0204335
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =4.00935 +/- 2.54204
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 315997), exposure 20093.5, 13 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000864402, 0.00223641 and 2.58724. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 315997 so gap is 58274.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 44 (315997) and the bin is not full 3 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=92566.6 whereas forward=28545.2
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 44 (315997) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 344542 - 344923


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 350302 - 350706 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 350706), exposure 4688.65
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.335289 bg counts (201), with cf=1.47205 and errBG= 0.0236495
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.8667 +/- 3.29179
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 350706), exposure 20878.3, 14 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000901556, 0.00221955 and 2.46191. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 350706 so gap is 92983, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 46 (350706) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=127275 whereas forward=5423.59
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 46 (350706) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 356129 - 356493


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 357568 - 357769 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 361885 - 363109 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 363109), exposure 6476.36
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.52736 bg counts (297), with cf=1.45936 and errBG= 0.0306006
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =9.4459 +/- 3.86136
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 363109), exposure 22666, 14 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000825663, 0.00216305 and 2.61977. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 363109 so gap is 105386, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 49 (363109) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=139679 whereas forward=4533.19
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 49 (363109) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 367642 - 369289


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 369289), exposure 8123.65
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.652606 bg counts (368), with cf=1.45936 and errBG= 0.0340195
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =9.26312 +/- 3.86142
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 369289), exposure 24313.3, 14 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000766965, 0.00201163 and 2.62284. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 369289 so gap is 111567, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 50 (369289) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=145859 whereas forward=4175.54
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 50 (369289) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 373465 - 375110


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 379225 - 380870 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 385042 - 385416 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 390805 - 391199 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 396682 - 396985 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 402742 - 402767 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 402767), exposure 12508.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 1.06993 bg counts (580), with cf=1.47422 and errBG= 0.0444262
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.6907 +/- 4.42315
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (154404 - 402767), exposure 28698.6, 15 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000694882, 0.00174366 and 2.50929. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 402767 so gap is 145044, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 56 (402767) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=179337 whereas forward=7185.73
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (154404 - 402767) = 154404- 402767
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 409953 - 410151


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 410151), exposure 12707
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 1.08195 bg counts (591), with cf=1.47422 and errBG= 0.0445056
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.673 +/- 4.42315
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 410151), exposure 198.077, 0 soft counts and 0 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -1.65602e-05, -4.41604e-05 and 2.66667. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 410151 so gap is 152428, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 57 (410151) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=186721 whereas forward=4472.66
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 57 (410151) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 414624 - 415970


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 415970), exposure 14053.4
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 1.12968 bg counts (635), with cf=1.47422 and errBG= 0.0448298
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.6026 +/- 4.42316
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 415970), exposure 1544.5, 0 soft counts and 0 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -1.47643e-05, -2.39219e-05 and 1.62026. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 415970 so gap is 158247, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 58 (415970) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=192540 whereas forward=3491.76
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 58 (415970) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 419462 - 420831


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 420831), exposure 15422.4
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 1.2464 bg counts (695), with cf=1.49757 and errBG= 0.0472788
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =13.1091 +/- 4.73627
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 420831), exposure 2913.48, 1 soft counts and 0 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000543134, -3.53848e-05 and -0.0651493. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 420831 so gap is 163108, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 59 (420831) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=197400 whereas forward=4711.22
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 59 (420831) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 425542 - 426771


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 426771), exposure 16651
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 1.35232 bg counts (751), with cf=1.50795 and errBG= 0.0493467
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.5482 +/- 5.00184
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 426771), exposure 4142.06, 1 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000361761, 0.000326908 and 0.903658. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 426771 so gap is 169048, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 60 (426771) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=203340 whereas forward=4531.86
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 60 (426771) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 431302 - 432531


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 432531), exposure 17879.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 1.43028 bg counts (791), with cf=1.52239 and errBG= 0.0508551
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.0913 +/- 5.27429
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 432531), exposure 5370.64, 1 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00026599, 0.000552792 and 2.07825. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 432531 so gap is 174808, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 61 (432531) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=209101 whereas forward=4596.31
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 61 (432531) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 437127 - 438351


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 442882 - 444111 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 444111), exposure 20331.7
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 1.55195 bg counts (909), with cf=1.52239 and errBG= 0.0514749
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.906 +/- 5.27431
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 444111), exposure 7822.78, 1 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000173588, 0.000362606 and 2.08888. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 444111 so gap is 186388, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 63 (444111) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=220681 whereas forward=4595.32
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 63 (444111) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 448706 - 449930


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 454462 - 455691 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 455691), exposure 22783.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 1.72806 bg counts (1027), with cf=1.52915 and errBG= 0.0539229
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.2365 +/- 5.51405
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 455691), exposure 10274.9, 1 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000119909, 0.000416823 and 3.47617. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 455691 so gap is 197968, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 65 (455691) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=232261 whereas forward=4598.72
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 65 (455691) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 460290 - 461511


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 466042 - 467271 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 467271), exposure 25233.5
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 1.89313 bg counts (1140), with cf=1.54072 and errBG= 0.0560695
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6533 +/- 5.76549
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 467271), exposure 12724.5, 2 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000222454, 0.000322546 and 1.44994. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 467271 so gap is 209548, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 67 (467271) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=243841 whereas forward=4600.32
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 67 (467271) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 471871 - 473089


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 477622 - 478851 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 478851), exposure 26762.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 1.96145 bg counts (1207), with cf=1.54072 and errBG= 0.0564578
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.548 +/- 5.76549
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 478851), exposure 14254, 2 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00019507, 0.000283483 and 1.45324. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 478851 so gap is 221128, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 69 (478851) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=255421 whereas forward=4650.63
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 69 (478851) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 483502 - 484730


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 489509 - 490730 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 495563 - 496431 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 501446 - 502670 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 502670), exposure 31303.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 2.19282 bg counts (1388), with cf=1.5468 and errBG= 0.0588583
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.8101 +/- 5.99141
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 502670), exposure 18794.7, 2 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00014158, 0.000287843 and 2.03309. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=257723 and stop= 502670 so gap is 244947, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 73 (502670) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (257723 - 502670), with lastBin= 0x19d4fe0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (182549 - 223430), exposure 10620.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 1.6571 bg counts (541), with cf=1.53475 and errBG= 0.0712445
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.7561 +/- 7.36123
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 42
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 512183
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19d4fe0 which has initial GTIBin: 809
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 512183 - 513530


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 517942 - 519291 to this bin
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 512183 - 519291
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 512183 - 519291 the cf is 1.64173
++tructures/grbBin.cpp::        binData:  line  405  INFO   >>  This bin is empty, so found a emptyBin CF of 1.64173
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 519291), exposure 2695.35
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 0 counts and 0.243137 bg counts (116), with cf=1.64173 and errBG= 0.0225747
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =-0.399167 +/- 0.0370617
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 519291), exposure 21490.1, 2 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000115438, 0.000241317 and 2.09045. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 519291 so gap is 7107.7, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 75 (519291) and the bin is not full 0 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=16621.3 whereas forward=4479.78
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 75 (519291) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 523771 - 525110


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 525110), exposure 4034.25
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.344091 bg counts (168), with cf=1.69348 and errBG= 0.0265472
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.11077 +/- 1.69408
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 525110), exposure 22829, 2 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000106066, 0.000296155 and 2.79217. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 525110 so gap is 12926.4, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 76 (525110) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=22440 whereas forward=4414.7
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 76 (525110) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 529524 - 530871


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 530871), exposure 5380.67
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.451847 bg counts (223), with cf=1.65391 and errBG= 0.0302579
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.56051 +/- 2.33952
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 530871), exposure 24175.4, 2 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.83687e-05, 0.000341047 and 3.46703. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 530871 so gap is 18687.5, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 77 (530871) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=28201.1 whereas forward=4471.41
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 77 (530871) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 535342 - 536689


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 541102 - 542330 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 546924 - 548150 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 553295 - 553909 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 553909), exposure 9796.02
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.699351 bg counts (468), with cf=1.65391 and errBG= 0.0323275
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.15116 +/- 2.3396
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 553909), exposure 28590.7, 2 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 7.70419e-05, 0.000280099 and 3.63567. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 553909 so gap is 41725.4, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 81 (553909) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=51239.1 whereas forward=5169.32
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 81 (553909) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 559078 - 559730


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 564262 - 565491 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 565491), exposure 11676.5
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.771547 bg counts (553), with cf=1.65391 and errBG= 0.0328095
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.03176 +/- 2.33962
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 565491), exposure 30471.2, 2 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 7.0675e-05, 0.000260483 and 3.68564. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 565491 so gap is 53307.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 83 (565491) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=62820.8 whereas forward=4591.97
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 83 (565491) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 570083 - 571311


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 571311), exposure 12905.1
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.877093 bg counts (608), with cf=1.63716 and errBG= 0.0355708
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =5.11269 +/- 3.27483
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 571311), exposure 31699.8, 2 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.65985e-05, 0.000348647 and 5.23506. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 571311 so gap is 59127.7, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 84 (571311) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=68641.3 whereas forward=4778.47
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 84 (571311) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 576090 - 577311


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 577311), exposure 14126.1
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.922692 bg counts (653), with cf=1.63716 and errBG= 0.0361077
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =5.03804 +/- 3.27485
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 577311), exposure 32920.8, 2 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.31345e-05, 0.000334407 and 5.29674. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 577311 so gap is 65127.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 85 (577311) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=74640.8 whereas forward=4772.93
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 85 (577311) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 582084 - 583310


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 583310), exposure 15352.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 1.0275 bg counts (707), with cf=1.65409 and errBG= 0.038643
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.57087 +/- 3.6992
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 583310), exposure 34146.9, 3 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000109375, 0.000319053 and 2.91706. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 583310 so gap is 71126.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 86 (583310) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=80639.9 whereas forward=4776.05
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 86 (583310) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 588086 - 589249


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 589249), exposure 16515.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 1.07561 bg counts (751), with cf=1.65409 and errBG= 0.0392496
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.49128 +/- 3.69922
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 589249), exposure 35310.3, 3 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00010482, 0.000307225 and 2.93098. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 589249 so gap is 77065.7, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 87 (589249) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=86579.3 whereas forward=3756.74
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 87 (589249) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 593006 - 594530


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 594530), exposure 18040
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 1.19761 bg counts (814), with cf=1.65593 and errBG= 0.0419763
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.95244 +/- 4.05679
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 594530), exposure 36834.7, 3 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.77e-05, 0.000336837 and 3.44767. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 594530 so gap is 82346.9, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 88 (594530) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=91860.5 whereas forward=4248.55
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 88 (594530) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 598779 - 600291


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 600291), exposure 19551.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 1.33477 bg counts (884), with cf=1.64702 and errBG= 0.044893
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =9.33077 +/- 4.35824
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 600291), exposure 38346.6, 3 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.16676e-05, 0.000361524 and 3.94385. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 600291 so gap is 88107.3, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 89 (600291) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=97620.9 whereas forward=4270.89
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 89 (600291) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 604562 - 606111


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 610347 - 611871 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 616129 - 617631 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 617631), exposure 24127.7
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 1.60825 bg counts (1085), with cf=1.64235 and errBG= 0.0488247
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.4975 +/- 4.64595
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 617631), exposure 42922.5, 4 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00011584, 0.000316541 and 2.73257. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 617631 so gap is 105447, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 92 (617631) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=114961 whereas forward=4281.13
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 92 (617631) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 621912 - 623449


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 627693 - 629210 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 629210), exposure 27181.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 1.82875 bg counts (1232), with cf=1.63557 and errBG= 0.0521012
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.7291 +/- 4.90746
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 629210), exposure 45976.4, 4 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000104539, 0.000325766 and 3.11623. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 629210 so gap is 117027, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 94 (629210) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=126541 whereas forward=4265.86
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 94 (629210) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 633476 - 635031


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 635031), exposure 28736.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 1.9042 bg counts (1301), with cf=1.63557 and errBG= 0.0527928
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.6057 +/- 4.90748
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 635031), exposure 47530.9, 4 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.99582e-05, 0.000313649 and 3.1378. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 635031 so gap is 122847, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 95 (635031) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=132361 whereas forward=4228.5
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 95 (635031) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 639259 - 640789


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 645044 - 646551 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 646551), exposure 31772.5
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 2.10132 bg counts (1429), with cf=1.63145 and errBG= 0.0555874
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.8863 +/- 5.15989
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 646551), exposure 50567.2, 4 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.08935e-05, 0.000323072 and 3.5544. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 646551 so gap is 134367, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 97 (646551) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=143881 whereas forward=4275.35
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 97 (646551) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 650826 - 652371


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 656606 - 658131 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 658131), exposure 34841.4
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 2.25234 bg counts (1550), with cf=1.62794 and errBG= 0.0572094
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.2407 +/- 5.40006
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 658131), exposure 53636.2, 4 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 8.33826e-05, 0.000332036 and 3.98208. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 658131 so gap is 145947, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 99 (658131) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=155461 whereas forward=4260.02
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 99 (658131) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 662391 - 663950


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 668176 - 669710 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 669710), exposure 37935.4
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 2.39707 bg counts (1683), with cf=1.62794 and errBG= 0.0584303
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.005 +/- 5.4001
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 669710), exposure 56730.2, 4 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 7.6995e-05, 0.00031156 and 4.0465. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 669710 so gap is 157527, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 101 (669710) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=167040 whereas forward=4244.97
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 101 (669710) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 673955 - 675469


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 675469), exposure 39449.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 2.46487 bg counts (1745), with cf=1.62794 and errBG= 0.059006
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =13.8947 +/- 5.40011
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 675469), exposure 58244.6, 4 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 7.40769e-05, 0.000302453 and 4.08296. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 675469 so gap is 163286, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 102 (675469) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=172800 whereas forward=370.916
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 102 (675469) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 675840 - 675916


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 675916), exposure 39525.1
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 2.48651 bg counts (1749), with cf=1.62794 and errBG= 0.0594558
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =13.8594 +/- 5.40013
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 675916), exposure 58319.8, 4 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 7.36692e-05, 0.000301762 and 4.09617. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 675916 so gap is 163732, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 103 (675916) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=173246 whereas forward=50.5472
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 103 (675916) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 675966 - 676249


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 676249), exposure 39808.4
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 2.57305 bg counts (1765), with cf=1.60539 and errBG= 0.0612458
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.1339 +/- 5.56209
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 676249), exposure 58603.1, 5 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.74828e-05, 0.000298504 and 3.06212. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 676249 so gap is 164066, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 104 (676249) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=173580 whereas forward=3495.53
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 104 (676249) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 679745 - 681289


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 681289), exposure 41352.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 2.71408 bg counts (1837), with cf=1.60352 and errBG= 0.063324
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.4937 +/- 5.78248
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 681289), exposure 60147.6, 5 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.32413e-05, 0.000315182 and 3.38028. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 681289 so gap is 169106, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 105 (681289) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=178620 whereas forward=4137.21
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 105 (681289) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 685427 - 687049


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 691247 - 692870 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 692870), exposure 44597.3
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 2.98871 bg counts (1969), with cf=1.59572 and errBG= 0.0673535
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.571 +/- 5.97161
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 692870), exposure 63392.1, 6 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000110139, 0.000294464 and 2.67357. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 692870 so gap is 180686, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 107 (692870) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=190200 whereas forward=5275.9
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 107 (692870) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 698146 - 699349


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 699349), exposure 45800.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 3.04868 bg counts (2024), with cf=1.59572 and errBG= 0.0677653
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.4753 +/- 5.97162
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 699349), exposure 64595.6, 6 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000107602, 0.000287965 and 2.67621. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 699349 so gap is 187166, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 108 (699349) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=196679 whereas forward=4617.67
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 108 (699349) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 703967 - 705170


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 709727 - 710390 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 710390), exposure 47581
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 3.13798 bg counts (2106), with cf=1.59572 and errBG= 0.0683787
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.3328 +/- 5.97164
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 710390), exposure 66375.8, 6 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000103825, 0.000278965 and 2.68688. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 710390 so gap is 198207, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 110 (710390) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=207720 whereas forward=5165.01
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 110 (710390) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 715555 - 716270


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 720168 - 721790 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 721790), exposure 49471.5
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 3.3089 bg counts (2200), with cf=1.58681 and errBG= 0.070546
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.5516 +/- 6.14671
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 721790), exposure 68266.3, 6 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.93288e-05, 0.000290659 and 2.92623. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=512183 and stop= 721790 so gap is 209606, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 112 (721790) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (512183 - 721790), with lastBin= 0x19967a0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (257723 - 502670), exposure 31303.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 2.19282 bg counts (1388), with cf=1.5468 and errBG= 0.0588583
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.8101 +/- 5.99141
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 43
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 725926
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x19967a0 which has initial GTIBin: 911
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 725926 - 727551


++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (725926 - 727551), exposure 1624.73
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.1972 bg counts (63), with cf=1.4781 and errBG= 0.0248449
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.66472 +/- 2.09067
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 727551), exposure 69891, 6 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.50171e-05, 0.000324295 and 3.41302. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=725926 and stop= 727551 so gap is 1624.73, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 113 (727551) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5761.2 whereas forward=4136.95
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 113 (727551) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  787  INFO   >>  I'm on the last event, so save the previous bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (512183 - 721790), exposure 49471.5
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 3.3089 bg counts (2200), with cf=1.58681 and errBG= 0.070546
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.5516 +/- 6.14671
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 44
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  903  INFO   >>  I have run out of background events
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x19967a0
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (725926 - 762051), exposure 11180.1
++taStructures/bin.cpp::        fullBin:  line  192  INFO   >>  Producing an upper limit of 13.9725 given bg=0.60769 and numCts= 2
++ctures/binMethod.cpp::        saveBin:  line  378  INFO   >>  Saving an upper limit, bin number: 45 with rate=0.00124977
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (409953 - 727551), exposure 79446.3, 6 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 8.02758e-05, 0.00028036 and 3.49246. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for PC mode.
++/genlc_cpp/genlc.cpp::           main:  line  397  INFO   >>  COMPLETE

