++lUtils/createLog.cpp::      createLog:  line   51  INFO   >>  Created FileAppender: 'genlc.log', level info
++/genlc_cpp/genlc.cpp::           main:  line  151  INFO   >>  Starting to run genlc.cpp, mode=0
++/genlc_cpp/genlc.cpp::           main:  line  152  INFO   >>  Argparsing reported: Selected GRB binning.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: WT, with files: wtsourcetotal.evt, wtbacktotal.evt, and wtcorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 71.6705 - 3000
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	71.6705 - 154.779
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - WT mode, suffix = 
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 30 ct/bin at rateFact=10 and binFact= 1.5 with minT 0.5 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file WTCURVE.qdp, reading from wtsourcetotal.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (71.6705 - 73.3002), exposure 1.62967
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 46 counts and 0 bg counts (0), with cf=1.14393 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.6209 +/- 7.76572
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=71.6705 and stop= 73.3002 so gap is 1.62967, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (71.6705 - 73.3002), with lastBin= 0 and workMinC was 45
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 73.9051), exposure 2.23457, 45 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 23.0367, 12.9435 and 0.561866. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 73.9051 so gap is 0.604904, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 73.9104), exposure 2.23991, 45 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 22.9818, 13.4234 and 0.584088. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 73.9104 so gap is 0.610241, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 73.9655), exposure 2.29506, 45 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 22.4295, 13.5992 and 0.60631. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 73.9655 so gap is 0.665393, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 73.9869), exposure 2.31641, 45 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 22.2228, 13.9677 and 0.628532. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 73.9869 so gap is 0.686742, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.1168), exposure 2.44628, 45 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 21.043, 13.6938 and 0.650754. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.1168 so gap is 0.816617, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.1684), exposure 2.49788, 46 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 21.0663, 13.411 and 0.636608. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.1684 so gap is 0.86821, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.1862), exposure 2.51567, 46 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 20.9173, 13.7708 and 0.658347. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.1862 so gap is 0.886001, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.2377), exposure 2.56726, 47 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 20.9425, 13.4941 and 0.644339. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.2377 so gap is 0.937595, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.2538), exposure 2.58327, 48 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 21.2555, 13.4104 and 0.630916. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.2538 so gap is 0.953607, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.2876), exposure 2.61708, 49 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 21.4181, 13.2372 and 0.61804. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.2876 so gap is 0.98741, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.3054), exposure 2.63487, 50 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 21.7076, 13.1478 and 0.605679. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.3054 so gap is 1.0052, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.3765), exposure 2.70603, 50 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 21.1367, 13.2248 and 0.625679. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.3765 so gap is 1.07636, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.3943), exposure 2.72382, 50 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 20.9987, 13.5584 and 0.645679. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.3943 so gap is 1.09416, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.4566), exposure 2.78609, 51 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 20.94, 13.2554 and 0.633019. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.4566 so gap is 1.15642, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.4708), exposure 2.80032, 52 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 21.242, 13.188 and 0.620845. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.4708 so gap is 1.17066, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.5313), exposure 2.86081, 52 soft counts and 34 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 20.7929, 13.309 and 0.640076. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.5313 so gap is 1.23115, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.5544), exposure 2.88394, 53 soft counts and 34 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 21.0228, 13.2023 and 0.627999. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.5544 so gap is 1.25427, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.6309), exposure 2.96044, 53 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 20.4795, 13.2475 and 0.646867. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.6309 so gap is 1.33078, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.6416), exposure 2.97112, 53 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 20.406, 13.585 and 0.665735. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.6416 so gap is 1.34145, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.6807), exposure 3.01026, 54 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 20.5206, 13.4083 and 0.653406. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.6807 so gap is 1.38059, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (73.3002 - 74.8017), exposure 1.50157
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0.716049 bg counts (1), with cf=1.14393 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =50.6579 +/- 7.722
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.8017), exposure 3.13124, 55 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 20.0931, 12.8903 and 0.641526. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=73.3002 and stop= 74.8017 so gap is 1.50157, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (73.3002 - 74.8017), with lastBin= 0xaf0fa0 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (71.6705 - 73.3002), exposure 1.62967
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 46 counts and 0 bg counts (0), with cf=1.14393 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.6209 +/- 7.76572
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.8658), exposure 3.19528, 55 soft counts and 37 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 19.6904, 12.9899 and 0.659708. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 74.8658 so gap is 0.0640475, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.9458), exposure 3.27534, 56 soft counts and 37 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 19.5583, 12.6724 and 0.647928. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 74.9458 so gap is 0.144107, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.9476), exposure 3.27712, 57 soft counts and 37 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 19.8968, 12.6655 and 0.636561. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 74.9476 so gap is 0.145886, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 74.9601), exposure 3.28958, 57 soft counts and 38 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 19.8215, 12.9653 and 0.654104. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 74.9601 so gap is 0.15834, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.0597), exposure 3.38921, 58 soft counts and 38 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 19.5763, 12.5842 and 0.642827. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.0597 so gap is 0.257969, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.1398), exposure 3.46926, 58 soft counts and 39 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 19.1246, 12.6235 and 0.660068. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.1398 so gap is 0.338029, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.1629), exposure 3.49239, 58 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 18.9979, 12.8675 and 0.677309. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.1629 so gap is 0.361157, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.2536), exposure 3.58313, 59 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 18.8361, 12.5416 and 0.66583. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.2536 so gap is 0.451891, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.3088), exposure 3.63828, 60 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 18.865, 12.3515 and 0.654733. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.3088 so gap is 0.507043, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.4564), exposure 3.78594, 61 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 18.4313, 11.8698 and 0.643999. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.4564 so gap is 0.654708, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.4867), exposure 3.81619, 62 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 18.585, 11.7757 and 0.633612. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.4867 so gap is 0.684953, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.5134), exposure 3.84288, 62 soft counts and 41 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 18.4559, 11.9916 and 0.649741. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.5134 so gap is 0.711639, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.524), exposure 3.85355, 63 soft counts and 41 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 18.7017, 11.9584 and 0.639428. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.524 so gap is 0.722314, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.5988), exposure 3.92827, 63 soft counts and 42 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 18.3459, 12.0221 and 0.655301. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.5988 so gap is 0.797036, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.6788), exposure 4.00833, 63 soft counts and 43 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 17.9795, 12.0674 and 0.671174. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.6788 so gap is 0.877096, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.7019), exposure 4.03146, 63 soft counts and 44 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 17.8764, 12.2819 and 0.687047. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.7019 so gap is 0.900224, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.7162), exposure 4.04569, 64 soft counts and 44 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 18.0962, 12.2387 and 0.676312. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.7162 so gap is 0.914457, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (71.6705 - 75.7286), exposure 4.05815, 64 soft counts and 45 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 18.0407, 12.483 and 0.691937. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 75.7286 so gap is 0.92691, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (71.6705 - 75.7286) = 71.6705- 75.7286
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (74.8017 - 76.5844), exposure 1.78267
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0.716049 bg counts (1), with cf=1.14393 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =50.6579 +/- 7.72122
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=74.8017 and stop= 76.5844 so gap is 1.78267, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (74.8017 - 76.5844), with lastBin= 0xaf2b10 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (73.3002 - 74.8017), exposure 1.50157
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0.716049 bg counts (1), with cf=1.14393 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =50.6579 +/- 7.722
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (76.5844 - 79.0449), exposure 2.46054
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.14393 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.477 +/- 7.6758
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=76.5844 and stop= 79.0449 so gap is 2.46054, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (76.5844 - 79.0449), with lastBin= 0xaf0fa0 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (74.8017 - 76.5844), exposure 1.78267
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0.716049 bg counts (1), with cf=1.14393 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =50.6579 +/- 7.72122
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.3616), exposure 3.63298, 45 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.1694, 9.85052 and 0.695199. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.3616 so gap is 0.31668, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.399), exposure 3.67034, 46 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.3368, 9.75025 and 0.680086. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.399 so gap is 0.354041, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.415), exposure 3.68636, 46 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.2745, 10.0182 and 0.701825. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.415 so gap is 0.370052, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.447), exposure 3.71838, 48 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.7669, 9.93193 and 0.672582. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.447 so gap is 0.402076, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.6445), exposure 3.91586, 48 soft counts and 34 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.0222, 9.72319 and 0.693416. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.6445 so gap is 0.599556, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.6872), exposure 3.95856, 48 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.8709, 9.90729 and 0.714249. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.6872 so gap is 0.642255, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.7157), exposure 3.98702, 48 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.7719, 10.1235 and 0.735082. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.7157 so gap is 0.67072, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.7174), exposure 3.9888, 49 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.0525, 10.119 and 0.720081. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.7174 so gap is 0.672499, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.7192), exposure 3.99058, 49 soft counts and 37 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.0463, 10.4011 and 0.740489. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.7192 so gap is 0.674278, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.7797), exposure 4.05107, 50 soft counts and 37 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.1189, 10.2458 and 0.725679. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.7797 so gap is 0.734768, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.8028), exposure 4.0742, 51 soft counts and 37 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.3195, 10.1876 and 0.71145. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.8028 so gap is 0.757896, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.9078), exposure 4.17917, 52 soft counts and 37 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.2336, 9.93175 and 0.697768. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.9078 so gap is 0.862863, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.9167), exposure 4.18806, 52 soft counts and 38 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.2034, 10.1838 and 0.716999. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.9167 so gap is 0.871758, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 79.9363), exposure 4.20763, 52 soft counts and 39 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.1373, 10.4083 and 0.73623. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 79.9363 so gap is 0.891328, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.0964), exposure 4.36775, 53 soft counts and 39 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.8809, 10.0267 and 0.722339. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.0964 so gap is 1.05145, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.1248), exposure 4.39622, 54 soft counts and 39 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.0513, 9.96182 and 0.708962. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.1248 so gap is 1.07991, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.1337), exposure 4.40511, 55 soft counts and 39 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.2826, 9.9417 and 0.696072. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.1337 so gap is 1.08881, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.2352), exposure 4.50652, 55 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.9612, 9.97182 and 0.714254. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.2352 so gap is 1.19022, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.3864), exposure 4.65775, 56 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.7535, 9.64806 and 0.701499. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.3864 so gap is 1.34144, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.486), exposure 4.75738, 57 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.7059, 9.44601 and 0.689192. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.486 so gap is 1.44108, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.5287), exposure 4.80008, 58 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.8223, 9.36198 and 0.677309. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.5287 so gap is 1.48377, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.5625), exposure 4.83388, 59 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.9623, 9.29651 and 0.66583. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.5625 so gap is 1.51758, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.5928), exposure 4.86413, 60 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.1107, 9.2387 and 0.654733. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.5928 so gap is 1.54782, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.6444), exposure 4.91572, 60 soft counts and 41 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.9626, 9.37444 and 0.671399. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.6444 so gap is 1.59942, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.6568), exposure 4.92818, 60 soft counts and 42 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.9273, 9.58288 and 0.688066. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.6568 so gap is 1.61187, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.671), exposure 4.94241, 61 soft counts and 42 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.1186, 9.55528 and 0.676786. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.671 so gap is 1.62611, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.6782), exposure 4.94953, 62 soft counts and 42 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.3294, 9.54154 and 0.66587. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.6782 so gap is 1.63322, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.8828), exposure 5.15413, 63 soft counts and 42 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.9825, 9.16278 and 0.655301. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.8828 so gap is 1.83782, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.9397), exposure 5.21106, 64 soft counts and 42 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.0493, 9.06267 and 0.645062. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.9397 so gap is 1.89475, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.9575), exposure 5.22885, 65 soft counts and 42 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.2203, 9.03183 and 0.635138. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.9575 so gap is 1.91255, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 80.9682), exposure 5.23952, 66 soft counts and 42 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.4096, 9.01343 and 0.625514. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 80.9682 so gap is 1.92322, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 81.0909), exposure 5.36228, 66 soft counts and 43 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.0797, 9.02042 and 0.640666. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 81.0909 so gap is 2.04598, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 81.1194), exposure 5.39075, 66 soft counts and 44 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 14.0054, 9.18499 and 0.655817. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 81.1194 so gap is 2.07445, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 81.2261), exposure 5.49748, 67 soft counts and 44 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.9416, 9.00667 and 0.646029. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 81.2261 so gap is 2.18118, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (75.7286 - 81.2919), exposure 5.56331, 67 soft counts and 45 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.7766, 9.10572 and 0.660954. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 81.2919 so gap is 2.247, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (75.7286 - 81.2919) = 75.7286- 81.2919
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (79.0449 - 81.5535), exposure 2.50854
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.14393 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.477 +/- 7.67473
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=79.0449 and stop= 81.5535 so gap is 2.50854, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (79.0449 - 81.5535), with lastBin= 0xaf2b10 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (76.5844 - 79.0449), exposure 2.46054
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.14393 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.477 +/- 7.6758
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81.5535 - 83.8307), exposure 2.27727
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0.716049 bg counts (1), with cf=1.11268 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.2738 +/- 7.50684
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=81.5535 and stop= 83.8307 so gap is 2.27727, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (81.5535 - 83.8307), with lastBin= 0xaf0fa0 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (79.0449 - 81.5535), exposure 2.50854
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.14393 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.477 +/- 7.67473
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 83.9695), exposure 2.67758, 32 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 13.3324, 7.61574 and 0.571221. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 83.9695 so gap is 0.138772, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 84.2649), exposure 2.97291, 33 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 12.3774, 6.85917 and 0.554167. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 84.2649 so gap is 0.434108, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 84.3396), exposure 3.04764, 34 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 12.1726, 6.69099 and 0.549678. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 84.3396 so gap is 0.508833, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 84.3645), exposure 3.07254, 34 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 12.0739, 6.99449 and 0.579307. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 84.3645 so gap is 0.53374, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 85.7593), exposure 4.46738, 45 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.8317, 6.77861 and 0.625813. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 85.7593 so gap is 1.92858, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 85.7629), exposure 4.47094, 45 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.8231, 7.01899 and 0.648522. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 85.7629 so gap is 1.93214, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 85.802), exposure 4.51008, 46 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.9728, 6.95807 and 0.634121. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 85.802 so gap is 1.97128, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 85.8127), exposure 4.52076, 47 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 11.19, 6.94164 and 0.620345. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 85.8127 so gap is 1.98195, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 85.8447), exposure 4.55278, 47 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 11.1113, 7.13417 and 0.642067. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 85.8447 so gap is 2.01398, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 85.8945), exposure 4.6026, 47 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.991, 7.29569 and 0.663788. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 85.8945 so gap is 2.06379, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 86.0529), exposure 4.76094, 48 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.8563, 7.05304 and 0.649675. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 86.0529 so gap is 2.22214, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 86.1596), exposure 4.86769, 48 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.6182, 7.1241 and 0.670934. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 86.1596 so gap is 2.32889, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 86.2486), exposure 4.95664, 49 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.6493, 6.99625 and 0.656966. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 86.2486 so gap is 2.41784, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 86.2788), exposure 4.98689, 49 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.5847, 7.17415 and 0.677782. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 86.2788 so gap is 2.44809, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 86.318), exposure 5.02603, 50 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.7209, 7.11828 and 0.66396. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 86.318 so gap is 2.48723, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 86.4496), exposure 5.15769, 51 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.6603, 6.93658 and 0.65069. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 86.4496 so gap is 2.61888, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 86.7752), exposure 5.48325, 51 soft counts and 34 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.0274, 6.72511 and 0.670674. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 86.7752 so gap is 2.94445, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 86.8464), exposure 5.55441, 51 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.89891, 6.83676 and 0.690658. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 86.8464 so gap is 3.01561, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 86.857), exposure 5.56509, 51 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.87993, 7.02108 and 0.710641. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 86.857 so gap is 3.02629, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 86.9673), exposure 5.67539, 52 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.88152, 6.88463 and 0.696717. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 86.9673 so gap is 3.13659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 86.994), exposure 5.70208, 53 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.028, 6.85241 and 0.683328. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 86.994 so gap is 3.16328, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.1008), exposure 5.80883, 54 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.0329, 6.72648 and 0.670444. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 87.1008 so gap is 3.27002, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.1025), exposure 5.8106, 55 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.2189, 6.72442 and 0.658037. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 87.1025 so gap is 3.2718, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.3054), exposure 6.01342, 56 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.057, 6.49762 and 0.646081. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 87.3054 so gap is 3.47462, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.332), exposure 6.04011, 57 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.1945, 6.46892 and 0.634552. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 87.332 so gap is 3.50131, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.4085), exposure 6.11661, 58 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.2466, 6.25837 and 0.610775. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 87.4085 so gap is 3.57781, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (83.8307 - 87.469), exposure 3.6383
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 2.14815 bg counts (3), with cf=1.09856 and errBG= 1.24023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =47.0755 +/- 7.49446
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.469), exposure 6.1771, 59 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.3241, 6.19709 and 0.600252. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=83.8307 and stop= 87.469 so gap is 3.6383, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (83.8307 - 87.469), with lastBin= 0xaf2b10 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81.5535 - 83.8307), exposure 2.27727
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0.716049 bg counts (1), with cf=1.11268 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.2738 +/- 7.50684
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.5473), exposure 6.25539, 59 soft counts and 37 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 10.1949, 6.2952 and 0.617483. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=87.469 and stop= 87.5473 so gap is 0.0782936, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.6754), exposure 6.38349, 59 soft counts and 38 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.99034, 6.34102 and 0.634714. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=87.469 and stop= 87.6754 so gap is 0.206391, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.7875), exposure 6.49558, 60 soft counts and 38 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.98711, 6.2316 and 0.623964. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=87.469 and stop= 87.7875 so gap is 0.318476, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.8498), exposure 6.55785, 60 soft counts and 39 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.89228, 6.33999 and 0.640903. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=87.469 and stop= 87.8498 so gap is 0.380746, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.8711), exposure 6.57919, 60 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.86018, 6.48644 and 0.657842. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=87.469 and stop= 87.8711 so gap is 0.402096, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 87.9868), exposure 6.69484, 61 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.85398, 6.37439 and 0.646885. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=87.469 and stop= 87.9868 so gap is 0.517739, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2919 - 88.2625), exposure 6.9706, 62 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 9.62178, 6.12222 and 0.636287. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=87.469 and stop= 88.2625 so gap is 0.793505, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (81.2919 - 88.2625) = 81.2919- 88.2625
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (87.469 - 91.4205), exposure 3.95143
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.09856 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.4354 +/- 7.36947
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=87.469 and stop= 91.4205 so gap is 3.95143, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (87.469 - 91.4205), with lastBin= 0xaf0fa0 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (83.8307 - 87.469), exposure 3.6383
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 2.14815 bg counts (3), with cf=1.09856 and errBG= 1.24023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =47.0755 +/- 7.49446
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 92.7851), exposure 4.52252, 30 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 7.2873, 4.8582 and 0.666667. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 92.7851 so gap is 1.36459, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 92.8883), exposure 4.62571, 30 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 7.12473, 4.82324 and 0.676972. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 92.8883 so gap is 1.46779, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 93.8561), exposure 5.59354, 34 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.69807, 4.59284 and 0.685696. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 93.8561 so gap is 2.43562, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 94.1087), exposure 5.84617, 35 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.60144, 4.39437 and 0.665668. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 94.1087 so gap is 2.68825, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 94.2813), exposure 6.01875, 36 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.59945, 4.26837 and 0.646776. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 94.2813 so gap is 2.86083, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 94.3756), exposure 6.11304, 36 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.49765, 4.38681 and 0.675139. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 94.3756 so gap is 2.95512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 94.429), exposure 6.16642, 37 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.62421, 4.34884 and 0.656507. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 94.429 so gap is 3.00849, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 94.4966), exposure 6.23402, 37 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.55237, 4.4824 and 0.684088. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 94.4966 so gap is 3.0761, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 94.8471), exposure 6.58451, 37 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.20359, 4.41491 and 0.71167. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 94.8471 so gap is 3.42659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 94.872), exposure 6.60942, 38 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.35077, 4.39828 and 0.692558. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 94.872 so gap is 3.4515, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 95.0018), exposure 6.7393, 39 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.39564, 4.31351 and 0.674446. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 95.0018 so gap is 3.58138, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 95.1531), exposure 6.89052, 39 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.25528, 4.38236 and 0.700586. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 95.1531 so gap is 3.7326, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (91.4205 - 95.2011), exposure 3.78064
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.716049 bg counts (1), with cf=1.11577 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.6742 +/- 6.16337
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 95.2011), exposure 6.93856, 39 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.21197, 4.51441 and 0.726727. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.4205 and stop= 95.2011 so gap is 3.78064, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (91.4205 - 95.2011), with lastBin= 0xaf2b10 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (87.469 - 91.4205), exposure 3.95143
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.09856 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.4354 +/- 7.36947
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 96.0159), exposure 7.75339, 45 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.43146, 4.91199 and 0.763744. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 96.0159 so gap is 0.814827, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 96.2063), exposure 7.94375, 45 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.27734, 4.93614 and 0.786343. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 96.2063 so gap is 1.00519, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 96.3504), exposure 8.08786, 46 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.30486, 4.84819 and 0.76896. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 96.3504 so gap is 1.1493, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 96.5675), exposure 8.30491, 47 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.27581, 4.72148 and 0.752329. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 96.5675 so gap is 1.36635, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 96.6938), exposure 8.43123, 47 soft counts and 37 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.18179, 4.7844 and 0.773951. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 96.6938 so gap is 1.49267, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 96.998), exposure 8.73546, 48 soft counts and 37 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.09554, 4.61777 and 0.757566. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 96.998 so gap is 1.7969, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 97.0798), exposure 8.8173, 48 soft counts and 38 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.03896, 4.70272 and 0.778731. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 97.0798 so gap is 1.87874, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 97.0976), exposure 8.8351, 49 soft counts and 38 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.15438, 4.69325 and 0.762587. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 97.0976 so gap is 1.89654, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 97.24), exposure 8.97743, 49 soft counts and 39 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.05681, 4.74438 and 0.783313. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 97.24 so gap is 2.03887, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 97.3432), exposure 9.08062, 49 soft counts and 40 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.98798, 4.81457 and 0.804039. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 97.3432 so gap is 2.14206, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 97.3627), exposure 9.10019, 49 soft counts and 41 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.97511, 4.92806 and 0.824766. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 97.3627 so gap is 2.16163, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 97.5086), exposure 9.24607, 49 soft counts and 42 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.88083, 4.9722 and 0.845492. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 97.5086 so gap is 2.30751, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 97.53), exposure 9.26742, 49 soft counts and 43 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.86728, 5.08235 and 0.866219. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 97.53 so gap is 2.32886, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 97.7043), exposure 9.44177, 50 soft counts and 43 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.87833, 4.9885 and 0.848626. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 97.7043 so gap is 2.50321, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 97.8911), exposure 9.62858, 51 soft counts and 43 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.88135, 4.89172 and 0.831734. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 97.8911 so gap is 2.69002, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 98.2167), exposure 9.95415, 52 soft counts and 43 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.80223, 4.73172 and 0.8155. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 98.2167 so gap is 3.01559, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 98.2487), exposure 9.98618, 53 soft counts and 43 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.89651, 4.71655 and 0.799889. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 98.2487 so gap is 3.04762, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 98.3057), exposure 10.0431, 53 soft counts and 44 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.86308, 4.80203 and 0.819029. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 98.3057 so gap is 3.10455, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (88.2625 - 98.4284), exposure 10.1659, 53 soft counts and 45 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.79228, 4.85491 and 0.838169. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 98.4284 so gap is 3.22731, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (88.2625 - 98.4284) = 88.2625- 98.4284
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (95.2011 - 98.8679), exposure 3.66675
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 31 counts and 0 bg counts (0), with cf=1.12724 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.9446 +/- 6.27625
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.2011 and stop= 98.8679 so gap is 3.66675, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (95.2011 - 98.8679), with lastBin= 0xaf0fa0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (91.4205 - 95.2011), exposure 3.78064
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.716049 bg counts (1), with cf=1.11577 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.6742 +/- 6.16337
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (98.8679 - 103.421), exposure 4.55277
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.716049 bg counts (1), with cf=1.12724 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.0102 +/- 6.22672
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98.8679 and stop= 103.421 so gap is 4.55277, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (98.8679 - 103.421), with lastBin= 0xaf2b10 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (95.2011 - 98.8679), exposure 3.66675
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 31 counts and 0 bg counts (0), with cf=1.12724 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.9446 +/- 6.27625
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 107.477), exposure 9.04861, 30 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.53097, 2.69671 and 0.76373. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=103.421 and stop= 107.477 so gap is 4.0564, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 108.269), exposure 9.84032, 30 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.24689, 2.59093 and 0.797973. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=103.421 and stop= 108.269 so gap is 4.84811, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 108.358), exposure 9.92928, 30 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.2178, 2.67791 and 0.832217. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=103.421 and stop= 108.358 so gap is 4.93706, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 108.482), exposure 10.0538, 31 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.28688, 2.64474 and 0.804635. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=103.421 and stop= 108.482 so gap is 5.0616, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 108.509), exposure 10.0805, 32 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.38681, 2.63773 and 0.778825. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=103.421 and stop= 108.509 so gap is 5.08829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 108.714), exposure 10.2851, 33 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.42591, 2.58526 and 0.75462. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=103.421 and stop= 108.714 so gap is 5.29288, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 108.774), exposure 10.3456, 34 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.51173, 2.57015 and 0.731876. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=103.421 and stop= 108.774 so gap is 5.35337, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 108.872), exposure 10.4434, 35 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.58367, 2.54607 and 0.710463. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=103.421 and stop= 108.872 so gap is 5.45122, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 109.528), exposure 11.0999, 35 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.37172, 2.49405 and 0.739697. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=103.421 and stop= 109.528 so gap is 6.10772, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (103.421 - 109.733), exposure 6.31232
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.716049 bg counts (1), with cf=1.09519 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.0716 +/- 6.04967
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 109.733), exposure 11.3045, 36 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.40755, 2.44891 and 0.718671. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=103.421 and stop= 109.733 so gap is 6.31232, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (103.421 - 109.733), with lastBin= 0xaf0fa0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (98.8679 - 103.421), exposure 4.55277
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.716049 bg counts (1), with cf=1.12724 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.0102 +/- 6.22672
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 109.97), exposure 11.5412, 37 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.43255, 2.3987 and 0.698809. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=109.733 and stop= 109.97 so gap is 0.236628, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 110.185), exposure 11.7564, 37 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.3697, 2.44784 and 0.726427. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=109.733 and stop= 110.185 so gap is 0.451899, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 110.32), exposure 11.8916, 38 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.42345, 2.42001 and 0.706891. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=109.733 and stop= 110.32 so gap is 0.58711, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 110.614), exposure 12.1852, 39 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.43082, 2.36171 and 0.688379. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=109.733 and stop= 110.614 so gap is 0.880662, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 110.857), exposure 12.4289, 39 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.36354, 2.40342 and 0.71455. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=109.733 and stop= 110.857 so gap is 1.1244, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 110.934), exposure 12.5054, 39 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.34297, 2.47621 and 0.740721. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=109.733 and stop= 110.934 so gap is 1.2009, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 111.197), exposure 12.7687, 39 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.27403, 2.51083 and 0.766892. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=109.733 and stop= 111.197 so gap is 1.46421, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 111.354), exposure 12.9253, 40 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.31907, 2.48041 and 0.747322. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=109.733 and stop= 111.354 so gap is 1.62077, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (98.4284 - 111.423), exposure 12.9947, 40 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.30135, 2.55137 and 0.772825. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=109.733 and stop= 111.423 so gap is 1.69016, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (98.4284 - 111.423) = 98.4284- 111.423
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (109.733 - 116.762), exposure 7.02931
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.1006 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.018 +/- 6.02824
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=109.733 and stop= 116.762 so gap is 7.02931, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (109.733 - 116.762), with lastBin= 0xaf2b10 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (103.421 - 109.733), exposure 6.31232
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.716049 bg counts (1), with cf=1.09519 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.0716 +/- 6.04967
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 12
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (116.762 - 125.747), exposure 8.98454
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.716049 bg counts (1), with cf=1.12247 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.8702 +/- 6.20032
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 125.747 so gap is 8.98454, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (116.762 - 125.747), with lastBin= 0xaf0fa0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (109.733 - 116.762), exposure 7.02931
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.1006 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.018 +/- 6.02824
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 13
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (111.423 - 131.915), exposure 20.4919, 30 soft counts and 37 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.62928, 1.96126 and 1.20376. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=125.747 and stop= 131.915 so gap is 6.16821, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (111.423 - 131.915) = 111.423- 131.915
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (125.747 - 136.526), exposure 10.7797
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.09547 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.8641 +/- 6.00015
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=125.747 and stop= 136.526 so gap is 10.7797, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (125.747 - 136.526), with lastBin= 0xaf2b10 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (116.762 - 125.747), exposure 8.98454
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.716049 bg counts (1), with cf=1.12247 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.8702 +/- 6.20032
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 14
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (136.526 - 147.263), exposure 10.737
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.09599 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.8796 +/- 6.00299
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=136.526 and stop= 147.263 so gap is 10.737, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (136.526 - 147.263), with lastBin= 0xaf0fa0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (125.747 - 136.526), exposure 10.7797
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.09547 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.8641 +/- 6.00015
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 15
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (147.263 - 154.779), exposure 7.51583
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 0.716049 bg counts (1), with cf=1.09696 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.2811 +/- 3.72205
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (131.915 - 154.779), exposure 22.8643, 28 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.30789, 1.29443 and 0.989709. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=147.263 and stop= 154.779 so gap is 7.51583, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (154.779) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  492  INFO   >>  Discarding leftover counts, as skip is set and I have no bin to carry back to
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 71.6705
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (154.779) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  787  INFO   >>  I'm on the last event, so save the previous bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (136.526 - 147.263), exposure 10.737
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.09599 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.8796 +/- 6.00299
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 16
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0xaf0fa0
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 71.6705 - 154.779
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 71.6705 - 154.779 the cf is 1.1101
++tructures/grbBin.cpp::        binData:  line  921  INFO   >>  This bin is empty, so found a emptyBin CF of 1.1101
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (71.6705 - 154.779), exposure 83.1088
++taStructures/bin.cpp::        fullBin:  line  192  INFO   >>  Producing an upper limit of 6.56626 given bg=0 and numCts= 0
++tructures/grbBin.cpp::        binData:  line  929  INFO   >>  Not saving this bin as it is an incomplete WT one
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (131.915 - 154.779), exposure 22.8643, 28 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.30789, 1.29443 and 0.989709. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for WT mode.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: WT, with files: wtsourcetotal_incbad.evt, wtbacktotal_incbad.evt, and wtcorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 71.6705 - 3000
++/SourceEventList.cpp::SourceEventList:  line   67  FATAL  >>  Can't open file wtsourcetotal_incbad.evt
++/genlc_cpp/genlc.cpp::           main:  line  388  WARN   >>  Unable to open the files for this mode, skipping
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: PC, with files: pcsourcetotal.evt, pcbacktotal.evt, and pccorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 156.453 - 394860
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	156.453 - 2062
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	5953.69 - 7829.16
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	12004.2 - 13617.2
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	18023.3 - 19399.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	24043.7 - 25182.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	28381.9 - 28931
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	30047.3 - 30965
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	34164.7 - 35187.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	35705 - 36733
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	39947 - 42529.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	45778 - 48302.2
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	51558.7 - 52381.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	57343.4 - 58140.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	63137.2 - 63899.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	64699.2 - 65644.3
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	68934.2 - 70481.2
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	81235.9 - 82620
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	86901.6 - 88380.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	92834.3 - 94200.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	98940 - 100319
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	116755 - 117675
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	191643 - 192851
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - PC mode, suffix = 
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 20 ct/bin at rateFact=10 and binFact= 1.5 with minT 2.51 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file PCCURVE.qdp, reading from pcsourcetotal.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (156.453 - 176.512), exposure 20.0584
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.030974 bg counts (1), with cf=2.60797 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.0786 +/- 11.6635
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=156.453 and stop= 176.512 so gap is 20.0584, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (156.453 - 176.512), with lastBin= 0 and workMinC was 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (176.512 - 216.629), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.15487 bg counts (5), with cf=2.66203 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.8283 +/- 11.9064
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=176.512 and stop= 216.629 so gap is 40.117, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (176.512 - 216.629), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (156.453 - 176.512), exposure 20.0584
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.030974 bg counts (1), with cf=2.60797 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.0786 +/- 11.6635
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (156.453 - 226.658), exposure 70.2047, 20 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.746078, 1.0142 and 1.35938. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=216.629 and stop= 226.658 so gap is 10.0292, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (156.453 - 226.658) = 156.453- 226.658
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (216.629 - 251.731), exposure 35.1023
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.68213 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.4765 +/- 11.9954
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=216.629 and stop= 251.731 so gap is 35.1023, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (216.629 - 251.731), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (176.512 - 216.629), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.15487 bg counts (5), with cf=2.66203 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.8283 +/- 11.9064
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (251.731 - 291.848), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.061948 bg counts (2), with cf=2.68231 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =56.1623 +/- 12.2924
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=251.731 and stop= 291.848 so gap is 40.117, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (251.731 - 291.848), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (216.629 - 251.731), exposure 35.1023
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.68213 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.4765 +/- 11.9954
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (226.658 - 311.906), exposure 85.2485, 20 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.627881, 0.840789 and 1.33909. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=291.848 and stop= 311.906 so gap is 20.0584, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (226.658 - 311.906) = 226.658- 311.906
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (291.848 - 331.965), exposure 40.1169
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.030974 bg counts (1), with cf=2.63497 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.2527 +/- 12.0752
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=291.848 and stop= 331.965 so gap is 40.1169, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (291.848 - 331.965), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (251.731 - 291.848), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.061948 bg counts (2), with cf=2.68231 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =56.1623 +/- 12.2924
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (331.965 - 412.199), exposure 80.2339
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.216818 bg counts (7), with cf=2.64794 and errBG= 0.0819495
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.3846 +/- 11.8439
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=331.965 and stop= 412.199 so gap is 80.2339, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (331.965 - 412.199), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (291.848 - 331.965), exposure 40.1169
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.030974 bg counts (1), with cf=2.63497 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.2527 +/- 12.0752
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (412.199 - 454.823), exposure 42.6243
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.123896 bg counts (4), with cf=2.67604 and errBG= 0.061948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.1893 +/- 11.9688
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.199 and stop= 454.823 so gap is 42.6243, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (412.199 - 454.823), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (331.965 - 412.199), exposure 80.2339
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.216818 bg counts (7), with cf=2.64794 and errBG= 0.0819495
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.3846 +/- 11.8439
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (311.906 - 482.403), exposure 170.497, 21 soft counts and 38 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.325948, 0.587553 and 1.8026. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=454.823 and stop= 482.403 so gap is 27.5804, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (311.906 - 482.403) = 311.906- 482.403
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (454.823 - 494.94), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.68496 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.9684 +/- 12.3054
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=454.823 and stop= 494.94 so gap is 40.117, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (454.823 - 494.94), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (412.199 - 454.823), exposure 42.6243
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.123896 bg counts (4), with cf=2.67604 and errBG= 0.061948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.1893 +/- 11.9688
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (494.94 - 572.667), exposure 77.7266
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.67835 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.8306 +/- 12.2752
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=494.94 and stop= 572.667 so gap is 77.7266, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (494.94 - 572.667), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (454.823 - 494.94), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.68496 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.9684 +/- 12.3054
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (482.403 - 605.261), exposure 122.858, 20 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.432761, 0.477699 and 1.10384. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=572.667 and stop= 605.261 so gap is 32.595, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (482.403 - 605.261) = 482.403- 605.261
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (572.667 - 635.349), exposure 62.6828
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.185844 bg counts (6), with cf=2.67165 and errBG= 0.0758705
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9364 +/- 11.9497
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=572.667 and stop= 635.349 so gap is 62.6828, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (572.667 - 635.349), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (494.94 - 572.667), exposure 77.7266
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.67835 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.8306 +/- 12.2752
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (635.349 - 688.003), exposure 52.6535
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.65617 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9588 +/- 11.8793
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=635.349 and stop= 688.003 so gap is 52.6535, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (635.349 - 688.003), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (572.667 - 635.349), exposure 62.6828
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.185844 bg counts (6), with cf=2.67165 and errBG= 0.0758705
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9364 +/- 11.9497
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (688.003 - 740.656), exposure 52.6535
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.030974 bg counts (1), with cf=2.65245 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9668 +/- 11.8624
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=688.003 and stop= 740.656 so gap is 52.6535, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (688.003 - 740.656), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (635.349 - 688.003), exposure 52.6535
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.65617 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9588 +/- 11.8793
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (605.261 - 778.266), exposure 173.004, 20 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.306942, 0.550421 and 1.79324. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=740.656 and stop= 778.266 so gap is 37.6096, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (605.261 - 778.266) = 605.261- 778.266
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (740.656 - 835.934), exposure 95.2778
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.15487 bg counts (5), with cf=2.67308 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.0475 +/- 11.9558
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=740.656 and stop= 835.934 so gap is 95.2778, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (740.656 - 835.934), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (688.003 - 740.656), exposure 52.6535
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.030974 bg counts (1), with cf=2.65245 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9668 +/- 11.8624
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 12
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (835.934 - 918.675), exposure 82.7413
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.64077 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.0471 +/- 12.1029
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=835.934 and stop= 918.675 so gap is 82.7413, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (835.934 - 918.675), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (740.656 - 835.934), exposure 95.2778
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.15487 bg counts (5), with cf=2.67308 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.0475 +/- 11.9558
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 13
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.266 - 991.387), exposure 213.121, 20 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.24869, 0.397903 and 1.6. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=918.675 and stop= 991.387 so gap is 72.712, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (778.266 - 991.387) = 778.266- 991.387
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (918.675 - 1011.45), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.69056 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.6445 +/- 12.0331
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=918.675 and stop= 1011.45 so gap is 92.7705, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (918.675 - 1011.45), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (835.934 - 918.675), exposure 82.7413
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.64077 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.0471 +/- 12.1029
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 14
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1011.45 - 1084.16), exposure 72.712
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.67327 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.2999 +/- 11.9558
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1011.45 and stop= 1084.16 so gap is 72.712, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1011.45 - 1084.16), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (918.675 - 1011.45), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.69056 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.6445 +/- 12.0331
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 15
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1084.16 - 1186.96), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.30974 bg counts (10), with cf=2.66241 and errBG= 0.0979484
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.4235 +/- 11.9095
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1084.16 and stop= 1186.96 so gap is 102.8, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1084.16 - 1186.96), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1011.45 - 1084.16), exposure 72.712
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.67327 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.2999 +/- 11.9558
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 16
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (991.387 - 1247.13), exposure 255.746, 20 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.207003, 0.371317 and 1.79378. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1186.96 and stop= 1247.13 so gap is 60.1755, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (991.387 - 1247.13) = 991.387- 1247.13
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1186.96 - 1287.25), exposure 100.293
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.123896 bg counts (4), with cf=2.65187 and errBG= 0.061948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.7088 +/- 11.8607
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1186.96 and stop= 1287.25 so gap is 100.293, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1186.96 - 1287.25), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1084.16 - 1186.96), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.30974 bg counts (10), with cf=2.66241 and errBG= 0.0979484
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.4235 +/- 11.9095
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 17
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1287.25 - 1425.15), exposure 137.902
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.247792 bg counts (8), with cf=2.65079 and errBG= 0.0876077
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.359 +/- 11.857
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1287.25 and stop= 1425.15 so gap is 137.902, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1287.25 - 1425.15), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1186.96 - 1287.25), exposure 100.293
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.123896 bg counts (4), with cf=2.65187 and errBG= 0.061948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.7088 +/- 11.8607
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 18
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1425.15 - 1482.82), exposure 57.6682
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.092922 bg counts (3), with cf=2.67746 and errBG= 0.0536486
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.3004 +/- 11.9748
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1247.13 - 1482.82), exposure 235.687, 20 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.22344, 0.291828 and 1.30607. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.15 and stop= 1482.82 so gap is 57.6682, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1425.15 - 1482.82), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1287.25 - 1425.15), exposure 137.902
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.247792 bg counts (8), with cf=2.65079 and errBG= 0.0876077
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.359 +/- 11.857
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 19
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1247.13 - 1482.82) = 1247.13- 1482.82
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1482.82 - 1625.74), exposure 142.917
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.402662 bg counts (13), with cf=2.616 and errBG= 0.111678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.8827 +/- 11.9916
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1482.82 and stop= 1625.74 so gap is 142.917, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1482.82 - 1625.74), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1425.15 - 1482.82), exposure 57.6682
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.092922 bg counts (3), with cf=2.67746 and errBG= 0.0536486
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.3004 +/- 11.9748
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1625.74 - 1741.07), exposure 115.336
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.216818 bg counts (7), with cf=2.61916 and errBG= 0.0819495
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =57.0536 +/- 12.2868
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1625.74 and stop= 1741.07 so gap is 115.336, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1625.74 - 1741.07), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1482.82 - 1625.74), exposure 142.917
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.402662 bg counts (13), with cf=2.616 and errBG= 0.111678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.8827 +/- 11.9916
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 21
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1482.82 - 1826.32), exposure 343.502, 20 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.150643, 0.271215 and 1.80039. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1741.07 and stop= 1826.32 so gap is 85.2486, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1482.82 - 1826.32) = 1482.82- 1826.32
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1741.07 - 1861.42), exposure 120.351
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.061948 bg counts (2), with cf=2.62924 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =57.6805 +/- 12.3328
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1741.07 and stop= 1861.42 so gap is 120.351, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1741.07 - 1861.42), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1625.74 - 1741.07), exposure 115.336
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.216818 bg counts (7), with cf=2.61916 and errBG= 0.0819495
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =57.0536 +/- 12.2868
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 22
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1861.42 - 1949.18), exposure 87.756
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.216818 bg counts (7), with cf=2.67562 and errBG= 0.0819495
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9323 +/- 11.9678
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1861.42 and stop= 1949.18 so gap is 87.756, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1861.42 - 1949.18), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1741.07 - 1861.42), exposure 120.351
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.061948 bg counts (2), with cf=2.62924 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =57.6805 +/- 12.3328
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 23
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1949.18 - 2062), exposure 112.82
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 18 counts and 0.185844 bg counts (6), with cf=2.60639 and errBG= 0.0758705
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.4306 +/- 11.0597
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1826.32 - 2062), exposure 235.679, 19 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.211057, 0.311136 and 1.47418. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1949.18 and stop= 2062 so gap is 112.82, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (2062) and the bin is not full 18 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=112.82 whereas forward=3891.69
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1861.42 - 2062), exposure 200.576
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 38 counts and 0.402662 bg counts (13), with cf=2.64283 and errBG= 0.111678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =99.3633 +/- 16.2942
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (2062) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1482.82 - 2062), exposure 579.18, 39 soft counts and 64 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.175226, 0.287458 and 1.6405. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1861.42 - 2062), with lastBin= 0 and workMinC was 17
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 5953.69
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1482.82 - 2062) = 1482.82- 2062
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 5953.69 - 7829.16


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 2, last was 1 so increasing dead to 0.000188291
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 3, last was 2 so increasing dead to 0.000408351
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5953.69 - 6126.7), exposure 173.004
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.11121 bg counts (5), with cf=2.63275 and errBG= 0.0497345
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.3621 +/- 11.7747
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5953.69 and stop= 6126.7 so gap is 173.004, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (5953.69 - 6126.7), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1861.42 - 2062), exposure 200.576
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 38 counts and 0.402662 bg counts (13), with cf=2.64283 and errBG= 0.111678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =99.3633 +/- 16.2942
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 24
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 4, last was 3 so increasing dead to 0.000440121
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6126.7 - 6262.09), exposure 135.394
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0679808 bg counts (3), with cf=1.85537 and errBG= 0.0392487
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.9812 +/- 8.29777
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (5953.69 - 6262.09), exposure 308.398, 20 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.130494, 0.159127 and 1.21942. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6126.7 and stop= 6262.09 so gap is 135.395, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6126.7 - 6262.09), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5953.69 - 6126.7), exposure 173.004
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.11121 bg counts (5), with cf=2.63275 and errBG= 0.0497345
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.3621 +/- 11.7747
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 25
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (5953.69 - 6262.09) = 5953.69- 6262.09
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6262.09 - 6362.39), exposure 100.292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139099 bg counts (6), with cf=1.22018 and errBG= 0.0567868
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.2339 +/- 5.45727
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6262.09 and stop= 6362.39 so gap is 100.292, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6262.09 - 6362.39), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6126.7 - 6262.09), exposure 135.394
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0679808 bg counts (3), with cf=1.85537 and errBG= 0.0392487
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.9812 +/- 8.29777
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 26
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6262.09 - 6455.16), exposure 193.063, 20 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.125714, 0.099454 and 0.791115. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6362.39 and stop= 6455.16 so gap is 92.7704, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6262.09 - 6457.66), exposure 195.57, 20 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.124102, 0.104504 and 0.842079. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6362.39 and stop= 6457.66 so gap is 95.2777, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6262.09 - 6460.17), exposure 198.077, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.122531, 0.109426 and 0.893043. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6362.39 and stop= 6460.17 so gap is 97.785, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6362.39 - 6465.19), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.208648 bg counts (9), with cf=1.22201 and errBG= 0.0695494
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1853 +/- 5.46567
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6262.09 - 6465.19), exposure 203.092, 21 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.125597, 0.112814 and 0.898226. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6362.39 and stop= 6465.19 so gap is 102.8, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6362.39 - 6465.19), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6262.09 - 6362.39), exposure 100.292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139099 bg counts (6), with cf=1.22018 and errBG= 0.0567868
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.2339 +/- 5.45727
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 27
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6262.09 - 6470.2), exposure 208.107, 21 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.12257, 0.11586 and 0.94525. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6465.19 and stop= 6470.2 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (6262.09 - 6470.2) = 6262.09- 6470.2
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6465.19 - 6588.04), exposure 122.858
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.21263 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.112 +/- 5.42339
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6465.19 and stop= 6588.04 so gap is 122.858, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6465.19 - 6588.04), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6362.39 - 6465.19), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.208648 bg counts (9), with cf=1.22201 and errBG= 0.0695494
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1853 +/- 5.46567
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 28
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6470.2 - 6668.28), exposure 198.077, 20 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.12149, 0.104038 and 0.856355. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6588.04 and stop= 6668.28 so gap is 80.234, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6588.04 - 6673.29), exposure 85.2485
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0463662 bg counts (2), with cf=1.21072 and errBG= 0.0327859
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1582 +/- 5.41464
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6470.2 - 6673.29), exposure 203.092, 20 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.11849, 0.113282 and 0.956042. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6588.04 and stop= 6673.29 so gap is 85.2485, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6588.04 - 6673.29), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6465.19 - 6588.04), exposure 122.858
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.21263 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.112 +/- 5.42339
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 29
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6470.2 - 6675.8), exposure 205.599, 20 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.116909, 0.117734 and 1.00706. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6673.29 and stop= 6675.8 so gap is 2.50734, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (6470.2 - 6675.8) = 6470.2- 6675.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 5, last was 4 so increasing dead to 0.00203985
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6673.29 - 6916.5), exposure 243.207
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.402302 bg counts (18), with cf=2.36558 and errBG= 0.0948235
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.3599 +/- 10.5816
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6673.29 and stop= 6916.5 so gap is 243.209, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6673.29 - 6916.5), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6588.04 - 6673.29), exposure 85.2485
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0463662 bg counts (2), with cf=1.21072 and errBG= 0.0327859
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1582 +/- 5.41464
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 30
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 6, last was 5 so increasing dead to 0.0010401
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6916.5 - 7079.48), exposure 162.974
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.178545 bg counts (8), with cf=1.68405 and errBG= 0.0631251
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.3803 +/- 7.53204
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6916.5 and stop= 7079.48 so gap is 162.975, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6916.5 - 7079.48), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6673.29 - 6916.5), exposure 243.207
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.402302 bg counts (18), with cf=2.36558 and errBG= 0.0948235
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.3599 +/- 10.5816
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 31
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6675.8 - 7099.54), exposure 423.732, 20 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0838933, 0.122028 and 1.45456. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7079.48 and stop= 7099.54 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (6675.8 - 7099.54) = 6675.8- 7099.54
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7079.48 - 7172.25), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.23722 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.601 +/- 5.53339
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7079.48 and stop= 7172.25 so gap is 92.7705, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7079.48 - 7172.25), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6916.5 - 7079.48), exposure 162.974
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.178545 bg counts (8), with cf=1.68405 and errBG= 0.0631251
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.3803 +/- 7.53204
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 32
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7172.25 - 7247.47), exposure 75.2193
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.22757 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.4091 +/- 5.49022
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7172.25 and stop= 7247.47 so gap is 75.2193, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7172.25 - 7247.47), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7079.48 - 7172.25), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.23722 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.601 +/- 5.53339
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 33
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7277.55), exposure 178.019, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.137761, 0.12359 and 0.897135. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7277.55 so gap is 30.0878, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7282.57), exposure 183.034, 21 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.140745, 0.120204 and 0.854057. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7282.57 so gap is 35.1024, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7290.09), exposure 190.556, 21 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.135189, 0.121951 and 0.902074. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7290.09 so gap is 42.6243, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7292.6), exposure 193.063, 22 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.139645, 0.120367 and 0.861948. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7292.6 so gap is 45.1316, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7295.11), exposure 195.57, 23 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.143987, 0.118824 and 0.82524. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7295.11 so gap is 47.639, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7297.61), exposure 198.078, 24 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.148219, 0.11732 and 0.791531. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7297.61 so gap is 50.1463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7302.63), exposure 203.092, 25 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.15065, 0.120373 and 0.799023. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7302.63 so gap is 55.1609, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (7099.54 - 7302.63) = 7099.54- 7302.63
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7247.47 - 7347.76), exposure 100.293
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.162282 bg counts (7), with cf=1.22001 and errBG= 0.0613368
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.2022 +/- 5.45656
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7347.76 so gap is 100.293, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7247.47 - 7347.76), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7172.25 - 7247.47), exposure 75.2193
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.22757 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.4091 +/- 5.49022
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 34
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7347.76 - 7448.05), exposure 100.292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139099 bg counts (6), with cf=1.23519 and errBG= 0.0567868
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.5319 +/- 5.52437
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7347.76 and stop= 7448.05 so gap is 100.292, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7347.76 - 7448.05), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7247.47 - 7347.76), exposure 100.293
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.162282 bg counts (7), with cf=1.22001 and errBG= 0.0613368
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.2022 +/- 5.45656
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 35
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 7, last was 6 so increasing dead to 0.00220001
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7448.05 - 7575.92), exposure 127.871
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.113609 bg counts (5), with cf=2.07781 and errBG= 0.0508074
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.3201 +/- 9.29285
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7448.05 and stop= 7575.92 so gap is 127.873, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7448.05 - 7575.92), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7347.76 - 7448.05), exposure 100.292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139099 bg counts (6), with cf=1.23519 and errBG= 0.0567868
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.5319 +/- 5.52437
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 36
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 7
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7302.63 - 7595.98), exposure 293.353, 20 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.105808, 0.191162 and 1.80668. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7575.92 and stop= 7595.98 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (7302.63 - 7595.98) = 7302.63- 7595.98
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7575.92 - 7696.28), exposure 120.351
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.113609 bg counts (5), with cf=2.22183 and errBG= 0.0508074
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.1842 +/- 9.93696
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7575.92 and stop= 7696.28 so gap is 120.351, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7575.92 - 7696.28), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7448.05 - 7575.92), exposure 127.871
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.113609 bg counts (5), with cf=2.07781 and errBG= 0.0508074
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.3201 +/- 9.29285
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 37
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 7
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 8, last was 7 so increasing dead to 0.00131994
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7696.28 - 7829.16), exposure 132.886
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.392729 bg counts (17), with cf=1.45435 and errBG= 0.0952508
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.6984 +/- 5.81903
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7595.98 - 7829.16), exposure 233.178, 12 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0890133, 0.147237 and 1.65411. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7696.28 and stop= 7829.16 so gap is 132.887, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 1 (7829.16) and the bin is not full 16 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=132.887 whereas forward=4175.05
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7575.92 - 7829.16), exposure 253.237
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 36 counts and 0.506338 bg counts (22), with cf=1.88073 and errBG= 0.107952
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =66.7538 +/- 11.2862
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 1 (7829.16) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7302.63 - 7829.16), exposure 526.532, 32 soft counts and 52 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0984137, 0.171722 and 1.7449. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7575.92 - 7829.16), with lastBin= 0 and workMinC was 15
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 12004.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (7302.63 - 7829.16) = 7302.63- 7829.16
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 12004.2 - 13617.2


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12004.2 - 12174.7), exposure 170.497
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.140995 bg counts (6), with cf=1.20298 and errBG= 0.0575609
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8901 +/- 5.38035
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12004.2 and stop= 12174.7 so gap is 170.497, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12004.2 - 12174.7), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7575.92 - 7829.16), exposure 253.237
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 36 counts and 0.506338 bg counts (22), with cf=1.88073 and errBG= 0.107952
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =66.7538 +/- 11.2862
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 38
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12174.7 - 12370.3), exposure 195.57
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.399485 bg counts (17), with cf=1.20285 and errBG= 0.0968895
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.7792 +/- 5.51336
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12174.7 and stop= 12370.3 so gap is 195.57, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12174.7 - 12370.3), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12004.2 - 12174.7), exposure 170.497
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.140995 bg counts (6), with cf=1.20298 and errBG= 0.0575609
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8901 +/- 5.38035
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 39
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (12004.2 - 12377.8), exposure 373.589, 20 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0634186, 0.0732786 and 1.15547. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12370.3 and stop= 12377.8 so gap is 7.52194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (12004.2 - 12377.8) = 12004.2- 12377.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12370.3 - 12483.1), exposure 112.829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0234991 bg counts (1), with cf=1.19924 and errBG= 0.0234991
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9566 +/- 5.36323
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12370.3 and stop= 12483.1 so gap is 112.829, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12370.3 - 12483.1), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12174.7 - 12370.3), exposure 195.57
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.399485 bg counts (17), with cf=1.20285 and errBG= 0.0968895
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.7792 +/- 5.51336
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 40
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12483.1 - 12633.5), exposure 150.439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.187993 bg counts (8), with cf=1.20313 and errBG= 0.0664656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8365 +/- 5.38117
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12483.1 and stop= 12633.5 so gap is 150.439, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12483.1 - 12633.5), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12370.3 - 12483.1), exposure 112.829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0234991 bg counts (1), with cf=1.19924 and errBG= 0.0234991
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9566 +/- 5.36323
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 41
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (12377.8 - 12698.7), exposure 320.936, 20 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0741611, 0.100369 and 1.3534. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12633.5 and stop= 12698.7 so gap is 65.1901, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (12377.8 - 12698.7) = 12377.8- 12698.7
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12633.5 - 12801.5), exposure 167.99
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.446484 bg counts (19), with cf=1.21274 and errBG= 0.10243
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.7133 +/- 5.42495
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12633.5 and stop= 12801.5 so gap is 167.99, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12633.5 - 12801.5), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12483.1 - 12633.5), exposure 150.439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.187993 bg counts (8), with cf=1.20313 and errBG= 0.0664656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8365 +/- 5.38117
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 42
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12801.5 - 12987.1), exposure 185.541
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.211492 bg counts (9), with cf=1.20879 and errBG= 0.0704974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9201 +/- 5.40654
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12801.5 and stop= 12987.1 so gap is 185.541, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12801.5 - 12987.1), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12633.5 - 12801.5), exposure 167.99
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.446484 bg counts (19), with cf=1.21274 and errBG= 0.10243
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.7133 +/- 5.42495
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 43
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (12698.7 - 13037.2), exposure 338.487, 20 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0707448, 0.0777863 and 1.09953. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12987.1 and stop= 13037.2 so gap is 50.1462, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (12698.7 - 13037.2) = 12698.7- 13037.2
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12987.1 - 13079.8), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.211492 bg counts (9), with cf=1.20708 and errBG= 0.0704974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8863 +/- 5.39889
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12987.1 and stop= 13079.8 so gap is 92.7705, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12987.1 - 13079.8), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12801.5 - 12987.1), exposure 185.541
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.211492 bg counts (9), with cf=1.20879 and errBG= 0.0704974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9201 +/- 5.40654
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 44
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13079.8 - 13210.2), exposure 130.38
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0469983 bg counts (2), with cf=1.209 and errBG= 0.0332328
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1231 +/- 5.40695
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13079.8 and stop= 13210.2 so gap is 130.38, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13079.8 - 13210.2), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12987.1 - 13079.8), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.211492 bg counts (9), with cf=1.20708 and errBG= 0.0704974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8863 +/- 5.39889
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 45
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (13037.2 - 13265.4), exposure 228.165, 18 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0946368, 0.0783682 and 0.828094. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13210.2 and stop= 13265.4 so gap is 55.1609, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (13037.2 - 13265.4) = 13037.2- 13265.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13210.2 - 13393.3), exposure 183.034
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.187993 bg counts (8), with cf=1.20219 and errBG= 0.0664656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.8068 +/- 4.65674
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13210.2 and stop= 13393.3 so gap is 183.034, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13210.2 - 13393.3), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13079.8 - 13210.2), exposure 130.38
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0469983 bg counts (2), with cf=1.209 and errBG= 0.0332328
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1231 +/- 5.40695
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 46
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 10, last was 9 so increasing dead to 26.8755
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 10 so increasing dead to 53.6868
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 12, last was 11 so increasing dead to 81.0743
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13393.3 - 13617.2), exposure 142.91
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 19 counts and 0.446484 bg counts (19), with cf=1.20154 and errBG= 0.10243
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.2928 +/- 5.23883
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (13265.4 - 13617.2), exposure 270.783, 10 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0424241, 0.088217 and 2.07941. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13393.3 and stop= 13617.2 so gap is 223.985, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 2 (13617.2) and the bin is not full 19 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=223.985 whereas forward=4406.02
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13210.2 - 13617.2), exposure 325.944
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 34 counts and 0.634477 bg counts (27), with cf=1.20182 and errBG= 0.122105
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =40.0995 +/- 7.00932
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 2 (13617.2) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (13037.2 - 13617.2), exposure 498.949, 28 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0662975, 0.0837138 and 1.2627. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13210.2 - 13617.2), with lastBin= 0 and workMinC was 13
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 18023.3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (13037.2 - 13617.2) = 13037.2- 13617.2
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 18023.3 - 19399.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18023.3 - 18261.5), exposure 238.194
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.181616 bg counts (13), with cf=1.71434 and errBG= 0.0503712
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =35.6899 +/- 7.85659
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18023.3 and stop= 18261.5 so gap is 238.194, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18023.3 - 18261.5), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13210.2 - 13617.2), exposure 325.944
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 34 counts and 0.634477 bg counts (27), with cf=1.20182 and errBG= 0.122105
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =40.0995 +/- 7.00932
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 47
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18261.5 - 18494.6), exposure 233.18
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.209557 bg counts (15), with cf=1.76034 and errBG= 0.0541073
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.8378 +/- 7.87304
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18261.5 and stop= 18494.6 so gap is 233.18, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18261.5 - 18494.6), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18023.3 - 18261.5), exposure 238.194
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.181616 bg counts (13), with cf=1.71434 and errBG= 0.0503712
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =35.6899 +/- 7.85659
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 48
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (18023.3 - 18607.5), exposure 584.203, 20 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.059109, 0.0911361 and 1.54183. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18494.6 and stop= 18607.5 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (18023.3 - 18607.5) = 18023.3- 18607.5
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18494.6 - 18700.2), exposure 205.599
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139704 bg counts (10), with cf=1.74818 and errBG= 0.0441784
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.7193 +/- 7.81847
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18494.6 and stop= 18700.2 so gap is 205.599, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18494.6 - 18700.2), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18261.5 - 18494.6), exposure 233.18
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.209557 bg counts (15), with cf=1.76034 and errBG= 0.0541073
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.8378 +/- 7.87304
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 49
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18700.2 - 19018.7), exposure 318.428
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.167645 bg counts (12), with cf=1.79138 and errBG= 0.048395
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.5704 +/- 6.93854
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18700.2 and stop= 19018.7 so gap is 318.428, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18700.2 - 19018.7), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18494.6 - 18700.2), exposure 205.599
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139704 bg counts (10), with cf=1.74818 and errBG= 0.0441784
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.7193 +/- 7.81847
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 50
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (18607.5 - 19091.4), exposure 483.911, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0585319, 0.0435764 and 0.74449. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19018.7 and stop= 19091.4 so gap is 72.712, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (18607.5 - 19269.4), exposure 661.93, 20 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0539224, 0.0533226 and 0.988877. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19018.7 and stop= 19269.4 so gap is 250.731, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (18607.5 - 19269.4) = 18607.5- 19269.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (19018.7 - 19399.8), exposure 381.106
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.32132 bg counts (23), with cf=1.8453 and errBG= 0.0669999
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.3131 +/- 8.25337
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (19269.4 - 19399.8), exposure 130.375, 2 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0282353, 0.0437007 and 1.54773. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19018.7 and stop= 19399.8 so gap is 381.106, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 3 (19399.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (18607.5 - 19399.8), exposure 792.305, 22 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0496963, 0.051735 and 1.04102. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (19018.7 - 19399.8), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18700.2 - 19018.7), exposure 318.428
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.167645 bg counts (12), with cf=1.79138 and errBG= 0.048395
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.5704 +/- 6.93854
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 51
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 24043.7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 14
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (18607.5 - 19399.8) = 18607.5- 19399.8
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 24043.7 - 25182.1


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24043.7 - 24261.8), exposure 218.136
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.135399 bg counts (9), with cf=1.28098 and errBG= 0.0451328
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0413 +/- 4.96155
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24043.7 and stop= 24261.8 so gap is 218.136, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (24043.7 - 24261.8), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (19018.7 - 19399.8), exposure 381.106
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.32132 bg counts (23), with cf=1.8453 and errBG= 0.0669999
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.3131 +/- 8.25337
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 52
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 14
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24261.8 - 24487.5), exposure 225.658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.150443 bg counts (10), with cf=1.27001 and errBG= 0.0475742
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8591 +/- 4.9191
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24261.8 and stop= 24487.5 so gap is 225.658, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (24261.8 - 24487.5), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24043.7 - 24261.8), exposure 218.136
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.135399 bg counts (9), with cf=1.28098 and errBG= 0.0451328
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0413 +/- 4.96155
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 53
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 14
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (24043.7 - 24530.1), exposure 486.418, 15 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0388497, 0.0468105 and 1.20491. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24487.5 and stop= 24530.1 so gap is 42.6242, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (24043.7 - 24530.1) = 24043.7- 24530.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24487.5 - 24685.6), exposure 198.077
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0601771 bg counts (4), with cf=1.26724 and errBG= 0.0300886
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9323 +/- 4.90814
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24487.5 and stop= 24685.6 so gap is 198.077, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (24487.5 - 24685.6), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24261.8 - 24487.5), exposure 225.658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.150443 bg counts (10), with cf=1.27001 and errBG= 0.0475742
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8591 +/- 4.9191
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 54
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 14
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24685.6 - 24881.1), exposure 195.57
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.21062 bg counts (14), with cf=1.26732 and errBG= 0.0562905
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7429 +/- 4.90885
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24685.6 and stop= 24881.1 so gap is 195.57, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (24685.6 - 24881.1), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24487.5 - 24685.6), exposure 198.077
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0601771 bg counts (4), with cf=1.26724 and errBG= 0.0300886
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9323 +/- 4.90814
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 55
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 14
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (24530.1 - 24926.3), exposure 396.155, 15 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0475441, 0.0443253 and 0.9323. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24881.1 and stop= 24926.3 so gap is 45.1316, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (24530.1 - 24976.4), exposure 446.301, 15 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0421168, 0.0421729 and 1.00133. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24881.1 and stop= 24976.4 so gap is 95.2777, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (24530.1 - 24976.4) = 24530.1- 24976.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24881.1 - 25121.8), exposure 240.702
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.436284 bg counts (29), with cf=1.2647 and errBG= 0.0810159
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.4188 +/- 4.89924
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24881.1 and stop= 25121.8 so gap is 240.702, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (24881.1 - 25121.8), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24685.6 - 24881.1), exposure 195.57
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.21062 bg counts (14), with cf=1.26732 and errBG= 0.0562905
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7429 +/- 4.90885
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 56
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 14
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 15, last was 14 so increasing dead to 27.6609
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (25121.8 - 25182.1), exposure 32.5914
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.63186 bg counts (42), with cf=1.26188 and errBG= 0.0974981
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =5.51206 +/- 2.82433
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (24976.4 - 25182.1), exposure 178.015, 12 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0785639, 0.0350145 and 0.445682. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25121.8 and stop= 25182.1 so gap is 60.2524, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 4 (25182.1) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=60.2524 whereas forward=3199.81
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24881.1 - 25182.1), exposure 273.293
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 1.06814 bg counts (71), with cf=1.264 and errBG= 0.126765
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9298 +/- 5.65503
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 4 (25182.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (24530.1 - 25182.1), exposure 624.316, 27 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0525098, 0.0401318 and 0.764272. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (24881.1 - 25182.1), with lastBin= 0 and workMinC was 13
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 28381.9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 16
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (24530.1 - 25182.1) = 24530.1- 25182.1
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 28381.9 - 28931


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28381.9 - 28692.8), exposure 310.906
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.128918 bg counts (15), with cf=1.33151 and errBG= 0.0332865
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.801 +/- 5.15711
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28381.9 and stop= 28692.8 so gap is 310.906, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28381.9 - 28692.8), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24881.1 - 25182.1), exposure 273.293
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 1.06814 bg counts (71), with cf=1.264 and errBG= 0.126765
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9298 +/- 5.65503
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 57
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 16
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28692.8 - 28931), exposure 238.193
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.171891 bg counts (20), with cf=1.33324 and errBG= 0.0384359
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.4367 +/- 3.77131
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28381.9 - 28931), exposure 549.099, 12 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0284468, 0.0266212 and 0.935823. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28692.8 and stop= 28931 so gap is 238.193, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 5 (28931) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=238.193 whereas forward=1116.31
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28381.9 - 28931), exposure 549.099
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.300809 bg counts (35), with cf=1.33211 and errBG= 0.0508459
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.2378 +/- 6.38894
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 5 (28931) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28381.9 - 28931), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 30047.3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 17
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 30047.3 - 30965


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28381.9 - 30147.6), exposure 649.391, 16 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0317821, 0.0262198 and 0.824986. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30047.3 and stop= 30147.6 so gap is 100.292, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28381.9 - 30157.6), exposure 659.42, 16 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0312987, 0.0277246 and 0.885807. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30047.3 and stop= 30157.6 so gap is 110.322, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28381.9 - 30160.1), exposure 661.928, 16 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0311802, 0.029577 and 0.948583. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30047.3 and stop= 30160.1 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (28381.9 - 30160.1) = 28381.9- 30160.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30047.3 - 30245.4), exposure 198.077
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.151501 bg counts (10), with cf=1.26245 and errBG= 0.0479089
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7454 +/- 4.88981
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30047.3 and stop= 30245.4 so gap is 198.077, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (30047.3 - 30245.4), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28381.9 - 28931), exposure 549.099
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.300809 bg counts (35), with cf=1.33211 and errBG= 0.0508459
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.2378 +/- 6.38894
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 58
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 17
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30245.4 - 30481.1), exposure 235.687
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.181801 bg counts (12), with cf=1.2586 and errBG= 0.0524815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.1674 +/- 5.18977
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30245.4 and stop= 30481.1 so gap is 235.687, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (30245.4 - 30481.1), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30047.3 - 30245.4), exposure 198.077
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.151501 bg counts (10), with cf=1.26245 and errBG= 0.0479089
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7454 +/- 4.88981
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 59
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 17
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (30160.1 - 30674.1), exposure 513.998, 15 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0364183, 0.0460029 and 1.26318. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30481.1 and stop= 30674.1 so gap is 193.063, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (30160.1 - 30674.1) = 30160.1- 30674.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30481.1 - 30719.3), exposure 238.194
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.227252 bg counts (15), with cf=1.26184 and errBG= 0.0586761
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6409 +/- 4.88765
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30481.1 and stop= 30719.3 so gap is 238.194, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (30481.1 - 30719.3), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30245.4 - 30481.1), exposure 235.687
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.181801 bg counts (12), with cf=1.2586 and errBG= 0.0524815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.1674 +/- 5.18977
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 60
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 17
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 19, last was 17 so increasing dead to 27.5214
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 19, last was 17 so increasing dead to 55.6248
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 20, last was 19 so increasing dead to 82.8063
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30719.3 - 30965), exposure 162.972
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.469654 bg counts (31), with cf=1.25391 and errBG= 0.0843523
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.18849 +/- 3.31923
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (30674.1 - 30965), exposure 208.104, 5 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0273893, 0.0418041 and 1.52629. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30719.3 and stop= 30965 so gap is 245.778, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 6 (30965) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=245.778 whereas forward=3199.67
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30481.1 - 30965), exposure 401.166
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.696905 bg counts (46), with cf=1.25932 and errBG= 0.102753
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.8274 +/- 5.90815
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 6 (30965) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (30160.1 - 30965), exposure 722.102, 20 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0338129, 0.0447932 and 1.32474. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (30481.1 - 30965), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 34164.7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (30160.1 - 30965) = 30160.1- 30965
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 34164.7 - 35187.7


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34164.7 - 34593.5), exposure 428.749
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.186854 bg counts (22), with cf=1.40176 and errBG= 0.0398374
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.7644 +/- 5.42927
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34164.7 and stop= 34593.5 so gap is 428.749, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34164.7 - 34593.5), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30481.1 - 30965), exposure 401.166
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.696905 bg counts (46), with cf=1.25932 and errBG= 0.102753
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.8274 +/- 5.90815
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 61
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34593.5 - 34881.8), exposure 288.34
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.135894 bg counts (16), with cf=1.38489 and errBG= 0.0339734
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.5851 +/- 5.36386
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34164.7 - 34881.8), exposure 717.09, 15 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0289428, 0.0287208 and 0.992329. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34593.5 and stop= 34881.8 so gap is 288.34, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34593.5 - 34881.8), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34164.7 - 34593.5), exposure 428.749
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.186854 bg counts (22), with cf=1.40176 and errBG= 0.0398374
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.7644 +/- 5.42927
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 62
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (34164.7 - 34881.8) = 34164.7- 34881.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34881.8 - 35157.6), exposure 275.804
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.212334 bg counts (25), with cf=1.37382 and errBG= 0.0424668
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.3156 +/- 5.32112
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34881.8 and stop= 35157.6 so gap is 275.804, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34881.8 - 35157.6), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34593.5 - 34881.8), exposure 288.34
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.135894 bg counts (16), with cf=1.38489 and errBG= 0.0339734
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.5851 +/- 5.36386
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 63
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 21
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (35157.6 - 35187.7), exposure 30.085
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0849335 bg counts (10), with cf=1.39722 and errBG= 0.0268583
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.27855 +/- 1.39773
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34881.8 - 35187.7), exposure 305.889, 5 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0221112, 0.0484886 and 2.19294. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35157.6 and stop= 35187.7 so gap is 30.085, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 7 (35187.7) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=30.085 whereas forward=517.359
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34881.8 - 35187.7), exposure 305.889
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.297267 bg counts (35), with cf=1.37529 and errBG= 0.0502474
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.5957 +/- 5.50158
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 7 (35187.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34164.7 - 35187.7), exposure 1022.98, 20 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0268994, 0.034631 and 1.28743. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34881.8 - 35187.7), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 35705
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 22
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (34164.7 - 35187.7) = 34164.7- 35187.7
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 35705 - 36733


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (35705 - 36033.5), exposure 328.458
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.203937 bg counts (24), with cf=1.38719 and errBG= 0.0416285
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.5249 +/- 5.37286
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35705 and stop= 36033.5 so gap is 328.458, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (35705 - 36033.5), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34881.8 - 35187.7), exposure 305.889
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.297267 bg counts (35), with cf=1.37529 and errBG= 0.0502474
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.5957 +/- 5.50158
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 64
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 22
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (36033.5 - 36306.8), exposure 273.297
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0934711 bg counts (11), with cf=1.40446 and errBG= 0.0281826
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.9578 +/- 6.28104
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=36033.5 and stop= 36306.8 so gap is 273.297, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (36033.5 - 36306.8), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (35705 - 36033.5), exposure 328.458
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.203937 bg counts (24), with cf=1.38719 and errBG= 0.0416285
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.5249 +/- 5.37286
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 65
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 22
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (35705 - 36324.4), exposure 619.306, 17 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0379931, 0.0424904 and 1.11837. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=36306.8 and stop= 36324.4 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (35705 - 36324.4) = 35705- 36324.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 23, last was 22 so increasing dead to 27.3841
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (36306.8 - 36733), exposure 371.078
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.747769 bg counts (88), with cf=1.39676 and errBG= 0.0797124
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.73289 +/- 3.69717
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (36324.4 - 36733), exposure 353.527, 3 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00950963, 0.0112884 and 1.18705. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=36306.8 and stop= 36733 so gap is 426.189, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 8 (36733) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=426.189 whereas forward=3214
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (36033.5 - 36733), exposure 644.375
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.84124 bg counts (99), with cf=1.40246 and errBG= 0.0845478
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.6867 +/- 7.28837
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 8 (36733) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (35705 - 36733), exposure 972.832, 20 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.02766, 0.0311501 and 1.12618. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (36033.5 - 36733), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 39947
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 25
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (35705 - 36733) = 35705- 36733
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 39947 - 42529.5


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (39947 - 40230.3), exposure 283.326
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121816 bg counts (14), with cf=1.30529 and errBG= 0.0325568
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4203 +/- 5.05553
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=39947 and stop= 40230.3 so gap is 283.326, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (39947 - 40230.3), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (36033.5 - 36733), exposure 644.375
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.84124 bg counts (99), with cf=1.40246 and errBG= 0.0845478
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.6867 +/- 7.28837
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 66
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 25
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40230.3 - 40563.8), exposure 333.472
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.217529 bg counts (25), with cf=1.31396 and errBG= 0.0435059
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4236 +/- 5.08927
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40230.3 and stop= 40563.8 so gap is 333.472, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (40230.3 - 40563.8), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (39947 - 40230.3), exposure 283.326
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121816 bg counts (14), with cf=1.30529 and errBG= 0.0325568
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4203 +/- 5.05553
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 67
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 25
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (39947 - 40784.4), exposure 837.441, 15 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0230164, 0.0372461 and 1.61824. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40563.8 and stop= 40784.4 so gap is 220.643, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (39947 - 40784.4) = 39947- 40784.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40563.8 - 40962.5), exposure 398.662
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.113115 bg counts (13), with cf=1.30203 and errBG= 0.0313725
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.6852 +/- 5.20827
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40563.8 and stop= 40962.5 so gap is 398.662, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (40563.8 - 40962.5), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40230.3 - 40563.8), exposure 333.472
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.217529 bg counts (25), with cf=1.31396 and errBG= 0.0435059
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4236 +/- 5.08927
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 68
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 25
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40962.5 - 41190.6), exposure 228.165
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0696094 bg counts (8), with cf=1.30539 and errBG= 0.0246106
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.49 +/- 5.05586
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40962.5 and stop= 41190.6 so gap is 228.165, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (40962.5 - 41190.6), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40563.8 - 40962.5), exposure 398.662
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.113115 bg counts (13), with cf=1.30203 and errBG= 0.0313725
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.6852 +/- 5.20827
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 69
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 25
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (40784.4 - 41476.5), exposure 692.017, 15 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0280171, 0.0261149 and 0.932103. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41190.6 and stop= 41476.5 so gap is 285.833, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (40784.4 - 41494), exposure 709.568, 16 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0292127, 0.0254529 and 0.871298. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41190.6 and stop= 41494 so gap is 303.384, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (40784.4 - 41519.1), exposure 734.641, 17 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0299808, 0.0245842 and 0.82. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41190.6 and stop= 41519.1 so gap is 328.457, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (40784.4 - 41524.1), exposure 739.656, 17 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0297775, 0.0261704 and 0.878866. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41190.6 and stop= 41524.1 so gap is 333.472, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (40784.4 - 41524.1) = 40784.4- 41524.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (41190.6 - 41762.3), exposure 571.667
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.208828 bg counts (24), with cf=1.30248 and errBG= 0.0426269
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.2652 +/- 5.04479
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41190.6 and stop= 41762.3 so gap is 571.667, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (41190.6 - 41762.3), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40962.5 - 41190.6), exposure 228.165
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0696094 bg counts (8), with cf=1.30539 and errBG= 0.0246106
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.49 +/- 5.05586
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 70
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 25
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (41762.3 - 42228.6), exposure 466.36
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.165322 bg counts (19), with cf=1.31097 and errBG= 0.0379275
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4478 +/- 5.0776
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41762.3 and stop= 42228.6 so gap is 466.36, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (41762.3 - 42228.6), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (41190.6 - 41762.3), exposure 571.667
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.208828 bg counts (24), with cf=1.30248 and errBG= 0.0426269
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.2652 +/- 5.04479
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 71
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 25
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (42228.6 - 42529.5), exposure 300.868
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 0.304541 bg counts (35), with cf=1.30615 and errBG= 0.0514768
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.3576 +/- 3.91902
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (41524.1 - 42529.5), exposure 1005.42, 13 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0164632, 0.0205777 and 1.24992. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=42228.6 and stop= 42529.5 so gap is 300.868, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 9 (42529.5) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=300.868 whereas forward=3248.51
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (41762.3 - 42529.5), exposure 767.228
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.469863 bg counts (54), with cf=1.30916 and errBG= 0.0639403
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.8047 +/- 6.4141
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 9 (42529.5) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (40784.4 - 42529.5), exposure 1745.08, 30 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0221067, 0.0229483 and 1.03807. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (41762.3 - 42529.5), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 45778
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (40784.4 - 42529.5) = 40784.4- 42529.5
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 45778 - 48302.2


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (45778 - 46053.8), exposure 275.804
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0865722 bg counts (11), with cf=1.31288 and errBG= 0.0261025
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5796 +/- 5.08489
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=45778 and stop= 46053.8 so gap is 275.804, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (45778 - 46053.8), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (41762.3 - 42529.5), exposure 767.228
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.469863 bg counts (54), with cf=1.30916 and errBG= 0.0639403
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.8047 +/- 6.4141
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 72
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46289.5), exposure 511.49, 15 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.038327, 0.0256974 and 0.670477. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46289.5 so gap is 235.687, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46297), exposure 519.012, 16 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0402859, 0.025325 and 0.62863. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46297 so gap is 243.209, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46317.1), exposure 539.071, 16 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0387869, 0.0268034 and 0.691041. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46317.1 so gap is 263.267, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46319.6), exposure 541.578, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0386074, 0.029108 and 0.753949. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46319.6 so gap is 265.774, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46362.2), exposure 584.202, 16 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0357905, 0.0292415 and 0.817018. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46362.2 so gap is 308.399, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46053.8 - 46372.3), exposure 318.428
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.110183 bg counts (14), with cf=1.32749 and errBG= 0.0294476
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7661 +/- 5.1415
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46372.3), exposure 594.231, 16 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0351865, 0.0310267 and 0.881781. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46372.3 so gap is 318.428, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (46053.8 - 46372.3), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (45778 - 46053.8), exposure 275.804
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0865722 bg counts (11), with cf=1.31288 and errBG= 0.0261025
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5796 +/- 5.08489
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 73
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46402.3), exposure 624.319, 16 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0334575, 0.0316407 and 0.945699. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46372.3 and stop= 46402.3 so gap is 30.0877, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (45778 - 46402.3) = 45778- 46402.3
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46372.3 - 46680.7), exposure 308.399
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.110183 bg counts (14), with cf=1.32022 and errBG= 0.0294476
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6578 +/- 5.11334
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46372.3 and stop= 46680.7 so gap is 308.399, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (46372.3 - 46680.7), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46053.8 - 46372.3), exposure 318.428
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.110183 bg counts (14), with cf=1.32749 and errBG= 0.0294476
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7661 +/- 5.1415
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 74
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46680.7 - 47127), exposure 446.301
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.173144 bg counts (22), with cf=1.32096 and errBG= 0.0369145
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5856 +/- 5.11627
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46680.7 and stop= 47127 so gap is 446.301, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (46680.7 - 47127), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46372.3 - 46680.7), exposure 308.399
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.110183 bg counts (14), with cf=1.32022 and errBG= 0.0294476
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6578 +/- 5.11334
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 75
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46402.3 - 47214.7), exposure 812.367, 15 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0240993, 0.02582 and 1.0714. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47127 and stop= 47214.7 so gap is 87.7558, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (46402.3 - 47214.7) = 46402.3- 47214.7
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47127 - 47548.2), exposure 421.228
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.141664 bg counts (18), with cf=1.31955 and errBG= 0.0333904
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6063 +/- 5.11078
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47127 and stop= 47548.2 so gap is 421.228, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (47127 - 47548.2), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46680.7 - 47127), exposure 446.301
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.173144 bg counts (22), with cf=1.32096 and errBG= 0.0369145
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5856 +/- 5.11627
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 76
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47548.2 - 47911.7), exposure 363.56
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.149534 bg counts (19), with cf=1.32489 and errBG= 0.0343054
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6753 +/- 5.13149
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47548.2 and stop= 47911.7 so gap is 363.56, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (47548.2 - 47911.7), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47127 - 47548.2), exposure 421.228
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.141664 bg counts (18), with cf=1.31955 and errBG= 0.0333904
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6063 +/- 5.11078
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 77
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (47214.7 - 47946.8), exposure 732.134, 15 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0268513, 0.0250026 and 0.931148. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47911.7 and stop= 47946.8 so gap is 35.1023, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (47214.7 - 47951.9), exposure 737.149, 15 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0266687, 0.0266219 and 0.998245. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47911.7 and stop= 47951.9 so gap is 40.1169, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (47214.7 - 47951.9) = 47214.7- 47951.9
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47911.7 - 48302.2), exposure 363.553
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 0.362029 bg counts (46), with cf=1.32754 and errBG= 0.0533783
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.1223 +/- 4.40351
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (47951.9 - 48302.2), exposure 323.436, 5 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0193503, 0.0162547 and 0.840024. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47911.7 and stop= 48302.2 so gap is 390.429, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 10 (48302.2) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=390.429 whereas forward=3256.51
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47548.2 - 48302.2), exposure 727.112
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.511563 bg counts (65), with cf=1.32601 and errBG= 0.0634516
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.798 +/- 6.76188
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 10 (48302.2) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (47214.7 - 48302.2), exposure 1060.58, 20 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0244372, 0.0234605 and 0.960031. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (47548.2 - 48302.2), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 51558.7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 28
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (47214.7 - 48302.2) = 47214.7- 48302.2
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 51558.7 - 52381.1


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (51558.7 - 52320.9), exposure 762.221
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.344861 bg counts (44), with cf=1.32488 and errBG= 0.0519898
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4163 +/- 5.13169
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=51558.7 and stop= 52320.9 so gap is 762.221, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (51558.7 - 52320.9), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47548.2 - 48302.2), exposure 727.112
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.511563 bg counts (65), with cf=1.32601 and errBG= 0.0634516
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.798 +/- 6.76188
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 78
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 28
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52320.9 - 52381.1), exposure 60.1738
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.0156755 bg counts (2), with cf=1.3489 and errBG= 0.0110843
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.67666 +/- 1.90769
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51558.7 - 52381.1), exposure 822.394, 7 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0111581, 0.0157056 and 1.40755. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52320.9 and stop= 52381.1 so gap is 60.1738, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 11 (52381.1) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=60.1738 whereas forward=4962.37
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (51558.7 - 52381.1), exposure 822.394
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.360537 bg counts (46), with cf=1.3277 and errBG= 0.0531582
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.0923 +/- 5.47471
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 11 (52381.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (51558.7 - 52381.1), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 57343.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 29
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 57343.4 - 58140.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57343.4 - 57651.8), exposure 308.399
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0859911 bg counts (11), with cf=1.34615 and errBG= 0.0259273
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.0765 +/- 5.21374
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57343.4 and stop= 57651.8 so gap is 308.399, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (57343.4 - 57651.8), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (51558.7 - 52381.1), exposure 822.394
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.360537 bg counts (46), with cf=1.3277 and errBG= 0.0531582
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.0923 +/- 5.47471
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 79
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 29
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51558.7 - 57722.1), exposure 1201, 15 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.016504, 0.0229736 and 1.392. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57651.8 and stop= 57722.1 so gap is 70.2046, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (51558.7 - 57722.1) = 51558.7- 57722.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57651.8 - 58140.8), exposure 488.922
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.171982 bg counts (22), with cf=1.34448 and errBG= 0.0366667
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.247 +/- 4.84783
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (57722.1 - 58140.8), exposure 418.718, 6 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0191093, 0.00954959 and 0.499734. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57651.8 and stop= 58140.8 so gap is 488.922, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 12 (58140.8) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=488.922 whereas forward=4996.46
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57343.4 - 58140.8), exposure 797.321
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.257973 bg counts (33), with cf=1.34537 and errBG= 0.0449074
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =37.3234 +/- 7.1193
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 12 (58140.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51558.7 - 58140.8), exposure 1619.72, 21 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0171776, 0.0195038 and 1.13542. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (57343.4 - 58140.8), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 63137.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 30
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (51558.7 - 58140.8) = 51558.7- 58140.8
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 63137.2 - 63899.4


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (63137.2 - 63558.5), exposure 421.228
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.214567 bg counts (27), with cf=1.31376 and errBG= 0.0412935
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4245 +/- 5.08845
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=63137.2 and stop= 63558.5 so gap is 421.228, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (63137.2 - 63558.5), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57343.4 - 58140.8), exposure 797.321
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.257973 bg counts (33), with cf=1.34537 and errBG= 0.0449074
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =37.3234 +/- 7.1193
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 80
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 30
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (63558.5 - 63899.4), exposure 340.992
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.18278 bg counts (23), with cf=1.31948 and errBG= 0.0381122
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.67573 +/- 3.23245
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (63137.2 - 63899.4), exposure 762.219, 7 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0118628, 0.0236921 and 1.99717. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=63558.5 and stop= 63899.4 so gap is 340.992, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 13 (63899.4) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=340.992 whereas forward=799.732
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (63137.2 - 63899.4), exposure 762.219
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.397347 bg counts (50), with cf=1.31539 and errBG= 0.0561934
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.1006 +/- 6.02835
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 13 (63899.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (63137.2 - 63899.4), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 64699.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 31
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 64699.2 - 65644.3


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (64699.2 - 65341), exposure 641.872
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.210921 bg counts (30), with cf=1.47806 and errBG= 0.0385088
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.8591 +/- 5.72478
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=64699.2 and stop= 65341 so gap is 641.872, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (64699.2 - 65341), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (63137.2 - 63899.4), exposure 762.219
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.397347 bg counts (50), with cf=1.31539 and errBG= 0.0561934
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.1006 +/- 6.02835
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 81
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 31
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (65341 - 65644.3), exposure 275.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.0773378 bg counts (11), with cf=1.4571 and errBG= 0.0233182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =5.7157 +/- 2.91439
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (63137.2 - 65644.3), exposure 1679.89, 13 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0105401, 0.0220031 and 2.08755. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=65341 and stop= 65644.3 so gap is 303.26, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 14 (65644.3) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=303.26 whereas forward=3289.91
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (64699.2 - 65644.3), exposure 917.672
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 19 counts and 0.288259 bg counts (41), with cf=1.47365 and errBG= 0.0450185
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.5745 +/- 6.42381
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 14 (65644.3) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (64699.2 - 65644.3), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 68934.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 33
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 68934.2 - 70481.2


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (63137.2 - 69017), exposure 1762.63, 15 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0124054, 0.0222862 and 1.79649. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=68934.2 and stop= 69017 so gap is 82.7411, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (63137.2 - 69017) = 63137.2- 69017
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68934.2 - 69719), exposure 784.787
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.284888 bg counts (37), with cf=2.04762 and errBG= 0.0468353
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.131 +/- 7.93098
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=68934.2 and stop= 69719 so gap is 784.787, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (68934.2 - 69719), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (64699.2 - 65644.3), exposure 917.672
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 19 counts and 0.288259 bg counts (41), with cf=1.47365 and errBG= 0.0450185
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.5745 +/- 6.42381
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 82
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 33
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (69719 - 70481.2), exposure 762.217
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 0.23869 bg counts (31), with cf=1.99866 and errBG= 0.04287
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.5081 +/- 6.62934
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (69017 - 70481.2), exposure 1464.26, 10 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0133752, 0.0174633 and 1.30565. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=69719 and stop= 70481.2 so gap is 762.217, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 15 (70481.2) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=762.217 whereas forward=10754.7
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68934.2 - 70481.2), exposure 1547
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.523578 bg counts (68), with cf=2.0269 and errBG= 0.0634932
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.6383 +/- 10.336
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 15 (70481.2) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (63137.2 - 70481.2), exposure 3226.9, 25 soft counts and 41 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0128483, 0.0201037 and 1.5647. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (68934.2 - 70481.2), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 81235.9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 34
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (63137.2 - 70481.2) = 63137.2- 70481.2
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 81235.9 - 82620


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81235.9 - 82043.3), exposure 807.353
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.405511 bg counts (46), with cf=1.30283 and errBG= 0.0597893
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0141 +/- 5.04644
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=81235.9 and stop= 82043.3 so gap is 807.353, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (81235.9 - 82043.3), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68934.2 - 70481.2), exposure 1547
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.523578 bg counts (68), with cf=2.0269 and errBG= 0.0634932
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.6383 +/- 10.336
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 83
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 34
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (82043.3 - 82620), exposure 576.677
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.220386 bg counts (25), with cf=1.30537 and errBG= 0.0440773
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.766 +/- 4.12833
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81235.9 - 82620), exposure 1384.03, 12 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0110192, 0.0119427 and 1.0838. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=82043.3 and stop= 82620 so gap is 576.677, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 16 (82620) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=576.677 whereas forward=4281.64
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81235.9 - 82620), exposure 1384.03
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.625897 bg counts (71), with cf=1.30384 and errBG= 0.0742803
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.78 +/- 6.51994
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 16 (82620) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (81235.9 - 82620), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 86901.6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 35
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 86901.6 - 88380.9


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81235.9 - 87037), exposure 1519.42, 15 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0126255, 0.0117186 and 0.92817. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=86901.6 and stop= 87037 so gap is 135.394, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81235.9 - 87104.7), exposure 1587.12, 15 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0120654, 0.0120649 and 0.999956. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=86901.6 and stop= 87104.7 so gap is 203.092, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (81235.9 - 87104.7) = 81235.9- 87104.7
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (86901.6 - 88127.7), exposure 1226.07
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.49643 bg counts (57), with cf=1.33174 and errBG= 0.0657537
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.315 +/- 5.15856
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=86901.6 and stop= 88127.7 so gap is 1226.07, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (86901.6 - 88127.7), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81235.9 - 82620), exposure 1384.03
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.625897 bg counts (71), with cf=1.30384 and errBG= 0.0742803
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.78 +/- 6.51994
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 84
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 35
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (88127.7 - 88380.9), exposure 253.233
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0348372 bg counts (4), with cf=1.35525 and errBG= 0.0174186
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.30804 +/- 1.35546
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (87104.7 - 88380.9), exposure 1276.22, 7 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0071398, 0.00391043 and 0.547694. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=88127.7 and stop= 88380.9 so gap is 253.233, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 17 (88380.9) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=253.233 whereas forward=4453.4
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (86901.6 - 88380.9), exposure 1479.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.531267 bg counts (61), with cf=1.33321 and errBG= 0.0680218
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.6231 +/- 5.33362
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 17 (88380.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81235.9 - 88380.9), exposure 2863.34, 22 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00986996, 0.00843215 and 0.854325. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (86901.6 - 88380.9), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 92834.3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 36
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (81235.9 - 88380.9) = 81235.9- 88380.9
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 92834.3 - 94200.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (92834.3 - 93889.9), exposure 1055.58
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.513736 bg counts (59), with cf=1.30945 and errBG= 0.0668827
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.969 +/- 5.07222
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=92834.3 and stop= 93889.9 so gap is 1055.58, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (92834.3 - 93889.9), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (86901.6 - 88380.9), exposure 1479.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.531267 bg counts (61), with cf=1.33321 and errBG= 0.0680218
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.6231 +/- 5.33362
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 85
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 36
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (93889.9 - 94200.8), exposure 310.901
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.113196 bg counts (13), with cf=1.32798 and errBG= 0.0313949
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.50564 +/- 1.87851
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 94200.8), exposure 1366.48, 11 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0102822, 0.00543334 and 0.528421. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=93889.9 and stop= 94200.8 so gap is 310.901, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 18 (94200.8) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=310.901 whereas forward=4739.22
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (92834.3 - 94200.8), exposure 1366.48
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.626932 bg counts (72), with cf=1.31163 and errBG= 0.0738846
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.4754 +/- 5.40884
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 18 (94200.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (92834.3 - 94200.8), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 98940
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 37
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 98940 - 100319


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 99253.4), exposure 1679.89, 15 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0114059, 0.00592793 and 0.519725. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99253.4 so gap is 313.414, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 99255.9), exposure 1682.4, 16 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0121646, 0.0059191 and 0.486584. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99255.9 so gap is 315.921, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 99378.8), exposure 1805.26, 17 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.012054, 0.005485 and 0.455035. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99378.8 so gap is 438.779, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 99391.3), exposure 1817.79, 18 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0126892, 0.00544718 and 0.429278. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99391.3 so gap is 451.316, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 99401.3), exposure 1827.82, 18 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0126195, 0.00613156 and 0.485878. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99401.3 so gap is 461.345, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 99454), exposure 1880.48, 18 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0122602, 0.00663618 and 0.541278. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99454 so gap is 513.999, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 99697.2), exposure 2123.69, 18 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0108296, 0.00646979 and 0.597416. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99697.2 so gap is 757.208, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 99830.1), exposure 2256.57, 19 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0107504, 0.0060738 and 0.564985. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99830.1 so gap is 890.096, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 99872.7), exposure 2299.2, 19 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0105413, 0.00652895 and 0.61937. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99872.7 so gap is 932.72, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (98940 - 99940.4), exposure 1000.42
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.421659 bg counts (49), with cf=1.30553 and errBG= 0.0602369
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0324 +/- 5.0569
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 99940.4), exposure 2366.9, 19 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.010235, 0.00687941 and 0.672145. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99940.4 so gap is 1000.42, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (98940 - 99940.4), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (92834.3 - 94200.8), exposure 1366.48
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.626932 bg counts (72), with cf=1.31163 and errBG= 0.0738846
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.4754 +/- 5.40884
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 86
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 37
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 100001), exposure 2427.07, 19 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00996734, 0.00723294 and 0.725663. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=99940.4 and stop= 100001 so gap is 60.1756, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 100056), exposure 2482.23, 19 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00974131, 0.00758902 and 0.779055. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=99940.4 and stop= 100056 so gap is 115.336, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (92834.3 - 100056) = 92834.3- 100056
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (99940.4 - 100319), exposure 320.929
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.197921 bg counts (23), with cf=1.3053 and errBG= 0.0412695
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.26813 +/- 2.91923
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (100056 - 100319), exposure 205.593, 0 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -0.000334847, 0.0187176 and -55.899. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=99940.4 and stop= 100319 so gap is 379.039, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 19 (100319) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=379.039 whereas forward=16435.2
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (98940 - 100319), exposure 1321.35
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.61958 bg counts (72), with cf=1.30547 and errBG= 0.0730182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.3005 +/- 5.83902
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 19 (100319) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (92834.3 - 100319), exposure 2687.83, 19 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00896268, 0.00844033 and 0.941719. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (98940 - 100319), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 116755
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 40
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (92834.3 - 100319) = 92834.3- 100319
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 116755 - 117675


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (116755 - 117675), exposure 837.438
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.775563 bg counts (88), with cf=1.28542 and errBG= 0.0826753
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.4281 +/- 4.45409
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (116755 - 117675), exposure 837.438, 4 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00520582, 0.0120252 and 2.30995. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116755 and stop= 117675 so gap is 920.564, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 20 (117675) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=0 and gapBack=17355.8 whereas forward=73967.7
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (98940 - 117675), exposure 2158.79
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 32 counts and 1.39514 bg counts (160), with cf=1.29795 and errBG= 0.110296
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =39.7236 +/- 7.34371
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 20 (117675) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (98940 - 117675), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 191643
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 44
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 191643 - 192851


++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (191643 - 192851), exposure 1208.52
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 0.187405 bg counts (45), with cf=1.52512 and errBG= 0.0279367
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.4905 +/- 5.05844
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (116755 - 192851), exposure 2045.96, 9 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00575099, 0.00932527 and 1.62151. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=191643 and stop= 192851 so gap is 1208.52, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  787  INFO   >>  I'm on the last event, so save the previous bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (98940 - 117675), exposure 2158.79
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 32 counts and 1.39514 bg counts (160), with cf=1.29795 and errBG= 0.110296
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =39.7236 +/- 7.34371
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 87
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0xaf2b10
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (191643 - 192851), exposure 1208.52
++taStructures/bin.cpp::   bayesian_bin:  line  273  INFO   >>  Making a Bayesian bin - I have 11 counts and 0.187405 bg counts, with cf=1.52512
++taStructures/bin.cpp::   bayesian_bin:  line  274  INFO   >>    Therefore net =16.4912 + 5.62923 -4.59825 and sigma=387.04
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 88
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (116755 - 192851), exposure 2045.96, 9 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00575099, 0.00932527 and 1.62151. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for PC mode.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: PC, with files: pcsourcetotal_incbad.evt, pcbacktotal_incbad.evt, and pccorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 156.453 - 394860
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	156.453 - 2062
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	5953.69 - 7829.16
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	12004.2 - 13617.2
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	18023.3 - 19399.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	22606 - 22763.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	24043.7 - 25182.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	28381.9 - 28931
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	30047.3 - 30965
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	34164.7 - 35187.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	35705 - 36733
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	39947 - 42529.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	45778 - 48302.2
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	51558.7 - 52381.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	53599.2 - 54080.6
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	57343.4 - 58140.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	59360.5 - 59877
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	63137.2 - 63899.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	64699.2 - 65644.3
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	68934.2 - 70481.2
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	81235.9 - 82620
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	86901.6 - 88380.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	92834.3 - 94200.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	98940 - 100319
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	104951 - 106127
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	109374 - 109499
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	110932 - 111905
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	115167 - 115441
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	116755 - 117675
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	120954 - 121696
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	168226 - 169730
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	174047 - 175514
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	179813 - 181278
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	185702 - 186539
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	191643 - 192851
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	197631 - 198631
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	203389 - 204396
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	208051 - 209415
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	249219 - 249254
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	249444 - 249519
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	249587 - 249900
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	301179 - 302699
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	306939 - 308458
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	312699 - 314219
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	318519 - 320039
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	324264 - 325199
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	330024 - 331561
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	365686 - 366240
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	371506 - 372032
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	376290 - 377579
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	382050 - 383339
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	387819 - 389100
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	393639 - 394860
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - PC mode, suffix = _incbad
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 20 ct/bin at rateFact=10 and binFact= 1.5 with minT 2.51 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file PCCURVE_incbad.qdp, reading from pcsourcetotal_incbad.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (156.453 - 176.512), exposure 20.0584
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.030974 bg counts (1), with cf=2.60797 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.0786 +/- 11.6635
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=156.453 and stop= 176.512 so gap is 20.0584, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (156.453 - 176.512), with lastBin= 0 and workMinC was 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (176.512 - 216.629), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.15487 bg counts (5), with cf=2.66203 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.8283 +/- 11.9064
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=176.512 and stop= 216.629 so gap is 40.117, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (176.512 - 216.629), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (156.453 - 176.512), exposure 20.0584
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.030974 bg counts (1), with cf=2.60797 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.0786 +/- 11.6635
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (156.453 - 226.658), exposure 70.2047, 20 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.746078, 1.0142 and 1.35938. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=216.629 and stop= 226.658 so gap is 10.0292, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (156.453 - 226.658) = 156.453- 226.658
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (216.629 - 251.731), exposure 35.1023
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.68213 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.4765 +/- 11.9954
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=216.629 and stop= 251.731 so gap is 35.1023, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (216.629 - 251.731), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (176.512 - 216.629), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.15487 bg counts (5), with cf=2.66203 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.8283 +/- 11.9064
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (251.731 - 291.848), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.061948 bg counts (2), with cf=2.68231 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =56.1623 +/- 12.2924
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=251.731 and stop= 291.848 so gap is 40.117, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (251.731 - 291.848), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (216.629 - 251.731), exposure 35.1023
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.68213 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.4765 +/- 11.9954
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (226.658 - 311.906), exposure 85.2485, 20 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.627881, 0.840789 and 1.33909. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=291.848 and stop= 311.906 so gap is 20.0584, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (226.658 - 311.906) = 226.658- 311.906
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (291.848 - 331.965), exposure 40.1169
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.030974 bg counts (1), with cf=2.63497 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.2527 +/- 12.0752
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=291.848 and stop= 331.965 so gap is 40.1169, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (291.848 - 331.965), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (251.731 - 291.848), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.061948 bg counts (2), with cf=2.68231 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =56.1623 +/- 12.2924
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (331.965 - 412.199), exposure 80.2339
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.216818 bg counts (7), with cf=2.64794 and errBG= 0.0819495
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.3846 +/- 11.8439
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=331.965 and stop= 412.199 so gap is 80.2339, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (331.965 - 412.199), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (291.848 - 331.965), exposure 40.1169
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.030974 bg counts (1), with cf=2.63497 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.2527 +/- 12.0752
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (412.199 - 454.823), exposure 42.6243
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.123896 bg counts (4), with cf=2.67604 and errBG= 0.061948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.1893 +/- 11.9688
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.199 and stop= 454.823 so gap is 42.6243, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (412.199 - 454.823), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (331.965 - 412.199), exposure 80.2339
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.216818 bg counts (7), with cf=2.64794 and errBG= 0.0819495
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.3846 +/- 11.8439
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (311.906 - 482.403), exposure 170.497, 21 soft counts and 38 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.325948, 0.587553 and 1.8026. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=454.823 and stop= 482.403 so gap is 27.5804, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (311.906 - 482.403) = 311.906- 482.403
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (454.823 - 494.94), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.68496 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.9684 +/- 12.3054
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=454.823 and stop= 494.94 so gap is 40.117, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (454.823 - 494.94), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (412.199 - 454.823), exposure 42.6243
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.123896 bg counts (4), with cf=2.67604 and errBG= 0.061948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.1893 +/- 11.9688
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (494.94 - 572.667), exposure 77.7266
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.67835 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.8306 +/- 12.2752
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=494.94 and stop= 572.667 so gap is 77.7266, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (494.94 - 572.667), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (454.823 - 494.94), exposure 40.117
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.68496 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.9684 +/- 12.3054
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (482.403 - 605.261), exposure 122.858, 20 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.432761, 0.477699 and 1.10384. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=572.667 and stop= 605.261 so gap is 32.595, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (482.403 - 605.261) = 482.403- 605.261
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (572.667 - 635.349), exposure 62.6828
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.185844 bg counts (6), with cf=2.67165 and errBG= 0.0758705
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9364 +/- 11.9497
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=572.667 and stop= 635.349 so gap is 62.6828, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (572.667 - 635.349), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (494.94 - 572.667), exposure 77.7266
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.67835 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.8306 +/- 12.2752
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (635.349 - 688.003), exposure 52.6535
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.65617 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9588 +/- 11.8793
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=635.349 and stop= 688.003 so gap is 52.6535, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (635.349 - 688.003), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (572.667 - 635.349), exposure 62.6828
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.185844 bg counts (6), with cf=2.67165 and errBG= 0.0758705
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9364 +/- 11.9497
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (688.003 - 740.656), exposure 52.6535
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.030974 bg counts (1), with cf=2.65245 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9668 +/- 11.8624
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=688.003 and stop= 740.656 so gap is 52.6535, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (688.003 - 740.656), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (635.349 - 688.003), exposure 52.6535
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.65617 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9588 +/- 11.8793
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (605.261 - 778.266), exposure 173.004, 20 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.306942, 0.550421 and 1.79324. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=740.656 and stop= 778.266 so gap is 37.6096, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (605.261 - 778.266) = 605.261- 778.266
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (740.656 - 835.934), exposure 95.2778
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.15487 bg counts (5), with cf=2.67308 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.0475 +/- 11.9558
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=740.656 and stop= 835.934 so gap is 95.2778, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (740.656 - 835.934), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (688.003 - 740.656), exposure 52.6535
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.030974 bg counts (1), with cf=2.65245 and errBG= 0.030974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9668 +/- 11.8624
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 12
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (835.934 - 918.675), exposure 82.7413
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.64077 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.0471 +/- 12.1029
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=835.934 and stop= 918.675 so gap is 82.7413, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (835.934 - 918.675), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (740.656 - 835.934), exposure 95.2778
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.15487 bg counts (5), with cf=2.67308 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.0475 +/- 11.9558
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 13
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.266 - 991.387), exposure 213.121, 20 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.24869, 0.397903 and 1.6. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=918.675 and stop= 991.387 so gap is 72.712, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (778.266 - 991.387) = 778.266- 991.387
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (918.675 - 1011.45), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.69056 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.6445 +/- 12.0331
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=918.675 and stop= 1011.45 so gap is 92.7705, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (918.675 - 1011.45), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (835.934 - 918.675), exposure 82.7413
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.15487 bg counts (5), with cf=2.64077 and errBG= 0.06926
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.0471 +/- 12.1029
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 14
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1011.45 - 1084.16), exposure 72.712
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.67327 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.2999 +/- 11.9558
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1011.45 and stop= 1084.16 so gap is 72.712, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1011.45 - 1084.16), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (918.675 - 1011.45), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.69056 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.6445 +/- 12.0331
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 15
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1084.16 - 1186.96), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.30974 bg counts (10), with cf=2.66241 and errBG= 0.0979484
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.4235 +/- 11.9095
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1084.16 and stop= 1186.96 so gap is 102.8, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1084.16 - 1186.96), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1011.45 - 1084.16), exposure 72.712
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.061948 bg counts (2), with cf=2.67327 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.2999 +/- 11.9558
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 16
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (991.387 - 1247.13), exposure 255.746, 20 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.207003, 0.371317 and 1.79378. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1186.96 and stop= 1247.13 so gap is 60.1755, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (991.387 - 1247.13) = 991.387- 1247.13
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1186.96 - 1287.25), exposure 100.293
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.123896 bg counts (4), with cf=2.65187 and errBG= 0.061948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.7088 +/- 11.8607
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1186.96 and stop= 1287.25 so gap is 100.293, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1186.96 - 1287.25), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1084.16 - 1186.96), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.30974 bg counts (10), with cf=2.66241 and errBG= 0.0979484
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.4235 +/- 11.9095
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 17
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1287.25 - 1425.15), exposure 137.902
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.247792 bg counts (8), with cf=2.65079 and errBG= 0.0876077
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.359 +/- 11.857
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1287.25 and stop= 1425.15 so gap is 137.902, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1287.25 - 1425.15), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1186.96 - 1287.25), exposure 100.293
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.123896 bg counts (4), with cf=2.65187 and errBG= 0.061948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.7088 +/- 11.8607
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 18
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1425.15 - 1482.82), exposure 57.6682
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.092922 bg counts (3), with cf=2.67746 and errBG= 0.0536486
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.3004 +/- 11.9748
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1247.13 - 1482.82), exposure 235.687, 20 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.22344, 0.291828 and 1.30607. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.15 and stop= 1482.82 so gap is 57.6682, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1425.15 - 1482.82), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1287.25 - 1425.15), exposure 137.902
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.247792 bg counts (8), with cf=2.65079 and errBG= 0.0876077
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.359 +/- 11.857
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 19
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1247.13 - 1482.82) = 1247.13- 1482.82
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1482.82 - 1625.74), exposure 142.917
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.402662 bg counts (13), with cf=2.616 and errBG= 0.111678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.8827 +/- 11.9916
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1482.82 and stop= 1625.74 so gap is 142.917, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1482.82 - 1625.74), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1425.15 - 1482.82), exposure 57.6682
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.092922 bg counts (3), with cf=2.67746 and errBG= 0.0536486
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.3004 +/- 11.9748
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1625.74 - 1741.07), exposure 115.336
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.216818 bg counts (7), with cf=2.61916 and errBG= 0.0819495
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =57.0536 +/- 12.2868
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1625.74 and stop= 1741.07 so gap is 115.336, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1625.74 - 1741.07), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1482.82 - 1625.74), exposure 142.917
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.402662 bg counts (13), with cf=2.616 and errBG= 0.111678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.8827 +/- 11.9916
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 21
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1482.82 - 1826.32), exposure 343.502, 20 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.150643, 0.271215 and 1.80039. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1741.07 and stop= 1826.32 so gap is 85.2486, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1482.82 - 1826.32) = 1482.82- 1826.32
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1741.07 - 1861.42), exposure 120.351
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.061948 bg counts (2), with cf=2.62924 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =57.6805 +/- 12.3328
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1741.07 and stop= 1861.42 so gap is 120.351, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1741.07 - 1861.42), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1625.74 - 1741.07), exposure 115.336
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.216818 bg counts (7), with cf=2.61916 and errBG= 0.0819495
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =57.0536 +/- 12.2868
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 22
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1861.42 - 1949.18), exposure 87.756
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.216818 bg counts (7), with cf=2.67562 and errBG= 0.0819495
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.9323 +/- 11.9678
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1861.42 and stop= 1949.18 so gap is 87.756, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1861.42 - 1949.18), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1741.07 - 1861.42), exposure 120.351
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.061948 bg counts (2), with cf=2.62924 and errBG= 0.0438039
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =57.6805 +/- 12.3328
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 23
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1949.18 - 2062), exposure 112.82
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 18 counts and 0.185844 bg counts (6), with cf=2.60639 and errBG= 0.0758705
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.4306 +/- 11.0597
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1826.32 - 2062), exposure 235.679, 19 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.211057, 0.311136 and 1.47418. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1949.18 and stop= 2062 so gap is 112.82, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (2062) and the bin is not full 18 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=112.82 whereas forward=3891.69
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1861.42 - 2062), exposure 200.576
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 38 counts and 0.402662 bg counts (13), with cf=2.64283 and errBG= 0.111678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =99.3633 +/- 16.2942
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (2062) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1482.82 - 2062), exposure 579.18, 39 soft counts and 64 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.175226, 0.287458 and 1.6405. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1861.42 - 2062), with lastBin= 0 and workMinC was 17
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 5953.69
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1482.82 - 2062) = 1482.82- 2062
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 5953.69 - 7829.16


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 2, last was 1 so increasing dead to 0.000188291
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 3, last was 2 so increasing dead to 0.000408351
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5953.69 - 6126.7), exposure 173.004
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.11121 bg counts (5), with cf=2.63275 and errBG= 0.0497345
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.3621 +/- 11.7747
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5953.69 and stop= 6126.7 so gap is 173.004, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (5953.69 - 6126.7), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1861.42 - 2062), exposure 200.576
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 38 counts and 0.402662 bg counts (13), with cf=2.64283 and errBG= 0.111678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =99.3633 +/- 16.2942
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 24
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 4, last was 3 so increasing dead to 0.000440121
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6126.7 - 6262.09), exposure 135.394
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0679808 bg counts (3), with cf=1.85537 and errBG= 0.0392487
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.9812 +/- 8.29777
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (5953.69 - 6262.09), exposure 308.398, 20 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.130494, 0.159127 and 1.21942. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6126.7 and stop= 6262.09 so gap is 135.395, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6126.7 - 6262.09), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5953.69 - 6126.7), exposure 173.004
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.11121 bg counts (5), with cf=2.63275 and errBG= 0.0497345
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =52.3621 +/- 11.7747
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 25
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (5953.69 - 6262.09) = 5953.69- 6262.09
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6262.09 - 6362.39), exposure 100.292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139099 bg counts (6), with cf=1.22018 and errBG= 0.0567868
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.2339 +/- 5.45727
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6262.09 and stop= 6362.39 so gap is 100.292, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6262.09 - 6362.39), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6126.7 - 6262.09), exposure 135.394
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0679808 bg counts (3), with cf=1.85537 and errBG= 0.0392487
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.9812 +/- 8.29777
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 26
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6262.09 - 6455.16), exposure 193.063, 20 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.125714, 0.099454 and 0.791115. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6362.39 and stop= 6455.16 so gap is 92.7704, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6262.09 - 6457.66), exposure 195.57, 20 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.124102, 0.104504 and 0.842079. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6362.39 and stop= 6457.66 so gap is 95.2777, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6262.09 - 6460.17), exposure 198.077, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.122531, 0.109426 and 0.893043. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6362.39 and stop= 6460.17 so gap is 97.785, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6362.39 - 6465.19), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.208648 bg counts (9), with cf=1.22201 and errBG= 0.0695494
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1853 +/- 5.46567
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6262.09 - 6465.19), exposure 203.092, 21 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.125597, 0.112814 and 0.898226. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6362.39 and stop= 6465.19 so gap is 102.8, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6362.39 - 6465.19), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6262.09 - 6362.39), exposure 100.292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139099 bg counts (6), with cf=1.22018 and errBG= 0.0567868
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.2339 +/- 5.45727
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 27
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6262.09 - 6470.2), exposure 208.107, 21 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.12257, 0.11586 and 0.94525. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6465.19 and stop= 6470.2 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (6262.09 - 6470.2) = 6262.09- 6470.2
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6465.19 - 6588.04), exposure 122.858
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.21263 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.112 +/- 5.42339
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6465.19 and stop= 6588.04 so gap is 122.858, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6465.19 - 6588.04), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6362.39 - 6465.19), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.208648 bg counts (9), with cf=1.22201 and errBG= 0.0695494
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1853 +/- 5.46567
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 28
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6470.2 - 6668.28), exposure 198.077, 20 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.12149, 0.104038 and 0.856355. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6588.04 and stop= 6668.28 so gap is 80.234, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6588.04 - 6673.29), exposure 85.2485
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0463662 bg counts (2), with cf=1.21072 and errBG= 0.0327859
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1582 +/- 5.41464
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6470.2 - 6673.29), exposure 203.092, 20 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.11849, 0.113282 and 0.956042. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6588.04 and stop= 6673.29 so gap is 85.2485, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6588.04 - 6673.29), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6465.19 - 6588.04), exposure 122.858
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.21263 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.112 +/- 5.42339
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 29
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6470.2 - 6675.8), exposure 205.599, 20 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.116909, 0.117734 and 1.00706. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6673.29 and stop= 6675.8 so gap is 2.50734, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (6470.2 - 6675.8) = 6470.2- 6675.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 5, last was 4 so increasing dead to 0.00203985
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6673.29 - 6916.5), exposure 243.207
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.402302 bg counts (18), with cf=2.36558 and errBG= 0.0948235
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.3599 +/- 10.5816
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6673.29 and stop= 6916.5 so gap is 243.209, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6673.29 - 6916.5), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6588.04 - 6673.29), exposure 85.2485
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0463662 bg counts (2), with cf=1.21072 and errBG= 0.0327859
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1582 +/- 5.41464
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 30
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 6, last was 5 so increasing dead to 0.0010401
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6916.5 - 7079.48), exposure 162.974
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.178545 bg counts (8), with cf=1.68405 and errBG= 0.0631251
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.3803 +/- 7.53204
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6916.5 and stop= 7079.48 so gap is 162.975, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6916.5 - 7079.48), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6673.29 - 6916.5), exposure 243.207
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.402302 bg counts (18), with cf=2.36558 and errBG= 0.0948235
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.3599 +/- 10.5816
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 31
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6675.8 - 7099.54), exposure 423.732, 20 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0838933, 0.122028 and 1.45456. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7079.48 and stop= 7099.54 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (6675.8 - 7099.54) = 6675.8- 7099.54
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7079.48 - 7172.25), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.23722 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.601 +/- 5.53339
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7079.48 and stop= 7172.25 so gap is 92.7705, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7079.48 - 7172.25), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6916.5 - 7079.48), exposure 162.974
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.178545 bg counts (8), with cf=1.68405 and errBG= 0.0631251
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.3803 +/- 7.53204
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 32
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7172.25 - 7247.47), exposure 75.2193
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.22757 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.4091 +/- 5.49022
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7172.25 and stop= 7247.47 so gap is 75.2193, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7172.25 - 7247.47), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7079.48 - 7172.25), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.23722 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.601 +/- 5.53339
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 33
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7277.55), exposure 178.019, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.137761, 0.12359 and 0.897135. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7277.55 so gap is 30.0878, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7282.57), exposure 183.034, 21 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.140745, 0.120204 and 0.854057. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7282.57 so gap is 35.1024, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7290.09), exposure 190.556, 21 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.135189, 0.121951 and 0.902074. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7290.09 so gap is 42.6243, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7292.6), exposure 193.063, 22 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.139645, 0.120367 and 0.861948. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7292.6 so gap is 45.1316, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7295.11), exposure 195.57, 23 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.143987, 0.118824 and 0.82524. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7295.11 so gap is 47.639, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7297.61), exposure 198.078, 24 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.148219, 0.11732 and 0.791531. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7297.61 so gap is 50.1463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7099.54 - 7302.63), exposure 203.092, 25 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.15065, 0.120373 and 0.799023. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7302.63 so gap is 55.1609, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (7099.54 - 7302.63) = 7099.54- 7302.63
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7247.47 - 7347.76), exposure 100.293
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.162282 bg counts (7), with cf=1.22001 and errBG= 0.0613368
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.2022 +/- 5.45656
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7247.47 and stop= 7347.76 so gap is 100.293, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7247.47 - 7347.76), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7172.25 - 7247.47), exposure 75.2193
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.115916 bg counts (5), with cf=1.22757 and errBG= 0.051839
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.4091 +/- 5.49022
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 34
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7347.76 - 7448.05), exposure 100.292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139099 bg counts (6), with cf=1.23519 and errBG= 0.0567868
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.5319 +/- 5.52437
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7347.76 and stop= 7448.05 so gap is 100.292, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7347.76 - 7448.05), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7247.47 - 7347.76), exposure 100.293
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.162282 bg counts (7), with cf=1.22001 and errBG= 0.0613368
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.2022 +/- 5.45656
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 35
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 7, last was 6 so increasing dead to 0.00220001
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7448.05 - 7575.92), exposure 127.871
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.113609 bg counts (5), with cf=2.07781 and errBG= 0.0508074
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.3201 +/- 9.29285
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7448.05 and stop= 7575.92 so gap is 127.873, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7448.05 - 7575.92), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7347.76 - 7448.05), exposure 100.292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139099 bg counts (6), with cf=1.23519 and errBG= 0.0567868
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.5319 +/- 5.52437
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 36
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 7
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7302.63 - 7595.98), exposure 293.353, 20 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.105808, 0.191162 and 1.80668. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7575.92 and stop= 7595.98 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (7302.63 - 7595.98) = 7302.63- 7595.98
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7575.92 - 7696.28), exposure 120.351
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.113609 bg counts (5), with cf=2.22183 and errBG= 0.0508074
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.1842 +/- 9.93696
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7575.92 and stop= 7696.28 so gap is 120.351, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7575.92 - 7696.28), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7448.05 - 7575.92), exposure 127.871
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.113609 bg counts (5), with cf=2.07781 and errBG= 0.0508074
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.3201 +/- 9.29285
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 37
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 7
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 8, last was 7 so increasing dead to 0.00131994
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7696.28 - 7829.16), exposure 132.886
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.392729 bg counts (17), with cf=1.45435 and errBG= 0.0952508
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.6984 +/- 5.81903
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7595.98 - 7829.16), exposure 233.178, 12 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0890133, 0.147237 and 1.65411. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7696.28 and stop= 7829.16 so gap is 132.887, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 1 (7829.16) and the bin is not full 16 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=132.887 whereas forward=4175.05
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7575.92 - 7829.16), exposure 253.237
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 36 counts and 0.506338 bg counts (22), with cf=1.88073 and errBG= 0.107952
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =66.7538 +/- 11.2862
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 1 (7829.16) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7302.63 - 7829.16), exposure 526.532, 32 soft counts and 52 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0984137, 0.171722 and 1.7449. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7575.92 - 7829.16), with lastBin= 0 and workMinC was 15
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 12004.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (7302.63 - 7829.16) = 7302.63- 7829.16
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 12004.2 - 13617.2


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12004.2 - 12174.7), exposure 170.497
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.140995 bg counts (6), with cf=1.20298 and errBG= 0.0575609
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8901 +/- 5.38035
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12004.2 and stop= 12174.7 so gap is 170.497, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12004.2 - 12174.7), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7575.92 - 7829.16), exposure 253.237
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 36 counts and 0.506338 bg counts (22), with cf=1.88073 and errBG= 0.107952
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =66.7538 +/- 11.2862
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 38
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12174.7 - 12370.3), exposure 195.57
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.399485 bg counts (17), with cf=1.20285 and errBG= 0.0968895
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.7792 +/- 5.51336
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12174.7 and stop= 12370.3 so gap is 195.57, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12174.7 - 12370.3), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12004.2 - 12174.7), exposure 170.497
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.140995 bg counts (6), with cf=1.20298 and errBG= 0.0575609
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8901 +/- 5.38035
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 39
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (12004.2 - 12377.8), exposure 373.589, 20 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0634186, 0.0732786 and 1.15547. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12370.3 and stop= 12377.8 so gap is 7.52194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (12004.2 - 12377.8) = 12004.2- 12377.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12370.3 - 12483.1), exposure 112.829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0234991 bg counts (1), with cf=1.19924 and errBG= 0.0234991
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9566 +/- 5.36323
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12370.3 and stop= 12483.1 so gap is 112.829, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12370.3 - 12483.1), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12174.7 - 12370.3), exposure 195.57
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.399485 bg counts (17), with cf=1.20285 and errBG= 0.0968895
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.7792 +/- 5.51336
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 40
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12483.1 - 12633.5), exposure 150.439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.187993 bg counts (8), with cf=1.20313 and errBG= 0.0664656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8365 +/- 5.38117
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12483.1 and stop= 12633.5 so gap is 150.439, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12483.1 - 12633.5), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12370.3 - 12483.1), exposure 112.829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0234991 bg counts (1), with cf=1.19924 and errBG= 0.0234991
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9566 +/- 5.36323
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 41
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (12377.8 - 12698.7), exposure 320.936, 20 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0741611, 0.100369 and 1.3534. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12633.5 and stop= 12698.7 so gap is 65.1901, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (12377.8 - 12698.7) = 12377.8- 12698.7
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12633.5 - 12801.5), exposure 167.99
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.446484 bg counts (19), with cf=1.21274 and errBG= 0.10243
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.7133 +/- 5.42495
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12633.5 and stop= 12801.5 so gap is 167.99, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12633.5 - 12801.5), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12483.1 - 12633.5), exposure 150.439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.187993 bg counts (8), with cf=1.20313 and errBG= 0.0664656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8365 +/- 5.38117
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 42
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12801.5 - 12987.1), exposure 185.541
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.211492 bg counts (9), with cf=1.20879 and errBG= 0.0704974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9201 +/- 5.40654
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12801.5 and stop= 12987.1 so gap is 185.541, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12801.5 - 12987.1), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12633.5 - 12801.5), exposure 167.99
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.446484 bg counts (19), with cf=1.21274 and errBG= 0.10243
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.7133 +/- 5.42495
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 43
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (12698.7 - 13037.2), exposure 338.487, 20 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0707448, 0.0777863 and 1.09953. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12987.1 and stop= 13037.2 so gap is 50.1462, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (12698.7 - 13037.2) = 12698.7- 13037.2
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12987.1 - 13079.8), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.211492 bg counts (9), with cf=1.20708 and errBG= 0.0704974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8863 +/- 5.39889
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12987.1 and stop= 13079.8 so gap is 92.7705, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12987.1 - 13079.8), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12801.5 - 12987.1), exposure 185.541
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.211492 bg counts (9), with cf=1.20879 and errBG= 0.0704974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9201 +/- 5.40654
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 44
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13079.8 - 13210.2), exposure 130.38
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0469983 bg counts (2), with cf=1.209 and errBG= 0.0332328
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1231 +/- 5.40695
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13079.8 and stop= 13210.2 so gap is 130.38, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13079.8 - 13210.2), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12987.1 - 13079.8), exposure 92.7705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.211492 bg counts (9), with cf=1.20708 and errBG= 0.0704974
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8863 +/- 5.39889
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 45
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (13037.2 - 13265.4), exposure 228.165, 18 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0946368, 0.0783682 and 0.828094. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13210.2 and stop= 13265.4 so gap is 55.1609, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (13037.2 - 13265.4) = 13037.2- 13265.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13210.2 - 13393.3), exposure 183.034
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.187993 bg counts (8), with cf=1.20219 and errBG= 0.0664656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.8068 +/- 4.65674
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13210.2 and stop= 13393.3 so gap is 183.034, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13210.2 - 13393.3), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13079.8 - 13210.2), exposure 130.38
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0469983 bg counts (2), with cf=1.209 and errBG= 0.0332328
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1231 +/- 5.40695
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 46
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 10, last was 9 so increasing dead to 26.8755
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 11, last was 10 so increasing dead to 53.6868
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 12, last was 11 so increasing dead to 81.0743
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13393.3 - 13617.2), exposure 142.91
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 19 counts and 0.446484 bg counts (19), with cf=1.20154 and errBG= 0.10243
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.2928 +/- 5.23883
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (13265.4 - 13617.2), exposure 270.783, 10 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0424241, 0.088217 and 2.07941. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13393.3 and stop= 13617.2 so gap is 223.985, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 2 (13617.2) and the bin is not full 19 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=223.985 whereas forward=4406.02
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13210.2 - 13617.2), exposure 325.944
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 34 counts and 0.634477 bg counts (27), with cf=1.20182 and errBG= 0.122105
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =40.0995 +/- 7.00932
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 2 (13617.2) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (13037.2 - 13617.2), exposure 498.949, 28 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0662975, 0.0837138 and 1.2627. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13210.2 - 13617.2), with lastBin= 0 and workMinC was 13
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 18023.3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (13037.2 - 13617.2) = 13037.2- 13617.2
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 18023.3 - 19399.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18023.3 - 18261.5), exposure 238.194
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.181616 bg counts (13), with cf=1.71434 and errBG= 0.0503712
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =35.6899 +/- 7.85659
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18023.3 and stop= 18261.5 so gap is 238.194, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18023.3 - 18261.5), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13210.2 - 13617.2), exposure 325.944
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 34 counts and 0.634477 bg counts (27), with cf=1.20182 and errBG= 0.122105
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =40.0995 +/- 7.00932
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 47
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18261.5 - 18494.6), exposure 233.18
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.209557 bg counts (15), with cf=1.76034 and errBG= 0.0541073
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.8378 +/- 7.87304
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18261.5 and stop= 18494.6 so gap is 233.18, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18261.5 - 18494.6), with lastBin= 0xaf0fa0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18023.3 - 18261.5), exposure 238.194
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.181616 bg counts (13), with cf=1.71434 and errBG= 0.0503712
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =35.6899 +/- 7.85659
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 48
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (18023.3 - 18607.5), exposure 584.203, 20 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.059109, 0.0911361 and 1.54183. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18494.6 and stop= 18607.5 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (18023.3 - 18607.5) = 18023.3- 18607.5
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18494.6 - 18700.2), exposure 205.599
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139704 bg counts (10), with cf=1.74818 and errBG= 0.0441784
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.7193 +/- 7.81847
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18494.6 and stop= 18700.2 so gap is 205.599, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18494.6 - 18700.2), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18261.5 - 18494.6), exposure 233.18
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.209557 bg counts (15), with cf=1.76034 and errBG= 0.0541073
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.8378 +/- 7.87304
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 49
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18700.2 - 19018.7), exposure 318.428
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.167645 bg counts (12), with cf=1.79138 and errBG= 0.048395
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.5704 +/- 6.93854
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18700.2 and stop= 19018.7 so gap is 318.428, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18700.2 - 19018.7), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18494.6 - 18700.2), exposure 205.599
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.139704 bg counts (10), with cf=1.74818 and errBG= 0.0441784
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.7193 +/- 7.81847
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 50
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (18607.5 - 19091.4), exposure 483.911, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0585319, 0.0435764 and 0.74449. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19018.7 and stop= 19091.4 so gap is 72.712, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (18607.5 - 19269.4), exposure 661.93, 20 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0539224, 0.0533226 and 0.988877. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19018.7 and stop= 19269.4 so gap is 250.731, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (18607.5 - 19269.4) = 18607.5- 19269.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (19018.7 - 19399.8), exposure 381.106
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.32132 bg counts (23), with cf=1.8453 and errBG= 0.0669999
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.3131 +/- 8.25337
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (19269.4 - 19399.8), exposure 130.375, 2 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0282353, 0.0437007 and 1.54773. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19018.7 and stop= 19399.8 so gap is 381.106, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 3 (19399.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (18607.5 - 19399.8), exposure 792.305, 22 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0496963, 0.051735 and 1.04102. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (19018.7 - 19399.8), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18700.2 - 19018.7), exposure 318.428
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.167645 bg counts (12), with cf=1.79138 and errBG= 0.048395
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.5704 +/- 6.93854
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 51
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 22606
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 14
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (18607.5 - 19399.8) = 18607.5- 19399.8
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 22606 - 22763.9


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22606 - 22763.9), exposure 157.96
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.162228 bg counts (19), with cf=1.33589 and errBG= 0.0372177
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.46273 +/- 2.98755
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22606 - 22763.9), exposure 157.96, 1 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00818679, 0.0327229 and 3.99704. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22606 and stop= 22763.9 so gap is 157.96, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 4 (22763.9) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=3364.15 whereas forward=1279.77
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 4 (22763.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 24043.7 - 25182.1


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22606 - 24151.5), exposure 265.774
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.177273 bg counts (20), with cf=1.30019 and errBG= 0.0396393
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.2724 +/- 5.03588
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22606 and stop= 24151.5 so gap is 1545.54, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (22606 - 24151.5), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (19018.7 - 19399.8), exposure 381.106
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.32132 bg counts (23), with cf=1.8453 and errBG= 0.0669999
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.3131 +/- 8.25337
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 52
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 15
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24151.5 - 24442.4), exposure 290.848
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.255753 bg counts (17), with cf=1.27005 and errBG= 0.0620291
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7259 +/- 4.91951
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24151.5 and stop= 24442.4 so gap is 290.848, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (24151.5 - 24442.4), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22606 - 24151.5), exposure 265.774
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.177273 bg counts (20), with cf=1.30019 and errBG= 0.0396393
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.2724 +/- 5.03588
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 53
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 15
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22606 - 24572.7), exposure 687.002, 17 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0312911, 0.0406432 and 1.29888. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24442.4 and stop= 24572.7 so gap is 130.38, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (22606 - 24572.7) = 22606- 24572.7
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24442.4 - 24635.4), exposure 193.063
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0752214 bg counts (5), with cf=1.26997 and errBG= 0.03364
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.954 +/- 4.91876
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24442.4 and stop= 24635.4 so gap is 193.063, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (24442.4 - 24635.4), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24151.5 - 24442.4), exposure 290.848
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.255753 bg counts (17), with cf=1.27005 and errBG= 0.0620291
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7259 +/- 4.91951
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 54
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 15
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24635.4 - 24841), exposure 205.599
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.165487 bg counts (11), with cf=1.27 and errBG= 0.0498962
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8399 +/- 4.9191
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24635.4 and stop= 24841 so gap is 205.599, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (24635.4 - 24841), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24442.4 - 24635.4), exposure 193.063
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0752214 bg counts (5), with cf=1.26997 and errBG= 0.03364
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.954 +/- 4.91876
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 55
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 15
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (24572.7 - 24996.5), exposure 423.735, 15 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0442188, 0.0474426 and 1.07291. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24841 and stop= 24996.5 so gap is 155.453, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (24572.7 - 24996.5) = 24572.7- 24996.5
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24841 - 25066.7), exposure 225.658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.180531 bg counts (12), with cf=1.26196 and errBG= 0.0521149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7016 +/- 4.88801
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=24841 and stop= 25066.7 so gap is 225.658, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (24841 - 25066.7), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24635.4 - 24841), exposure 205.599
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.165487 bg counts (11), with cf=1.27 and errBG= 0.0498962
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8399 +/- 4.9191
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 56
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 15
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 16, last was 15 so increasing dead to 27.6609
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (25066.7 - 25182.1), exposure 87.7522
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.932745 bg counts (62), with cf=1.266 and errBG= 0.118459
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.4792 +/- 4.00626
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (24996.5 - 25182.1), exposure 157.957, 11 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0806691, 0.0314708 and 0.390122. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25066.7 and stop= 25182.1 so gap is 115.413, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 5 (25182.1) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=115.413 whereas forward=3199.81
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24841 - 25182.1), exposure 313.41
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 1.11328 bg counts (74), with cf=1.26358 and errBG= 0.129416
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.1828 +/- 6.32001
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 5 (25182.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (24572.7 - 25182.1), exposure 581.692, 26 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.05412, 0.0431053 and 0.796477. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (24841 - 25182.1), with lastBin= 0 and workMinC was 13
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 28381.9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 17
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (24572.7 - 25182.1) = 24572.7- 25182.1
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 28381.9 - 28931


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28381.9 - 28692.8), exposure 310.906
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.128918 bg counts (15), with cf=1.33151 and errBG= 0.0332865
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.801 +/- 5.15711
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28381.9 and stop= 28692.8 so gap is 310.906, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28381.9 - 28692.8), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (24841 - 25182.1), exposure 313.41
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 1.11328 bg counts (74), with cf=1.26358 and errBG= 0.129416
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.1828 +/- 6.32001
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 57
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 17
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28692.8 - 28931), exposure 238.193
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.171891 bg counts (20), with cf=1.33324 and errBG= 0.0384359
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.4367 +/- 3.77131
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28381.9 - 28931), exposure 549.099, 12 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0284468, 0.0266212 and 0.935823. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28692.8 and stop= 28931 so gap is 238.193, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 6 (28931) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=238.193 whereas forward=1116.31
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28381.9 - 28931), exposure 549.099
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.300809 bg counts (35), with cf=1.33211 and errBG= 0.0508459
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.2378 +/- 6.38894
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 6 (28931) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28381.9 - 28931), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 30047.3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 18
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 30047.3 - 30965


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28381.9 - 30147.6), exposure 649.391, 16 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0317821, 0.0262198 and 0.824986. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30047.3 and stop= 30147.6 so gap is 100.292, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28381.9 - 30157.6), exposure 659.42, 16 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0312987, 0.0277246 and 0.885807. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30047.3 and stop= 30157.6 so gap is 110.322, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28381.9 - 30160.1), exposure 661.928, 16 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0311802, 0.029577 and 0.948583. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30047.3 and stop= 30160.1 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (28381.9 - 30160.1) = 28381.9- 30160.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30047.3 - 30245.4), exposure 198.077
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.151501 bg counts (10), with cf=1.26245 and errBG= 0.0479089
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7454 +/- 4.88981
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30047.3 and stop= 30245.4 so gap is 198.077, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (30047.3 - 30245.4), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28381.9 - 28931), exposure 549.099
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.300809 bg counts (35), with cf=1.33211 and errBG= 0.0508459
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.2378 +/- 6.38894
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 58
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 18
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30245.4 - 30481.1), exposure 235.687
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.181801 bg counts (12), with cf=1.2586 and errBG= 0.0524815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.1674 +/- 5.18977
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30245.4 and stop= 30481.1 so gap is 235.687, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (30245.4 - 30481.1), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30047.3 - 30245.4), exposure 198.077
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.151501 bg counts (10), with cf=1.26245 and errBG= 0.0479089
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7454 +/- 4.88981
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 59
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 18
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (30160.1 - 30674.1), exposure 513.998, 15 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0364183, 0.0460029 and 1.26318. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30481.1 and stop= 30674.1 so gap is 193.063, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (30160.1 - 30674.1) = 30160.1- 30674.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30481.1 - 30719.3), exposure 238.194
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.227252 bg counts (15), with cf=1.26184 and errBG= 0.0586761
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6409 +/- 4.88765
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30481.1 and stop= 30719.3 so gap is 238.194, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (30481.1 - 30719.3), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30245.4 - 30481.1), exposure 235.687
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.181801 bg counts (12), with cf=1.2586 and errBG= 0.0524815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.1674 +/- 5.18977
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 60
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 18
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 20, last was 18 so increasing dead to 27.5214
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 20, last was 18 so increasing dead to 55.6248
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 21, last was 20 so increasing dead to 82.8063
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30719.3 - 30965), exposure 162.972
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.469654 bg counts (31), with cf=1.25391 and errBG= 0.0843523
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.18849 +/- 3.31923
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (30674.1 - 30965), exposure 208.104, 5 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0273893, 0.0418041 and 1.52629. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=30719.3 and stop= 30965 so gap is 245.778, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 7 (30965) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=245.778 whereas forward=3199.67
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30481.1 - 30965), exposure 401.166
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.696905 bg counts (46), with cf=1.25932 and errBG= 0.102753
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.8274 +/- 5.90815
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 7 (30965) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (30160.1 - 30965), exposure 722.102, 20 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0338129, 0.0447932 and 1.32474. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (30481.1 - 30965), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 34164.7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 22
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (30160.1 - 30965) = 30160.1- 30965
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 34164.7 - 35187.7


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34164.7 - 34593.5), exposure 428.749
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.186854 bg counts (22), with cf=1.40176 and errBG= 0.0398374
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.7644 +/- 5.42927
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34164.7 and stop= 34593.5 so gap is 428.749, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34164.7 - 34593.5), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (30481.1 - 30965), exposure 401.166
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.696905 bg counts (46), with cf=1.25932 and errBG= 0.102753
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.8274 +/- 5.90815
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 61
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 22
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34593.5 - 34881.8), exposure 288.34
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.135894 bg counts (16), with cf=1.38489 and errBG= 0.0339734
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.5851 +/- 5.36386
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34164.7 - 34881.8), exposure 717.09, 15 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0289428, 0.0287208 and 0.992329. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34593.5 and stop= 34881.8 so gap is 288.34, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34593.5 - 34881.8), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34164.7 - 34593.5), exposure 428.749
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.186854 bg counts (22), with cf=1.40176 and errBG= 0.0398374
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.7644 +/- 5.42927
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 62
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 22
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (34164.7 - 34881.8) = 34164.7- 34881.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34881.8 - 35157.6), exposure 275.804
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.212334 bg counts (25), with cf=1.37382 and errBG= 0.0424668
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.3156 +/- 5.32112
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34881.8 and stop= 35157.6 so gap is 275.804, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34881.8 - 35157.6), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34593.5 - 34881.8), exposure 288.34
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.135894 bg counts (16), with cf=1.38489 and errBG= 0.0339734
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.5851 +/- 5.36386
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 63
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 22
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (35157.6 - 35187.7), exposure 30.085
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0849335 bg counts (10), with cf=1.39722 and errBG= 0.0268583
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.27855 +/- 1.39773
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34881.8 - 35187.7), exposure 305.889, 5 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0221112, 0.0484886 and 2.19294. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35157.6 and stop= 35187.7 so gap is 30.085, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 8 (35187.7) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=30.085 whereas forward=517.359
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34881.8 - 35187.7), exposure 305.889
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.297267 bg counts (35), with cf=1.37529 and errBG= 0.0502474
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.5957 +/- 5.50158
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 8 (35187.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34164.7 - 35187.7), exposure 1022.98, 20 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0268994, 0.034631 and 1.28743. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34881.8 - 35187.7), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 35705
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 23
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (34164.7 - 35187.7) = 34164.7- 35187.7
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 35705 - 36733


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (35705 - 36033.5), exposure 328.458
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.203937 bg counts (24), with cf=1.38719 and errBG= 0.0416285
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.5249 +/- 5.37286
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35705 and stop= 36033.5 so gap is 328.458, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (35705 - 36033.5), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34881.8 - 35187.7), exposure 305.889
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.297267 bg counts (35), with cf=1.37529 and errBG= 0.0502474
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.5957 +/- 5.50158
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 64
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 23
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (36033.5 - 36306.8), exposure 273.297
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0934711 bg counts (11), with cf=1.40446 and errBG= 0.0281826
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.9578 +/- 6.28104
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=36033.5 and stop= 36306.8 so gap is 273.297, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (36033.5 - 36306.8), with lastBin= 0xaf2b10 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (35705 - 36033.5), exposure 328.458
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.203937 bg counts (24), with cf=1.38719 and errBG= 0.0416285
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.5249 +/- 5.37286
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 65
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 23
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (35705 - 36324.4), exposure 619.306, 17 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0379931, 0.0424904 and 1.11837. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=36306.8 and stop= 36324.4 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (35705 - 36324.4) = 35705- 36324.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 24, last was 23 so increasing dead to 27.3841
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (36306.8 - 36733), exposure 371.078
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.747769 bg counts (88), with cf=1.39676 and errBG= 0.0797124
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.73289 +/- 3.69717
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (36324.4 - 36733), exposure 353.527, 3 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00950963, 0.0112884 and 1.18705. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=36306.8 and stop= 36733 so gap is 426.189, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 9 (36733) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=426.189 whereas forward=3214
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (36033.5 - 36733), exposure 644.375
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.84124 bg counts (99), with cf=1.40246 and errBG= 0.0845478
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.6867 +/- 7.28837
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 9 (36733) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (35705 - 36733), exposure 972.832, 20 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.02766, 0.0311501 and 1.12618. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (36033.5 - 36733), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 39947
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (35705 - 36733) = 35705- 36733
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 39947 - 42529.5


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (39947 - 40230.3), exposure 283.326
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121816 bg counts (14), with cf=1.30529 and errBG= 0.0325568
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4203 +/- 5.05553
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=39947 and stop= 40230.3 so gap is 283.326, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (39947 - 40230.3), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (36033.5 - 36733), exposure 644.375
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.84124 bg counts (99), with cf=1.40246 and errBG= 0.0845478
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.6867 +/- 7.28837
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 66
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40230.3 - 40563.8), exposure 333.472
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.217529 bg counts (25), with cf=1.31396 and errBG= 0.0435059
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4236 +/- 5.08927
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40230.3 and stop= 40563.8 so gap is 333.472, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (40230.3 - 40563.8), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (39947 - 40230.3), exposure 283.326
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.121816 bg counts (14), with cf=1.30529 and errBG= 0.0325568
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4203 +/- 5.05553
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 67
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (39947 - 40784.4), exposure 837.441, 15 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0230164, 0.0372461 and 1.61824. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40563.8 and stop= 40784.4 so gap is 220.643, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (39947 - 40784.4) = 39947- 40784.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40563.8 - 40962.5), exposure 398.662
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.113115 bg counts (13), with cf=1.30203 and errBG= 0.0313725
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.6852 +/- 5.20827
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40563.8 and stop= 40962.5 so gap is 398.662, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (40563.8 - 40962.5), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40230.3 - 40563.8), exposure 333.472
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.217529 bg counts (25), with cf=1.31396 and errBG= 0.0435059
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4236 +/- 5.08927
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 68
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40962.5 - 41190.6), exposure 228.165
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0696094 bg counts (8), with cf=1.30539 and errBG= 0.0246106
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.49 +/- 5.05586
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40962.5 and stop= 41190.6 so gap is 228.165, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (40962.5 - 41190.6), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40563.8 - 40962.5), exposure 398.662
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.113115 bg counts (13), with cf=1.30203 and errBG= 0.0313725
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.6852 +/- 5.20827
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 69
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (40784.4 - 41476.5), exposure 692.017, 15 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0280171, 0.0261149 and 0.932103. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41190.6 and stop= 41476.5 so gap is 285.833, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (40784.4 - 41494), exposure 709.568, 16 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0292127, 0.0254529 and 0.871298. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41190.6 and stop= 41494 so gap is 303.384, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (40784.4 - 41519.1), exposure 734.641, 17 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0299808, 0.0245842 and 0.82. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41190.6 and stop= 41519.1 so gap is 328.457, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (40784.4 - 41524.1), exposure 739.656, 17 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0297775, 0.0261704 and 0.878866. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41190.6 and stop= 41524.1 so gap is 333.472, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (40784.4 - 41524.1) = 40784.4- 41524.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (41190.6 - 41762.3), exposure 571.667
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.208828 bg counts (24), with cf=1.30248 and errBG= 0.0426269
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.2652 +/- 5.04479
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41190.6 and stop= 41762.3 so gap is 571.667, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (41190.6 - 41762.3), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40962.5 - 41190.6), exposure 228.165
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0696094 bg counts (8), with cf=1.30539 and errBG= 0.0246106
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.49 +/- 5.05586
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 70
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (41762.3 - 42228.6), exposure 466.36
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.165322 bg counts (19), with cf=1.31097 and errBG= 0.0379275
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4478 +/- 5.0776
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=41762.3 and stop= 42228.6 so gap is 466.36, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (41762.3 - 42228.6), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (41190.6 - 41762.3), exposure 571.667
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.208828 bg counts (24), with cf=1.30248 and errBG= 0.0426269
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.2652 +/- 5.04479
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 71
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 26
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (42228.6 - 42529.5), exposure 300.868
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 0.304541 bg counts (35), with cf=1.30615 and errBG= 0.0514768
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.3576 +/- 3.91902
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (41524.1 - 42529.5), exposure 1005.42, 13 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0164632, 0.0205777 and 1.24992. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=42228.6 and stop= 42529.5 so gap is 300.868, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 10 (42529.5) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=300.868 whereas forward=3248.51
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (41762.3 - 42529.5), exposure 767.228
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.469863 bg counts (54), with cf=1.30916 and errBG= 0.0639403
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.8047 +/- 6.4141
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 10 (42529.5) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (40784.4 - 42529.5), exposure 1745.08, 30 soft counts and 31 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0221067, 0.0229483 and 1.03807. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (41762.3 - 42529.5), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 45778
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 27
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (40784.4 - 42529.5) = 40784.4- 42529.5
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 45778 - 48302.2


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (45778 - 46053.8), exposure 275.804
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0865722 bg counts (11), with cf=1.31288 and errBG= 0.0261025
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5796 +/- 5.08489
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=45778 and stop= 46053.8 so gap is 275.804, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (45778 - 46053.8), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (41762.3 - 42529.5), exposure 767.228
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.469863 bg counts (54), with cf=1.30916 and errBG= 0.0639403
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.8047 +/- 6.4141
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 72
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 27
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46289.5), exposure 511.49, 15 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.038327, 0.0256974 and 0.670477. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46289.5 so gap is 235.687, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46297), exposure 519.012, 16 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0402859, 0.025325 and 0.62863. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46297 so gap is 243.209, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46317.1), exposure 539.071, 16 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0387869, 0.0268034 and 0.691041. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46317.1 so gap is 263.267, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46319.6), exposure 541.578, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0386074, 0.029108 and 0.753949. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46319.6 so gap is 265.774, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46362.2), exposure 584.202, 16 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0357905, 0.0292415 and 0.817018. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46362.2 so gap is 308.399, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46053.8 - 46372.3), exposure 318.428
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.110183 bg counts (14), with cf=1.32749 and errBG= 0.0294476
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7661 +/- 5.1415
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46372.3), exposure 594.231, 16 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0351865, 0.0310267 and 0.881781. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46053.8 and stop= 46372.3 so gap is 318.428, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (46053.8 - 46372.3), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (45778 - 46053.8), exposure 275.804
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0865722 bg counts (11), with cf=1.31288 and errBG= 0.0261025
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5796 +/- 5.08489
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 73
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 27
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (45778 - 46402.3), exposure 624.319, 16 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0334575, 0.0316407 and 0.945699. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46372.3 and stop= 46402.3 so gap is 30.0877, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (45778 - 46402.3) = 45778- 46402.3
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46372.3 - 46680.7), exposure 308.399
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.110183 bg counts (14), with cf=1.32022 and errBG= 0.0294476
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6578 +/- 5.11334
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46372.3 and stop= 46680.7 so gap is 308.399, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (46372.3 - 46680.7), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46053.8 - 46372.3), exposure 318.428
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.110183 bg counts (14), with cf=1.32749 and errBG= 0.0294476
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7661 +/- 5.1415
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 74
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 27
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46680.7 - 47127), exposure 446.301
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.173144 bg counts (22), with cf=1.32096 and errBG= 0.0369145
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5856 +/- 5.11627
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46680.7 and stop= 47127 so gap is 446.301, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (46680.7 - 47127), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46372.3 - 46680.7), exposure 308.399
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.110183 bg counts (14), with cf=1.32022 and errBG= 0.0294476
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6578 +/- 5.11334
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 75
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 27
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46402.3 - 47214.7), exposure 812.367, 15 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0240993, 0.02582 and 1.0714. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47127 and stop= 47214.7 so gap is 87.7558, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (46402.3 - 47214.7) = 46402.3- 47214.7
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47127 - 47548.2), exposure 421.228
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.141664 bg counts (18), with cf=1.31955 and errBG= 0.0333904
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6063 +/- 5.11078
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47127 and stop= 47548.2 so gap is 421.228, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (47127 - 47548.2), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46680.7 - 47127), exposure 446.301
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.173144 bg counts (22), with cf=1.32096 and errBG= 0.0369145
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5856 +/- 5.11627
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 76
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 27
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47548.2 - 47911.7), exposure 363.56
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.149534 bg counts (19), with cf=1.32489 and errBG= 0.0343054
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6753 +/- 5.13149
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47548.2 and stop= 47911.7 so gap is 363.56, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (47548.2 - 47911.7), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47127 - 47548.2), exposure 421.228
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.141664 bg counts (18), with cf=1.31955 and errBG= 0.0333904
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6063 +/- 5.11078
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 77
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 27
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (47214.7 - 47946.8), exposure 732.134, 15 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0268513, 0.0250026 and 0.931148. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47911.7 and stop= 47946.8 so gap is 35.1023, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (47214.7 - 47951.9), exposure 737.149, 15 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0266687, 0.0266219 and 0.998245. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47911.7 and stop= 47951.9 so gap is 40.1169, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (47214.7 - 47951.9) = 47214.7- 47951.9
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47911.7 - 48302.2), exposure 363.553
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 0.362029 bg counts (46), with cf=1.32754 and errBG= 0.0533783
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.1223 +/- 4.40351
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (47951.9 - 48302.2), exposure 323.436, 5 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0193503, 0.0162547 and 0.840024. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=47911.7 and stop= 48302.2 so gap is 390.429, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 11 (48302.2) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=390.429 whereas forward=3256.51
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47548.2 - 48302.2), exposure 727.112
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.511563 bg counts (65), with cf=1.32601 and errBG= 0.0634516
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.798 +/- 6.76188
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 11 (48302.2) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (47214.7 - 48302.2), exposure 1060.58, 20 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0244372, 0.0234605 and 0.960031. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (47548.2 - 48302.2), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 51558.7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 29
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (47214.7 - 48302.2) = 47214.7- 48302.2
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 51558.7 - 52381.1


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (51558.7 - 52320.9), exposure 762.221
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.344861 bg counts (44), with cf=1.32488 and errBG= 0.0519898
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4163 +/- 5.13169
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=51558.7 and stop= 52320.9 so gap is 762.221, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (51558.7 - 52320.9), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (47548.2 - 48302.2), exposure 727.112
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.511563 bg counts (65), with cf=1.32601 and errBG= 0.0634516
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.798 +/- 6.76188
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 78
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 29
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52320.9 - 52381.1), exposure 60.1738
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.0156755 bg counts (2), with cf=1.3489 and errBG= 0.0110843
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.67666 +/- 1.90769
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51558.7 - 52381.1), exposure 822.394, 7 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0111581, 0.0157056 and 1.40755. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52320.9 and stop= 52381.1 so gap is 60.1738, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 12 (52381.1) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=60.1738 whereas forward=1218.13
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (51558.7 - 52381.1), exposure 822.394
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.360537 bg counts (46), with cf=1.3277 and errBG= 0.0531582
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.0923 +/- 5.47471
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 12 (52381.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (51558.7 - 52381.1), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 53599.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 30
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 53599.2 - 54080.6


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (53599.2 - 54080.6), exposure 481.402
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 0.209778 bg counts (30), with cf=1.80774 and errBG= 0.0383001
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5059 +/- 5.99599
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51558.7 - 54080.6), exposure 1303.8, 14 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0159993, 0.0159006 and 0.99383. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=53599.2 and stop= 54080.6 so gap is 481.402, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 13 (54080.6) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 17 counts, because gotBinThisOrb=0 and gapBack=1699.53 whereas forward=3262.84
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (51558.7 - 54080.6), exposure 1303.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.570315 bg counts (76), with cf=1.51629 and errBG= 0.0654196
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.5913 +/- 8.02406
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 13 (54080.6) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (51558.7 - 54080.6), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 57343.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 31
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 57343.4 - 58140.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51558.7 - 57423.7), exposure 1384.03, 15 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0160366, 0.0178502 and 1.11309. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57343.4 and stop= 57423.7 so gap is 80.2339, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (51558.7 - 57423.7) = 51558.7- 57423.7
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57343.4 - 57651.8), exposure 308.399
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0859911 bg counts (11), with cf=1.34615 and errBG= 0.0259273
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.0765 +/- 5.21374
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57343.4 and stop= 57651.8 so gap is 308.399, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (57343.4 - 57651.8), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (51558.7 - 54080.6), exposure 1303.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.570315 bg counts (76), with cf=1.51629 and errBG= 0.0654196
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.5913 +/- 8.02406
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 79
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 31
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57651.8 - 58140.8), exposure 488.922
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.171982 bg counts (22), with cf=1.34448 and errBG= 0.0366667
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.247 +/- 4.84783
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (57423.7 - 58140.8), exposure 717.088, 13 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.024145, 0.0205192 and 0.849831. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57651.8 and stop= 58140.8 so gap is 488.922, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 14 (58140.8) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=488.922 whereas forward=1219.7
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57343.4 - 58140.8), exposure 797.321
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.257973 bg counts (33), with cf=1.34537 and errBG= 0.0449074
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =37.3234 +/- 7.1193
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 14 (58140.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51558.7 - 58140.8), exposure 2101.12, 28 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0188051, 0.018766 and 0.997917. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (57343.4 - 58140.8), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 59360.5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 32
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (51558.7 - 58140.8) = 51558.7- 58140.8
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 59360.5 - 59877


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (59360.5 - 59877), exposure 516.504
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.182412 bg counts (26), with cf=2.31357 and errBG= 0.0357739
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.7729 +/- 6.12168
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (59360.5 - 59877), exposure 516.504, 6 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.02657, 0.0039716 and 0.149477. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=59360.5 and stop= 59877 so gap is 516.504, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 15 (59877) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 28 counts, because gotBinThisOrb=0 and gapBack=1736.2 whereas forward=3260.26
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57343.4 - 59877), exposure 1313.83
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 35 counts and 0.440385 bg counts (59), with cf=1.53901 and errBG= 0.0573333
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.1877 +/- 9.10535
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 15 (59877) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (57343.4 - 59877), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 63137.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 33
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 63137.2 - 63899.4


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (63137.2 - 63558.5), exposure 421.228
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.214567 bg counts (27), with cf=1.31376 and errBG= 0.0412935
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.4245 +/- 5.08845
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=63137.2 and stop= 63558.5 so gap is 421.228, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (63137.2 - 63558.5), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57343.4 - 59877), exposure 1313.83
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 35 counts and 0.440385 bg counts (59), with cf=1.53901 and errBG= 0.0573333
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.1877 +/- 9.10535
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 80
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 33
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (63558.5 - 63899.4), exposure 340.992
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.18278 bg counts (23), with cf=1.31948 and errBG= 0.0381122
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.67573 +/- 3.23245
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (59360.5 - 63899.4), exposure 1278.72, 13 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.01779, 0.0157879 and 0.887458. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=63558.5 and stop= 63899.4 so gap is 340.992, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 16 (63899.4) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=340.992 whereas forward=799.732
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (63137.2 - 63899.4), exposure 762.219
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.397347 bg counts (50), with cf=1.31539 and errBG= 0.0561934
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.1006 +/- 6.02835
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 16 (63899.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (63137.2 - 63899.4), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 64699.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 34
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 64699.2 - 65644.3


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (59360.5 - 64937.4), exposure 1516.92, 15 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0169562, 0.0152625 and 0.900115. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=64699.2 and stop= 64937.4 so gap is 238.194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (59360.5 - 64937.4) = 59360.5- 64937.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (64699.2 - 65341), exposure 641.872
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.210921 bg counts (30), with cf=1.47806 and errBG= 0.0385088
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.8591 +/- 5.72478
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=64699.2 and stop= 65341 so gap is 641.872, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (64699.2 - 65341), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (63137.2 - 63899.4), exposure 762.219
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.397347 bg counts (50), with cf=1.31539 and errBG= 0.0561934
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.1006 +/- 6.02835
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 81
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 34
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (65341 - 65644.3), exposure 275.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.0773378 bg counts (11), with cf=1.4571 and errBG= 0.0233182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =5.7157 +/- 2.91439
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (64937.4 - 65644.3), exposure 679.477, 4 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00837868, 0.0234692 and 2.80106. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=65341 and stop= 65644.3 so gap is 303.26, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 17 (65644.3) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=303.26 whereas forward=3289.91
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (64699.2 - 65644.3), exposure 917.672
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 19 counts and 0.288259 bg counts (41), with cf=1.47365 and errBG= 0.0450185
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.5745 +/- 6.42381
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 17 (65644.3) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (59360.5 - 65644.3), exposure 2196.39, 19 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0142954, 0.0177985 and 1.24505. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (64699.2 - 65644.3), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 68934.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 36
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (59360.5 - 65644.3) = 59360.5- 65644.3
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 68934.2 - 70481.2


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68934.2 - 69719), exposure 784.787
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.284888 bg counts (37), with cf=2.04762 and errBG= 0.0468353
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.131 +/- 7.93098
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=68934.2 and stop= 69719 so gap is 784.787, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (68934.2 - 69719), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (64699.2 - 65644.3), exposure 917.672
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 19 counts and 0.288259 bg counts (41), with cf=1.47365 and errBG= 0.0450185
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.5745 +/- 6.42381
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 82
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 36
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (69719 - 70481.2), exposure 762.217
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 0.23869 bg counts (31), with cf=1.99866 and errBG= 0.04287
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.5081 +/- 6.62934
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68934.2 - 70481.2), exposure 1547, 12 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0153579, 0.0180216 and 1.17344. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=69719 and stop= 70481.2 so gap is 762.217, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 18 (70481.2) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=762.217 whereas forward=10754.7
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68934.2 - 70481.2), exposure 1547
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.523578 bg counts (68), with cf=2.0269 and errBG= 0.0634932
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.6383 +/- 10.336
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 18 (70481.2) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (68934.2 - 70481.2), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 81235.9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 37
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 81235.9 - 82620


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68934.2 - 81632.1), exposure 1943.16, 16 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0148704, 0.0155552 and 1.04605. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=81235.9 and stop= 81632.1 so gap is 396.154, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (68934.2 - 81632.1) = 68934.2- 81632.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81235.9 - 82043.3), exposure 807.353
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.405511 bg counts (46), with cf=1.30283 and errBG= 0.0597893
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0141 +/- 5.04644
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=81235.9 and stop= 82043.3 so gap is 807.353, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (81235.9 - 82043.3), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68934.2 - 70481.2), exposure 1547
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.523578 bg counts (68), with cf=2.0269 and errBG= 0.0634932
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.6383 +/- 10.336
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 83
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 37
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (82043.3 - 82620), exposure 576.677
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.220386 bg counts (25), with cf=1.30537 and errBG= 0.0440773
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.766 +/- 4.12833
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81632.1 - 82620), exposure 987.876, 8 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0102481, 0.0143033 and 1.3957. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=82043.3 and stop= 82620 so gap is 576.677, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 19 (82620) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=576.677 whereas forward=4281.64
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81235.9 - 82620), exposure 1384.03
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.625897 bg counts (71), with cf=1.30384 and errBG= 0.0742803
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.78 +/- 6.51994
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 19 (82620) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68934.2 - 82620), exposure 2931.03, 24 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0133039, 0.0151409 and 1.13808. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (81235.9 - 82620), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 86901.6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 38
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (68934.2 - 82620) = 68934.2- 82620
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 86901.6 - 88380.9


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (86901.6 - 88127.7), exposure 1226.07
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.49643 bg counts (57), with cf=1.33174 and errBG= 0.0657537
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.315 +/- 5.15856
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=86901.6 and stop= 88127.7 so gap is 1226.07, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (86901.6 - 88127.7), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81235.9 - 82620), exposure 1384.03
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.625897 bg counts (71), with cf=1.30384 and errBG= 0.0742803
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.78 +/- 6.51994
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 84
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 38
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (88127.7 - 88380.9), exposure 253.233
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0348372 bg counts (4), with cf=1.35525 and errBG= 0.0174186
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.30804 +/- 1.35546
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 88380.9), exposure 1479.31, 10 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00879496, 0.00514513 and 0.585009. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=88127.7 and stop= 88380.9 so gap is 253.233, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 20 (88380.9) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=253.233 whereas forward=4453.4
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (86901.6 - 88380.9), exposure 1479.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.531267 bg counts (61), with cf=1.33321 and errBG= 0.0680218
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.6231 +/- 5.33362
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 20 (88380.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (86901.6 - 88380.9), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 92834.3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 39
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 92834.3 - 94200.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 93039.9), exposure 1684.91, 15 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0115719, 0.00682239 and 0.589564. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=92834.3 and stop= 93039.9 so gap is 205.599, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 93160.3), exposure 1805.26, 16 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0115062, 0.00634826 and 0.551726. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=92834.3 and stop= 93160.3 so gap is 325.95, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 93446.1), exposure 2091.09, 16 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0098839, 0.00604499 and 0.6116. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=92834.3 and stop= 93446.1 so gap is 611.783, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 93461.1), exposure 2106.13, 17 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0104284, 0.00600181 and 0.575526. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=92834.3 and stop= 93461.1 so gap is 626.827, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 93553.9), exposure 2198.9, 18 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0105721, 0.00573279 and 0.542256. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=92834.3 and stop= 93553.9 so gap is 719.598, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 93616.6), exposure 2261.59, 19 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0108519, 0.00556877 and 0.513159. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=92834.3 and stop= 93616.6 so gap is 782.281, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 93676.8), exposure 2321.76, 19 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0105608, 0.00598263 and 0.566495. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=92834.3 and stop= 93676.8 so gap is 842.456, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (92834.3 - 93889.9), exposure 1055.58
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.513736 bg counts (59), with cf=1.30945 and errBG= 0.0668827
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.969 +/- 5.07222
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 93889.9), exposure 2534.88, 20 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0101701, 0.00544768 and 0.535659. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=92834.3 and stop= 93889.9 so gap is 1055.58, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (92834.3 - 93889.9), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (86901.6 - 88380.9), exposure 1479.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.531267 bg counts (61), with cf=1.33321 and errBG= 0.0680218
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.6231 +/- 5.33362
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 85
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 39
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 94098), exposure 2742.99, 21 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00987368, 0.00500906 and 0.507315. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=93889.9 and stop= 94098 so gap is 208.107, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (93889.9 - 94200.8), exposure 310.901
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.113196 bg counts (13), with cf=1.32798 and errBG= 0.0313949
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.50564 +/- 1.87851
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 94200.8), exposure 2845.79, 21 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00950895, 0.0052834 and 0.555624. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=93889.9 and stop= 94200.8 so gap is 310.901, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 21 (94200.8) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=310.901 whereas forward=4739.22
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (92834.3 - 94200.8), exposure 1366.48
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.626932 bg counts (72), with cf=1.31163 and errBG= 0.0738846
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.4754 +/- 5.40884
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 21 (94200.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (92834.3 - 94200.8), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 98940
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 40
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 98940 - 100319


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 98970.1), exposure 2875.87, 21 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00940157, 0.00568266 and 0.604438. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 98970.1 so gap is 30.0876, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 99045.3), exposure 2951.09, 22 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00958914, 0.00553009 and 0.576704. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99045.3 so gap is 105.307, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 99072.9), exposure 2978.67, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00950035, 0.00591765 and 0.622888. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99072.9 so gap is 132.887, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 99080.4), exposure 2986.19, 23 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00991386, 0.00590274 and 0.595403. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99080.4 so gap is 140.409, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 99213.3), exposure 3119.08, 24 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00989933, 0.00563665 and 0.569397. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99213.3 so gap is 273.297, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 99253.4), exposure 3159.2, 25 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0101832, 0.00556146 and 0.546142. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99253.4 so gap is 313.414, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 99255.9), exposure 3161.71, 26 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0105879, 0.00555705 and 0.524848. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99255.9 so gap is 315.921, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 99378.8), exposure 3284.56, 27 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0105862, 0.00533185 and 0.503662. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99378.8 so gap is 438.779, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 99391.3), exposure 3297.1, 28 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.010942, 0.00531158 and 0.485432. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99391.3 so gap is 451.316, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 99401.3), exposure 3307.13, 28 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0109088, 0.00569044 and 0.521638. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99401.3 so gap is 461.345, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (86901.6 - 99401.3) = 86901.6- 99401.3
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (98940 - 99940.4), exposure 1000.42
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.421659 bg counts (49), with cf=1.30553 and errBG= 0.0602369
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0324 +/- 5.0569
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98940 and stop= 99940.4 so gap is 1000.42, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (98940 - 99940.4), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (92834.3 - 94200.8), exposure 1366.48
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.626932 bg counts (72), with cf=1.31163 and errBG= 0.0738846
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.4754 +/- 5.40884
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 86
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 40
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (99940.4 - 100319), exposure 320.929
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.197921 bg counts (23), with cf=1.3053 and errBG= 0.0412695
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.26813 +/- 2.91923
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (99401.3 - 100319), exposure 860.002, 1 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00119121, 0.0133465 and 11.2042. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=99940.4 and stop= 100319 so gap is 379.039, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 22 (100319) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=379.039 whereas forward=4631.86
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (98940 - 100319), exposure 1321.35
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.61958 bg counts (72), with cf=1.30547 and errBG= 0.0730182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.3005 +/- 5.83902
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 22 (100319) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (86901.6 - 100319), exposure 4167.13, 29 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00890282, 0.00727115 and 0.816725. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (98940 - 100319), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 104951
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 43
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (86901.6 - 100319) = 86901.6- 100319
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 104951 - 106127


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (104951 - 106127), exposure 1175.92
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.259681 bg counts (62), with cf=3.08775 and errBG= 0.0329795
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.8124 +/- 8.17004
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (104951 - 106127), exposure 1175.92, 2 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00495912, 0.0127387 and 2.56874. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=104951 and stop= 106127 so gap is 1175.92, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 23 (106127) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5807.79 whereas forward=3246.38
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 23 (106127) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 109374 - 109499


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (104951 - 109499), exposure 1301.29
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.267354 bg counts (69), with cf=3.08775 and errBG= 0.0321856
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.7887 +/- 8.17001
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (104951 - 109499), exposure 1301.29, 2 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00447875, 0.0114959 and 2.56677. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=104951 and stop= 109499 so gap is 4547.67, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 24 (109499) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=9179.53 whereas forward=1432.78
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 24 (109499) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 110932 - 111905


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (104951 - 111641), exposure 2010.86
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.44532 bg counts (101), with cf=2.15402 and errBG= 0.044311
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.351 +/- 8.34302
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=104951 and stop= 111641 so gap is 6690.02, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (104951 - 111641), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (98940 - 100319), exposure 1321.35
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.61958 bg counts (72), with cf=1.30547 and errBG= 0.0730182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.3005 +/- 5.83902
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 87
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 45
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (111641 - 111905), exposure 235.684
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.150159 bg counts (27), with cf=1.337 and errBG= 0.0288982
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.13624 +/- 1.33756
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (104951 - 111905), exposure 2246.54, 8 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00607118, 0.00835918 and 1.37686. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=111641 and stop= 111905 so gap is 263.224, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 25 (111905) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=263.224 whereas forward=3262.64
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (104951 - 111905), exposure 2246.54
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.595479 bg counts (128), with cf=2.10295 and errBG= 0.0526334
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.395 +/- 8.41254
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 25 (111905) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (104951 - 111905), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 115167
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 47
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 115167 - 115441


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (115167 - 115441), exposure 273.296
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.146329 bg counts (17), with cf=1.3321 and errBG= 0.0354899
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =5.13349 +/- 2.66463
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (104951 - 115441), exposure 2519.84, 11 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00698153, 0.00790655 and 1.13249. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=115167 and stop= 115441 so gap is 273.296, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 26 (115441) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=3535.93 whereas forward=1314.2
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 26 (115441) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 116755 - 117675


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (115167 - 117414), exposure 932.718
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.419538 bg counts (48), with cf=1.2981 and errBG= 0.0605551
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9269 +/- 5.02812
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=115167 and stop= 117414 so gap is 2246.92, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (115167 - 117414), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (104951 - 111905), exposure 2246.54
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.595479 bg counts (128), with cf=2.10295 and errBG= 0.0526334
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.395 +/- 8.41254
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 88
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 48
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (117414 - 117675), exposure 178.016
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.502353 bg counts (57), with cf=1.28199 and errBG= 0.0665383
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =0.63798 +/- 1.28483
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (104951 - 117675), exposure 3357.27, 15 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00650095, 0.00895643 and 1.37771. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=117414 and stop= 117675 so gap is 261.142, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 27 (117675) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=261.142 whereas forward=3278.35
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (115167 - 117675), exposure 1110.73
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.921891 bg counts (105), with cf=1.29709 and errBG= 0.0899674
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5577 +/- 5.18967
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (115167 - 117675), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 120954
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 52
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (104951 - 117675) = 104951- 117675
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 120954 - 121696


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (120954 - 121696), exposure 742.161
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.195235 bg counts (36), with cf=1.46524 and errBG= 0.0325391
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.50538 +/- 3.58941
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (120954 - 121696), exposure 742.161, 0 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -0.000153453, 0.0116851 and -76.148. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=120954 and stop= 121696 so gap is 742.161, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 28 (121696) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 16 counts, because gotBinThisOrb=0 and gapBack=4020.51 whereas forward=46530.2
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (115167 - 121696), exposure 1852.89
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 1.11713 bg counts (141), with cf=1.34295 and errBG= 0.094079
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =28.0447 +/- 6.30026
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 28 (121696) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (115167 - 121696), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 168226
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 53
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 168226 - 169730


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (168226 - 169730), exposure 1504.38
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.137952 bg counts (61), with cf=3.89196 and errBG= 0.0176629
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =3.35505 +/- 3.89256
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (120954 - 169730), exposure 2246.54, 0 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -8.08941e-05, 0.0055236 and -68.2818. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=168226 and stop= 169730 so gap is 1504.38, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 29 (169730) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=48034.6 whereas forward=4316.52
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 29 (169730) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 174047 - 175514


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (168226 - 175514), exposure 2971.15
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.175832 bg counts (128), with cf=3.89196 and errBG= 0.0155415
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =3.20763 +/- 3.89243
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (120954 - 175514), exposure 3713.31, 0 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -5.47264e-05, 0.00333376 and -60.9168. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=168226 and stop= 175514 so gap is 7287.67, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 30 (175514) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=53817.9 whereas forward=4299.78
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 30 (175514) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 179813 - 181278


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (168226 - 181278), exposure 4407.83
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 1.16039 bg counts (358), with cf=1.69014 and errBG= 0.0613287
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.6303 +/- 5.60653
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (120954 - 181278), exposure 5149.99, 4 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000858748, 0.00405709 and 4.72443. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=168226 and stop= 181278 so gap is 13051.6, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 31 (181278) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=59581.9 whereas forward=4424.28
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 31 (181278) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 185702 - 186539


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (168226 - 186539), exposure 5245.27
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 1.29705 bg counts (400), with cf=1.65748 and errBG= 0.0648527
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.0549 +/- 6.20265
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (120954 - 186539), exposure 5987.43, 6 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00123495, 0.00372487 and 3.01622. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=168226 and stop= 186539 so gap is 18313.3, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 32 (186539) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=64843.6 whereas forward=5103.62
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 32 (186539) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 191643 - 192851


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (168226 - 191693), exposure 5295.42
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.31371 bg counts (404), with cf=1.64773 and errBG= 0.0653596
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.5513 +/- 6.38255
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=168226 and stop= 191693 so gap is 23467.1, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (168226 - 191693), with lastBin= 0xaf2b10 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (115167 - 121696), exposure 1852.89
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 1.11713 bg counts (141), with cf=1.34295 and errBG= 0.094079
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =28.0447 +/- 6.30026
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 89
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 58
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (191693 - 192851), exposure 1158.37
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.170747 bg counts (41), with cf=1.52651 and errBG= 0.0266661
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.0044 +/- 4.82741
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (120954 - 192851), exposure 7195.95, 11 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00206543, 0.0043527 and 2.1074. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=191693 and stop= 192851 so gap is 1158.37, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 33 (192851) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=1158.37 whereas forward=4779.12
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (168226 - 192851), exposure 6453.79
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 1.48446 bg counts (445), with cf=1.59924 and errBG= 0.0703701
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =37.6071 +/- 7.997
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 33 (192851) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (168226 - 192851), with lastBin= 0 and workMinC was 8
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 197631
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 59
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 197631 - 198631


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (197631 - 198631), exposure 972.832
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.194653 bg counts (35), with cf=1.37628 and errBG= 0.0329024
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.61348 +/- 3.07778
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (120954 - 198631), exposure 8168.78, 13 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00214816, 0.004316 and 2.00916. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=197631 and stop= 198631 so gap is 1000.46, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 34 (198631) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5779.58 whereas forward=4758.3
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 34 (198631) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 203389 - 204396


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (197631 - 204396), exposure 1895.52
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 0.558667 bg counts (101), with cf=1.38212 and errBG= 0.0555895
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.667 +/- 4.14709
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (120954 - 204396), exposure 9091.47, 14 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.002049, 0.00431241 and 2.10465. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=197631 and stop= 204396 so gap is 6765.1, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 35 (204396) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=11544.2 whereas forward=3655.12
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 35 (204396) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 208051 - 209415


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (120954 - 209124), exposure 10164.6, 15 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00196483, 0.00412957 and 2.10174. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=197631 and stop= 209124 so gap is 11493.3, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (120954 - 209124) = 120954- 209124
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (197631 - 209415), exposure 3259.49
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.75182 bg counts (161), with cf=1.40387 and errBG= 0.0592517
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.1949 +/- 5.06241
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (209124 - 209415), exposure 290.844, 1 soft counts and 0 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00489714, -2.21371e-05 and -0.0045204. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=197631 and stop= 209415 so gap is 11784.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 36 (209415) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 25 counts, because gotBinThisOrb=0 and gapBack=16563.3 whereas forward=39804.3
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (168226 - 209415), exposure 9713.28
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 38 counts and 2.23628 bg counts (606), with cf=1.5324 and errBG= 0.0908426
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =54.8045 +/- 9.4474
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 36 (209415) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (120954 - 209415), exposure 10455.4, 16 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00204673, 0.00401374 and 1.96105. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (168226 - 209415), with lastBin= 0 and workMinC was 8
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 249219
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 66
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (120954 - 209415) = 120954- 209415
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 249219 - 249254


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (249219 - 249254), exposure 35.1022
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0074651 bg counts (1), with cf=1.3309 and errBG= 0.0074651
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.32097 +/- 1.33094
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 249254), exposure 35.1022, 1 soft counts and 0 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.037915, -0.000212668 and -0.00560905. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=249219 and stop= 249254 so gap is 35.1022, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 37 (249254) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=39839.4 whereas forward=189.944
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 37 (249254) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 249444 - 249519


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (249219 - 249519), exposure 110.321
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0373255 bg counts (5), with cf=1.3309 and errBG= 0.0166925
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.28122 +/- 1.33109
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 249519), exposure 110.321, 1 soft counts and 0 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0119738, -0.000270668 and -0.022605. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=249219 and stop= 249519 so gap is 300.265, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 38 (249519) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=40104.5 whereas forward=67.6557
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 38 (249519) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 249587 - 249900


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (249219 - 249900), exposure 423.734
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.171697 bg counts (23), with cf=1.35438 and errBG= 0.0358013
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =5.18497 +/- 2.70919
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 249900), exposure 423.734, 4 soft counts and 0 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0125227, -0.000211409 and -0.016882. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=249219 and stop= 249900 so gap is 681.334, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 39 (249900) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 38 counts, because gotBinThisOrb=0 and gapBack=40485.6 whereas forward=51278.8
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (168226 - 249900), exposure 10137
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 42 counts and 2.40798 bg counts (629), with cf=1.51545 and errBG= 0.0960123
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =59.9997 +/- 9.82232
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 39 (249900) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (168226 - 249900), with lastBin= 0 and workMinC was 8
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 301179
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf2b10 which has initial GTIBin: 69
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 301179 - 302699


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301179 - 302699), exposure 1519.42
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.202538 bg counts (67), with cf=1.45437 and errBG= 0.024744
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.9773 +/- 3.25228
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 302699), exposure 1943.16, 7 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00493192, 0.00132421 and 0.268498. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=301179 and stop= 302699 so gap is 1519.42, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 40 (302699) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=52798.2 whereas forward=4240.41
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 40 (302699) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 306939 - 308458


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301179 - 308458), exposure 3011.27
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.350525 bg counts (120), with cf=1.47214 and errBG= 0.0319984
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =9.78893 +/- 3.89519
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 308458), exposure 3435, 7 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00276489, 0.00159247 and 0.575959. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=301179 and stop= 308458 so gap is 7278.53, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 41 (308458) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=58557.3 whereas forward=4241.5
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 41 (308458) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 312699 - 314219


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301179 - 314219), exposure 4530.69
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.483212 bg counts (170), with cf=1.50824 and errBG= 0.0370607
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.3536 +/- 4.76979
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 314219), exposure 4954.42, 10 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00286381, 0.00107954 and 0.376959. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=301179 and stop= 314219 so gap is 13039.5, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 42 (314219) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=64318.3 whereas forward=4300.58
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 42 (314219) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 318519 - 320039


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301179 - 320039), exposure 6050.11
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 0.684631 bg counts (239), with cf=1.50368 and errBG= 0.0442851
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.022 +/- 5.62663
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 320039), exposure 6473.85, 13 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00286143, 0.00103227 and 0.360751. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=301179 and stop= 320039 so gap is 18859.5, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 43 (320039) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=70138.3 whereas forward=4225.19
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 43 (320039) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 324264 - 325199


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301179 - 324567), exposure 6353.5
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.732053 bg counts (254), with cf=1.50657 and errBG= 0.0459331
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.4956 +/- 5.83532
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=301179 and stop= 324567 so gap is 23388, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (301179 - 324567), with lastBin= 0xaf0fa0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (168226 - 249900), exposure 10137
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 42 counts and 2.40798 bg counts (629), with cf=1.51545 and errBG= 0.0960123
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =59.9997 +/- 9.82232
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 90
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 74
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 324635), exposure 6844.93, 15 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00314683, 0.000968113 and 0.307647. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=324567 and stop= 324635 so gap is 67.6974, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 324863), exposure 7073.09, 15 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00304268, 0.00114472 and 0.376222. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=324567 and stop= 324863 so gap is 295.862, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (324567 - 325199), exposure 631.84
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 3 counts and 0.0790354 bg counts (25), with cf=1.49286 and errBG= 0.0158071
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =4.36058 +/- 2.58581
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 325199), exposure 7409.07, 15 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00289904, 0.00129059 and 0.445177. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=324567 and stop= 325199 so gap is 631.84, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 44 (325199) and the bin is not full 3 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=631.84 whereas forward=4824.78
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301179 - 325199), exposure 6985.34
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 18 counts and 0.811088 bg counts (279), with cf=1.50428 and errBG= 0.0485586
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.857 +/- 6.38254
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 44 (325199) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (301179 - 325199), with lastBin= 0 and workMinC was 7
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 330024
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 75
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 330024 - 331561


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 330059), exposure 7444.17, 16 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0030803, 0.00128387 and 0.416799. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=330024 and stop= 330059 so gap is 35.1022, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 330307), exposure 7692.4, 17 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00316953, 0.00123816 and 0.390644. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=330024 and stop= 330307 so gap is 283.326, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 330771), exposure 8156.25, 18 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00316222, 0.00116025 and 0.36691. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=330024 and stop= 330771 so gap is 747.178, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 331077), exposure 8462.14, 19 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0032178, 0.0011122 and 0.345639. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=330024 and stop= 331077 so gap is 1053.07, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (330024 - 331561), exposure 1536.97
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.215761 bg counts (68), with cf=1.45567 and errBG= 0.0261649
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.96427 +/- 3.2552
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 331561), exposure 8946.05, 19 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00304061, 0.0012076 and 0.397155. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=330024 and stop= 331561 so gap is 1536.97, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 45 (331561) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 18 counts, because gotBinThisOrb=0 and gapBack=6361.75 whereas forward=34125.2
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301179 - 331561), exposure 8522.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 1.02685 bg counts (347), with cf=1.49371 and errBG= 0.0551241
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.8216 +/- 7.16407
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 45 (331561) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (301179 - 331561), with lastBin= 0 and workMinC was 7
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 365686
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0xaf0fa0 which has initial GTIBin: 76
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 365686 - 366240


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 365686 - 366240
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 365686 - 366240 the cf is 1.4691
++tructures/grbBin.cpp::        binData:  line  405  INFO   >>  This bin is empty, so found a emptyBin CF of 1.4691
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (365686 - 366240), exposure 554.113
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 0 counts and 0.0979736 bg counts (30), with cf=1.4691 and errBG= 0.0178874
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =-0.143933 +/- 0.0262784
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 366240), exposure 9500.16, 19 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00285568, 0.00112954 and 0.39554. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=365686 and stop= 366240 so gap is 554.113, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 46 (366240) and the bin is not full 0 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=34679.3 whereas forward=5265.69
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 46 (366240) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 371506 - 372032


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (365686 - 372032), exposure 1053.07
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.189416 bg counts (58), with cf=1.47152 and errBG= 0.0248715
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.19279 +/- 1.47197
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 372032), exposure 9999.11, 19 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00270454, 0.00121557 and 0.449456. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=365686 and stop= 372032 so gap is 6345.76, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 47 (372032) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=40470.9 whereas forward=4258.65
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 47 (372032) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 376290 - 377579


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 376303), exposure 10011.6, 19 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00270115, 0.00137932 and 0.510642. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=365686 and stop= 376303 so gap is 10616.9, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (365686 - 377579), exposure 2341.82
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 3 counts and 0.304768 bg counts (109), with cf=1.81451 and errBG= 0.0291915
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =4.89053 +/- 3.14327
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 377579), exposure 11287.9, 20 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00259081, 0.00121467 and 0.468839. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=365686 and stop= 377579 so gap is 11893.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 48 (377579) and the bin is not full 3 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=46018.3 whereas forward=4470.87
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 48 (377579) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 382050 - 383339


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 382589), exposure 11826.9, 20 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00246937, 0.00127656 and 0.516956. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=365686 and stop= 382589 so gap is 16903.1, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 382870), exposure 12107.8, 20 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00241087, 0.00136318 and 0.565432. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=365686 and stop= 382870 so gap is 17183.9, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (365686 - 383339), exposure 3630.57
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.485021 bg counts (164), with cf=1.62271 and errBG= 0.0378738
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.9492 +/- 3.97528
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 383339), exposure 12576.6, 20 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00231547, 0.00142097 and 0.613683. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=365686 and stop= 383339 so gap is 17652.8, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 49 (383339) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=51778 whereas forward=4480.25
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 49 (383339) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 387819 - 389100


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 387894), exposure 12651.8, 21 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00260597, 0.00141199 and 0.541829. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=365686 and stop= 387894 so gap is 22208.3, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 388529), exposure 13286.2, 21 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00247742, 0.00155679 and 0.628393. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=365686 and stop= 388529 so gap is 22842.6, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (365686 - 389100), exposure 4911.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 0.613287 bg counts (221), with cf=2.16147 and errBG= 0.0412541
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.1276 +/- 6.48501
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (249219 - 389100), exposure 13857.8, 21 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00237231, 0.00168567 and 0.710559. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=365686 and stop= 389100 so gap is 23414.3, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 50 (389100) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=57539.4 whereas forward=4538.97
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (249219 - 389100) = 249219- 389100
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 393639 - 394860


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 83, last was 82 so increasing dead to 2.50852
++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (365686 - 394860), exposure 6130.35
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.798479 bg counts (280), with cf=1.98131 and errBG= 0.0477182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.1937 +/- 6.8641
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (393639 - 394860), exposure 1218.55, 2 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00227827, 0.00105019 and 0.460957. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=365686 and stop= 394860 so gap is 29174.3, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  787  INFO   >>  I'm on the last event, so save the previous bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301179 - 331561), exposure 8522.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 1.02685 bg counts (347), with cf=1.49371 and errBG= 0.0551241
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.8216 +/- 7.16407
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 91
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0xaf0fa0
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (365686 - 394860), exposure 6130.35
++taStructures/bin.cpp::   bayesian_bin:  line  273  INFO   >>  Making a Bayesian bin - I have 12 counts and 0.798479 bg counts, with cf=1.98131
++taStructures/bin.cpp::   bayesian_bin:  line  274  INFO   >>    Therefore net =22.1946 + 7.60228 -6.26291 and sigma=234.743
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 92
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (393639 - 394860), exposure 1218.55, 2 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00227827, 0.00105019 and 0.460957. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for PC mode.
++/genlc_cpp/genlc.cpp::           main:  line  397  INFO   >>  COMPLETE

