++lUtils/createLog.cpp::      createLog:  line   51  INFO   >>  Created FileAppender: 'genlc.log', level info
++/genlc_cpp/genlc.cpp::           main:  line  151  INFO   >>  Starting to run genlc.cpp, mode=0
++/genlc_cpp/genlc.cpp::           main:  line  152  INFO   >>  Argparsing reported: Selected GRB binning.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: WT, with files: wtsourcetotal.evt, wtbacktotal.evt, and wtcorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 384.053 - 3000
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	384.053 - 445.812
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - WT mode, suffix = 
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 30 ct/bin at rateFact=10 and binFact= 1.5 with minT 0.5 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file WTCURVE.qdp, reading from wtsourcetotal.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (384.053 - 389.282), exposure 5.22884
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 44 counts and 0 bg counts (0), with cf=1.14873 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =50.5442 +/- 7.63003
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=384.053 and stop= 389.282 so gap is 5.22884, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (384.053 - 389.282), with lastBin= 0 and workMinC was 30
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 389.561), exposure 5.50816, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.25653, 3.33681 and 0.533333. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 389.561 so gap is 0.279324, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 389.771), exposure 5.7181, 31 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.22771, 3.2143 and 0.516129. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 389.771 so gap is 0.489261, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 389.808), exposure 5.75546, 32 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.38688, 3.19344 and 0.5. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 389.808 so gap is 0.526623, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 390.255), exposure 6.20202, 35 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.48266, 3.14872 and 0.485714. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 390.255 so gap is 0.973185, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 390.458), exposure 6.40482, 36 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.45675, 3.04902 and 0.472222. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 390.458 so gap is 1.17599, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 390.618), exposure 6.56495, 37 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.47425, 2.97465 and 0.459459. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 390.618 so gap is 1.33611, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 390.737), exposure 6.68415, 38 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.53065, 2.9216 and 0.447368. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 390.737 so gap is 1.45531, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 390.993), exposure 6.94034, 38 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.28957, 2.97927 and 0.473684. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 390.993 so gap is 1.71151, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 391.143), exposure 7.08979, 38 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.157, 3.0785 and 0.5. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 391.143 so gap is 1.86095, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 391.273), exposure 7.21967, 39 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.20535, 3.02312 and 0.487179. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 391.273 so gap is 1.99083, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 391.317), exposure 7.26415, 40 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.32549, 3.00461 and 0.475. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 391.317 so gap is 2.03531, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 391.326), exposure 7.27304, 41 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.4757, 3.00093 and 0.463415. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 391.326 so gap is 2.0442, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 391.358), exposure 7.30507, 41 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.44731, 3.14503 and 0.487805. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 391.358 so gap is 2.07623, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 391.49), exposure 7.43672, 41 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.33317, 3.24382 and 0.512195. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 391.49 so gap is 2.20788, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 391.497), exposure 7.44384, 42 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.48143, 3.24072 and 0.5. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 391.497 so gap is 2.215, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 391.682), exposure 7.62887, 43 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.47481, 3.16212 and 0.488372. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 391.682 so gap is 2.40003, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 391.824), exposure 7.7712, 44 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.50404, 3.1042 and 0.477273. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 391.824 so gap is 2.54236, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 391.975), exposure 7.92243, 45 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.52489, 3.04495 and 0.466667. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 391.975 so gap is 2.69359, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 392.039), exposure 7.98647, 46 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.61639, 3.02053 and 0.456522. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 392.039 so gap is 2.75764, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 392.054), exposure 8.00071, 47 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.7482, 3.01515 and 0.446809. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 392.054 so gap is 2.77187, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 392.516), exposure 8.46327, 47 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.37938, 2.98609 and 0.468085. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 392.516 so gap is 3.23443, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 392.53), exposure 8.4775, 48 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.50417, 2.98108 and 0.458333. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 392.53 so gap is 3.24866, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 392.662), exposure 8.60916, 48 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.40471, 3.06892 and 0.479167. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 392.662 so gap is 3.38032, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 392.678), exposure 8.62517, 48 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.39282, 3.19641 and 0.5. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 392.678 so gap is 3.39633, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 392.728), exposure 8.67498, 48 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.35611, 3.31047 and 0.520833. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 392.728 so gap is 3.44615, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (389.282 - 392.749), exposure 3.4675
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.14873 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.462 +/- 6.29548
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 392.749), exposure 8.69633, 49 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.4726, 3.30235 and 0.510204. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=389.282 and stop= 392.749 so gap is 3.4675, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (389.282 - 392.749), with lastBin= 0x2075fa0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (384.053 - 389.282), exposure 5.22884
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 44 counts and 0 bg counts (0), with cf=1.14873 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =50.5442 +/- 7.63003
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2075fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 392.772), exposure 8.71946, 50 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.58717, 3.29359 and 0.5. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.749 and stop= 392.772 so gap is 0.0231287, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 392.783), exposure 8.73014, 50 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.57912, 3.42114 and 0.52. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.749 and stop= 392.783 so gap is 0.0338035, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 392.853), exposure 8.79952, 50 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.52724, 3.52471 and 0.54. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.749 and stop= 392.853 so gap is 0.10319, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 393.128), exposure 9.07529, 51 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.45548, 3.41761 and 0.529412. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.749 and stop= 393.128 so gap is 0.378955, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 393.308), exposure 9.25498, 51 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.33014, 3.47537 and 0.54902. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.749 and stop= 393.308 so gap is 0.558647, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 393.865), exposure 9.81185, 51 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.97087, 3.3952 and 0.568627. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.749 and stop= 393.865 so gap is 1.11552, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 393.909), exposure 9.85633, 52 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.06048, 3.37988 and 0.557692. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.749 and stop= 393.909 so gap is 1.15999, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 394.139), exposure 10.0858, 53 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.03646, 3.30297 and 0.54717. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.749 and stop= 394.139 so gap is 1.3895, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (384.053 - 394.151), exposure 10.0983, 53 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 6.02902, 3.41265 and 0.566038. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.749 and stop= 394.151 so gap is 1.40196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (384.053 - 394.151) = 384.053- 394.151
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (392.749 - 398.074), exposure 5.32491
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.16619 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.9856 +/- 6.38988
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.749 and stop= 398.074 so gap is 5.32491, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (392.749 - 398.074), with lastBin= 0x2077c90 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (389.282 - 392.749), exposure 3.4675
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.14873 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.462 +/- 6.29548
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 403.933), exposure 9.78162, 30 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.60344, 2.39961 and 0.665924. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=398.074 and stop= 403.933 so gap is 5.85867, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (398.074 - 403.961), exposure 5.88714
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.17492 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =35.2475 +/- 6.4372
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 403.961), exposure 9.81009, 31 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.71275, 2.39265 and 0.644442. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=398.074 and stop= 403.961 so gap is 5.88714, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (398.074 - 403.961), with lastBin= 0x2075fa0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (392.749 - 398.074), exposure 5.32491
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.16619 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.9856 +/- 6.38988
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2075fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 404.451), exposure 10.2994, 33 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.76453, 2.50714 and 0.665991. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 404.451 so gap is 0.489262, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 405.15), exposure 10.9986, 36 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.84568, 2.66823 and 0.693825. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 405.15 so gap is 1.18846, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 405.346), exposure 11.1943, 37 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.88013, 2.62159 and 0.675644. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 405.346 so gap is 1.38417, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 405.479), exposure 11.3277, 38 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.9349, 2.5907 and 0.658391. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 405.479 so gap is 1.5176, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 405.522), exposure 11.3704, 38 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.92012, 2.68108 and 0.683927. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 405.522 so gap is 1.5603, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 405.737), exposure 11.5857, 39 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.94553, 2.7295 and 0.691797. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 405.737 so gap is 1.77557, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 405.879), exposure 11.728, 40 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.99469, 2.69638 and 0.67499. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 405.879 so gap is 1.9179, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 406.059), exposure 11.9077, 41 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.03, 2.65569 and 0.65898. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 406.059 so gap is 2.09759, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 406.32), exposure 12.1692, 42 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.03692, 2.59862 and 0.643713. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 406.32 so gap is 2.35911, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 406.337), exposure 12.1852, 43 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.12502, 2.5952 and 0.629136. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 406.337 so gap is 2.37512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 406.578), exposure 12.4272, 44 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.1363, 2.54467 and 0.615205. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 406.578 so gap is 2.61709, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 406.61), exposure 12.4592, 45 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.21702, 2.53813 and 0.601878. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 406.61 so gap is 2.64911, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 406.868), exposure 12.7172, 46 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.22097, 2.48664 and 0.589116. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 406.868 so gap is 2.90708, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 406.895), exposure 12.7439, 47 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.30145, 2.48144 and 0.576884. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 406.895 so gap is 2.93377, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 407.137), exposure 12.9858, 48 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.30895, 2.4352 and 0.56515. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 407.137 so gap is 3.17573, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 407.205), exposure 13.0534, 48 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.28663, 2.50978 and 0.585491. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 407.205 so gap is 3.24334, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 407.516), exposure 13.3648, 48 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.18677, 2.53648 and 0.605832. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 407.516 so gap is 3.55469, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (394.151 - 407.648), exposure 13.4964, 48 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.14593, 2.59607 and 0.626173. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 407.648 so gap is 3.68634, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (394.151 - 407.648) = 394.151- 407.648
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (403.961 - 408.464), exposure 4.50295
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.15043 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.5129 +/- 6.30287
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=403.961 and stop= 408.464 so gap is 4.50295, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (403.961 - 408.464), with lastBin= 0x2077c90 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (398.074 - 403.961), exposure 5.88714
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.17492 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =35.2475 +/- 6.4372
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (408.464 - 412.77), exposure 4.30549
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.641975 bg counts (1), with cf=1.13819 and errBG= 0.641975
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.415 +/- 6.27824
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=408.464 and stop= 412.77 so gap is 4.30549, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (408.464 - 412.77), with lastBin= 0x2075fa0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (403.961 - 408.464), exposure 4.50295
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.15043 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.5129 +/- 6.30287
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2075fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 413.884), exposure 6.23583, 30 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.47572, 1.52554 and 0.278601. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 413.884 so gap is 1.11374, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 414.22), exposure 6.57208, 30 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.19557, 1.62067 and 0.311934. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 414.22 so gap is 1.44999, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 414.679), exposure 7.03109, 31 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.01827, 1.51487 and 0.301872. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 414.679 so gap is 1.909, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 414.821), exposure 7.17341, 32 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.07737, 1.48482 and 0.292438. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 414.821 so gap is 2.05132, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 414.908), exposure 7.26059, 32 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.01641, 1.62375 and 0.323688. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 414.908 so gap is 2.1385, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 415.275), exposure 7.62709, 33 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.92458, 1.54573 and 0.31388. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 415.275 so gap is 2.505, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 415.382), exposure 7.73384, 33 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.85661, 1.67156 and 0.344183. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 415.382 so gap is 2.61175, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 415.419), exposure 7.7712, 34 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.97972, 1.66352 and 0.33406. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 415.419 so gap is 2.64911, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 415.538), exposure 7.8904, 35 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.04875, 1.63839 and 0.324515. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 415.538 so gap is 2.76831, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 415.693), exposure 8.04519, 36 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.09308, 1.60687 and 0.315501. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 415.693 so gap is 2.9231, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 415.746), exposure 8.09856, 37 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.20006, 1.59628 and 0.306974. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 415.746 so gap is 2.97647, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 415.773), exposure 8.12525, 38 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.32306, 1.59104 and 0.298895. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 415.773 so gap is 3.00316, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 415.812), exposure 8.16439, 39 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.43695, 1.58341 and 0.291231. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 415.812 so gap is 3.0423, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 415.91), exposure 8.26224, 40 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.51032, 1.56466 and 0.283951. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 415.91 so gap is 3.14015, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 415.956), exposure 8.3085, 41 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.61629, 1.55595 and 0.277042. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 415.956 so gap is 3.18641, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 416.022), exposure 8.37433, 42 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.70772, 1.54372 and 0.270461. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 416.022 so gap is 3.25224, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 416.024), exposure 8.3761, 43 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.84205, 1.54339 and 0.264186. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 416.024 so gap is 3.25401, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 416.598), exposure 8.95076, 44 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.51221, 1.4443 and 0.262018. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 416.598 so gap is 3.82867, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 416.956), exposure 9.30837, 45 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.42242, 1.38881 and 0.256124. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 416.956 so gap is 4.18628, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 416.97), exposure 9.3226, 45 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.41414, 1.50849 and 0.278621. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 416.97 so gap is 4.20051, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 416.981), exposure 9.33328, 46 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.52959, 1.50677 and 0.272491. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 416.981 so gap is 4.21119, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 417.063), exposure 9.41512, 46 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.48153, 1.61427 and 0.294493. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 417.063 so gap is 4.29303, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 417.44), exposure 9.79229, 46 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.27039, 1.66805 and 0.316494. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 417.44 so gap is 4.6702, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 417.561), exposure 9.91328, 47 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.3206, 1.64769 and 0.309681. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 417.561 so gap is 4.79119, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (412.77 - 417.661), exposure 4.89082
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.641975 bg counts (1), with cf=1.13715 and errBG= 0.641975
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.3845 +/- 6.2722
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 417.661), exposure 10.0129, 47 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.26766, 1.74469 and 0.331208. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412.77 and stop= 417.661 so gap is 4.89082, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (412.77 - 417.661), with lastBin= 0x2077c90 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (408.464 - 412.77), exposure 4.30549
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.641975 bg counts (1), with cf=1.13819 and errBG= 0.641975
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.415 +/- 6.27824
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 417.675), exposure 10.0271, 47 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.26019, 1.85545 and 0.352735. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 417.675 so gap is 0.0142331, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 417.774), exposure 10.1268, 47 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.20843, 1.94932 and 0.374262. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 417.774 so gap is 0.113864, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 418.175), exposure 10.5271, 48 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.11823, 1.87519 and 0.366375. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 418.175 so gap is 0.51417, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 418.401), exposure 10.753, 49 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.11627, 1.83579 and 0.358814. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 418.401 so gap is 0.74012, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 418.468), exposure 10.8206, 49 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.0843, 1.92925 and 0.379452. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 418.468 so gap is 0.807727, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 418.474), exposure 10.826, 50 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.18667, 1.9283 and 0.37178. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 418.474 so gap is 0.813064, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 418.488), exposure 10.8402, 51 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 5.2846, 1.92577 and 0.364411. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 418.488 so gap is 0.827297, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 419.424), exposure 11.776, 51 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.86464, 1.86915 and 0.384231. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 419.424 so gap is 1.76312, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 419.748), exposure 12.0998, 51 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.73446, 1.91296 and 0.404051. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 419.748 so gap is 2.08692, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 419.883), exposure 12.235, 52 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.77493, 1.89182 and 0.396199. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 419.883 so gap is 2.22214, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 419.897), exposure 12.2493, 53 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.86208, 1.88962 and 0.388646. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 419.897 so gap is 2.23637, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 420.134), exposure 12.4859, 53 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.76993, 1.94475 and 0.40771. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 420.134 so gap is 2.473, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 420.308), exposure 12.6603, 54 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.79392, 1.91797 and 0.400083. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 420.308 so gap is 2.64735, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 420.333), exposure 12.6852, 55 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.87401, 1.9142 and 0.392736. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 420.333 so gap is 2.67226, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 420.363), exposure 12.7154, 55 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.86242, 1.99894 and 0.4111. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 420.363 so gap is 2.7025, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 420.614), exposure 12.9663, 56 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.85591, 1.96027 and 0.403687. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 420.614 so gap is 2.95336, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 420.685), exposure 13.0374, 57 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.91649, 1.94957 and 0.396536. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 420.685 so gap is 3.02453, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 420.897), exposure 13.2492, 57 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.83793, 2.00411 and 0.414249. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 420.897 so gap is 3.23624, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 420.904), exposure 13.2563, 58 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.92098, 2.00303 and 0.407039. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 420.904 so gap is 3.24336, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 421.278), exposure 13.6299, 59 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.86939, 1.94813 and 0.400076. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 421.278 so gap is 3.61698, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 421.294), exposure 13.6459, 59 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.86367, 2.02904 and 0.417183. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 421.294 so gap is 3.63299, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 421.619), exposure 13.9715, 60 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.8316, 1.98176 and 0.410167. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 421.619 so gap is 3.95857, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 421.922), exposure 14.2739, 61 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.80876, 1.93977 and 0.403382. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 421.922 so gap is 4.26102, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 422.107), exposure 14.459, 62 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.82575, 1.91495 and 0.396818. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 422.107 so gap is 4.44605, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 422.123), exposure 14.475, 63 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.89885, 1.91283 and 0.390465. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 422.123 so gap is 4.46207, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 422.329), exposure 14.6814, 64 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.90731, 1.88594 and 0.384311. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 422.329 so gap is 4.66845, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 422.516), exposure 14.8682, 65 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.92202, 1.86224 and 0.378349. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 422.516 so gap is 4.85525, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 422.966), exposure 15.3183, 65 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.77739, 1.88164 and 0.393864. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 422.966 so gap is 5.30537, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 423.082), exposure 15.4339, 66 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.81516, 1.86754 and 0.387847. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 423.082 so gap is 5.42101, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (417.661 - 423.368), exposure 5.70744
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.13535 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.0606 +/- 6.21958
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 423.368), exposure 15.7204, 67 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.79965, 1.83352 and 0.38201. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=417.661 and stop= 423.368 so gap is 5.70744, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (417.661 - 423.368), with lastBin= 0x2075fa0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (412.77 - 417.661), exposure 4.89082
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.641975 bg counts (1), with cf=1.13715 and errBG= 0.641975
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.3845 +/- 6.2722
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2075fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 423.445), exposure 15.7969, 68 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.84828, 1.82464 and 0.376347. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 423.445 so gap is 0.0765001, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 423.516), exposure 15.868, 69 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.89808, 1.81645 and 0.37085. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 423.516 so gap is 0.147665, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 423.893), exposure 16.2452, 70 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.80932, 1.77428 and 0.368925. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 423.893 so gap is 0.524841, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 423.998), exposure 16.3502, 70 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.77844, 1.83233 and 0.383457. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 423.998 so gap is 0.62981, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 424.019), exposure 16.3715, 71 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.84156, 1.82994 and 0.377965. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 424.019 so gap is 0.65116, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 424.121), exposure 16.4729, 72 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.88068, 1.81867 and 0.372627. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 424.121 so gap is 0.75257, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 424.245), exposure 16.5975, 73 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.91247, 1.80503 and 0.367438. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 424.245 so gap is 0.877109, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 424.601), exposure 16.9533, 74 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.87633, 1.76714 and 0.362392. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 424.601 so gap is 1.23294, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 425.181), exposure 17.5333, 75 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.77978, 1.70869 and 0.357482. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 425.181 so gap is 1.81293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 425.263), exposure 17.6151, 76 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.82203, 1.70075 and 0.352704. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 425.263 so gap is 1.89477, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 425.339), exposure 17.6916, 76 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.80118, 1.75757 and 0.366071. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 425.339 so gap is 1.97128, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 425.386), exposure 17.7379, 77 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.85266, 1.75299 and 0.361242. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 425.386 so gap is 2.01753, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 425.395), exposure 17.7468, 78 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.91421, 1.75211 and 0.356539. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 425.395 so gap is 2.02643, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 425.839), exposure 18.1916, 79 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.85647, 1.70927 and 0.351957. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 425.839 so gap is 2.47121, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 426.063), exposure 18.4157, 79 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.79735, 1.75011 and 0.364809. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 426.063 so gap is 2.69538, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (407.648 - 426.446), exposure 18.7982, 79 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.69973, 1.7749 and 0.37766. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 426.446 so gap is 3.0779, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (407.648 - 426.446) = 407.648- 426.446
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (423.368 - 428.88), exposure 5.51173
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.641975 bg counts (1), with cf=1.13503 and errBG= 0.641975
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.3221 +/- 6.26021
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=423.368 and stop= 428.88 so gap is 5.51173, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (423.368 - 428.88), with lastBin= 0x2077c90 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (417.661 - 423.368), exposure 5.70744
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.13535 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.0606 +/- 6.21958
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 434.415), exposure 7.9687, 30 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.18024, 1.85105 and 0.442809. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=428.88 and stop= 434.415 so gap is 5.53486, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (428.88 - 434.77), exposure 5.89069
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.641975 bg counts (1), with cf=1.13465 and errBG= 0.641975
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.3111 +/- 6.2581
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 434.77), exposure 8.32453, 31 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.13786, 1.77193 and 0.428223. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=428.88 and stop= 434.77 so gap is 5.89069, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (428.88 - 434.77), with lastBin= 0x2075fa0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (423.368 - 428.88), exposure 5.51173
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.641975 bg counts (1), with cf=1.13503 and errBG= 0.641975
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.3221 +/- 6.26021
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2075fa0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 435.009), exposure 8.56293, 32 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.15517, 1.72259 and 0.414567. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 435.009 so gap is 0.238404, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 435.121), exposure 8.67501, 33 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.23228, 1.70034 and 0.401755. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 435.121 so gap is 0.350489, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 435.495), exposure 9.04863, 34 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.18292, 1.63013 and 0.389711. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 435.495 so gap is 0.724108, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 435.737), exposure 9.29059, 34 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.07398, 1.70981 and 0.419689. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 435.737 so gap is 0.96607, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 435.785), exposure 9.33863, 34 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.05302, 1.82251 and 0.449667. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 435.785 so gap is 1.01411, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 435.84), exposure 9.39378, 35 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.15002, 1.81181 and 0.436579. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 435.84 so gap is 1.06926, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 435.879), exposure 9.43293, 35 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.1328, 1.92458 and 0.465685. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 435.879 so gap is 1.1084, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 436.265), exposure 9.819, 35 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.9703, 1.96446 and 0.49479. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 436.265 so gap is 1.49447, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 436.404), exposure 9.95777, 37 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.14286, 1.93709 and 0.467572. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 436.404 so gap is 1.63324, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 436.42), exposure 9.97378, 38 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.24997, 1.93398 and 0.455056. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 436.42 so gap is 1.64926, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 436.973), exposure 10.5271, 38 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.02659, 1.94011 and 0.481824. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 436.973 so gap is 2.20257, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 437.014), exposure 10.568, 38 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.011, 2.03996 and 0.508592. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 437.014 so gap is 2.24349, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 437.03), exposure 10.584, 39 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.11214, 2.03688 and 0.495333. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 437.03 so gap is 2.2595, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 437.541), exposure 11.0946, 39 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.92288, 2.04533 and 0.521384. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 437.541 so gap is 2.77011, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 438.158), exposure 11.712, 40 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.81291, 1.93752 and 0.508146. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 438.158 so gap is 3.38747, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 438.183), exposure 11.7369, 40 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.80482, 2.03001 and 0.533536. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 438.183 so gap is 3.41238, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 438.313), exposure 11.8668, 40 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.76318, 2.10333 and 0.558925. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 438.313 so gap is 3.54225, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 438.537), exposure 12.091, 41 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.78718, 2.06434 and 0.545085. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 438.537 so gap is 3.76643, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 438.603), exposure 12.1568, 42 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.85994, 2.05316 and 0.531915. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 438.603 so gap is 3.83225, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 438.795), exposure 12.3489, 43 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.89169, 2.02121 and 0.519365. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 438.795 so gap is 4.0244, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 438.907), exposure 12.461, 43 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.85669, 2.09402 and 0.542958. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 438.907 so gap is 4.13649, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 439.192), exposure 12.7457, 44 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.85951, 2.04725 and 0.530443. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 439.192 so gap is 4.42115, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 439.281), exposure 12.8346, 44 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.83276, 2.1214 and 0.553492. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 439.281 so gap is 4.5101, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 439.426), exposure 12.9805, 45 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.87703, 2.09756 and 0.541022. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 439.426 so gap is 4.65599, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 439.574), exposure 13.1282, 46 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.91979, 2.07397 and 0.529101. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 439.574 so gap is 4.80366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 440.092), exposure 13.6459, 47 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.85416, 1.99528 and 0.517695. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 440.092 so gap is 5.32139, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 440.163), exposure 13.7171, 47 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.83416, 2.06758 and 0.539253. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 440.163 so gap is 5.39255, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 440.181), exposure 13.7349, 48 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.91175, 2.06491 and 0.527873. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 440.181 so gap is 5.41034, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (434.77 - 440.183), exposure 5.41212
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.1342 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.026 +/- 6.21309
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 440.183), exposure 13.7366, 49 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.99378, 2.06464 and 0.516963. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=434.77 and stop= 440.183 so gap is 5.41212, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (434.77 - 440.183), with lastBin= 0x2077c90 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (428.88 - 434.77), exposure 5.89069
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.641975 bg counts (1), with cf=1.13465 and errBG= 0.641975
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.3111 +/- 6.2581
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 440.417), exposure 13.9715, 49 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.92665, 2.11109 and 0.53763. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 440.417 so gap is 0.234845, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 441.271), exposure 14.8255, 50 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.77694, 1.98948 and 0.526744. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 441.271 so gap is 1.08883, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 441.35), exposure 14.9038, 51 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.83318, 1.97903 and 0.51629. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 441.35 so gap is 1.16711, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 441.505), exposure 15.0585, 51 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.79378, 2.03398 and 0.536137. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 441.505 so gap is 1.3219, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 441.658), exposure 15.2116, 52 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.83015, 2.01352 and 0.525703. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 441.658 so gap is 1.4749, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 442.079), exposure 15.6332, 52 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.72685, 2.03174 and 0.545163. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 442.079 so gap is 1.89655, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 442.488), exposure 16.0424, 53 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.70247, 1.97992 and 0.534757. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 442.488 so gap is 2.30574, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 443.004), exposure 16.5583, 53 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.5871, 1.9867 and 0.553846. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 443.004 so gap is 2.82169, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 443.447), exposure 17.0013, 54 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.56032, 1.93493 and 0.543471. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 443.447 so gap is 3.26469, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 443.454), exposure 17.0085, 55 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.62549, 1.93412 and 0.533479. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 443.454 so gap is 3.27181, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 443.972), exposure 17.5262, 56 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.58309, 1.87699 and 0.523847. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 443.972 so gap is 3.78953, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (426.446 - 444.255), exposure 17.8091, 56 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.52617, 1.91084 and 0.541901. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 444.255 so gap is 4.07242, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (426.446 - 444.255) = 426.446- 444.255
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (440.183 - 445.812), exposure 5.62938
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0 bg counts (0), with cf=1.13381 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.0071 +/- 4.39152
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (444.255 - 445.812), exposure 1.55697, 1 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.728216, 1.45643 and 2. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=440.183 and stop= 445.812 so gap is 5.62938, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (445.812) and the bin is not full 15 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  492  INFO   >>  Discarding leftover counts, as skip is set and I have no bin to carry back to
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 384.053
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (445.812) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  787  INFO   >>  I'm on the last event, so save the previous bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (434.77 - 440.183), exposure 5.41212
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.1342 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.026 +/- 6.21309
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x2077c90
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 384.053 - 445.812
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 384.053 - 445.812 the cf is 1.14462
++tructures/grbBin.cpp::        binData:  line  921  INFO   >>  This bin is empty, so found a emptyBin CF of 1.14462
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (384.053 - 445.812), exposure 61.759
++taStructures/bin.cpp::        fullBin:  line  192  INFO   >>  Producing an upper limit of 6.77045 given bg=0 and numCts= 0
++tructures/grbBin.cpp::        binData:  line  929  INFO   >>  Not saving this bin as it is an incomplete WT one
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (444.255 - 445.812), exposure 1.55697, 1 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.728216, 1.45643 and 2. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for WT mode.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: WT, with files: wtsourcetotal_incbad.evt, wtbacktotal_incbad.evt, and wtcorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 384.053 - 3000
++/SourceEventList.cpp::SourceEventList:  line   67  FATAL  >>  Can't open file wtsourcetotal_incbad.evt
++/genlc_cpp/genlc.cpp::           main:  line  388  WARN   >>  Unable to open the files for this mode, skipping
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: PC, with files: pcsourcetotal.evt, pcbacktotal.evt, and pccorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 447.49 - 441841
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	447.49 - 2864.54
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	6160.11 - 8642.34
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	11930.8 - 12136.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	12324.3 - 12397
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	12471.4 - 14419.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	17730.7 - 18342.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	19032 - 20197.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	23487.5 - 24212.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	35059.9 - 36153.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	40824.4 - 42213.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	46600.8 - 48378.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	52376.4 - 54550.2
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	63943.9 - 66418.6
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	295322 - 296102
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - PC mode, suffix = 
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 20 ct/bin at rateFact=10 and binFact= 1.5 with minT 2.51 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file PCCURVE.qdp, reading from pcsourcetotal.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (447.49 - 457.52), exposure 10.0292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.15511 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.1021 +/- 9.63792
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=447.49 and stop= 457.52 so gap is 10.0292, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (447.49 - 457.52), with lastBin= 0 and workMinC was 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (457.52 - 470.056), exposure 12.5366
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0 bg counts (0), with cf=2.14364 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.0164 +/- 9.82338
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (447.49 - 470.056), exposure 22.5658, 21 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.00301, 1.90194 and 0.949544. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=457.52 and stop= 470.056 so gap is 12.5366, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (457.52 - 470.056), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (447.49 - 457.52), exposure 10.0292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.15511 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.1021 +/- 9.63792
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (447.49 - 470.056) = 447.49- 470.056
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (470.056 - 485.1), exposure 15.044
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.138006 bg counts (5), with cf=2.23028 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.4492 +/- 11.1522
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=470.056 and stop= 485.1 so gap is 15.044, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (470.056 - 485.1), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (457.52 - 470.056), exposure 12.5366
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0 bg counts (0), with cf=2.14364 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.0164 +/- 9.82338
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (470.056 - 495.13), exposure 25.0732, 20 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.74478, 1.64361 and 0.942017. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=485.1 and stop= 495.13 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (470.056 - 497.637), exposure 27.5805, 22 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.73888, 1.64693 and 0.947122. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=485.1 and stop= 497.637 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (470.056 - 497.637) = 470.056- 497.637
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (485.1 - 500.144), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.0552023 bg counts (2), with cf=2.14643 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.2494 +/- 10.2943
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=485.1 and stop= 500.144 so gap is 15.0439, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (485.1 - 500.144), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (470.056 - 485.1), exposure 15.044
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.138006 bg counts (5), with cf=2.23028 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.4492 +/- 11.1522
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (500.144 - 522.71), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.19675 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.8892 +/- 10.0675
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=500.144 and stop= 522.71 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (500.144 - 522.71), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (485.1 - 500.144), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.0552023 bg counts (2), with cf=2.14643 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.2494 +/- 10.2943
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (497.637 - 530.232), exposure 32.5952, 20 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.33734, 1.06786 and 0.798496. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=522.71 and stop= 530.232 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (497.637 - 532.739), exposure 35.1025, 22 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.35983, 1.17119 and 0.861278. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=522.71 and stop= 532.739 so gap is 10.0292, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (497.637 - 535.247), exposure 37.6098, 25 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.43679, 1.14899 and 0.799692. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=522.71 and stop= 535.247 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (497.637 - 535.247) = 497.637- 535.247
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (522.71 - 537.754), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.0276011 bg counts (1), with cf=2.10909 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.3417 +/- 9.89266
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=522.71 and stop= 537.754 so gap is 15.0439, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (522.71 - 537.754), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (500.144 - 522.71), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.19675 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.8892 +/- 10.0675
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (537.754 - 555.305), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.17813 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.4424 +/- 9.74128
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=537.754 and stop= 555.305 so gap is 17.5512, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (537.754 - 555.305), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (522.71 - 537.754), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.0276011 bg counts (1), with cf=2.10909 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.3417 +/- 9.89266
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (535.247 - 570.349), exposure 35.1025, 21 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.2752, 1.10841 and 0.869204. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=555.305 and stop= 570.349 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (535.247 - 572.856), exposure 37.6098, 22 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.24707, 1.03451 and 0.829555. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=555.305 and stop= 572.856 so gap is 17.5513, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (535.247 - 575.364), exposure 40.1172, 23 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.22246, 0.969857 and 0.793365. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=555.305 and stop= 575.364 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (555.305 - 577.871), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0 bg counts (0), with cf=2.1266 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.0385 +/- 10.4182
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (535.247 - 577.871), exposure 42.6245, 28 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.40152, 0.963001 and 0.687111. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=555.305 and stop= 577.871 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (555.305 - 577.871), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (537.754 - 555.305), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.17813 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.4424 +/- 9.74128
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (535.247 - 582.886), exposure 47.6391, 31 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.38932, 0.905906 and 0.652047. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=577.871 and stop= 582.886 so gap is 5.01468, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (535.247 - 582.886) = 535.247- 582.886
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (577.871 - 602.944), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.16887 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.3666 +/- 9.93954
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=577.871 and stop= 602.944 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (577.871 - 602.944), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (555.305 - 577.871), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0 bg counts (0), with cf=2.1266 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.0385 +/- 10.4182
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 620.496), exposure 37.6098, 21 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.20115, 0.73774 and 0.614197. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=602.944 and stop= 620.496 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 623.003), exposure 40.1171, 22 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.1793, 0.691632 and 0.586474. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=602.944 and stop= 623.003 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (602.944 - 625.51), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.13746 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.7291 +/- 10.0264
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 625.51), exposure 42.6245, 23 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.15864, 0.801247 and 0.691543. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=602.944 and stop= 625.51 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (602.944 - 625.51), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (577.871 - 602.944), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.16887 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.3666 +/- 9.93954
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 628.018), exposure 45.1317, 23 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.09427, 0.851367 and 0.778023. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=625.51 and stop= 628.018 so gap is 2.50728, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 630.525), exposure 47.6391, 24 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.08262, 0.851258 and 0.786293. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=625.51 and stop= 630.525 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 633.032), exposure 50.1464, 26 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.1146, 0.85234 and 0.764707. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=625.51 and stop= 633.032 so gap is 7.52194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (582.886 - 633.032) = 582.886- 633.032
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (625.51 - 648.076), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.110405 bg counts (4), with cf=2.18249 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =47.7737 +/- 10.2375
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=625.51 and stop= 648.076 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (625.51 - 648.076), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (602.944 - 625.51), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.13746 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.7291 +/- 10.0264
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (648.076 - 668.135), exposure 20.0586
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0276011 bg counts (1), with cf=2.16498 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.4048 +/- 9.92135
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=648.076 and stop= 668.135 so gap is 20.0586, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (648.076 - 668.135), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (625.51 - 648.076), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.110405 bg counts (4), with cf=2.18249 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =47.7737 +/- 10.2375
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (633.032 - 673.149), exposure 40.1171, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.07612, 0.971432 and 0.902721. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=668.135 and stop= 673.149 so gap is 5.01462, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (633.032 - 675.657), exposure 42.6245, 20 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.01281, 1.01371 and 1.00088. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=668.135 and stop= 675.657 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (633.032 - 675.657) = 633.032- 675.657
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (668.135 - 693.208), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.15064 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9853 +/- 9.85599
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=668.135 and stop= 693.208 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (668.135 - 693.208), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (648.076 - 668.135), exposure 20.0586
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0276011 bg counts (1), with cf=2.16498 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.4048 +/- 9.92135
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 12
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 705.744), exposure 30.0878, 22 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.57739, 0.275082 and 0.17439. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 705.744 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 708.252), exposure 32.5952, 24 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.58852, 0.253921 and 0.159848. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 708.252 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 710.759), exposure 35.1025, 25 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.53604, 0.296765 and 0.193201. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 710.759 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 713.266), exposure 37.6098, 27 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.54748, 0.333898 and 0.215768. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 713.266 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 715.774), exposure 40.1171, 29 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.55601, 0.313029 and 0.201174. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 715.774 so gap is 22.5659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 718.281), exposure 42.6245, 29 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.46448, 0.343457 and 0.234524. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 718.281 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (693.208 - 720.788), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.193208 bg counts (7), with cf=2.15045 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.1954 +/- 10.5362
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 720.788), exposure 45.1317, 32 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.52702, 0.420286 and 0.275233. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 720.788 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (693.208 - 720.788), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (668.135 - 693.208), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.15064 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9853 +/- 9.85599
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 13
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 723.296), exposure 47.6391, 33 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.49209, 0.398165 and 0.266851. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 723.296 so gap is 2.50734, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 728.31), exposure 52.6537, 34 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.3911, 0.360245 and 0.258964. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 728.31 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 733.325), exposure 57.6684, 38 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.41846, 0.328919 and 0.231885. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 733.325 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 735.832), exposure 60.1757, 38 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.35936, 0.35075 and 0.258027. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 735.832 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 740.847), exposure 65.1903, 38 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.25479, 0.35664 and 0.284223. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 740.847 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 743.354), exposure 67.6976, 39 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.23997, 0.436645 and 0.352142. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 743.354 so gap is 22.5659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 745.862), exposure 70.205, 40 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.22621, 0.482096 and 0.39316. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 745.862 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 748.369), exposure 72.7123, 43 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.26988, 0.465472 and 0.366547. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 748.369 so gap is 27.5806, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (720.788 - 750.876), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.138006 bg counts (5), with cf=2.15117 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7266 +/- 9.62125
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 750.876), exposure 75.2196, 43 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.22756, 0.508834 and 0.41451. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 750.876 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (720.788 - 750.876), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (693.208 - 720.788), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.193208 bg counts (7), with cf=2.15045 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.1954 +/- 10.5362
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 14
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 755.891), exposure 80.2342, 44 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.17844, 0.477032 and 0.4048. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 755.891 so gap is 5.01466, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 758.398), exposure 82.7416, 45 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.1695, 0.462576 and 0.395534. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 758.398 so gap is 7.522, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 760.906), exposure 85.2489, 47 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.18521, 0.448971 and 0.378813. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 760.906 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 763.413), exposure 87.7562, 48 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.175, 0.435468 and 0.37061. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 763.413 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 768.427), exposure 92.7708, 49 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.13451, 0.411929 and 0.36309. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 768.427 so gap is 17.5513, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 775.949), exposure 100.293, 49 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.04942, 0.401718 and 0.3828. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 775.949 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 778.457), exposure 102.8, 50 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.04458, 0.412676 and 0.395064. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 778.457 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (675.657 - 778.457) = 675.657- 778.457
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (750.876 - 796.008), exposure 45.1318
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.110405 bg counts (4), with cf=2.15702 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.3734 +/- 10.3454
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 796.008 so gap is 45.1318, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (750.876 - 796.008), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (720.788 - 750.876), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.138006 bg counts (5), with cf=2.15117 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7266 +/- 9.62125
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 15
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (796.008 - 826.096), exposure 30.0879
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.16277 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.2555 +/- 9.67222
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=796.008 and stop= 826.096 so gap is 30.0879, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (796.008 - 826.096), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (750.876 - 796.008), exposure 45.1318
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.110405 bg counts (4), with cf=2.15702 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.3734 +/- 10.3454
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 16
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 833.618), exposure 55.161, 21 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.820273, 0.702672 and 0.856632. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 833.618 so gap is 7.52194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 836.125), exposure 57.6684, 23 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.858775, 0.671089 and 0.781449. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 836.125 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 838.632), exposure 60.1757, 26 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.929606, 0.643127 and 0.691827. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 838.632 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 841.14), exposure 62.683, 27 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.927248, 0.617401 and 0.665843. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 841.14 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 843.647), exposure 65.1903, 27 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.891585, 0.627143 and 0.703401. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 843.647 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 846.154), exposure 67.6976, 28 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.89081, 0.636161 and 0.714138. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 846.154 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (778.457 - 846.154) = 778.457- 846.154
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (826.096 - 853.676), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.15785 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.0767 +/- 9.88924
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 853.676 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (826.096 - 853.676), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (796.008 - 826.096), exposure 30.0879
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.16277 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.2555 +/- 9.67222
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 17
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (853.676 - 893.793), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0828034 bg counts (3), with cf=2.14398 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7021 +/- 9.58872
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=853.676 and stop= 893.793 so gap is 40.1171, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (853.676 - 893.793), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (826.096 - 853.676), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.15785 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.0767 +/- 9.88924
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 18
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 906.33), exposure 60.1757, 20 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.711315, 0.425929 and 0.598791. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 906.33 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 911.345), exposure 65.1903, 23 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.756295, 0.393166 and 0.519858. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 911.345 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 913.852), exposure 67.6976, 25 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.792287, 0.378604 and 0.477862. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 913.852 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 918.867), exposure 72.7123, 26 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.766624, 0.382287 and 0.498663. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 918.867 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 921.374), exposure 75.2196, 27 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.768792, 0.397268 and 0.516744. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 921.374 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 923.881), exposure 77.7269, 28 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.770819, 0.384453 and 0.498759. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 923.881 so gap is 30.0879, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 926.389), exposure 80.2342, 28 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.746732, 0.39843 and 0.533566. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 926.389 so gap is 32.5951, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 928.896), exposure 82.7415, 28 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.723387, 0.41156 and 0.568934. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 928.896 so gap is 35.1025, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 933.911), exposure 87.7562, 29 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.706827, 0.387369 and 0.548039. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 933.911 so gap is 40.1171, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 936.418), exposure 90.2635, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.71128, 0.376609 and 0.52948. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 936.418 so gap is 42.6244, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (893.793 - 941.433), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.14133 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.7316 +/- 9.81353
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 941.433), exposure 95.2781, 32 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.719766, 0.356787 and 0.495699. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 941.433 so gap is 47.639, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (893.793 - 941.433), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (853.676 - 893.793), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0828034 bg counts (3), with cf=2.14398 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7021 +/- 9.58872
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 19
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 943.94), exposure 97.7855, 32 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.70131, 0.369404 and 0.526734. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=941.433 and stop= 943.94 so gap is 2.50736, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 946.447), exposure 100.293, 32 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.683777, 0.403789 and 0.590528. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=941.433 and stop= 946.447 so gap is 5.0147, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 948.954), exposure 102.8, 33 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.68838, 0.393941 and 0.572273. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=941.433 and stop= 948.954 so gap is 7.52198, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 951.462), exposure 105.307, 33 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.67199, 0.404624 and 0.602127. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=941.433 and stop= 951.462 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (846.154 - 951.462) = 846.154- 951.462
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (941.433 - 984.057), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.110405 bg counts (4), with cf=2.13821 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.5281 +/- 9.56308
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=941.433 and stop= 984.057 so gap is 42.6244, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (941.433 - 984.057), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (893.793 - 941.433), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.14133 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.7316 +/- 9.81353
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1019.16), exposure 67.6976, 20 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.632839, 0.405196 and 0.640283. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=984.057 and stop= 1019.16 so gap is 35.1025, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (984.057 - 1021.67), exposure 37.6098
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.15277 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9705 +/- 9.86596
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1021.67), exposure 70.2049, 21 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.640732, 0.451714 and 0.704997. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=984.057 and stop= 1021.67 so gap is 37.6098, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (984.057 - 1021.67), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (941.433 - 984.057), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.110405 bg counts (4), with cf=2.13821 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.5281 +/- 9.56308
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 21
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1026.68), exposure 75.2195, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.626479, 0.4216 and 0.672968. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1026.68 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1029.19), exposure 77.7269, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.661356, 0.408 and 0.616914. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1029.19 so gap is 7.52198, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1031.7), exposure 80.2342, 25 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.666908, 0.421475 and 0.631983. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1031.7 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1034.2), exposure 82.7415, 25 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.646699, 0.434132 and 0.671305. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1034.2 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1036.71), exposure 85.2489, 25 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.627678, 0.470724 and 0.749945. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1036.71 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1041.73), exposure 90.2635, 25 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.592807, 0.46805 and 0.789548. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1041.73 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (951.462 - 1041.73) = 951.462- 1041.73
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1021.67 - 1066.8), exposure 45.1317
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0276011 bg counts (1), with cf=2.13829 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7068 +/- 9.56292
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1066.8 so gap is 45.1317, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1021.67 - 1066.8), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (984.057 - 1021.67), exposure 37.6098
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.15277 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9705 +/- 9.86596
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 22
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1066.8 - 1114.44), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.13143 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.5974 +/- 9.99818
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1114.44), exposure 72.7122, 21 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.616403, 0.349645 and 0.567235. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1066.8 and stop= 1114.44 so gap is 47.639, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1066.8 - 1114.44), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1021.67 - 1066.8), exposure 45.1317
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0276011 bg counts (1), with cf=2.13829 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7068 +/- 9.56292
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 23
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1116.94), exposure 75.2196, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.624211, 0.394701 and 0.632319. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1116.94 so gap is 2.50734, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1121.96), exposure 80.2342, 23 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.611934, 0.396767 and 0.648382. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1121.96 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1131.99), exposure 90.2635, 24 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.567515, 0.425368 and 0.749527. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1131.99 so gap is 17.5513, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1139.51), exposure 97.7854, 24 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.523861, 0.415013 and 0.792221. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1139.51 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1142.02), exposure 100.293, 24 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.510764, 0.425709 and 0.833475. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1142.02 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1041.73 - 1142.02) = 1041.73- 1142.02
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1114.44 - 1167.09), exposure 52.6537
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.14353 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7523 +/- 9.58654
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1167.09 so gap is 52.6537, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1114.44 - 1167.09), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1066.8 - 1114.44), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.13143 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.5974 +/- 9.99818
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 24
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1167.09 - 1209.72), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0276011 bg counts (1), with cf=2.1412 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9062 +/- 9.8124
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1167.09 and stop= 1209.72 so gap is 42.6244, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1167.09 - 1209.72), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1114.44 - 1167.09), exposure 52.6537
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.14353 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7523 +/- 9.58654
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 25
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1224.76), exposure 82.7415, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.514836, 0.385665 and 0.749101. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1224.76 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1234.79), exposure 92.7707, 20 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.459178, 0.367535 and 0.800419. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1234.79 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1239.8), exposure 97.7854, 21 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.457987, 0.348687 and 0.761346. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1239.8 so gap is 30.0878, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1247.33), exposure 105.307, 22 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.445822, 0.323781 and 0.726255. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1247.33 so gap is 37.6098, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1249.83), exposure 107.815, 23 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.455525, 0.316251 and 0.694256. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1249.83 so gap is 40.1171, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1254.85), exposure 112.829, 24 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.453919, 0.302195 and 0.665748. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1254.85 so gap is 45.1317, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1257.35), exposure 115.337, 25 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.462285, 0.313861 and 0.678933. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1257.35 so gap is 47.6391, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1259.86), exposure 117.844, 27 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.488142, 0.306683 and 0.628265. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1259.86 so gap is 50.1463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1262.37), exposure 120.351, 27 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.477972, 0.317551 and 0.66437. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1262.37 so gap is 52.6537, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1269.89), exposure 127.873, 28 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.466559, 0.29841 and 0.639597. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1269.89 so gap is 60.1756, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1274.91), exposure 132.888, 28 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.448953, 0.303315 and 0.675606. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1274.91 so gap is 65.1903, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1287.44), exposure 145.424, 28 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.409846, 0.291793 and 0.711959. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1287.44 so gap is 77.7268, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1142.02 - 1287.44) = 1142.02- 1287.44
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1209.72 - 1302.49), exposure 92.7708
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.193208 bg counts (7), with cf=2.13642 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.3157 +/- 9.55564
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1302.49 so gap is 92.7708, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1209.72 - 1302.49), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1167.09 - 1209.72), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0276011 bg counts (1), with cf=2.1412 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9062 +/- 9.8124
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 26
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1302.49 - 1362.66), exposure 60.1755
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.13604 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6799 +/- 9.78908
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1302.49 and stop= 1362.66 so gap is 60.1755, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1302.49 - 1362.66), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1209.72 - 1302.49), exposure 92.7708
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.193208 bg counts (7), with cf=2.13642 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.3157 +/- 9.55564
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 27
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1377.71), exposure 90.2634, 20 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.470722, 0.188944 and 0.401392. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1377.71 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1382.72), exposure 95.278, 20 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.445947, 0.201181 and 0.451132. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1382.72 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1385.23), exposure 97.7854, 22 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.477732, 0.196023 and 0.41032. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1385.23 so gap is 22.5659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1390.24), exposure 102.8, 22 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.454428, 0.227576 and 0.500797. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1390.24 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1392.75), exposure 105.307, 23 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.463881, 0.222158 and 0.478911. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1392.75 so gap is 30.0878, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1395.26), exposure 107.815, 24 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.472894, 0.216991 and 0.458858. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1395.26 so gap is 32.5951, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1397.76), exposure 110.322, 24 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.461614, 0.231411 and 0.501309. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1397.76 so gap is 35.1025, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1400.27), exposure 112.829, 25 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.470277, 0.226269 and 0.48114. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1400.27 so gap is 37.6098, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1407.79), exposure 120.351, 26 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.458417, 0.228679 and 0.498845. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1407.79 so gap is 45.1317, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1420.33), exposure 132.888, 26 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.41517, 0.223003 and 0.537137. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1420.33 so gap is 57.6683, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1422.84), exposure 135.395, 27 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.422798, 0.218873 and 0.517679. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1422.84 so gap is 60.1756, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1362.66 - 1425.34), exposure 62.6829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.165607 bg counts (6), with cf=2.12494 and errBG= 0.0676087
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.1468 +/- 9.50409
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1425.34), exposure 137.902, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.415111, 0.245394 and 0.591154. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1425.34 so gap is 62.6829, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1362.66 - 1425.34), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1302.49 - 1362.66), exposure 60.1755
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.13604 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6799 +/- 9.78908
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 28
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1430.36), exposure 142.917, 28 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.415467, 0.251706 and 0.605839. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.34 and stop= 1430.36 so gap is 5.01462, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1432.87), exposure 145.424, 30 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.437698, 0.262064 and 0.598731. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.34 and stop= 1432.87 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1437.88), exposure 150.439, 31 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.437316, 0.267536 and 0.611768. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.34 and stop= 1437.88 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1442.9), exposure 155.454, 32 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.436806, 0.272503 and 0.623855. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.34 and stop= 1442.9 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1287.44 - 1442.9) = 1287.44- 1442.9
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1425.34 - 1472.98), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.15462 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.9734 +/- 9.63612
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.34 and stop= 1472.98 so gap is 47.639, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1425.34 - 1472.98), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1362.66 - 1425.34), exposure 62.6829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.165607 bg counts (6), with cf=2.12494 and errBG= 0.0676087
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.1468 +/- 9.50409
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 29
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1472.98 - 1545.7), exposure 72.7122
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.12542 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.4658 +/- 9.96995
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1472.98 and stop= 1545.7 so gap is 72.7122, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1472.98 - 1545.7), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1425.34 - 1472.98), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.15462 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.9734 +/- 9.63612
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 30
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1563.25), exposure 120.351, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.354228, 0.317893 and 0.897426. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1563.25 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1570.77), exposure 127.873, 20 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.332926, 0.316217 and 0.949811. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1570.77 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1583.31), exposure 140.41, 21 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.317095, 0.287983 and 0.908193. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1583.31 so gap is 37.6098, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1585.81), exposure 142.917, 22 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.326429, 0.282518 and 0.865482. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1585.81 so gap is 40.117, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1588.32), exposure 145.424, 23 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.335441, 0.277647 and 0.827708. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1588.32 so gap is 42.6244, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1590.83), exposure 147.932, 23 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.329756, 0.287332 and 0.871348. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1590.83 so gap is 45.1317, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1442.9 - 1590.83) = 1442.9- 1590.83
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1545.7 - 1648.5), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.276011 bg counts (10), with cf=2.15566 and errBG= 0.0872825
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6739 +/- 9.88027
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1648.5 so gap is 102.8, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1545.7 - 1648.5), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1472.98 - 1545.7), exposure 72.7122
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.12542 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.4658 +/- 9.96995
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 31
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1721.21), exposure 130.38, 21 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.348236, 0.14728 and 0.422931. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1648.5 and stop= 1721.21 so gap is 72.7121, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1648.5 - 1733.74), exposure 85.2487
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.193208 bg counts (7), with cf=2.16277 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.8376 +/- 9.67351
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1733.74), exposure 142.917, 22 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.332509, 0.132697 and 0.399078. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1648.5 and stop= 1733.74 so gap is 85.2487, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1648.5 - 1733.74), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1545.7 - 1648.5), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.276011 bg counts (10), with cf=2.15566 and errBG= 0.0872825
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6739 +/- 9.88027
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 32
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1756.31), exposure 165.483, 23 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.299325, 0.127484 and 0.425905. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1756.31 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1761.33), exposure 170.497, 24 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.302673, 0.123386 and 0.407655. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1761.33 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1766.34), exposure 175.512, 24 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.294025, 0.132045 and 0.449095. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1766.34 so gap is 32.5951, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1776.37), exposure 185.541, 25 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.289836, 0.13661 and 0.471336. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1776.37 so gap is 42.6243, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1781.38), exposure 190.556, 25 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.282209, 0.14441 and 0.511714. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1781.38 so gap is 47.639, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1783.89), exposure 193.063, 25 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.278544, 0.153517 and 0.55114. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1783.89 so gap is 50.1463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1788.91), exposure 198.078, 26 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.282195, 0.14963 and 0.530238. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1788.91 so gap is 55.1609, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1793.92), exposure 203.092, 27 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.285995, 0.156702 and 0.547918. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1793.92 so gap is 60.1755, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1803.95), exposure 213.122, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.272256, 0.159198 and 0.584737. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1803.95 so gap is 70.2048, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1808.96), exposure 218.136, 28 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.27564, 0.155539 and 0.564282. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1808.96 so gap is 75.2194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1811.47), exposure 220.644, 29 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.28204, 0.153771 and 0.54521. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1811.47 so gap is 77.7267, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1813.98), exposure 223.151, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.288626, 0.152043 and 0.526783. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1813.98 so gap is 80.234, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1816.49), exposure 225.658, 30 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.285419, 0.16 and 0.560578. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1816.49 so gap is 82.7414, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1818.99), exposure 228.166, 31 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.291824, 0.158242 and 0.54225. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1818.99 so gap is 85.2486, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1821.5), exposure 230.673, 33 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.307526, 0.156522 and 0.508969. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1821.5 so gap is 87.756, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1733.74 - 1846.57), exposure 112.829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.193208 bg counts (7), with cf=2.15856 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =47.0714 +/- 10.1258
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1846.57), exposure 255.746, 34 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.285555, 0.158463 and 0.55493. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1846.57 so gap is 112.829, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1733.74 - 1846.57), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1648.5 - 1733.74), exposure 85.2487
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.193208 bg counts (7), with cf=2.16277 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.8376 +/- 9.67351
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 33
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1854.1), exposure 263.268, 35 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.285445, 0.153936 and 0.539282. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1846.57 and stop= 1854.1 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1864.12), exposure 273.297, 36 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.282616, 0.164014 and 0.580342. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1846.57 and stop= 1864.12 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1590.83 - 1864.12) = 1590.83- 1864.12
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1846.57 - 1956.9), exposure 110.322
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.220809 bg counts (8), with cf=2.15835 and errBG= 0.0780678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.6903 +/- 9.65388
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1846.57 and stop= 1956.9 so gap is 110.322, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1846.57 - 1956.9), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1733.74 - 1846.57), exposure 112.829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.193208 bg counts (7), with cf=2.15856 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =47.0714 +/- 10.1258
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 34
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2032.11), exposure 167.99, 20 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.254721, 0.112268 and 0.440747. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2032.11 so gap is 75.2194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2039.64), exposure 175.512, 21 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.256048, 0.107456 and 0.419672. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2039.64 so gap is 82.7413, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2052.17), exposure 188.048, 22 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.250035, 0.100292 and 0.401114. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2052.17 so gap is 95.2779, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2057.19), exposure 193.063, 23 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.254577, 0.0976874 and 0.383725. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2057.19 so gap is 100.293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2072.23), exposure 208.107, 24 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.246154, 0.0906256 and 0.368166. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2072.23 so gap is 115.336, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2077.25), exposure 213.122, 25 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.250004, 0.0884933 and 0.353967. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2077.25 so gap is 120.351, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2079.75), exposure 215.629, 26 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.256902, 0.0874643 and 0.340458. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2079.75 so gap is 122.858, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1956.9 - 2084.77), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.303613 bg counts (11), with cf=2.14331 and errBG= 0.0915426
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2155 +/- 9.58719
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2084.77), exposure 220.643, 27 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.260773, 0.0854765 and 0.327781. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2084.77 so gap is 127.873, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1956.9 - 2084.77), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1846.57 - 1956.9), exposure 110.322
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.220809 bg counts (8), with cf=2.15835 and errBG= 0.0780678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.6903 +/- 9.65388
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 35
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2087.28), exposure 223.151, 27 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.257577, 0.0941179 and 0.365397. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2087.28 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2094.8), exposure 230.673, 28 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.258437, 0.0907911 and 0.351308. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2094.8 so gap is 10.0292, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2099.81), exposure 235.687, 28 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.252938, 0.0979228 and 0.387141. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2099.81 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2104.83), exposure 240.702, 28 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.247422, 0.104633 and 0.422892. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2104.83 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2107.33), exposure 243.209, 29 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.253529, 0.103554 and 0.408451. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2107.33 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2112.35), exposure 248.224, 30 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.25689, 0.101462 and 0.394964. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2112.35 so gap is 27.5804, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2139.93), exposure 275.804, 31 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.238652, 0.0908861 and 0.380831. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2139.93 so gap is 55.1609, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2152.47), exposure 288.341, 32 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.235806, 0.0867289 and 0.367798. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2152.47 so gap is 67.6974, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2162.49), exposure 298.37, 33 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.235028, 0.0838137 and 0.356612. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2162.49 so gap is 77.7267, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2165), exposure 300.877, 33 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.233069, 0.0903779 and 0.387773. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2165 so gap is 80.2339, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2170.02), exposure 305.892, 34 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.236394, 0.0888963 and 0.376051. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2170.02 so gap is 85.2486, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2180.05), exposure 315.921, 34 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.22889, 0.0930237 and 0.406413. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2180.05 so gap is 95.2778, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2182.55), exposure 318.429, 35 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.233984, 0.0922913 and 0.394433. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2182.55 so gap is 97.7851, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2190.08), exposure 325.951, 36 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.234915, 0.0901615 and 0.383804. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2190.08 so gap is 105.307, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2197.6), exposure 333.472, 37 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.236115, 0.0881278 and 0.373241. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2197.6 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2205.12), exposure 340.994, 38 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.237102, 0.0923815 and 0.389627. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2205.12 so gap is 120.351, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2215.15), exposure 351.024, 39 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.236448, 0.0894036 and 0.378111. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2215.15 so gap is 130.38, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2217.66), exposure 353.531, 40 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.240848, 0.0887696 and 0.36857. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2217.66 so gap is 132.887, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2084.77 - 2225.18), exposure 140.409
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.276011 bg counts (10), with cf=2.14192 and errBG= 0.0872825
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2473 +/- 9.5808
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2225.18), exposure 361.053, 41 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.241687, 0.0869202 and 0.359639. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2225.18 so gap is 140.409, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2084.77 - 2225.18), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1956.9 - 2084.77), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.303613 bg counts (11), with cf=2.14331 and errBG= 0.0915426
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2155 +/- 9.58719
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 36
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2245.24), exposure 381.111, 42 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.234551, 0.0823454 and 0.351076. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2245.24 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2247.74), exposure 383.619, 43 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.238566, 0.0816524 and 0.342263. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2247.74 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2262.79), exposure 398.663, 43 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.229267, 0.0839296 and 0.366078. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2262.79 so gap is 37.6097, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2267.8), exposure 403.677, 43 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.226419, 0.0883345 and 0.390138. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2267.8 so gap is 42.6243, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2282.85), exposure 418.721, 44 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.223411, 0.0851608 and 0.381185. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2282.85 so gap is 57.6682, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2287.86), exposure 423.736, 45 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.225953, 0.084153 and 0.372437. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2287.86 so gap is 62.6828, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2300.4), exposure 436.272, 45 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.219324, 0.0965063 and 0.440017. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2300.4 so gap is 75.2194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1864.12 - 2300.4) = 1864.12- 2300.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2225.18 - 2365.59), exposure 140.409
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.165607 bg counts (6), with cf=2.16532 and errBG= 0.0676087
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.9478 +/- 9.68471
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2365.59 so gap is 140.409, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2225.18 - 2365.59), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2084.77 - 2225.18), exposure 140.409
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.276011 bg counts (10), with cf=2.14192 and errBG= 0.0872825
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2473 +/- 9.5808
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 37
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2483.43), exposure 183.034, 20 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.236351, 0.0928338 and 0.392779. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2365.59 and stop= 2483.43 so gap is 117.844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2498.47), exposure 198.077, 21 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.228825, 0.0857832 and 0.374886. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2365.59 and stop= 2498.47 so gap is 132.887, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2506), exposure 205.599, 21 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.220161, 0.0928022 and 0.42152. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2365.59 and stop= 2506 so gap is 140.409, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2365.59 - 2518.53), exposure 152.946
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.331214 bg counts (12), with cf=2.17217 and errBG= 0.0956131
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.724 +/- 9.71647
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2518.53), exposure 218.136, 21 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.207233, 0.0977567 and 0.471724. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2365.59 and stop= 2518.53 so gap is 152.946, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2365.59 - 2518.53), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2225.18 - 2365.59), exposure 140.409
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.165607 bg counts (6), with cf=2.16532 and errBG= 0.0676087
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.9478 +/- 9.68471
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 38
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2521.04), exposure 220.643, 22 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.215051, 0.106818 and 0.496709. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2521.04 so gap is 2.50736, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2526.05), exposure 225.658, 23 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.220236, 0.104444 and 0.474238. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2526.05 so gap is 7.52194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2531.07), exposure 230.672, 24 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.224933, 0.102174 and 0.45424. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2531.07 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2546.11), exposure 245.716, 25 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.219588, 0.0959181 and 0.43681. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2546.11 so gap is 27.5804, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2551.13), exposure 250.731, 25 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.214956, 0.102497 and 0.476829. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2551.13 so gap is 32.5951, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2553.64), exposure 253.225, 25 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.212601, 0.109901 and 0.516937. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2553.64 so gap is 35.1023, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 1, last was 0 so increasing dead to 0.0129083
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2561.16), exposure 260.747, 26 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.211186, 0.106731 and 0.505387. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2561.16 so gap is 42.6243, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2566.17), exposure 265.762, 26 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.207201, 0.109336 and 0.527679. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2566.17 so gap is 47.6389, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2576.2), exposure 275.791, 27 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.204125, 0.10536 and 0.516153. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2576.2 so gap is 57.6682, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2578.71), exposure 278.298, 27 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.202286, 0.108817 and 0.537937. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2578.71 so gap is 60.1754, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2581.22), exposure 280.806, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.200479, 0.112209 and 0.559702. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2581.22 so gap is 62.6828, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2591.24), exposure 290.835, 28 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.197799, 0.108339 and 0.547725. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2591.24 so gap is 72.712, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2606.29), exposure 305.879, 29 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.191898, 0.103011 and 0.536801. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2606.29 so gap is 87.7559, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2613.81), exposure 313.401, 29 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.187292, 0.104446 and 0.557664. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2613.81 so gap is 95.2778, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2616.32), exposure 315.908, 30 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.189693, 0.103617 and 0.546234. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2616.32 so gap is 97.7851, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2631.36), exposure 330.952, 31 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.184787, 0.098907 and 0.53525. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2631.36 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2636.38), exposure 335.967, 32 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.185687, 0.0972686 and 0.52383. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2636.38 so gap is 117.844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2641.39), exposure 340.981, 32 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.182957, 0.0994371 and 0.543501. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2641.39 so gap is 122.858, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2518.53 - 2648.91), exposure 130.367
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.166514 bg counts (6), with cf=1.56126 and errBG= 0.0679789
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.9652 +/- 6.98296
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2648.91), exposure 348.503, 32 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.179008, 0.100803 and 0.563121. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2648.91 so gap is 130.38, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2518.53 - 2648.91), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2365.59 - 2518.53), exposure 152.946
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.331214 bg counts (12), with cf=2.17217 and errBG= 0.0956131
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.724 +/- 9.71647
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 39
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2661.45), exposure 361.04, 33 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.176194, 0.0971579 and 0.551426. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2648.91 and stop= 2661.45 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (2300.4 - 2661.45) = 2300.4- 2661.45
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2648.91 - 2709.09), exposure 60.1754
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.196382 bg counts (7), with cf=1.21884 and errBG= 0.0742253
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.3562 +/- 5.58614
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2648.91 and stop= 2709.09 so gap is 60.1754, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2648.91 - 2709.09), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2518.53 - 2648.91), exposure 130.367
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.166514 bg counts (6), with cf=1.56126 and errBG= 0.0679789
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.9652 +/- 6.98296
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 40
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2794.34), exposure 132.887, 21 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.191259, 0.0807512 and 0.422209. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2794.34 so gap is 85.2485, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2799.35), exposure 137.902, 22 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.19315, 0.0778148 and 0.402872. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2799.35 so gap is 90.2632, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2814.4), exposure 152.946, 23 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.182116, 0.0701608 and 0.385253. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2814.4 so gap is 105.307, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2816.9), exposure 155.453, 23 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.179179, 0.0846952 and 0.472684. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2816.9 so gap is 107.814, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2819.41), exposure 157.961, 23 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.176335, 0.0910593 and 0.516399. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2819.41 so gap is 110.322, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2821.92), exposure 160.468, 24 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.181167, 0.0894229 and 0.493593. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2821.92 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2824.42), exposure 162.975, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.17838, 0.0955184 and 0.535477. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2824.42 so gap is 115.336, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2826.93), exposure 165.482, 24 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.175678, 0.101439 and 0.577417. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2826.93 so gap is 117.844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2709.09 - 2834.45), exposure 125.365
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.280545 bg counts (10), with cf=1.22345 and errBG= 0.0887163
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1258 +/- 5.47252
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2834.45), exposure 173.004, 26 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.182134, 0.0970288 and 0.532732. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2834.45 so gap is 125.365, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2709.09 - 2834.45), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2648.91 - 2709.09), exposure 60.1754
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.196382 bg counts (7), with cf=1.21884 and errBG= 0.0742253
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.3562 +/- 5.58614
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 41
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2841.98), exposure 180.526, 26 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.174546, 0.0997427 and 0.571442. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2834.45 and stop= 2841.98 so gap is 7.52192, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2844.48), exposure 183.034, 27 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.178819, 0.0983763 and 0.550146. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2834.45 and stop= 2844.48 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2849.5), exposure 188.048, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.17405, 0.102232 and 0.587369. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2834.45 and stop= 2849.5 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2854.51), exposure 193.063, 29 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.18215, 0.0995763 and 0.546672. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2834.45 and stop= 2854.51 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2834.45 - 2864.54), exposure 30.0866
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0 bg counts (0), with cf=1.2245 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.347 +/- 2.9994
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2864.54), exposure 203.091, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.179323, 0.0946595 and 0.527871. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2834.45 and stop= 2864.54 so gap is 30.0866, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (2864.54) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=30.0866 whereas forward=3295.57
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2709.09 - 2864.54), exposure 155.452
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.280545 bg counts (10), with cf=1.22369 and errBG= 0.0887163
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.4728 +/- 6.24059
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (2864.54) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2864.54), exposure 564.131, 63 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.177408, 0.0962032 and 0.54227. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2709.09 - 2864.54), with lastBin= 0 and workMinC was 15
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 6160.11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (2300.4 - 2864.54) = 2300.4- 2864.54
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 6160.11 - 8642.34


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6160.11 - 6393.29), exposure 233.181
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0886769 bg counts (7), with cf=1.97906 and errBG= 0.0335167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =39.4056 +/- 8.85086
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6160.11 and stop= 6393.29 so gap is 233.181, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6160.11 - 6393.29), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2709.09 - 2864.54), exposure 155.452
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.280545 bg counts (10), with cf=1.22369 and errBG= 0.0887163
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.4728 +/- 6.24059
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 42
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6533.7), exposure 373.591, 19 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0999466, 0.041868 and 0.418904. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6533.7 so gap is 140.41, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6561.28), exposure 401.171, 20 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0974853, 0.0389272 and 0.399313. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6561.28 so gap is 167.991, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6563.79), exposure 403.678, 20 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0968798, 0.043672 and 0.450785. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6563.79 so gap is 170.498, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6573.82), exposure 413.708, 20 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0945312, 0.0475072 and 0.502556. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6573.82 so gap is 180.527, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6581.34), exposure 421.23, 21 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0976499, 0.0466588 and 0.477818. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6581.34 so gap is 188.049, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6623.96), exposure 463.854, 22 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0928363, 0.0464774 and 0.500639. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6623.96 so gap is 230.673, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6674.11), exposure 514.001, 23 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0875721, 0.0418943 and 0.478397. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6674.11 so gap is 280.82, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6393.29 - 6694.17), exposure 300.878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.177354 bg counts (14), with cf=1.95921 and errBG= 0.0473998
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.0407 +/- 7.58855
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6694.17), exposure 534.059, 24 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0878381, 0.0403208 and 0.459035. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6694.17 so gap is 300.878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6393.29 - 6694.17), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6160.11 - 6393.29), exposure 233.181
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0886769 bg counts (7), with cf=1.97906 and errBG= 0.0335167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =39.4056 +/- 8.85086
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 43
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6706.7), exposure 546.596, 25 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0892859, 0.039396 and 0.441234. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6706.7 so gap is 12.5365, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6716.73), exposure 556.625, 26 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0911316, 0.0386861 and 0.424508. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6716.73 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6724.26), exposure 564.147, 27 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0932821, 0.0381258 and 0.408716. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6724.26 so gap is 30.0878, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6734.28), exposure 574.176, 27 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0916527, 0.0408747 and 0.445974. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6734.28 so gap is 40.1171, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6741.81), exposure 581.698, 28 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0938385, 0.04376 and 0.466333. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6741.81 so gap is 47.639, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6744.31), exposure 584.206, 29 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0968292, 0.0435722 and 0.44999. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6744.31 so gap is 50.1464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6794.46), exposure 634.352, 29 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0890181, 0.0432006 and 0.485302. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6794.46 so gap is 100.293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6809.5), exposure 649.396, 29 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0869559, 0.0451972 and 0.519771. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6809.5 so gap is 115.337, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6812.01), exposure 651.903, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0896068, 0.0480091 and 0.535775. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6812.01 so gap is 117.844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6822.04), exposure 661.932, 30 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0882491, 0.050186 and 0.568686. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6822.04 so gap is 127.873, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6837.08), exposure 676.976, 30 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0862513, 0.0517733 and 0.60026. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6837.08 so gap is 142.917, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6839.59), exposure 679.484, 31 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0886986, 0.0515822 and 0.581545. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6839.59 so gap is 145.424, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6844.61), exposure 684.498, 32 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0908276, 0.0512043 and 0.563753. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6844.61 so gap is 150.439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6852.13), exposure 692.02, 32 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0898403, 0.0533967 and 0.594351. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6852.13 so gap is 157.961, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6877.2), exposure 717.093, 33 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0892763, 0.0515297 and 0.577193. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6877.2 so gap is 183.034, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6917.32), exposure 757.211, 34 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0870775, 0.0487997 and 0.560416. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6917.32 so gap is 223.151, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6694.17 - 6924.84), exposure 230.673
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.215358 bg counts (17), with cf=1.93744 and errBG= 0.052232
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =38.3316 +/- 8.6651
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6924.84), exposure 764.732, 36 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0913369, 0.0482871 and 0.528671. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6924.84 so gap is 230.673, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6694.17 - 6924.84), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6393.29 - 6694.17), exposure 300.878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.177354 bg counts (14), with cf=1.95921 and errBG= 0.0473998
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.0407 +/- 7.58855
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 44
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6942.39), exposure 782.284, 36 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.089256, 0.0497232 and 0.557085. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6924.84 and stop= 6942.39 so gap is 17.5513, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (6160.11 - 6942.39) = 6160.11- 6942.39
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6924.84 - 7278.37), exposure 353.532
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 18 counts and 0.215358 bg counts (17), with cf=1.91827 and errBG= 0.052232
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.1157 +/- 8.13913
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6924.84 and stop= 7278.37 so gap is 353.532, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6924.84 - 7278.37), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6694.17 - 6924.84), exposure 230.673
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.215358 bg counts (17), with cf=1.93744 and errBG= 0.052232
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =38.3316 +/- 8.6651
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 45
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7478.96), exposure 536.566, 15 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0532251, 0.0417104 and 0.783661. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7278.37 and stop= 7478.96 so gap is 200.585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7499.02), exposure 556.624, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0546735, 0.0402074 and 0.735408. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7278.37 and stop= 7499.02 so gap is 220.644, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7511.55), exposure 569.161, 16 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0534266, 0.0427052 and 0.799326. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7278.37 and stop= 7511.55 so gap is 233.18, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7278.37 - 7584.27), exposure 305.892
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.177354 bg counts (14), with cf=1.90212 and errBG= 0.0473998
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.0965 +/- 7.609
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7584.27), exposure 641.873, 19 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0562921, 0.040717 and 0.723318. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7278.37 and stop= 7584.27 so gap is 305.892, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7278.37 - 7584.27), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6924.84 - 7278.37), exposure 353.532
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 18 counts and 0.215358 bg counts (17), with cf=1.91827 and errBG= 0.052232
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.1157 +/- 8.13913
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 46
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7599.31), exposure 656.917, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0580997, 0.0397846 and 0.684765. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7599.31 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7629.4), exposure 687.004, 21 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0583644, 0.0380422 and 0.651805. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7629.4 so gap is 45.1316, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7644.44), exposure 702.048, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0597394, 0.0371928 and 0.622584. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7644.44 so gap is 60.1755, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7659.48), exposure 717.092, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0584861, 0.038994 and 0.666722. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7659.48 so gap is 75.2194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7667.01), exposure 724.614, 22 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.057879, 0.0412091 and 0.711987. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7667.01 so gap is 82.7413, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7717.15), exposure 774.76, 23 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.056573, 0.0384798 and 0.68018. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7717.15 so gap is 132.888, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (6942.39 - 7717.15) = 6942.39- 7717.15
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7584.27 - 7925.26), exposure 340.994
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.253362 bg counts (20), with cf=1.90764 and errBG= 0.0566536
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =37.6695 +/- 8.53191
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7925.26 so gap is 340.994, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7584.27 - 7925.26), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7278.37 - 7584.27), exposure 305.892
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.177354 bg counts (14), with cf=1.90212 and errBG= 0.0473998
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.0965 +/- 7.609
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 47
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7925.26 - 8258.73), exposure 333.472
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.329371 bg counts (26), with cf=1.87771 and errBG= 0.064595
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.5472 +/- 7.27335
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7717.15 - 8258.73), exposure 541.579, 17 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0581657, 0.0412464 and 0.709119. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7925.26 and stop= 8258.73 so gap is 333.472, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7925.26 - 8258.73), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7584.27 - 7925.26), exposure 340.994
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.253362 bg counts (20), with cf=1.90764 and errBG= 0.0566536
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =37.6695 +/- 8.53191
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 48
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7717.15 - 8384.1), exposure 666.945, 20 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0558639, 0.0564964 and 1.01132. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=8258.73 and stop= 8384.1 so gap is 125.365, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (7717.15 - 8384.1) = 7717.15- 8384.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8258.73 - 8549.58), exposure 290.848
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.291367 bg counts (23), with cf=1.9344 and errBG= 0.0607542
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =38.1243 +/- 8.65168
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=8258.73 and stop= 8549.58 so gap is 290.848, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (8258.73 - 8549.58), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7925.26 - 8258.73), exposure 333.472
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.329371 bg counts (26), with cf=1.87771 and errBG= 0.064595
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.5472 +/- 7.27335
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 49
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8549.58 - 8642.34), exposure 92.7557
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.0380044 bg counts (3), with cf=1.91387 and errBG= 0.0219418
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =13.3243 +/- 5.06379
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (8384.1 - 8642.34), exposure 258.238, 11 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0803523, 0.0371707 and 0.462596. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=8549.58 and stop= 8642.34 so gap is 92.7557, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 1 (8642.34) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=92.7557 whereas forward=3288.43
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8258.73 - 8642.34), exposure 383.604
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.329371 bg counts (26), with cf=1.92907 and errBG= 0.064595
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.4496 +/- 10.0245
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 1 (8642.34) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7717.15 - 8642.34), exposure 925.183, 31 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0626986, 0.0511033 and 0.815063. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (8258.73 - 8642.34), with lastBin= 0 and workMinC was 14
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 11930.8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (7717.15 - 8642.34) = 7717.15- 8642.34
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 11930.8 - 12136.4


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11930.8 - 12136.4), exposure 205.599
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.135279 bg counts (18), with cf=1.31582 and errBG= 0.0318855
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.9276 +/- 4.74444
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12136.4), exposure 205.599, 7 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0445398, 0.037794 and 0.848544. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=11930.8 and stop= 12136.4 so gap is 205.599, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 2 (12136.4) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=3494.03 whereas forward=187.909
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 2 (12136.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 12324.3 - 12397


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11930.8 - 12356.9), exposure 238.194
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.142794 bg counts (19), with cf=1.3161 and errBG= 0.0327592
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5536 +/- 5.09742
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=11930.8 and stop= 12356.9 so gap is 426.103, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (11930.8 - 12356.9), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8258.73 - 8642.34), exposure 383.604
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.329371 bg counts (26), with cf=1.92907 and errBG= 0.064595
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.4496 +/- 10.0245
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 50
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12356.9 - 12397), exposure 40.1166
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.0375774 bg counts (5), with cf=1.29599 and errBG= 0.0168051
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.54327 +/- 1.83293
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12397), exposure 278.31, 9 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0421453, 0.0372502 and 0.883853. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12356.9 and stop= 12397 so gap is 40.1166, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 3 (12397) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=40.1166 whereas forward=74.3775
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11930.8 - 12397), exposure 278.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.180371 bg counts (24), with cf=1.31374 and errBG= 0.0368181
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.0965 +/- 5.41689
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 3 (12397) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (11930.8 - 12397), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 12471.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 12471.4 - 14419.5


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12737.1), exposure 544.086, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0384017, 0.028585 and 0.744368. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12471.4 and stop= 12737.1 so gap is 265.776, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12747.2), exposure 554.115, 17 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0401232, 0.0280676 and 0.699536. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12471.4 and stop= 12747.2 so gap is 275.805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12762.2), exposure 569.159, 18 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0413399, 0.0273257 and 0.661001. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12471.4 and stop= 12762.2 so gap is 290.849, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12787.3), exposure 594.232, 18 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0395956, 0.0283536 and 0.716079. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12471.4 and stop= 12787.3 so gap is 315.922, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12471.4 - 12804.8), exposure 333.473
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0901857 bg counts (12), with cf=1.31596 and errBG= 0.0260344
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6207 +/- 5.09681
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12804.8), exposure 611.784, 19 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0406496, 0.0275402 and 0.677502. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12471.4 and stop= 12804.8 so gap is 333.473, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12471.4 - 12804.8), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11930.8 - 12397), exposure 278.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.180371 bg counts (24), with cf=1.31374 and errBG= 0.0368181
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.0965 +/- 5.41689
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 51
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12832.4), exposure 639.364, 19 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0388651, 0.0284471 and 0.731946. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12804.8 and stop= 12832.4 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12837.4), exposure 644.379, 19 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0385626, 0.0302218 and 0.783707. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12804.8 and stop= 12837.4 so gap is 32.5951, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (11930.8 - 12837.4) = 11930.8- 12837.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12804.8 - 13338.9), exposure 534.058
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.195402 bg counts (26), with cf=1.31896 and errBG= 0.0383215
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5267 +/- 5.10858
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12804.8 and stop= 13338.9 so gap is 534.058, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12804.8 - 13338.9), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12471.4 - 12804.8), exposure 333.473
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0901857 bg counts (12), with cf=1.31596 and errBG= 0.0260344
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6207 +/- 5.09681
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 52
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13338.9 - 13647.3), exposure 308.399
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0901857 bg counts (12), with cf=1.31304 and errBG= 0.0260344
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5771 +/- 5.08549
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13338.9 and stop= 13647.3 so gap is 308.399, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13338.9 - 13647.3), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12804.8 - 13338.9), exposure 534.058
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.195402 bg counts (26), with cf=1.31896 and errBG= 0.0383215
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5267 +/- 5.10858
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 53
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (12837.4 - 13732.5), exposure 895.111, 19 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0276249, 0.0219014 and 0.792816. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13647.3 and stop= 13732.5 so gap is 85.2486, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (12837.4 - 13732.5) = 12837.4- 13732.5
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13647.3 - 13933.1), exposure 285.834
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.135279 bg counts (18), with cf=1.3185 and errBG= 0.0318855
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5991 +/- 5.1067
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13647.3 and stop= 13933.1 so gap is 285.834, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13647.3 - 13933.1), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13338.9 - 13647.3), exposure 308.399
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0901857 bg counts (12), with cf=1.31304 and errBG= 0.0260344
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5771 +/- 5.08549
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 54
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13933.1 - 14419.5), exposure 486.407
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.255526 bg counts (34), with cf=1.2997 and errBG= 0.0438224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.6648 +/- 4.11039
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (13732.5 - 14419.5), exposure 686.992, 14 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0264751, 0.00908699 and 0.343228. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13933.1 and stop= 14419.5 so gap is 486.407, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 4 (14419.5) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=486.407 whereas forward=3311.16
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13647.3 - 14419.5), exposure 772.241
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.390805 bg counts (52), with cf=1.31098 and errBG= 0.0541948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.2621 +/- 6.55527
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 4 (14419.5) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (12837.4 - 14419.5), exposure 1582.1, 33 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0271256, 0.0163355 and 0.602219. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13647.3 - 14419.5), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 17730.7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (12837.4 - 14419.5) = 12837.4- 14419.5
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 17730.7 - 18342.5


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17730.7 - 18079.2), exposure 348.517
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.15507 bg counts (20), with cf=2.18585 and errBG= 0.0346748
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.4489 +/- 8.46612
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17730.7 and stop= 18079.2 so gap is 348.517, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17730.7 - 18079.2), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13647.3 - 14419.5), exposure 772.241
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.390805 bg counts (52), with cf=1.31098 and errBG= 0.0541948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.2621 +/- 6.55527
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 55
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18079.2 - 18342.5), exposure 263.264
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.0697817 bg counts (9), with cf=2.21021 and errBG= 0.0232606
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.8968 +/- 4.94244
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 18342.5), exposure 611.781, 14 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0503897, 0.0204628 and 0.406092. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18079.2 and stop= 18342.5 so gap is 263.264, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 5 (18342.5) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=263.264 whereas forward=689.536
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17730.7 - 18342.5), exposure 611.781
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.224852 bg counts (29), with cf=2.19194 and errBG= 0.041754
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.346 +/- 9.8031
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 5 (18342.5) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17730.7 - 18342.5), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 19032
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 7
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 19032 - 20197.9


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19167.4), exposure 747.176, 15 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0442255, 0.0259113 and 0.58589. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19167.4 so gap is 135.395, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19190), exposure 769.742, 16 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0459566, 0.0251299 and 0.546818. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19190 so gap is 157.961, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19495.9), exposure 1075.63, 16 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0327593, 0.0201186 and 0.614133. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19495.9 so gap is 463.853, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19536), exposure 1115.75, 16 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0315352, 0.0213503 and 0.677032. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19536 so gap is 503.969, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19571.1), exposure 1150.85, 17 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0325401, 0.0206698 and 0.635209. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19571.1 so gap is 539.072, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19583.6), exposure 1163.39, 18 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0340607, 0.020447 and 0.600311. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19583.6 so gap is 551.608, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19869.5), exposure 1449.22, 19 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0287156, 0.0163676 and 0.56999. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19869.5 so gap is 837.442, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19949.7), exposure 1529.46, 19 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0271979, 0.0170625 and 0.627345. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19949.7 so gap is 917.675, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 20014.9), exposure 1594.65, 19 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.026032, 0.0177469 and 0.681735. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 20014.9 so gap is 982.865, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 20077.6), exposure 1657.33, 19 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0250058, 0.0184234 and 0.736764. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 20077.6 so gap is 1045.55, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 20115.2), exposure 1694.94, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0257766, 0.0179844 and 0.697703. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 20115.2 so gap is 1083.16, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (19032 - 20157.8), exposure 1125.78
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.500895 bg counts (65), with cf=2.28607 and errBG= 0.0621284
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.146 +/- 8.85507
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 20157.8), exposure 1737.56, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0251343, 0.0188981 and 0.751884. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 20157.8 so gap is 1125.78, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (19032 - 20157.8), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17730.7 - 18342.5), exposure 611.781
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.224852 bg counts (29), with cf=2.19194 and errBG= 0.041754
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.346 +/- 9.8031
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 56
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 7
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17730.7 - 20157.8) = 17730.7- 20157.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (20157.8 - 20197.9), exposure 40.1125
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.00770608 bg counts (1), with cf=2.39126 and errBG= 0.00770608
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.37283 +/- 2.39133
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20157.8 - 20197.9), exposure 40.1125, 0 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0, 0.0591543 and inf. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=20157.8 and stop= 20197.9 so gap is 40.1125, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 6 (20197.9) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=40.1125 whereas forward=3289.6
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (19032 - 20197.9), exposure 1165.89
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.508601 bg counts (66), with cf=2.29265 and errBG= 0.0626045
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =35.5163 +/- 9.17172
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 6 (20197.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 20197.9), exposure 1777.68, 20 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0245672, 0.0198057 and 0.806185. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (19032 - 20197.9), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 23487.5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 8
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17730.7 - 20197.9) = 17730.7- 20197.9
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 23487.5 - 24212.1


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23487.5 - 24212.1), exposure 724.61
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 0.29768 bg counts (37), with cf=1.28801 and errBG= 0.0489384
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.6488 +/- 4.81971
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 24212.1), exposure 724.61, 14 soft counts and 0 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0245278, -0.000133237 and -0.00543209. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23487.5 and stop= 24212.1 so gap is 724.61, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 7 (24212.1) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 16 counts, because gotBinThisOrb=0 and gapBack=4014.21 whereas forward=10847.8
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (19032 - 24212.1), exposure 1890.5
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.806282 bg counts (103), with cf=1.82382 and errBG= 0.0794453
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.244 +/- 9.99051
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 7 (24212.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (19032 - 24212.1), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 35059.9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 35059.9 - 36153.1


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35160.2), exposure 824.902, 15 soft counts and 0 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0231401, -0.000117038 and -0.0050578. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35160.2 so gap is 100.292, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35255.5), exposure 920.18, 15 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0207239, 0.00128326 and 0.0619216. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35255.5 so gap is 195.57, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35268), exposure 932.716, 16 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0218853, 0.00125909 and 0.0575312. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35268 so gap is 208.107, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35300.6), exposure 965.312, 17 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0225357, 0.0012032 and 0.053391. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35300.6 so gap is 240.702, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35418.4), exposure 1083.16, 18 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.021287, 0.00106038 and 0.0498136. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35418.4 so gap is 358.546, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35431), exposure 1095.69, 19 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0222667, 0.00104236 and 0.0468126. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35431 so gap is 371.082, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35566.4), exposure 1231.09, 20 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0209074, 0.000906752 and 0.0433699. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35566.4 so gap is 506.477, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35611.5), exposure 1276.22, 20 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0201582, 0.0019263 and 0.0955588. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35611.5 so gap is 551.609, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35634.1), exposure 1298.78, 21 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0208451, 0.00188786 and 0.090566. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35634.1 so gap is 574.175, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35684.2), exposure 1348.93, 22 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.021061, 0.0018129 and 0.0860785. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35684.2 so gap is 624.321, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35792), exposure 1456.75, 23 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.020415, 0.00165658 and 0.0811452. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35792 so gap is 732.136, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35809.6), exposure 1474.3, 24 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0210855, 0.0016281 and 0.0772145. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35809.6 so gap is 749.687, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35970.1), exposure 1634.76, 25 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0198042, 0.00145645 and 0.0735423. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 35970.1 so gap is 910.155, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 36007.7), exposure 1672.37, 26 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0201537, 0.0014237 and 0.0706419. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 36007.7 so gap is 947.765, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (35059.9 - 36153.1), exposure 1093.18
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.32683 bg counts (68), with cf=1.34338 and errBG= 0.039634
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7117 +/- 5.20317
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 36153.1), exposure 1817.79, 26 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0185172, 0.0020325 and 0.109763. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35059.9 and stop= 36153.1 so gap is 1093.18, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 8 (36153.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (35059.9 - 36153.1), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (19032 - 24212.1), exposure 1890.5
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.806282 bg counts (103), with cf=1.82382 and errBG= 0.0794453
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =53.244 +/- 9.99051
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 57
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 40824.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 10
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 40824.4 - 42213.4


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 40922.2), exposure 1915.58, 26 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0175522, 0.00261131 and 0.148774. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 40922.2 so gap is 97.7847, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 40944.7), exposure 1938.14, 26 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0173381, 0.00326022 and 0.188038. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 40944.7 so gap is 120.351, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41022.5), exposure 2015.87, 26 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0166555, 0.00379013 and 0.22756. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41022.5 so gap is 198.078, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41142.8), exposure 2136.22, 27 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0163239, 0.00354974 and 0.217456. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41142.8 so gap is 318.429, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41175.4), exposure 2168.82, 28 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.016685, 0.00349639 and 0.209553. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41175.4 so gap is 351.024, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41348.4), exposure 2341.82, 28 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0154241, 0.00380792 and 0.246881. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41348.4 so gap is 524.029, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41358.4), exposure 2351.85, 28 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0153584, 0.00435125 and 0.283315. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41358.4 so gap is 534.059, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41423.6), exposure 2417.04, 29 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0154877, 0.00422992 and 0.273115. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41423.6 so gap is 599.249, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41438.7), exposure 2432.09, 30 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0159316, 0.00419194 and 0.263121. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41438.7 so gap is 614.293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41506.4), exposure 2499.78, 30 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0154888, 0.00460036 and 0.297011. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41506.4 so gap is 681.99, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41604.2), exposure 2597.57, 31 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0154208, 0.00441981 and 0.286613. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41604.2 so gap is 779.776, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41724.5), exposure 2717.92, 31 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0147241, 0.00472388 and 0.320827. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41724.5 so gap is 900.127, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41732), exposure 2725.44, 32 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0151662, 0.00471084 and 0.310614. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41732 so gap is 907.649, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40824.4 - 42213.4), exposure 1389.04
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.503123 bg counts (70), with cf=1.33393 and errBG= 0.0601347
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.3378 +/- 5.1669
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 42213.4), exposure 3206.84, 34 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0137181, 0.00396176 and 0.288797. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 42213.4 so gap is 1389.04, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 9 (42213.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (40824.4 - 42213.4), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (35059.9 - 36153.1), exposure 1093.18
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.32683 bg counts (68), with cf=1.34338 and errBG= 0.039634
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7117 +/- 5.20317
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 58
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 46600.8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 11
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 46600.8 - 48378.4


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 46721.1), exposure 3327.19, 35 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0136212, 0.00380879 and 0.279623. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 46721.1 so gap is 120.35, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 46956.8), exposure 3562.88, 36 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0130823, 0.00355142 and 0.271467. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 46956.8 so gap is 356.039, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 47059.6), exposure 3665.68, 37 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0130798, 0.00345007 and 0.263772. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 47059.6 so gap is 458.839, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 47445.7), exposure 4051.8, 38 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0121486, 0.00310542 and 0.25562. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 47445.7 so gap is 844.966, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 47503.4), exposure 4109.47, 38 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0119781, 0.00338746 and 0.282805. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 47503.4 so gap is 902.634, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 47538.5), exposure 4144.57, 39 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0122136, 0.00335721 and 0.274875. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 47538.5 so gap is 937.737, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 47731.6), exposure 4337.64, 40 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0119735, 0.00320185 and 0.267412. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 47731.6 so gap is 1130.8, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 47829.4), exposure 4435.42, 40 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0117052, 0.00342796 and 0.292858. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 47829.4 so gap is 1228.59, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 47919.6), exposure 4525.69, 40 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0114689, 0.00365458 and 0.318651. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 47919.6 so gap is 1318.85, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 48137.8), exposure 4743.82, 41 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0112168, 0.00348381 and 0.31059. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 48137.8 so gap is 1536.99, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 48150.3), exposure 4756.36, 41 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0111872, 0.00375799 and 0.335919. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 48150.3 so gap is 1549.52, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46600.8 - 48378.4), exposure 1777.68
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.467038 bg counts (97), with cf=1.35705 and errBG= 0.0474206
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.6508 +/- 4.7014
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 48378.4), exposure 4984.51, 42 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0109435, 0.00357174 and 0.326379. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 48378.4 so gap is 1777.68, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 10 (48378.4) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=6165.01 whereas forward=3997.94
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 10 (48378.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 52376.4 - 54550.2


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 52391.4), exposure 4999.56, 43 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0111763, 0.00356099 and 0.318619. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 52391.4 so gap is 5790.66, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 52411.5), exposure 5019.61, 44 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0113907, 0.00354487 and 0.311209. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 52411.5 so gap is 5810.72, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46600.8 - 52506.8), exposure 1908.06
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.516727 bg counts (104), with cf=1.34933 and errBG= 0.0506693
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5427 +/- 5.22636
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 52506.8), exposure 5114.89, 45 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0114269, 0.00347884 and 0.304442. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 52506.8 so gap is 5906, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (46600.8 - 52506.8), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40824.4 - 42213.4), exposure 1389.04
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.503123 bg counts (70), with cf=1.33393 and errBG= 0.0601347
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.3378 +/- 5.1669
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 59
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 12
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 52526.8), exposure 5134.95, 46 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.011638, 0.0034634 and 0.297593. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 52526.8 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 52584.5), exposure 5192.62, 47 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0117519, 0.00342493 and 0.291437. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 52584.5 so gap is 77.7269, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 52704.8), exposure 5312.97, 47 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.011475, 0.00359009 and 0.312861. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 52704.8 so gap is 198.078, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (23487.5 - 52704.8) = 23487.5- 52704.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52506.8 - 54016.2), exposure 1509.4
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.61756 bg counts (87), with cf=1.31853 and errBG= 0.0662094
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9637 +/- 5.1074
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 54016.2 so gap is 1509.4, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (52506.8 - 54016.2), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46600.8 - 52506.8), exposure 1908.06
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.516727 bg counts (104), with cf=1.34933 and errBG= 0.0506693
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5427 +/- 5.22636
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 60
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 12
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (54016.2 - 54550.2), exposure 534.044
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.298132 bg counts (42), with cf=1.31851 and errBG= 0.0460028
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.19944 +/- 2.94889
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (52704.8 - 54550.2), exposure 1845.37, 12 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00828, 0.00329725 and 0.398219. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=54016.2 and stop= 54550.2 so gap is 534.044, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 11 (54550.2) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=534.044 whereas forward=9393.64
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52506.8 - 54550.2), exposure 2043.45
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.915692 bg counts (129), with cf=1.31853 and errBG= 0.0806222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.1632 +/- 5.89759
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 11 (54550.2) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 54550.2), exposure 7158.34, 59 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0106512, 0.00351431 and 0.329944. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (52506.8 - 54550.2), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 63943.9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (23487.5 - 54550.2) = 23487.5- 54550.2
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 63943.9 - 66418.6


++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (63943.9 - 66418.6), exposure 2474.71
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 0.449431 bg counts (140), with cf=1.4372 and errBG= 0.0379838
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.1633 +/- 4.76698
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (63943.9 - 66418.6), exposure 2474.71, 9 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00508509, 0.00104237 and 0.204987. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=63943.9 and stop= 66418.6 so gap is 2474.71, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 12 (66418.6) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=0 and gapBack=11868.3 whereas forward=228904
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52506.8 - 66418.6), exposure 4518.15
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 31 counts and 1.36512 bg counts (269), with cf=1.36064 and errBG= 0.083233
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =40.3223 +/- 7.57656
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 12 (66418.6) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  810  INFO   >>  The current bin is full, and there are orbits left, so writing this bin, which ends at the end of orbit 12 with stop = 66418.6 = 66418.6
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52506.8 - 66418.6), exposure 4518.15
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 31 counts and 1.36512 bg counts (269), with cf=1.36064 and errBG= 0.083233
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =40.3223 +/- 7.57656
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 61
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 295322
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 14
++tructures/grbBin.cpp::        binData:  line  903  INFO   >>  I have run out of background events
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x207c900
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 295322 - 296102
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 295322 - 296102 the cf is 1.59898
++tructures/grbBin.cpp::        binData:  line  921  INFO   >>  This bin is empty, so found a emptyBin CF of 1.59898
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (295322 - 296102), exposure 779.77
++taStructures/bin.cpp::        fullBin:  line  192  INFO   >>  Producing an upper limit of 9.45796 given bg=0.294796 and numCts= 0
++ctures/binMethod.cpp::        saveBin:  line  378  INFO   >>  Saving an upper limit, bin number: 62 with rate=0.0121292
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (63943.9 - 66418.6), exposure 3254.48, 9 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00375838, 0.000770758 and 0.205077. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for PC mode.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: PC, with files: pcsourcetotal_incbad.evt, pcbacktotal_incbad.evt, and pccorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 447.49 - 441841
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	447.49 - 2864.54
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	6160.11 - 8642.34
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	11930.8 - 12136.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	12324.3 - 12397
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	12471.4 - 14419.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	17730.7 - 18342.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	19032 - 20197.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	23487.5 - 24212.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	25534.6 - 25975.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	29277.2 - 30169.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	31710 - 31752.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	35059.9 - 36153.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	40824.4 - 42213.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	46600.8 - 48378.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	52376.4 - 54550.2
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	58360.7 - 60639.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	63943.9 - 66418.6
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	106263 - 106858
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	110130 - 110762
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	112410 - 112636
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	115908 - 116702
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	121727 - 122702
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	127469 - 128821
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	133243 - 135001
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	140380 - 141182
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	144795 - 144903
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	146140 - 147299
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	150592 - 151023
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	152317 - 153077
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	156399 - 158683
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	186915 - 187623
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	192784 - 193383
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	221615 - 221702
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	238895 - 239642
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	245127 - 245403
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	250475 - 251162
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	256235 - 256985
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	268070 - 268502
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	273216 - 274324
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	279536 - 280082
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	289658 - 290042
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	295322 - 296102
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	308015 - 308461
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	314363 - 314641
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	319829 - 320523
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	325356 - 326284
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	330097 - 330541
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	337583 - 337861
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	347231 - 347761
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	359998 - 360961
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	412702 - 412983
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	418466 - 418742
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	422899 - 424501
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	428659 - 430261
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	434479 - 436081
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	440239 - 441841
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - PC mode, suffix = _incbad
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 20 ct/bin at rateFact=10 and binFact= 1.5 with minT 2.51 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file PCCURVE_incbad.qdp, reading from pcsourcetotal_incbad.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (447.49 - 457.52), exposure 10.0292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.15511 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.1021 +/- 9.63792
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=447.49 and stop= 457.52 so gap is 10.0292, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (447.49 - 457.52), with lastBin= 0 and workMinC was 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (457.52 - 470.056), exposure 12.5366
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0 bg counts (0), with cf=2.14364 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.0164 +/- 9.82338
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (447.49 - 470.056), exposure 22.5658, 21 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.00301, 1.90194 and 0.949544. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=457.52 and stop= 470.056 so gap is 12.5366, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (457.52 - 470.056), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (447.49 - 457.52), exposure 10.0292
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.15511 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.1021 +/- 9.63792
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (447.49 - 470.056) = 447.49- 470.056
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (470.056 - 485.1), exposure 15.044
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.138006 bg counts (5), with cf=2.23028 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.4492 +/- 11.1522
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=470.056 and stop= 485.1 so gap is 15.044, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (470.056 - 485.1), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (457.52 - 470.056), exposure 12.5366
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0 bg counts (0), with cf=2.14364 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.0164 +/- 9.82338
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (470.056 - 495.13), exposure 25.0732, 20 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.74478, 1.64361 and 0.942017. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=485.1 and stop= 495.13 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (470.056 - 497.637), exposure 27.5805, 22 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.73888, 1.64693 and 0.947122. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=485.1 and stop= 497.637 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (470.056 - 497.637) = 470.056- 497.637
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (485.1 - 500.144), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.0552023 bg counts (2), with cf=2.14643 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.2494 +/- 10.2943
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=485.1 and stop= 500.144 so gap is 15.0439, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (485.1 - 500.144), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (470.056 - 485.1), exposure 15.044
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.138006 bg counts (5), with cf=2.23028 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =55.4492 +/- 11.1522
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (500.144 - 522.71), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.19675 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.8892 +/- 10.0675
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=500.144 and stop= 522.71 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (500.144 - 522.71), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (485.1 - 500.144), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.0552023 bg counts (2), with cf=2.14643 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.2494 +/- 10.2943
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (497.637 - 530.232), exposure 32.5952, 20 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.33734, 1.06786 and 0.798496. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=522.71 and stop= 530.232 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (497.637 - 532.739), exposure 35.1025, 22 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.35983, 1.17119 and 0.861278. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=522.71 and stop= 532.739 so gap is 10.0292, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (497.637 - 535.247), exposure 37.6098, 25 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.43679, 1.14899 and 0.799692. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=522.71 and stop= 535.247 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (497.637 - 535.247) = 497.637- 535.247
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (522.71 - 537.754), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.0276011 bg counts (1), with cf=2.10909 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.3417 +/- 9.89266
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=522.71 and stop= 537.754 so gap is 15.0439, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (522.71 - 537.754), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (500.144 - 522.71), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.19675 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.8892 +/- 10.0675
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (537.754 - 555.305), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.17813 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.4424 +/- 9.74128
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=537.754 and stop= 555.305 so gap is 17.5512, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (537.754 - 555.305), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (522.71 - 537.754), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.0276011 bg counts (1), with cf=2.10909 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.3417 +/- 9.89266
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (535.247 - 570.349), exposure 35.1025, 21 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.2752, 1.10841 and 0.869204. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=555.305 and stop= 570.349 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (535.247 - 572.856), exposure 37.6098, 22 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.24707, 1.03451 and 0.829555. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=555.305 and stop= 572.856 so gap is 17.5513, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (535.247 - 575.364), exposure 40.1172, 23 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.22246, 0.969857 and 0.793365. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=555.305 and stop= 575.364 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (555.305 - 577.871), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0 bg counts (0), with cf=2.1266 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.0385 +/- 10.4182
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (535.247 - 577.871), exposure 42.6245, 28 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.40152, 0.963001 and 0.687111. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=555.305 and stop= 577.871 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (555.305 - 577.871), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (537.754 - 555.305), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.17813 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.4424 +/- 9.74128
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (535.247 - 582.886), exposure 47.6391, 31 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.38932, 0.905906 and 0.652047. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=577.871 and stop= 582.886 so gap is 5.01468, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (535.247 - 582.886) = 535.247- 582.886
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (577.871 - 602.944), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.16887 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.3666 +/- 9.93954
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=577.871 and stop= 602.944 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (577.871 - 602.944), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (555.305 - 577.871), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0 bg counts (0), with cf=2.1266 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.0385 +/- 10.4182
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 620.496), exposure 37.6098, 21 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.20115, 0.73774 and 0.614197. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=602.944 and stop= 620.496 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 623.003), exposure 40.1171, 22 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.1793, 0.691632 and 0.586474. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=602.944 and stop= 623.003 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (602.944 - 625.51), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.13746 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.7291 +/- 10.0264
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 625.51), exposure 42.6245, 23 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.15864, 0.801247 and 0.691543. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=602.944 and stop= 625.51 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (602.944 - 625.51), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (577.871 - 602.944), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.16887 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.3666 +/- 9.93954
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 628.018), exposure 45.1317, 23 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.09427, 0.851367 and 0.778023. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=625.51 and stop= 628.018 so gap is 2.50728, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 630.525), exposure 47.6391, 24 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.08262, 0.851258 and 0.786293. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=625.51 and stop= 630.525 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (582.886 - 633.032), exposure 50.1464, 26 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.1146, 0.85234 and 0.764707. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=625.51 and stop= 633.032 so gap is 7.52194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (582.886 - 633.032) = 582.886- 633.032
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (625.51 - 648.076), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.110405 bg counts (4), with cf=2.18249 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =47.7737 +/- 10.2375
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=625.51 and stop= 648.076 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (625.51 - 648.076), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (602.944 - 625.51), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.13746 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.7291 +/- 10.0264
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (648.076 - 668.135), exposure 20.0586
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0276011 bg counts (1), with cf=2.16498 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.4048 +/- 9.92135
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=648.076 and stop= 668.135 so gap is 20.0586, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (648.076 - 668.135), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (625.51 - 648.076), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.110405 bg counts (4), with cf=2.18249 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =47.7737 +/- 10.2375
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (633.032 - 673.149), exposure 40.1171, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.07612, 0.971432 and 0.902721. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=668.135 and stop= 673.149 so gap is 5.01462, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (633.032 - 675.657), exposure 42.6245, 20 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.01281, 1.01371 and 1.00088. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=668.135 and stop= 675.657 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (633.032 - 675.657) = 633.032- 675.657
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (668.135 - 693.208), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.15064 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9853 +/- 9.85599
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=668.135 and stop= 693.208 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (668.135 - 693.208), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (648.076 - 668.135), exposure 20.0586
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0276011 bg counts (1), with cf=2.16498 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.4048 +/- 9.92135
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 12
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 705.744), exposure 30.0878, 22 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.57739, 0.275082 and 0.17439. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 705.744 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 708.252), exposure 32.5952, 24 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.58852, 0.253921 and 0.159848. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 708.252 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 710.759), exposure 35.1025, 25 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.53604, 0.296765 and 0.193201. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 710.759 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 713.266), exposure 37.6098, 27 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.54748, 0.333898 and 0.215768. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 713.266 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 715.774), exposure 40.1171, 29 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.55601, 0.313029 and 0.201174. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 715.774 so gap is 22.5659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 718.281), exposure 42.6245, 29 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.46448, 0.343457 and 0.234524. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 718.281 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (693.208 - 720.788), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.193208 bg counts (7), with cf=2.15045 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.1954 +/- 10.5362
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 720.788), exposure 45.1317, 32 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.52702, 0.420286 and 0.275233. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=693.208 and stop= 720.788 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (693.208 - 720.788), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (668.135 - 693.208), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.15064 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9853 +/- 9.85599
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 13
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 723.296), exposure 47.6391, 33 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.49209, 0.398165 and 0.266851. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 723.296 so gap is 2.50734, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 728.31), exposure 52.6537, 34 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.3911, 0.360245 and 0.258964. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 728.31 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 733.325), exposure 57.6684, 38 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.41846, 0.328919 and 0.231885. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 733.325 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 735.832), exposure 60.1757, 38 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.35936, 0.35075 and 0.258027. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 735.832 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 740.847), exposure 65.1903, 38 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.25479, 0.35664 and 0.284223. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 740.847 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 743.354), exposure 67.6976, 39 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.23997, 0.436645 and 0.352142. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 743.354 so gap is 22.5659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 745.862), exposure 70.205, 40 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.22621, 0.482096 and 0.39316. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 745.862 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 748.369), exposure 72.7123, 43 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.26988, 0.465472 and 0.366547. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 748.369 so gap is 27.5806, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (720.788 - 750.876), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.138006 bg counts (5), with cf=2.15117 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7266 +/- 9.62125
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 750.876), exposure 75.2196, 43 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.22756, 0.508834 and 0.41451. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=720.788 and stop= 750.876 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (720.788 - 750.876), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (693.208 - 720.788), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.193208 bg counts (7), with cf=2.15045 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.1954 +/- 10.5362
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 14
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 755.891), exposure 80.2342, 44 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.17844, 0.477032 and 0.4048. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 755.891 so gap is 5.01466, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 758.398), exposure 82.7416, 45 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.1695, 0.462576 and 0.395534. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 758.398 so gap is 7.522, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 760.906), exposure 85.2489, 47 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.18521, 0.448971 and 0.378813. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 760.906 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 763.413), exposure 87.7562, 48 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.175, 0.435468 and 0.37061. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 763.413 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 768.427), exposure 92.7708, 49 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.13451, 0.411929 and 0.36309. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 768.427 so gap is 17.5513, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 775.949), exposure 100.293, 49 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.04942, 0.401718 and 0.3828. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 775.949 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (675.657 - 778.457), exposure 102.8, 50 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.04458, 0.412676 and 0.395064. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 778.457 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (675.657 - 778.457) = 675.657- 778.457
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (750.876 - 796.008), exposure 45.1318
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.110405 bg counts (4), with cf=2.15702 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.3734 +/- 10.3454
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.876 and stop= 796.008 so gap is 45.1318, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (750.876 - 796.008), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (720.788 - 750.876), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.138006 bg counts (5), with cf=2.15117 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7266 +/- 9.62125
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 15
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (796.008 - 826.096), exposure 30.0879
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.16277 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.2555 +/- 9.67222
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=796.008 and stop= 826.096 so gap is 30.0879, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (796.008 - 826.096), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (750.876 - 796.008), exposure 45.1318
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.110405 bg counts (4), with cf=2.15702 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.3734 +/- 10.3454
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 16
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 833.618), exposure 55.161, 21 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.820273, 0.702672 and 0.856632. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 833.618 so gap is 7.52194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 836.125), exposure 57.6684, 23 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.858775, 0.671089 and 0.781449. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 836.125 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 838.632), exposure 60.1757, 26 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.929606, 0.643127 and 0.691827. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 838.632 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 841.14), exposure 62.683, 27 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.927248, 0.617401 and 0.665843. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 841.14 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 843.647), exposure 65.1903, 27 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.891585, 0.627143 and 0.703401. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 843.647 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (778.457 - 846.154), exposure 67.6976, 28 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.89081, 0.636161 and 0.714138. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 846.154 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (778.457 - 846.154) = 778.457- 846.154
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (826.096 - 853.676), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.15785 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.0767 +/- 9.88924
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=826.096 and stop= 853.676 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (826.096 - 853.676), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (796.008 - 826.096), exposure 30.0879
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.16277 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.2555 +/- 9.67222
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 17
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (853.676 - 893.793), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0828034 bg counts (3), with cf=2.14398 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7021 +/- 9.58872
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=853.676 and stop= 893.793 so gap is 40.1171, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (853.676 - 893.793), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (826.096 - 853.676), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.15785 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =45.0767 +/- 9.88924
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 18
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 906.33), exposure 60.1757, 20 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.711315, 0.425929 and 0.598791. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 906.33 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 911.345), exposure 65.1903, 23 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.756295, 0.393166 and 0.519858. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 911.345 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 913.852), exposure 67.6976, 25 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.792287, 0.378604 and 0.477862. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 913.852 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 918.867), exposure 72.7123, 26 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.766624, 0.382287 and 0.498663. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 918.867 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 921.374), exposure 75.2196, 27 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.768792, 0.397268 and 0.516744. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 921.374 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 923.881), exposure 77.7269, 28 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.770819, 0.384453 and 0.498759. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 923.881 so gap is 30.0879, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 926.389), exposure 80.2342, 28 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.746732, 0.39843 and 0.533566. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 926.389 so gap is 32.5951, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 928.896), exposure 82.7415, 28 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.723387, 0.41156 and 0.568934. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 928.896 so gap is 35.1025, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 933.911), exposure 87.7562, 29 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.706827, 0.387369 and 0.548039. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 933.911 so gap is 40.1171, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 936.418), exposure 90.2635, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.71128, 0.376609 and 0.52948. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 936.418 so gap is 42.6244, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (893.793 - 941.433), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.14133 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.7316 +/- 9.81353
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 941.433), exposure 95.2781, 32 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.719766, 0.356787 and 0.495699. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=893.793 and stop= 941.433 so gap is 47.639, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (893.793 - 941.433), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (853.676 - 893.793), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0828034 bg counts (3), with cf=2.14398 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7021 +/- 9.58872
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 19
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 943.94), exposure 97.7855, 32 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.70131, 0.369404 and 0.526734. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=941.433 and stop= 943.94 so gap is 2.50736, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 946.447), exposure 100.293, 32 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.683777, 0.403789 and 0.590528. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=941.433 and stop= 946.447 so gap is 5.0147, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 948.954), exposure 102.8, 33 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.68838, 0.393941 and 0.572273. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=941.433 and stop= 948.954 so gap is 7.52198, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (846.154 - 951.462), exposure 105.307, 33 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.67199, 0.404624 and 0.602127. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=941.433 and stop= 951.462 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (846.154 - 951.462) = 846.154- 951.462
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (941.433 - 984.057), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.110405 bg counts (4), with cf=2.13821 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.5281 +/- 9.56308
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=941.433 and stop= 984.057 so gap is 42.6244, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (941.433 - 984.057), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (893.793 - 941.433), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.14133 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.7316 +/- 9.81353
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1019.16), exposure 67.6976, 20 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.632839, 0.405196 and 0.640283. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=984.057 and stop= 1019.16 so gap is 35.1025, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (984.057 - 1021.67), exposure 37.6098
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.15277 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9705 +/- 9.86596
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1021.67), exposure 70.2049, 21 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.640732, 0.451714 and 0.704997. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=984.057 and stop= 1021.67 so gap is 37.6098, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (984.057 - 1021.67), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (941.433 - 984.057), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.110405 bg counts (4), with cf=2.13821 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.5281 +/- 9.56308
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 21
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1026.68), exposure 75.2195, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.626479, 0.4216 and 0.672968. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1026.68 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1029.19), exposure 77.7269, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.661356, 0.408 and 0.616914. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1029.19 so gap is 7.52198, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1031.7), exposure 80.2342, 25 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.666908, 0.421475 and 0.631983. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1031.7 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1034.2), exposure 82.7415, 25 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.646699, 0.434132 and 0.671305. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1034.2 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1036.71), exposure 85.2489, 25 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.627678, 0.470724 and 0.749945. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1036.71 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (951.462 - 1041.73), exposure 90.2635, 25 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.592807, 0.46805 and 0.789548. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1041.73 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (951.462 - 1041.73) = 951.462- 1041.73
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1021.67 - 1066.8), exposure 45.1317
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0276011 bg counts (1), with cf=2.13829 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7068 +/- 9.56292
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1021.67 and stop= 1066.8 so gap is 45.1317, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1021.67 - 1066.8), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (984.057 - 1021.67), exposure 37.6098
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.110405 bg counts (4), with cf=2.15277 and errBG= 0.0552023
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9705 +/- 9.86596
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 22
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1066.8 - 1114.44), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.13143 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.5974 +/- 9.99818
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1114.44), exposure 72.7122, 21 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.616403, 0.349645 and 0.567235. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1066.8 and stop= 1114.44 so gap is 47.639, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1066.8 - 1114.44), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1021.67 - 1066.8), exposure 45.1317
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0276011 bg counts (1), with cf=2.13829 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7068 +/- 9.56292
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 23
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1116.94), exposure 75.2196, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.624211, 0.394701 and 0.632319. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1116.94 so gap is 2.50734, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1121.96), exposure 80.2342, 23 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.611934, 0.396767 and 0.648382. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1121.96 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1131.99), exposure 90.2635, 24 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.567515, 0.425368 and 0.749527. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1131.99 so gap is 17.5513, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1139.51), exposure 97.7854, 24 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.523861, 0.415013 and 0.792221. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1139.51 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1041.73 - 1142.02), exposure 100.293, 24 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.510764, 0.425709 and 0.833475. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1142.02 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1041.73 - 1142.02) = 1041.73- 1142.02
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1114.44 - 1167.09), exposure 52.6537
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.14353 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7523 +/- 9.58654
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1114.44 and stop= 1167.09 so gap is 52.6537, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1114.44 - 1167.09), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1066.8 - 1114.44), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.13143 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.5974 +/- 9.99818
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 24
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1167.09 - 1209.72), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0276011 bg counts (1), with cf=2.1412 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9062 +/- 9.8124
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1167.09 and stop= 1209.72 so gap is 42.6244, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1167.09 - 1209.72), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1114.44 - 1167.09), exposure 52.6537
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.14353 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.7523 +/- 9.58654
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 25
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1224.76), exposure 82.7415, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.514836, 0.385665 and 0.749101. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1224.76 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1234.79), exposure 92.7707, 20 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.459178, 0.367535 and 0.800419. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1234.79 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1239.8), exposure 97.7854, 21 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.457987, 0.348687 and 0.761346. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1239.8 so gap is 30.0878, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1247.33), exposure 105.307, 22 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.445822, 0.323781 and 0.726255. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1247.33 so gap is 37.6098, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1249.83), exposure 107.815, 23 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.455525, 0.316251 and 0.694256. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1249.83 so gap is 40.1171, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1254.85), exposure 112.829, 24 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.453919, 0.302195 and 0.665748. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1254.85 so gap is 45.1317, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1257.35), exposure 115.337, 25 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.462285, 0.313861 and 0.678933. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1257.35 so gap is 47.6391, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1259.86), exposure 117.844, 27 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.488142, 0.306683 and 0.628265. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1259.86 so gap is 50.1463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1262.37), exposure 120.351, 27 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.477972, 0.317551 and 0.66437. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1262.37 so gap is 52.6537, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1269.89), exposure 127.873, 28 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.466559, 0.29841 and 0.639597. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1269.89 so gap is 60.1756, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1274.91), exposure 132.888, 28 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.448953, 0.303315 and 0.675606. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1274.91 so gap is 65.1903, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1142.02 - 1287.44), exposure 145.424, 28 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.409846, 0.291793 and 0.711959. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1287.44 so gap is 77.7268, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1142.02 - 1287.44) = 1142.02- 1287.44
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1209.72 - 1302.49), exposure 92.7708
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.193208 bg counts (7), with cf=2.13642 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.3157 +/- 9.55564
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1209.72 and stop= 1302.49 so gap is 92.7708, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1209.72 - 1302.49), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1167.09 - 1209.72), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0276011 bg counts (1), with cf=2.1412 and errBG= 0.0276011
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.9062 +/- 9.8124
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 26
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1302.49 - 1362.66), exposure 60.1755
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.13604 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6799 +/- 9.78908
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1302.49 and stop= 1362.66 so gap is 60.1755, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1302.49 - 1362.66), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1209.72 - 1302.49), exposure 92.7708
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.193208 bg counts (7), with cf=2.13642 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.3157 +/- 9.55564
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 27
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1377.71), exposure 90.2634, 20 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.470722, 0.188944 and 0.401392. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1377.71 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1382.72), exposure 95.278, 20 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.445947, 0.201181 and 0.451132. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1382.72 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1385.23), exposure 97.7854, 22 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.477732, 0.196023 and 0.41032. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1385.23 so gap is 22.5659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1390.24), exposure 102.8, 22 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.454428, 0.227576 and 0.500797. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1390.24 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1392.75), exposure 105.307, 23 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.463881, 0.222158 and 0.478911. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1392.75 so gap is 30.0878, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1395.26), exposure 107.815, 24 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.472894, 0.216991 and 0.458858. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1395.26 so gap is 32.5951, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1397.76), exposure 110.322, 24 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.461614, 0.231411 and 0.501309. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1397.76 so gap is 35.1025, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1400.27), exposure 112.829, 25 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.470277, 0.226269 and 0.48114. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1400.27 so gap is 37.6098, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1407.79), exposure 120.351, 26 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.458417, 0.228679 and 0.498845. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1407.79 so gap is 45.1317, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1420.33), exposure 132.888, 26 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.41517, 0.223003 and 0.537137. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1420.33 so gap is 57.6683, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1422.84), exposure 135.395, 27 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.422798, 0.218873 and 0.517679. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1422.84 so gap is 60.1756, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1362.66 - 1425.34), exposure 62.6829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.165607 bg counts (6), with cf=2.12494 and errBG= 0.0676087
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.1468 +/- 9.50409
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1425.34), exposure 137.902, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.415111, 0.245394 and 0.591154. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1362.66 and stop= 1425.34 so gap is 62.6829, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1362.66 - 1425.34), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1302.49 - 1362.66), exposure 60.1755
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0828034 bg counts (3), with cf=2.13604 and errBG= 0.0478066
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6799 +/- 9.78908
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 28
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1430.36), exposure 142.917, 28 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.415467, 0.251706 and 0.605839. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.34 and stop= 1430.36 so gap is 5.01462, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1432.87), exposure 145.424, 30 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.437698, 0.262064 and 0.598731. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.34 and stop= 1432.87 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1437.88), exposure 150.439, 31 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.437316, 0.267536 and 0.611768. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.34 and stop= 1437.88 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1287.44 - 1442.9), exposure 155.454, 32 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.436806, 0.272503 and 0.623855. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.34 and stop= 1442.9 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1287.44 - 1442.9) = 1287.44- 1442.9
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1425.34 - 1472.98), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.15462 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.9734 +/- 9.63612
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1425.34 and stop= 1472.98 so gap is 47.639, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1425.34 - 1472.98), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1362.66 - 1425.34), exposure 62.6829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.165607 bg counts (6), with cf=2.12494 and errBG= 0.0676087
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.1468 +/- 9.50409
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 29
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1472.98 - 1545.7), exposure 72.7122
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.12542 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.4658 +/- 9.96995
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1472.98 and stop= 1545.7 so gap is 72.7122, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1472.98 - 1545.7), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1425.34 - 1472.98), exposure 47.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0552023 bg counts (2), with cf=2.15462 and errBG= 0.0390339
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.9734 +/- 9.63612
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 30
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1563.25), exposure 120.351, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.354228, 0.317893 and 0.897426. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1563.25 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1570.77), exposure 127.873, 20 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.332926, 0.316217 and 0.949811. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1570.77 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1583.31), exposure 140.41, 21 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.317095, 0.287983 and 0.908193. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1583.31 so gap is 37.6098, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1585.81), exposure 142.917, 22 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.326429, 0.282518 and 0.865482. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1585.81 so gap is 40.117, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1588.32), exposure 145.424, 23 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.335441, 0.277647 and 0.827708. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1588.32 so gap is 42.6244, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1442.9 - 1590.83), exposure 147.932, 23 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.329756, 0.287332 and 0.871348. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1590.83 so gap is 45.1317, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1442.9 - 1590.83) = 1442.9- 1590.83
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1545.7 - 1648.5), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.276011 bg counts (10), with cf=2.15566 and errBG= 0.0872825
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6739 +/- 9.88027
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1545.7 and stop= 1648.5 so gap is 102.8, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1545.7 - 1648.5), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1472.98 - 1545.7), exposure 72.7122
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.138006 bg counts (5), with cf=2.12542 and errBG= 0.061718
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =46.4658 +/- 9.96995
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 31
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1721.21), exposure 130.38, 21 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.348236, 0.14728 and 0.422931. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1648.5 and stop= 1721.21 so gap is 72.7121, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1648.5 - 1733.74), exposure 85.2487
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.193208 bg counts (7), with cf=2.16277 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.8376 +/- 9.67351
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1733.74), exposure 142.917, 22 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.332509, 0.132697 and 0.399078. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1648.5 and stop= 1733.74 so gap is 85.2487, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1648.5 - 1733.74), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1545.7 - 1648.5), exposure 102.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.276011 bg counts (10), with cf=2.15566 and errBG= 0.0872825
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6739 +/- 9.88027
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 32
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1756.31), exposure 165.483, 23 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.299325, 0.127484 and 0.425905. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1756.31 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1761.33), exposure 170.497, 24 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.302673, 0.123386 and 0.407655. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1761.33 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1766.34), exposure 175.512, 24 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.294025, 0.132045 and 0.449095. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1766.34 so gap is 32.5951, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1776.37), exposure 185.541, 25 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.289836, 0.13661 and 0.471336. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1776.37 so gap is 42.6243, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1781.38), exposure 190.556, 25 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.282209, 0.14441 and 0.511714. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1781.38 so gap is 47.639, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1783.89), exposure 193.063, 25 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.278544, 0.153517 and 0.55114. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1783.89 so gap is 50.1463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1788.91), exposure 198.078, 26 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.282195, 0.14963 and 0.530238. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1788.91 so gap is 55.1609, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1793.92), exposure 203.092, 27 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.285995, 0.156702 and 0.547918. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1793.92 so gap is 60.1755, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1803.95), exposure 213.122, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.272256, 0.159198 and 0.584737. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1803.95 so gap is 70.2048, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1808.96), exposure 218.136, 28 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.27564, 0.155539 and 0.564282. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1808.96 so gap is 75.2194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1811.47), exposure 220.644, 29 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.28204, 0.153771 and 0.54521. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1811.47 so gap is 77.7267, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1813.98), exposure 223.151, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.288626, 0.152043 and 0.526783. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1813.98 so gap is 80.234, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1816.49), exposure 225.658, 30 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.285419, 0.16 and 0.560578. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1816.49 so gap is 82.7414, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1818.99), exposure 228.166, 31 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.291824, 0.158242 and 0.54225. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1818.99 so gap is 85.2486, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1821.5), exposure 230.673, 33 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.307526, 0.156522 and 0.508969. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1821.5 so gap is 87.756, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1733.74 - 1846.57), exposure 112.829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.193208 bg counts (7), with cf=2.15856 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =47.0714 +/- 10.1258
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1846.57), exposure 255.746, 34 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.285555, 0.158463 and 0.55493. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1733.74 and stop= 1846.57 so gap is 112.829, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1733.74 - 1846.57), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1648.5 - 1733.74), exposure 85.2487
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.193208 bg counts (7), with cf=2.16277 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.8376 +/- 9.67351
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 33
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1854.1), exposure 263.268, 35 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.285445, 0.153936 and 0.539282. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1846.57 and stop= 1854.1 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1590.83 - 1864.12), exposure 273.297, 36 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.282616, 0.164014 and 0.580342. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1846.57 and stop= 1864.12 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1590.83 - 1864.12) = 1590.83- 1864.12
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1846.57 - 1956.9), exposure 110.322
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.220809 bg counts (8), with cf=2.15835 and errBG= 0.0780678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.6903 +/- 9.65388
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1846.57 and stop= 1956.9 so gap is 110.322, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1846.57 - 1956.9), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1733.74 - 1846.57), exposure 112.829
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.193208 bg counts (7), with cf=2.15856 and errBG= 0.0730257
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =47.0714 +/- 10.1258
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 34
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2032.11), exposure 167.99, 20 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.254721, 0.112268 and 0.440747. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2032.11 so gap is 75.2194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2039.64), exposure 175.512, 21 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.256048, 0.107456 and 0.419672. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2039.64 so gap is 82.7413, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2052.17), exposure 188.048, 22 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.250035, 0.100292 and 0.401114. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2052.17 so gap is 95.2779, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2057.19), exposure 193.063, 23 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.254577, 0.0976874 and 0.383725. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2057.19 so gap is 100.293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2072.23), exposure 208.107, 24 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.246154, 0.0906256 and 0.368166. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2072.23 so gap is 115.336, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2077.25), exposure 213.122, 25 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.250004, 0.0884933 and 0.353967. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2077.25 so gap is 120.351, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2079.75), exposure 215.629, 26 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.256902, 0.0874643 and 0.340458. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2079.75 so gap is 122.858, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1956.9 - 2084.77), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.303613 bg counts (11), with cf=2.14331 and errBG= 0.0915426
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2155 +/- 9.58719
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2084.77), exposure 220.643, 27 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.260773, 0.0854765 and 0.327781. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1956.9 and stop= 2084.77 so gap is 127.873, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1956.9 - 2084.77), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1846.57 - 1956.9), exposure 110.322
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.220809 bg counts (8), with cf=2.15835 and errBG= 0.0780678
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.6903 +/- 9.65388
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 35
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2087.28), exposure 223.151, 27 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.257577, 0.0941179 and 0.365397. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2087.28 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2094.8), exposure 230.673, 28 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.258437, 0.0907911 and 0.351308. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2094.8 so gap is 10.0292, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2099.81), exposure 235.687, 28 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.252938, 0.0979228 and 0.387141. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2099.81 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2104.83), exposure 240.702, 28 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.247422, 0.104633 and 0.422892. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2104.83 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2107.33), exposure 243.209, 29 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.253529, 0.103554 and 0.408451. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2107.33 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2112.35), exposure 248.224, 30 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.25689, 0.101462 and 0.394964. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2112.35 so gap is 27.5804, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2139.93), exposure 275.804, 31 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.238652, 0.0908861 and 0.380831. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2139.93 so gap is 55.1609, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2152.47), exposure 288.341, 32 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.235806, 0.0867289 and 0.367798. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2152.47 so gap is 67.6974, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2162.49), exposure 298.37, 33 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.235028, 0.0838137 and 0.356612. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2162.49 so gap is 77.7267, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2165), exposure 300.877, 33 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.233069, 0.0903779 and 0.387773. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2165 so gap is 80.2339, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2170.02), exposure 305.892, 34 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.236394, 0.0888963 and 0.376051. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2170.02 so gap is 85.2486, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2180.05), exposure 315.921, 34 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.22889, 0.0930237 and 0.406413. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2180.05 so gap is 95.2778, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2182.55), exposure 318.429, 35 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.233984, 0.0922913 and 0.394433. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2182.55 so gap is 97.7851, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2190.08), exposure 325.951, 36 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.234915, 0.0901615 and 0.383804. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2190.08 so gap is 105.307, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2197.6), exposure 333.472, 37 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.236115, 0.0881278 and 0.373241. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2197.6 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2205.12), exposure 340.994, 38 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.237102, 0.0923815 and 0.389627. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2205.12 so gap is 120.351, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2215.15), exposure 351.024, 39 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.236448, 0.0894036 and 0.378111. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2215.15 so gap is 130.38, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2217.66), exposure 353.531, 40 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.240848, 0.0887696 and 0.36857. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2217.66 so gap is 132.887, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2084.77 - 2225.18), exposure 140.409
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.276011 bg counts (10), with cf=2.14192 and errBG= 0.0872825
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2473 +/- 9.5808
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2225.18), exposure 361.053, 41 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.241687, 0.0869202 and 0.359639. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2084.77 and stop= 2225.18 so gap is 140.409, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2084.77 - 2225.18), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1956.9 - 2084.77), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.303613 bg counts (11), with cf=2.14331 and errBG= 0.0915426
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2155 +/- 9.58719
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 36
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2245.24), exposure 381.111, 42 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.234551, 0.0823454 and 0.351076. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2245.24 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2247.74), exposure 383.619, 43 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.238566, 0.0816524 and 0.342263. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2247.74 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2262.79), exposure 398.663, 43 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.229267, 0.0839296 and 0.366078. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2262.79 so gap is 37.6097, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2267.8), exposure 403.677, 43 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.226419, 0.0883345 and 0.390138. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2267.8 so gap is 42.6243, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2282.85), exposure 418.721, 44 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.223411, 0.0851608 and 0.381185. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2282.85 so gap is 57.6682, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2287.86), exposure 423.736, 45 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.225953, 0.084153 and 0.372437. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2287.86 so gap is 62.6828, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1864.12 - 2300.4), exposure 436.272, 45 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.219324, 0.0965063 and 0.440017. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2300.4 so gap is 75.2194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1864.12 - 2300.4) = 1864.12- 2300.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2225.18 - 2365.59), exposure 140.409
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.165607 bg counts (6), with cf=2.16532 and errBG= 0.0676087
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.9478 +/- 9.68471
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2225.18 and stop= 2365.59 so gap is 140.409, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2225.18 - 2365.59), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2084.77 - 2225.18), exposure 140.409
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.276011 bg counts (10), with cf=2.14192 and errBG= 0.0872825
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2473 +/- 9.5808
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 37
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2483.43), exposure 183.034, 20 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.236351, 0.0928338 and 0.392779. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2365.59 and stop= 2483.43 so gap is 117.844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2498.47), exposure 198.077, 21 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.228825, 0.0857832 and 0.374886. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2365.59 and stop= 2498.47 so gap is 132.887, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2506), exposure 205.599, 21 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.220161, 0.0928022 and 0.42152. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2365.59 and stop= 2506 so gap is 140.409, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2365.59 - 2518.53), exposure 152.946
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.331214 bg counts (12), with cf=2.17217 and errBG= 0.0956131
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.724 +/- 9.71647
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2518.53), exposure 218.136, 21 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.207233, 0.0977567 and 0.471724. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2365.59 and stop= 2518.53 so gap is 152.946, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2365.59 - 2518.53), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2225.18 - 2365.59), exposure 140.409
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.165607 bg counts (6), with cf=2.16532 and errBG= 0.0676087
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.9478 +/- 9.68471
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 38
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2521.04), exposure 220.643, 22 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.215051, 0.106818 and 0.496709. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2521.04 so gap is 2.50736, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2526.05), exposure 225.658, 23 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.220236, 0.104444 and 0.474238. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2526.05 so gap is 7.52194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2531.07), exposure 230.672, 24 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.224933, 0.102174 and 0.45424. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2531.07 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2546.11), exposure 245.716, 25 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.219588, 0.0959181 and 0.43681. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2546.11 so gap is 27.5804, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2551.13), exposure 250.731, 25 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.214956, 0.102497 and 0.476829. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2551.13 so gap is 32.5951, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2553.64), exposure 253.225, 25 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.212601, 0.109901 and 0.516937. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2553.64 so gap is 35.1023, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 1, last was 0 so increasing dead to 0.0129083
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2561.16), exposure 260.747, 26 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.211186, 0.106731 and 0.505387. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2561.16 so gap is 42.6243, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2566.17), exposure 265.762, 26 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.207201, 0.109336 and 0.527679. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2566.17 so gap is 47.6389, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2576.2), exposure 275.791, 27 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.204125, 0.10536 and 0.516153. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2576.2 so gap is 57.6682, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2578.71), exposure 278.298, 27 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.202286, 0.108817 and 0.537937. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2578.71 so gap is 60.1754, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2581.22), exposure 280.806, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.200479, 0.112209 and 0.559702. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2581.22 so gap is 62.6828, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2591.24), exposure 290.835, 28 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.197799, 0.108339 and 0.547725. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2591.24 so gap is 72.712, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2606.29), exposure 305.879, 29 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.191898, 0.103011 and 0.536801. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2606.29 so gap is 87.7559, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2613.81), exposure 313.401, 29 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.187292, 0.104446 and 0.557664. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2613.81 so gap is 95.2778, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2616.32), exposure 315.908, 30 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.189693, 0.103617 and 0.546234. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2616.32 so gap is 97.7851, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2631.36), exposure 330.952, 31 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.184787, 0.098907 and 0.53525. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2631.36 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2636.38), exposure 335.967, 32 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.185687, 0.0972686 and 0.52383. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2636.38 so gap is 117.844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2641.39), exposure 340.981, 32 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.182957, 0.0994371 and 0.543501. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2641.39 so gap is 122.858, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2518.53 - 2648.91), exposure 130.367
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.166514 bg counts (6), with cf=1.56126 and errBG= 0.0679789
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.9652 +/- 6.98296
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2648.91), exposure 348.503, 32 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.179008, 0.100803 and 0.563121. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2518.53 and stop= 2648.91 so gap is 130.38, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2518.53 - 2648.91), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2365.59 - 2518.53), exposure 152.946
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.331214 bg counts (12), with cf=2.17217 and errBG= 0.0956131
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.724 +/- 9.71647
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 39
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2661.45), exposure 361.04, 33 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.176194, 0.0971579 and 0.551426. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2648.91 and stop= 2661.45 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (2300.4 - 2661.45) = 2300.4- 2661.45
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2648.91 - 2709.09), exposure 60.1754
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.196382 bg counts (7), with cf=1.21884 and errBG= 0.0742253
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.3562 +/- 5.58614
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2648.91 and stop= 2709.09 so gap is 60.1754, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2648.91 - 2709.09), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2518.53 - 2648.91), exposure 130.367
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.166514 bg counts (6), with cf=1.56126 and errBG= 0.0679789
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.9652 +/- 6.98296
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 40
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2794.34), exposure 132.887, 21 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.191259, 0.0807512 and 0.422209. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2794.34 so gap is 85.2485, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2799.35), exposure 137.902, 22 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.19315, 0.0778148 and 0.402872. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2799.35 so gap is 90.2632, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2814.4), exposure 152.946, 23 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.182116, 0.0701608 and 0.385253. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2814.4 so gap is 105.307, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2816.9), exposure 155.453, 23 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.179179, 0.0846952 and 0.472684. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2816.9 so gap is 107.814, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2819.41), exposure 157.961, 23 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.176335, 0.0910593 and 0.516399. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2819.41 so gap is 110.322, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2821.92), exposure 160.468, 24 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.181167, 0.0894229 and 0.493593. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2821.92 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2824.42), exposure 162.975, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.17838, 0.0955184 and 0.535477. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2824.42 so gap is 115.336, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2826.93), exposure 165.482, 24 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.175678, 0.101439 and 0.577417. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2826.93 so gap is 117.844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2709.09 - 2834.45), exposure 125.365
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.280545 bg counts (10), with cf=1.22345 and errBG= 0.0887163
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1258 +/- 5.47252
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2834.45), exposure 173.004, 26 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.182134, 0.0970288 and 0.532732. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2709.09 and stop= 2834.45 so gap is 125.365, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2709.09 - 2834.45), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2648.91 - 2709.09), exposure 60.1754
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.196382 bg counts (7), with cf=1.21884 and errBG= 0.0742253
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.3562 +/- 5.58614
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 41
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2841.98), exposure 180.526, 26 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.174546, 0.0997427 and 0.571442. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2834.45 and stop= 2841.98 so gap is 7.52192, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2844.48), exposure 183.034, 27 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.178819, 0.0983763 and 0.550146. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2834.45 and stop= 2844.48 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2849.5), exposure 188.048, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.17405, 0.102232 and 0.587369. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2834.45 and stop= 2849.5 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2854.51), exposure 193.063, 29 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.18215, 0.0995763 and 0.546672. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2834.45 and stop= 2854.51 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2834.45 - 2864.54), exposure 30.0866
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0 bg counts (0), with cf=1.2245 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.347 +/- 2.9994
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2661.45 - 2864.54), exposure 203.091, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.179323, 0.0946595 and 0.527871. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=2834.45 and stop= 2864.54 so gap is 30.0866, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (2864.54) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=30.0866 whereas forward=3295.57
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2709.09 - 2864.54), exposure 155.452
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.280545 bg counts (10), with cf=1.22369 and errBG= 0.0887163
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.4728 +/- 6.24059
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (2864.54) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (2300.4 - 2864.54), exposure 564.131, 63 soft counts and 35 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.177408, 0.0962032 and 0.54227. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (2709.09 - 2864.54), with lastBin= 0 and workMinC was 15
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 6160.11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (2300.4 - 2864.54) = 2300.4- 2864.54
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 6160.11 - 8642.34


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6160.11 - 6393.29), exposure 233.181
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0886769 bg counts (7), with cf=1.97906 and errBG= 0.0335167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =39.4056 +/- 8.85086
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6160.11 and stop= 6393.29 so gap is 233.181, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6160.11 - 6393.29), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (2709.09 - 2864.54), exposure 155.452
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.280545 bg counts (10), with cf=1.22369 and errBG= 0.0887163
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.4728 +/- 6.24059
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 42
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6533.7), exposure 373.591, 19 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0999466, 0.041868 and 0.418904. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6533.7 so gap is 140.41, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6561.28), exposure 401.171, 20 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0974853, 0.0389272 and 0.399313. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6561.28 so gap is 167.991, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6563.79), exposure 403.678, 20 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0968798, 0.043672 and 0.450785. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6563.79 so gap is 170.498, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6573.82), exposure 413.708, 20 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0945312, 0.0475072 and 0.502556. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6573.82 so gap is 180.527, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6581.34), exposure 421.23, 21 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0976499, 0.0466588 and 0.477818. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6581.34 so gap is 188.049, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6623.96), exposure 463.854, 22 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0928363, 0.0464774 and 0.500639. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6623.96 so gap is 230.673, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6674.11), exposure 514.001, 23 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0875721, 0.0418943 and 0.478397. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6674.11 so gap is 280.82, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6393.29 - 6694.17), exposure 300.878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.177354 bg counts (14), with cf=1.95921 and errBG= 0.0473998
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.0407 +/- 7.58855
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6694.17), exposure 534.059, 24 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0878381, 0.0403208 and 0.459035. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6393.29 and stop= 6694.17 so gap is 300.878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6393.29 - 6694.17), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6160.11 - 6393.29), exposure 233.181
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0886769 bg counts (7), with cf=1.97906 and errBG= 0.0335167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =39.4056 +/- 8.85086
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 43
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6706.7), exposure 546.596, 25 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0892859, 0.039396 and 0.441234. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6706.7 so gap is 12.5365, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6716.73), exposure 556.625, 26 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0911316, 0.0386861 and 0.424508. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6716.73 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6724.26), exposure 564.147, 27 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0932821, 0.0381258 and 0.408716. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6724.26 so gap is 30.0878, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6734.28), exposure 574.176, 27 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0916527, 0.0408747 and 0.445974. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6734.28 so gap is 40.1171, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6741.81), exposure 581.698, 28 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0938385, 0.04376 and 0.466333. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6741.81 so gap is 47.639, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6744.31), exposure 584.206, 29 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0968292, 0.0435722 and 0.44999. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6744.31 so gap is 50.1464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6794.46), exposure 634.352, 29 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0890181, 0.0432006 and 0.485302. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6794.46 so gap is 100.293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6809.5), exposure 649.396, 29 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0869559, 0.0451972 and 0.519771. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6809.5 so gap is 115.337, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6812.01), exposure 651.903, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0896068, 0.0480091 and 0.535775. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6812.01 so gap is 117.844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6822.04), exposure 661.932, 30 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0882491, 0.050186 and 0.568686. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6822.04 so gap is 127.873, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6837.08), exposure 676.976, 30 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0862513, 0.0517733 and 0.60026. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6837.08 so gap is 142.917, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6839.59), exposure 679.484, 31 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0886986, 0.0515822 and 0.581545. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6839.59 so gap is 145.424, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6844.61), exposure 684.498, 32 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0908276, 0.0512043 and 0.563753. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6844.61 so gap is 150.439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6852.13), exposure 692.02, 32 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0898403, 0.0533967 and 0.594351. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6852.13 so gap is 157.961, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6877.2), exposure 717.093, 33 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0892763, 0.0515297 and 0.577193. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6877.2 so gap is 183.034, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6917.32), exposure 757.211, 34 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0870775, 0.0487997 and 0.560416. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6917.32 so gap is 223.151, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6694.17 - 6924.84), exposure 230.673
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.215358 bg counts (17), with cf=1.93744 and errBG= 0.052232
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =38.3316 +/- 8.6651
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6924.84), exposure 764.732, 36 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0913369, 0.0482871 and 0.528671. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6694.17 and stop= 6924.84 so gap is 230.673, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6694.17 - 6924.84), with lastBin= 0x2077c90 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6393.29 - 6694.17), exposure 300.878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.177354 bg counts (14), with cf=1.95921 and errBG= 0.0473998
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.0407 +/- 7.58855
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 44
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6160.11 - 6942.39), exposure 782.284, 36 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.089256, 0.0497232 and 0.557085. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6924.84 and stop= 6942.39 so gap is 17.5513, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (6160.11 - 6942.39) = 6160.11- 6942.39
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6924.84 - 7278.37), exposure 353.532
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 18 counts and 0.215358 bg counts (17), with cf=1.91827 and errBG= 0.052232
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.1157 +/- 8.13913
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6924.84 and stop= 7278.37 so gap is 353.532, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6924.84 - 7278.37), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6694.17 - 6924.84), exposure 230.673
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.215358 bg counts (17), with cf=1.93744 and errBG= 0.052232
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =38.3316 +/- 8.6651
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 45
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7478.96), exposure 536.566, 15 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0532251, 0.0417104 and 0.783661. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7278.37 and stop= 7478.96 so gap is 200.585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7499.02), exposure 556.624, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0546735, 0.0402074 and 0.735408. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7278.37 and stop= 7499.02 so gap is 220.644, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7511.55), exposure 569.161, 16 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0534266, 0.0427052 and 0.799326. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7278.37 and stop= 7511.55 so gap is 233.18, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7278.37 - 7584.27), exposure 305.892
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.177354 bg counts (14), with cf=1.90212 and errBG= 0.0473998
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.0965 +/- 7.609
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7584.27), exposure 641.873, 19 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0562921, 0.040717 and 0.723318. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7278.37 and stop= 7584.27 so gap is 305.892, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7278.37 - 7584.27), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6924.84 - 7278.37), exposure 353.532
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 18 counts and 0.215358 bg counts (17), with cf=1.91827 and errBG= 0.052232
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.1157 +/- 8.13913
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 46
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7599.31), exposure 656.917, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0580997, 0.0397846 and 0.684765. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7599.31 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7629.4), exposure 687.004, 21 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0583644, 0.0380422 and 0.651805. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7629.4 so gap is 45.1316, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7644.44), exposure 702.048, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0597394, 0.0371928 and 0.622584. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7644.44 so gap is 60.1755, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7659.48), exposure 717.092, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0584861, 0.038994 and 0.666722. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7659.48 so gap is 75.2194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7667.01), exposure 724.614, 22 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.057879, 0.0412091 and 0.711987. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7667.01 so gap is 82.7413, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6942.39 - 7717.15), exposure 774.76, 23 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.056573, 0.0384798 and 0.68018. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7717.15 so gap is 132.888, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (6942.39 - 7717.15) = 6942.39- 7717.15
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7584.27 - 7925.26), exposure 340.994
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.253362 bg counts (20), with cf=1.90764 and errBG= 0.0566536
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =37.6695 +/- 8.53191
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7584.27 and stop= 7925.26 so gap is 340.994, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7584.27 - 7925.26), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7278.37 - 7584.27), exposure 305.892
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.177354 bg counts (14), with cf=1.90212 and errBG= 0.0473998
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =30.0965 +/- 7.609
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 47
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7925.26 - 8258.73), exposure 333.472
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.329371 bg counts (26), with cf=1.87771 and errBG= 0.064595
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.5472 +/- 7.27335
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7717.15 - 8258.73), exposure 541.579, 17 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0581657, 0.0412464 and 0.709119. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=7925.26 and stop= 8258.73 so gap is 333.472, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (7925.26 - 8258.73), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7584.27 - 7925.26), exposure 340.994
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.253362 bg counts (20), with cf=1.90764 and errBG= 0.0566536
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =37.6695 +/- 8.53191
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 48
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7717.15 - 8384.1), exposure 666.945, 20 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0558639, 0.0564964 and 1.01132. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=8258.73 and stop= 8384.1 so gap is 125.365, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (7717.15 - 8384.1) = 7717.15- 8384.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8258.73 - 8549.58), exposure 290.848
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.291367 bg counts (23), with cf=1.9344 and errBG= 0.0607542
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =38.1243 +/- 8.65168
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=8258.73 and stop= 8549.58 so gap is 290.848, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (8258.73 - 8549.58), with lastBin= 0x207c900 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (7925.26 - 8258.73), exposure 333.472
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.329371 bg counts (26), with cf=1.87771 and errBG= 0.064595
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.5472 +/- 7.27335
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 49
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8549.58 - 8642.34), exposure 92.7557
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.0380044 bg counts (3), with cf=1.91387 and errBG= 0.0219418
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =13.3243 +/- 5.06379
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (8384.1 - 8642.34), exposure 258.238, 11 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0803523, 0.0371707 and 0.462596. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=8549.58 and stop= 8642.34 so gap is 92.7557, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 1 (8642.34) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=92.7557 whereas forward=3288.43
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8258.73 - 8642.34), exposure 383.604
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.329371 bg counts (26), with cf=1.92907 and errBG= 0.064595
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.4496 +/- 10.0245
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 1 (8642.34) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (7717.15 - 8642.34), exposure 925.183, 31 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0626986, 0.0511033 and 0.815063. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (8258.73 - 8642.34), with lastBin= 0 and workMinC was 14
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 11930.8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (7717.15 - 8642.34) = 7717.15- 8642.34
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 11930.8 - 12136.4


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11930.8 - 12136.4), exposure 205.599
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.135279 bg counts (18), with cf=1.31582 and errBG= 0.0318855
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.9276 +/- 4.74444
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12136.4), exposure 205.599, 7 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0445398, 0.037794 and 0.848544. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=11930.8 and stop= 12136.4 so gap is 205.599, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 2 (12136.4) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=3494.03 whereas forward=187.909
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 2 (12136.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 12324.3 - 12397


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11930.8 - 12356.9), exposure 238.194
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.142794 bg counts (19), with cf=1.3161 and errBG= 0.0327592
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5536 +/- 5.09742
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=11930.8 and stop= 12356.9 so gap is 426.103, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (11930.8 - 12356.9), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (8258.73 - 8642.34), exposure 383.604
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 27 counts and 0.329371 bg counts (26), with cf=1.92907 and errBG= 0.064595
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =51.4496 +/- 10.0245
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 50
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12356.9 - 12397), exposure 40.1166
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.0375774 bg counts (5), with cf=1.29599 and errBG= 0.0168051
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.54327 +/- 1.83293
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12397), exposure 278.31, 9 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0421453, 0.0372502 and 0.883853. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12356.9 and stop= 12397 so gap is 40.1166, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 3 (12397) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=40.1166 whereas forward=74.3775
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11930.8 - 12397), exposure 278.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.180371 bg counts (24), with cf=1.31374 and errBG= 0.0368181
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.0965 +/- 5.41689
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 3 (12397) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (11930.8 - 12397), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 12471.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 12471.4 - 14419.5


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12737.1), exposure 544.086, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0384017, 0.028585 and 0.744368. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12471.4 and stop= 12737.1 so gap is 265.776, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12747.2), exposure 554.115, 17 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0401232, 0.0280676 and 0.699536. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12471.4 and stop= 12747.2 so gap is 275.805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12762.2), exposure 569.159, 18 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0413399, 0.0273257 and 0.661001. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12471.4 and stop= 12762.2 so gap is 290.849, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12787.3), exposure 594.232, 18 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0395956, 0.0283536 and 0.716079. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12471.4 and stop= 12787.3 so gap is 315.922, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12471.4 - 12804.8), exposure 333.473
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0901857 bg counts (12), with cf=1.31596 and errBG= 0.0260344
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6207 +/- 5.09681
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12804.8), exposure 611.784, 19 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0406496, 0.0275402 and 0.677502. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12471.4 and stop= 12804.8 so gap is 333.473, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12471.4 - 12804.8), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11930.8 - 12397), exposure 278.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.180371 bg counts (24), with cf=1.31374 and errBG= 0.0368181
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.0965 +/- 5.41689
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 51
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12832.4), exposure 639.364, 19 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0388651, 0.0284471 and 0.731946. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12804.8 and stop= 12832.4 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (11930.8 - 12837.4), exposure 644.379, 19 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0385626, 0.0302218 and 0.783707. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12804.8 and stop= 12837.4 so gap is 32.5951, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (11930.8 - 12837.4) = 11930.8- 12837.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12804.8 - 13338.9), exposure 534.058
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.195402 bg counts (26), with cf=1.31896 and errBG= 0.0383215
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5267 +/- 5.10858
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=12804.8 and stop= 13338.9 so gap is 534.058, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (12804.8 - 13338.9), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12471.4 - 12804.8), exposure 333.473
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0901857 bg counts (12), with cf=1.31596 and errBG= 0.0260344
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.6207 +/- 5.09681
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 52
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13338.9 - 13647.3), exposure 308.399
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0901857 bg counts (12), with cf=1.31304 and errBG= 0.0260344
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5771 +/- 5.08549
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13338.9 and stop= 13647.3 so gap is 308.399, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13338.9 - 13647.3), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (12804.8 - 13338.9), exposure 534.058
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.195402 bg counts (26), with cf=1.31896 and errBG= 0.0383215
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5267 +/- 5.10858
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 53
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (12837.4 - 13732.5), exposure 895.111, 19 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0276249, 0.0219014 and 0.792816. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13647.3 and stop= 13732.5 so gap is 85.2486, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (12837.4 - 13732.5) = 12837.4- 13732.5
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13647.3 - 13933.1), exposure 285.834
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.135279 bg counts (18), with cf=1.3185 and errBG= 0.0318855
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5991 +/- 5.1067
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13647.3 and stop= 13933.1 so gap is 285.834, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13647.3 - 13933.1), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13338.9 - 13647.3), exposure 308.399
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0901857 bg counts (12), with cf=1.31304 and errBG= 0.0260344
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5771 +/- 5.08549
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 54
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13933.1 - 14419.5), exposure 486.407
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.255526 bg counts (34), with cf=1.2997 and errBG= 0.0438224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.6648 +/- 4.11039
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (13732.5 - 14419.5), exposure 686.992, 14 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0264751, 0.00908699 and 0.343228. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=13933.1 and stop= 14419.5 so gap is 486.407, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 4 (14419.5) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=486.407 whereas forward=3311.16
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13647.3 - 14419.5), exposure 772.241
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.390805 bg counts (52), with cf=1.31098 and errBG= 0.0541948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.2621 +/- 6.55527
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 4 (14419.5) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (12837.4 - 14419.5), exposure 1582.1, 33 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0271256, 0.0163355 and 0.602219. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (13647.3 - 14419.5), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 17730.7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (12837.4 - 14419.5) = 12837.4- 14419.5
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 17730.7 - 18342.5


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17730.7 - 18079.2), exposure 348.517
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.15507 bg counts (20), with cf=2.18585 and errBG= 0.0346748
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.4489 +/- 8.46612
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17730.7 and stop= 18079.2 so gap is 348.517, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17730.7 - 18079.2), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (13647.3 - 14419.5), exposure 772.241
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 0.390805 bg counts (52), with cf=1.31098 and errBG= 0.0541948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.2621 +/- 6.55527
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 55
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18079.2 - 18342.5), exposure 263.264
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.0697817 bg counts (9), with cf=2.21021 and errBG= 0.0232606
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.8968 +/- 4.94244
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 18342.5), exposure 611.781, 14 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0503897, 0.0204628 and 0.406092. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18079.2 and stop= 18342.5 so gap is 263.264, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 5 (18342.5) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=263.264 whereas forward=689.536
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17730.7 - 18342.5), exposure 611.781
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.224852 bg counts (29), with cf=2.19194 and errBG= 0.041754
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.346 +/- 9.8031
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 5 (18342.5) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17730.7 - 18342.5), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 19032
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 7
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 19032 - 20197.9


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19167.4), exposure 747.176, 15 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0442255, 0.0259113 and 0.58589. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19167.4 so gap is 135.395, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19190), exposure 769.742, 16 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0459566, 0.0251299 and 0.546818. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19190 so gap is 157.961, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19495.9), exposure 1075.63, 16 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0327593, 0.0201186 and 0.614133. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19495.9 so gap is 463.853, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19536), exposure 1115.75, 16 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0315352, 0.0213503 and 0.677032. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19536 so gap is 503.969, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19571.1), exposure 1150.85, 17 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0325401, 0.0206698 and 0.635209. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19571.1 so gap is 539.072, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19583.6), exposure 1163.39, 18 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0340607, 0.020447 and 0.600311. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19583.6 so gap is 551.608, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19869.5), exposure 1449.22, 19 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0287156, 0.0163676 and 0.56999. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19869.5 so gap is 837.442, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 19949.7), exposure 1529.46, 19 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0271979, 0.0170625 and 0.627345. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 19949.7 so gap is 917.675, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 20014.9), exposure 1594.65, 19 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.026032, 0.0177469 and 0.681735. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 20014.9 so gap is 982.865, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 20077.6), exposure 1657.33, 19 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0250058, 0.0184234 and 0.736764. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 20077.6 so gap is 1045.55, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 20115.2), exposure 1694.94, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0257766, 0.0179844 and 0.697703. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 20115.2 so gap is 1083.16, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (19032 - 20157.8), exposure 1125.78
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.500895 bg counts (65), with cf=2.28607 and errBG= 0.0621284
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.146 +/- 8.85507
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 20157.8), exposure 1737.56, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0251343, 0.0188981 and 0.751884. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=19032 and stop= 20157.8 so gap is 1125.78, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (19032 - 20157.8), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17730.7 - 18342.5), exposure 611.781
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.224852 bg counts (29), with cf=2.19194 and errBG= 0.041754
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.346 +/- 9.8031
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 56
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 7
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17730.7 - 20157.8) = 17730.7- 20157.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (20157.8 - 20197.9), exposure 40.1125
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.00770608 bg counts (1), with cf=2.39126 and errBG= 0.00770608
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.37283 +/- 2.39133
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (20157.8 - 20197.9), exposure 40.1125, 0 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0, 0.0591543 and inf. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=20157.8 and stop= 20197.9 so gap is 40.1125, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 6 (20197.9) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=40.1125 whereas forward=3289.6
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (19032 - 20197.9), exposure 1165.89
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.508601 bg counts (66), with cf=2.29265 and errBG= 0.0626045
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =35.5163 +/- 9.17172
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 6 (20197.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17730.7 - 20197.9), exposure 1777.68, 20 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0245672, 0.0198057 and 0.806185. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (19032 - 20197.9), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 23487.5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 8
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17730.7 - 20197.9) = 17730.7- 20197.9
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 23487.5 - 24212.1


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23487.5 - 24212.1), exposure 724.61
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 0.29768 bg counts (37), with cf=1.28801 and errBG= 0.0489384
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.6488 +/- 4.81971
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 24212.1), exposure 724.61, 14 soft counts and 0 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0245278, -0.000133237 and -0.00543209. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23487.5 and stop= 24212.1 so gap is 724.61, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 7 (24212.1) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=4014.21 whereas forward=1322.44
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 7 (24212.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 25534.6 - 25975.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23487.5 - 25544.6), exposure 734.639
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.29768 bg counts (37), with cf=1.29067 and errBG= 0.0489384
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9759 +/- 4.99916
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23487.5 and stop= 25544.6 so gap is 2057.08, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (23487.5 - 25544.6), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (19032 - 20197.9), exposure 1165.89
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.508601 bg counts (66), with cf=2.29265 and errBG= 0.0626045
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =35.5163 +/- 9.17172
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 57
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 9
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 25642.4), exposure 832.424, 16 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0244263, 0.00296255 and 0.121285. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25544.6 and stop= 25642.4 so gap is 97.785, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 25720.1), exposure 910.15, 17 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0237634, 0.00267513 and 0.112574. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25544.6 and stop= 25720.1 so gap is 175.512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 25730.1), exposure 920.18, 18 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.024889, 0.00264598 and 0.106311. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25544.6 and stop= 25730.1 so gap is 185.541, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 25772.8), exposure 962.804, 18 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0237764, 0.00384307 and 0.161634. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25544.6 and stop= 25772.8 so gap is 228.165, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 25802.8), exposure 992.892, 18 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0230456, 0.0050514 and 0.219192. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25544.6 and stop= 25802.8 so gap is 258.253, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 25817.9), exposure 1007.94, 18 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0227016, 0.00629357 and 0.27723. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25544.6 and stop= 25817.9 so gap is 273.297, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 25825.4), exposure 1015.46, 19 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0238414, 0.00624695 and 0.262021. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25544.6 and stop= 25825.4 so gap is 280.819, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 25860.5), exposure 1050.56, 20 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0242892, 0.00603822 and 0.248597. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25544.6 and stop= 25860.5 so gap is 315.921, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (25544.6 - 25975.8), exposure 431.256
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 11 counts and 0.175804 bg counts (22), with cf=1.30836 and errBG= 0.0374816
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.1619 +/- 4.33961
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 25975.8), exposure 1165.89, 21 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0229894, 0.00543191 and 0.23628. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=25544.6 and stop= 25975.8 so gap is 431.256, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 8 (25975.8) and the bin is not full 11 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=431.256 whereas forward=3301.32
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23487.5 - 25975.8), exposure 1165.89
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.473485 bg counts (59), with cf=1.29816 and errBG= 0.0616425
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.1374 +/- 6.61981
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 8 (25975.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (23487.5 - 25975.8), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 29277.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 10
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 29277.2 - 30169.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 29324.8), exposure 1213.53, 22 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0235383, 0.00520994 and 0.221339. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 29324.8 so gap is 47.6387, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 29372.4), exposure 1261.17, 23 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0241781, 0.00500893 and 0.207169. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 29372.4 so gap is 95.2778, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 29675.8), exposure 1564.56, 23 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0194479, 0.00535603 and 0.275404. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 29675.8 so gap is 398.663, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 29873.9), exposure 1762.64, 24 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0184337, 0.00474749 and 0.257544. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 29873.9 so gap is 596.741, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 29954.1), exposure 1842.87, 25 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0187803, 0.00453126 and 0.241277. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 29954.1 so gap is 676.975, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 30132.2), exposure 2020.89, 26 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0181026, 0.00411181 and 0.227139. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 30132.2 so gap is 854.994, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 30144.7), exposure 2033.43, 27 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0190039, 0.00408358 and 0.214881. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 30144.7 so gap is 867.531, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 31710 - 31752.7 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29277.2 - 31752.7), exposure 935.223
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.212122 bg counts (55), with cf=2.01775 and errBG= 0.0286025
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.714 +/- 5.70736
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 31752.7), exposure 2101.12, 28 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0193201, 0.00394923 and 0.204411. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 31752.7 so gap is 2475.51, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 10 (31752.7) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5776.82 whereas forward=3307.23
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 10 (31752.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 35059.9 - 36153.1


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35160.2), exposure 2201.41, 29 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.019037, 0.00376931 and 0.197999. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 35160.2 so gap is 5883.03, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35255.5), exposure 2296.69, 29 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.018238, 0.00418435 and 0.22943. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 35255.5 so gap is 5978.31, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35268), exposure 2309.22, 30 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0187217, 0.00415865 and 0.222129. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 35268 so gap is 5990.84, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35300.6), exposure 2341.82, 31 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0190349, 0.00409488 and 0.215125. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 35300.6 so gap is 6023.44, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35418.4), exposure 2459.66, 32 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0186518, 0.00389309 and 0.208725. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 35418.4 so gap is 6141.28, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35431), exposure 2472.2, 33 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0191003, 0.00387056 and 0.202645. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 35431 so gap is 6153.82, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29277.2 - 35566.4), exposure 1441.7
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.346699 bg counts (83), with cf=1.70235 and errBG= 0.0380551
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.945 +/- 6.59349
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35566.4), exposure 2607.59, 34 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0186238, 0.00365903 and 0.196471. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29277.2 and stop= 35566.4 so gap is 6289.21, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (29277.2 - 35566.4), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23487.5 - 25975.8), exposure 1165.89
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 26 counts and 0.473485 bg counts (59), with cf=1.29816 and errBG= 0.0616425
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.1374 +/- 6.61981
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 58
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 12
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35611.5), exposure 2652.73, 34 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0183016, 0.00410414 and 0.22425. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35566.4 and stop= 35611.5 so gap is 45.1317, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35634.1), exposure 2675.29, 35 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0186515, 0.00406697 and 0.21805. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35566.4 and stop= 35634.1 so gap is 67.6975, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35684.2), exposure 2725.44, 36 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0187992, 0.00398964 and 0.212224. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35566.4 and stop= 35684.2 so gap is 117.844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35792), exposure 2833.25, 37 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0185532, 0.00382576 and 0.206204. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35566.4 and stop= 35792 so gap is 225.658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35809.6), exposure 2850.8, 38 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0189121, 0.00379741 and 0.200793. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35566.4 and stop= 35809.6 so gap is 243.21, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 35970.1), exposure 3011.27, 39 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0183311, 0.00358824 and 0.195747. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35566.4 and stop= 35970.1 so gap is 403.678, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 36007.7), exposure 3048.88, 40 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0185411, 0.00354398 and 0.191142. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35566.4 and stop= 36007.7 so gap is 441.288, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (35566.4 - 36153.1), exposure 586.705
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.192253 bg counts (40), with cf=1.34469 and errBG= 0.0303979
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.499 +/- 3.80357
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 36153.1), exposure 3194.3, 40 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0176819, 0.00379453 and 0.214599. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35566.4 and stop= 36153.1 so gap is 586.705, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 11 (36153.1) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=586.705 whereas forward=4671.31
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29277.2 - 36153.1), exposure 2028.41
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.538952 bg counts (123), with cf=1.57794 and errBG= 0.0485957
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =35.4423 +/- 7.56795
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 11 (36153.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (29277.2 - 36153.1), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 40824.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 13
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 40824.4 - 42213.4


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 40922.2), exposure 3292.08, 40 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0171442, 0.00407956 and 0.237955. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 40922.2 so gap is 97.7847, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 40944.7), exposure 3314.65, 40 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0170213, 0.00444971 and 0.26142. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 40944.7 so gap is 120.351, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41022.5), exposure 3392.38, 40 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0166222, 0.00473799 and 0.28504. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41022.5 so gap is 198.078, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41142.8), exposure 3512.73, 41 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0164217, 0.0045586 and 0.277596. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41142.8 so gap is 318.429, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41175.4), exposure 3545.32, 42 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0166422, 0.00451669 and 0.271399. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41175.4 so gap is 351.024, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41348.4), exposure 3718.33, 42 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0158486, 0.00466575 and 0.294396. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41348.4 so gap is 524.029, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41358.4), exposure 3728.36, 42 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0158059, 0.00500664 and 0.316757. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41358.4 so gap is 534.059, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41423.6), exposure 3793.55, 43 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.015881, 0.00491799 and 0.309678. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41423.6 so gap is 599.249, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41438.7), exposure 3808.59, 44 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0161632, 0.00489073 and 0.302585. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41438.7 so gap is 614.293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 41506.4), exposure 3876.29, 44 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.015873, 0.00514218 and 0.323958. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 41506.4 so gap is 681.99, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (23487.5 - 41506.4) = 23487.5- 41506.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40824.4 - 42213.4), exposure 1389.04
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.503123 bg counts (70), with cf=1.33393 and errBG= 0.0601347
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.3378 +/- 5.1669
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (41506.4 - 42213.4), exposure 707.054, 4 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00745653, 0.0017001 and 0.228002. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=40824.4 and stop= 42213.4 so gap is 1389.04, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 12 (42213.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (23487.5 - 42213.4), exposure 4583.34, 48 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0145741, 0.00461102 and 0.316384. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (40824.4 - 42213.4), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29277.2 - 36153.1), exposure 2028.41
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.538952 bg counts (123), with cf=1.57794 and errBG= 0.0485957
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =35.4423 +/- 7.56795
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 59
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 46600.8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 14
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (23487.5 - 42213.4) = 23487.5- 42213.4
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 46600.8 - 48378.4


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46600.8 - 48378.4), exposure 1777.68
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.467038 bg counts (97), with cf=1.35705 and errBG= 0.0474206
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =15.6508 +/- 4.7014
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 48378.4), exposure 1777.68, 8 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00593648, 0.00286802 and 0.483118. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 48378.4 so gap is 1777.68, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 13 (48378.4) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=6165.01 whereas forward=3997.94
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 13 (48378.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 52376.4 - 54550.2


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46600.8 - 52506.8), exposure 1908.06
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.516727 bg counts (104), with cf=1.34933 and errBG= 0.0506693
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5427 +/- 5.22636
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=46600.8 and stop= 52506.8 so gap is 5906, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (46600.8 - 52506.8), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (40824.4 - 42213.4), exposure 1389.04
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.503123 bg counts (70), with cf=1.33393 and errBG= 0.0601347
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.3378 +/- 5.1669
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 60
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 15
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 53083.4), exposure 2484.74, 16 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0083537, 0.00359824 and 0.430736. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 53083.4 so gap is 576.683, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 53203.8), exposure 2605.09, 17 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00846317, 0.0034138 and 0.403372. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 53203.8 so gap is 697.035, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 53213.8), exposure 2615.12, 18 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00892759, 0.00340071 and 0.380922. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 53213.8 so gap is 707.064, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 53231.4), exposure 2632.67, 18 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00886807, 0.00387857 and 0.437363. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 53231.4 so gap is 724.615, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 53344.2), exposure 2745.5, 19 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00898099, 0.00371573 and 0.413732. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 53344.2 so gap is 837.444, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 53421.9), exposure 2823.23, 20 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00919442, 0.00360337 and 0.391908. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 53421.9 so gap is 915.171, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 53715.3), exposure 3116.58, 21 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00873118, 0.00324294 and 0.37142. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 53715.3 so gap is 1208.53, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52506.8 - 54016.2), exposure 1509.4
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.61756 bg counts (87), with cf=1.31853 and errBG= 0.0662094
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9637 +/- 5.1074
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 54016.2), exposure 3417.46, 22 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00832908, 0.00293804 and 0.352744. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52506.8 and stop= 54016.2 so gap is 1509.4, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (52506.8 - 54016.2), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (46600.8 - 52506.8), exposure 1908.06
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.516727 bg counts (104), with cf=1.34933 and errBG= 0.0506693
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5427 +/- 5.22636
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 61
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 15
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 54098.9), exposure 3500.2, 22 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00812408, 0.00323222 and 0.397857. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=54016.2 and stop= 54098.9 so gap is 82.7413, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 54229.3), exposure 3630.58, 23 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00817202, 0.00311354 and 0.381. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=54016.2 and stop= 54229.3 so gap is 213.121, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 54274.4), exposure 3675.71, 24 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00842808, 0.00307017 and 0.364279. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=54016.2 and stop= 54274.4 so gap is 258.253, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 54427.4), exposure 3828.66, 25 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0084285, 0.00292777 and 0.347365. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=54016.2 and stop= 54427.4 so gap is 411.199, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (54016.2 - 54550.2), exposure 534.044
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.298132 bg counts (42), with cf=1.31851 and errBG= 0.0460028
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.19944 +/- 2.94889
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 54550.2), exposure 3951.5, 25 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00816168, 0.00315128 and 0.386107. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=54016.2 and stop= 54550.2 so gap is 534.044, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 14 (54550.2) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=534.044 whereas forward=3810.44
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52506.8 - 54550.2), exposure 2043.45
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.915692 bg counts (129), with cf=1.31853 and errBG= 0.0806222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.1632 +/- 5.89759
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 14 (54550.2) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (52506.8 - 54550.2), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 58360.7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 16
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 58360.7 - 60639.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 59343.5), exposure 4934.37, 25 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00651402, 0.00280255 and 0.430234. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 59343.5 so gap is 982.862, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 59393.7), exposure 4984.51, 26 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00674351, 0.00277351 and 0.411286. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 59393.7 so gap is 1033.01, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 60238.6), exposure 5829.48, 26 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00574955, 0.0026097 and 0.453897. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 60238.6 so gap is 1877.97, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 60341.4), exposure 5932.28, 26 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00564921, 0.00281023 and 0.497455. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 60341.4 so gap is 1980.77, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (58360.7 - 60639.8), exposure 2279.14
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.353545 bg counts (113), with cf=1.47744 and errBG= 0.0332587
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.86488 +/- 3.30403
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 60639.8), exposure 6230.64, 27 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00560722, 0.00267154 and 0.476447. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 60639.8 so gap is 2279.14, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 15 (60639.8) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=6089.58 whereas forward=3304.06
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 15 (60639.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 63943.9 - 66418.6


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 64184.6), exposure 6471.34, 28 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00561537, 0.00256879 and 0.457457. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 64184.6 so gap is 5823.9, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 64347.5), exposure 6634.32, 29 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00568977, 0.00250107 and 0.439573. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 64347.5 so gap is 5986.87, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 64455.3), exposure 6742.13, 30 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00581138, 0.00245912 and 0.423156. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 64455.3 so gap is 6094.69, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 65500.9), exposure 7787.68, 30 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00501221, 0.00229997 and 0.458873. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 65500.9 so gap is 7140.24, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 65651.3), exposure 7938.12, 31 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00509773, 0.00225417 and 0.442191. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 65651.3 so gap is 7290.67, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 65957.2), exposure 8244.01, 32 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00507633, 0.00216733 and 0.426948. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 65957.2 so gap is 7596.57, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 65994.8), exposure 8281.62, 33 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00522595, 0.00215749 and 0.412841. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 65994.8 so gap is 7634.18, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 66225.5), exposure 8512.29, 34 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00525009, 0.00209386 and 0.398822. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 66225.5 so gap is 7864.85, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 66248.1), exposure 8534.86, 35 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00540385, 0.00208832 and 0.38645. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 66248.1 so gap is 7887.41, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (58360.7 - 66381), exposure 4716.24
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.786925 bg counts (248), with cf=1.45093 and errBG= 0.0499698
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =20.6222 +/- 5.61989
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 66381), exposure 8667.75, 36 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00548433, 0.00205377 and 0.374479. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58360.7 and stop= 66381 so gap is 8020.3, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (58360.7 - 66381), with lastBin= 0x2077c90 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52506.8 - 54550.2), exposure 2043.45
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.915692 bg counts (129), with cf=1.31853 and errBG= 0.0806222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.1632 +/- 5.89759
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 62
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 17
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (66381 - 66418.6), exposure 37.6006
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0160511 bg counts (5), with cf=1.43252 and errBG= 0.00717827
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.40953 +/- 1.43256
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 66418.6), exposure 8705.35, 36 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00545812, 0.00220897 and 0.404712. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=66381 and stop= 66418.6 so gap is 37.6006, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 16 (66418.6) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=37.6006 whereas forward=39844.9
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (58360.7 - 66418.6), exposure 4753.84
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.802976 bg counts (253), with cf=1.44978 and errBG= 0.0504827
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.0323 +/- 5.79958
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 16 (66418.6) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (58360.7 - 66418.6), with lastBin= 0 and workMinC was 7
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 106263
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x2077c90 which has initial GTIBin: 18
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 106263 - 106858


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 106266), exposure 8707.85, 37 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00565373, 0.00220833 and 0.390598. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 106266 so gap is 2.5073, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 106858), exposure 594.23
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.0612377 bg counts (27), with cf=1.73413 and errBG= 0.0117852
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =3.36206 +/- 2.45251
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (46600.8 - 106858), exposure 9299.58, 37 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00528828, 0.00224897 and 0.425275. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 106858 so gap is 594.23, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 17 (106858) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=40439.1 whereas forward=3272.15
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (46600.8 - 106858) = 46600.8- 106858
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 110130 - 110762


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 112410 - 112636 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 112636), exposure 1451.73
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 3 counts and 0.166374 bg counts (69), with cf=1.6394 and errBG= 0.020029
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =4.64546 +/- 2.83972
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 112636), exposure 857.497, 0 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -6.84653e-05, 0.00161241 and -23.5507. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 112636 so gap is 6372.46, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 19 (112636) and the bin is not full 3 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=46217.4 whereas forward=3271.72
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 19 (112636) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 115908 - 116702


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 116702), exposure 2246.54
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.303886 bg counts (112), with cf=1.60443 and errBG= 0.0287146
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =5.93015 +/- 3.20919
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 116702), exposure 1652.31, 1 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00078749, 0.000780663 and 0.99133. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 116702 so gap is 10439, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 20 (116702) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=50283.9 whereas forward=5024.16
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 20 (116702) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 121727 - 122702


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 122702), exposure 3219.37
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.330003 bg counts (159), with cf=1.60443 and errBG= 0.0261709
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =5.88825 +/- 3.20913
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 122702), exposure 2625.14, 1 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000487408, 0.000484918 and 0.994892. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 122702 so gap is 16438.5, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 21 (122702) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=56283.4 whereas forward=4767.51
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 21 (122702) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 127469 - 128821


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 133243 - 135001 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 135001), exposure 6328.43
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.54345 bg counts (316), with cf=1.6192 and errBG= 0.0305715
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.21606 +/- 3.62099
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 135001), exposure 5734.2, 2 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000484203, 0.000194791 and 0.402292. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 135001 so gap is 28737.4, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 23 (135001) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=68582.3 whereas forward=5378.96
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 23 (135001) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 140380 - 141182


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 141182), exposure 7130.76
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.561413 bg counts (352), with cf=1.6192 and errBG= 0.0299234
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.18697 +/- 3.62097
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 141182), exposure 6536.53, 2 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000422343, 0.00016911 and 0.400409. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 141182 so gap is 34918.7, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 24 (141182) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=74763.6 whereas forward=3612.63
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 24 (141182) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 144795 - 144903


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 144903), exposure 7238.58
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.566857 bg counts (357), with cf=1.6192 and errBG= 0.0300012
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.17816 +/- 3.62097
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 144903), exposure 6644.35, 2 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000414708, 0.000165891 and 0.400018. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 144903 so gap is 38639.1, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 25 (144903) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=78484.1 whereas forward=1237.66
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 25 (144903) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 146140 - 147299


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 147299), exposure 8396.95
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.745943 bg counts (413), with cf=1.55789 and errBG= 0.0367055
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.301 +/- 4.40674
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 147299), exposure 7802.72, 4 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00070723, 0.000314546 and 0.444757. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 147299 so gap is 41035.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 26 (147299) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=80880.1 whereas forward=3292.98
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 26 (147299) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 150592 - 151023


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 151023), exposure 8828.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 0.864268 bg counts (450), with cf=1.54493 and errBG= 0.040742
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.5691 +/- 4.63521
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 151023), exposure 8233.97, 5 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000833615, 0.000288925 and 0.346593. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 151023 so gap is 44759.4, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 27 (151023) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=84604.3 whereas forward=1294.11
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 27 (151023) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 152317 - 153077


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 153077), exposure 9587.92
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.964063 bg counts (482), with cf=1.55987 and errBG= 0.0439118
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.0949 +/- 4.93322
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 153077), exposure 8993.69, 5 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000753326, 0.000442782 and 0.587769. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 153077 so gap is 46813.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 28 (153077) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=86658.1 whereas forward=3322.45
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 28 (153077) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 156399 - 158683


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 158683), exposure 11872.1
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 1.17613 bg counts (669), with cf=2.11233 and errBG= 0.0454717
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.8635 +/- 7.31794
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 158683), exposure 11277.8, 6 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000968328, 0.000753776 and 0.77843. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 158683 so gap is 52419.8, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 29 (158683) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=92264.7 whereas forward=28232.1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 29 (158683) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 186915 - 187623


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 192784 - 193383 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 193383), exposure 13178.4
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 1.25975 bg counts (747), with cf=2.11233 and errBG= 0.046092
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.6869 +/- 7.31796
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 193383), exposure 12584.1, 6 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000860365, 0.00066831 and 0.776775. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 193383 so gap is 87119.4, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 31 (193383) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=126964 whereas forward=28231.9
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 31 (193383) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 221615 - 221702


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 221702), exposure 13266.1
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 1.26402 bg counts (751), with cf=2.11233 and errBG= 0.0461247
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.6779 +/- 7.31796
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 221702), exposure 12671.9, 6 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000854235, 0.000663069 and 0.776214. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 221702 so gap is 115439, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 32 (221702) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=155284 whereas forward=17192.8
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 32 (221702) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 238895 - 239642


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 239642), exposure 14013.3
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 1.30817 bg counts (792), with cf=2.11233 and errBG= 0.046484
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.5846 +/- 7.31797
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 239642), exposure 13419.1, 6 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000802598, 0.000623037 and 0.776275. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 239642 so gap is 133379, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 33 (239642) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=173224 whereas forward=5484.61
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 33 (239642) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 245127 - 245403


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 250475 - 251162 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 251162), exposure 14976.1
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 1.36445 bg counts (844), with cf=2.11233 and errBG= 0.0469663
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.4657 +/- 7.31798
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 251162), exposure 14381.9, 6 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000745049, 0.0005764 and 0.773641. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 251162 so gap is 144899, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 35 (251162) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=184744 whereas forward=5072.65
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 35 (251162) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 256235 - 256985


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 256985), exposure 15725.8
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 1.48685 bg counts (882), with cf=2.06624 and errBG= 0.0500648
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.7889 +/- 7.45064
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 256985), exposure 15131.6, 7 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00080292, 0.00053907 and 0.671387. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 256985 so gap is 150721, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 36 (256985) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=190566 whereas forward=11085.5
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 36 (256985) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 268070 - 268502


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 273216 - 274324 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 279536 - 280082 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 280082), exposure 17811.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 1.60116 bg counts (991), with cf=2.06624 and errBG= 0.0508624
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.5527 +/- 7.45067
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 280082), exposure 17217.6, 7 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000699543, 0.000465216 and 0.665029. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 280082 so gap is 173819, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 39 (280082) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=213664 whereas forward=9576
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 39 (280082) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 289658 - 290042


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 295322 - 296102 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 296102), exposure 18975.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 1.91535 bg counts (1116), with cf=2.06624 and errBG= 0.0573345
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.9035 +/- 7.45087
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 296102), exposure 18381, 7 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000628134, 0.000427951 and 0.681306. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 296102 so gap is 189839, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 41 (296102) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=229684 whereas forward=11912.6
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 41 (296102) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 308015 - 308461


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 308461), exposure 19421.5
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 1.97748 bg counts (1136), with cf=2.02551 and errBG= 0.0586708
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.3517 +/- 7.57968
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 308461), exposure 18827.3, 8 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000692929, 0.000413807 and 0.597185. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 308461 so gap is 202198, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 42 (308461) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=242042 whereas forward=5901.66
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 42 (308461) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 314363 - 314641


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 314641), exposure 19699.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 2.07271 bg counts (1156), with cf=1.98744 and errBG= 0.060962
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.6922 +/- 7.69826
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 314641), exposure 19105.6, 9 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000757736, 0.000401133 and 0.529384. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=106263 and stop= 314641 so gap is 208377, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 43 (314641) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (106263 - 314641), with lastBin= 0x207c900 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (58360.7 - 66418.6), exposure 4753.84
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.802976 bg counts (253), with cf=1.44978 and errBG= 0.0504827
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.0323 +/- 5.79958
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 63
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 319829
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 46
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 319829 - 320523


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 319829 - 320523
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 319829 - 320523 the cf is 2.02616
++tructures/grbBin.cpp::        binData:  line  405  INFO   >>  This bin is empty, so found a emptyBin CF of 2.02616
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (319829 - 320523), exposure 694.522
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 0 counts and 0.0453371 bg counts (43), with cf=2.02616 and errBG= 0.00691384
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =-0.0918602 +/- 0.0140086
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 320523), exposure 19800.1, 9 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000728399, 0.000385126 and 0.528729. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=319829 and stop= 320523 so gap is 694.522, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 44 (320523) and the bin is not full 0 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5882.47 whereas forward=4832.68
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 44 (320523) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 325356 - 326284


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 330097 - 330541 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 337583 - 337861 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 347231 - 347761 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 359998 - 360961 to this bin
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 319829 - 360961
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 319829 - 360961 the cf is 3.20381
++tructures/grbBin.cpp::        binData:  line  405  INFO   >>  This bin is empty, so found a emptyBin CF of 3.20381
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (319829 - 360961), exposure 3836.17
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 0 counts and 0.246809 bg counts (208), with cf=3.20381 and errBG= 0.0171131
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =-0.790727 +/- 0.0548271
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 360961), exposure 22941.8, 9 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000621082, 0.000321019 and 0.516871. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=319829 and stop= 360961 so gap is 41132, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 49 (360961) and the bin is not full 0 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=0 and gapBack=46320 whereas forward=51740.9
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 360961), exposure 23536
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 2.31952 bg counts (1364), with cf=1.98744 and errBG= 0.0628044
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.2017 +/- 7.69832
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 49 (360961) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (106263 - 360961), with lastBin= 0 and workMinC was 6
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 412702
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x207c900 which has initial GTIBin: 53
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 412702 - 412983


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 412702 - 412983
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 412702 - 412983 the cf is 2.02023
++tructures/grbBin.cpp::        binData:  line  405  INFO   >>  This bin is empty, so found a emptyBin CF of 2.02023
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (412702 - 412983), exposure 280.818
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 0 counts and 0.0228512 bg counts (21), with cf=2.02023 and errBG= 0.00498654
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =-0.0461648 +/- 0.010074
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 412983), exposure 23222.6, 9 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000612879, 0.000315661 and 0.515046. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412702 and stop= 412983 so gap is 280.818, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 50 (412983) and the bin is not full 0 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=52021.7 whereas forward=5483.74
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 50 (412983) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 418466 - 418742


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 422899 - 424501 to this bin
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 428659 - 430261 to this bin
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 412702 - 430261
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 412702 - 430261 the cf is 2.70409
++tructures/grbBin.cpp::        binData:  line  405  INFO   >>  This bin is empty, so found a emptyBin CF of 2.70409
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (412702 - 430261), exposure 3760.95
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 0 counts and 0.180928 bg counts (217), with cf=2.70409 and errBG= 0.0122822
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =-0.489245 +/- 0.0332121
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 430261), exposure 26702.7, 9 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000527718, 0.000267097 and 0.506136. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412702 and stop= 430261 so gap is 17559.4, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 53 (430261) and the bin is not full 0 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=69300.3 whereas forward=4217.64
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 53 (430261) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 434479 - 436081


++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (412702 - 436081), exposure 5363.11
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.401891 bg counts (331), with cf=1.65504 and errBG= 0.0220899
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =0.989895 +/- 1.65544
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 436081), exposure 28304.9, 10 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0005505, 0.000242018 and 0.439632. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=412702 and stop= 436081 so gap is 23379.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 54 (436081) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=75120.1 whereas forward=4158.25
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 54 (436081) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  787  INFO   >>  I'm on the last event, so save the previous bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (106263 - 360961), exposure 23536
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 2.31952 bg counts (1364), with cf=1.98744 and errBG= 0.0628044
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.2017 +/- 7.69832
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 64
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  903  INFO   >>  I have run out of background events
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x207c900
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (412702 - 441841), exposure 6965.28
++taStructures/bin.cpp::        fullBin:  line  192  INFO   >>  Producing an upper limit of 12.7157 given bg=0.580348 and numCts= 1
++ctures/binMethod.cpp::        saveBin:  line  378  INFO   >>  Saving an upper limit, bin number: 65 with rate=0.00182558
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (110130 - 436081), exposure 29907.1, 10 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000513085, 0.000225083 and 0.438686. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for PC mode.
++/genlc_cpp/genlc.cpp::           main:  line  397  INFO   >>  COMPLETE

