++lUtils/createLog.cpp::      createLog:  line   51  INFO   >>  Created FileAppender: 'genlc.log', level info
++/genlc_cpp/genlc.cpp::           main:  line  151  INFO   >>  Starting to run genlc.cpp, mode=0
++/genlc_cpp/genlc.cpp::           main:  line  152  INFO   >>  Argparsing reported: Selected GRB binning.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: WT, with files: wtsourcetotal.evt, wtbacktotal.evt, and wtcorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 81.2057 - 3000
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	81.2057 - 130.152
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - WT mode, suffix = 
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 30 ct/bin at rateFact=10 and binFact= 1.5 with minT 0.5 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file WTCURVE.qdp, reading from wtsourcetotal.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81.2057 - 84.0025), exposure 2.79679
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.09173 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.128 +/- 7.32359
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=81.2057 and stop= 84.0025 so gap is 2.79679, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (81.2057 - 84.0025), with lastBin= 0 and workMinC was 45
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (84.0025 - 86.8047), exposure 2.80215
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.09173 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.128 +/- 7.32359
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=84.0025 and stop= 86.8047 so gap is 2.80215, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (84.0025 - 86.8047), with lastBin= 0x1ec1500 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81.2057 - 84.0025), exposure 2.79679
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.09173 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.128 +/- 7.32359
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1500 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (81.2057 - 87.3651), exposure 6.15937, 45 soft counts and 54 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 7.97615, 9.57138 and 1.2. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=86.8047 and stop= 87.3651 so gap is 0.560427, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (81.2057 - 87.3651) = 81.2057- 87.3651
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (86.8047 - 89.3239), exposure 2.51925
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.09173 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.128 +/- 7.32359
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=86.8047 and stop= 89.3239 so gap is 2.51925, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (86.8047 - 89.3239), with lastBin= 0x1ec3420 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (84.0025 - 86.8047), exposure 2.80215
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.09173 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.128 +/- 7.32359
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (89.3239 - 91.9962), exposure 2.67225
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0.716049 bg counts (1), with cf=1.09177 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.348 +/- 7.36545
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.3239 and stop= 91.9962 so gap is 2.67225, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (89.3239 - 91.9962), with lastBin= 0x1ec1500 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (86.8047 - 89.3239), exposure 2.51925
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.09173 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.128 +/- 7.32359
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1500 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (87.3651 - 94.3625), exposure 6.99734, 45 soft counts and 71 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 7.02224, 10.8552 and 1.54582. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.9962 and stop= 94.3625 so gap is 2.36626, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (87.3651 - 94.3625) = 87.3651- 94.3625
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (91.9962 - 95.0243), exposure 3.0281
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0.716049 bg counts (1), with cf=1.09216 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.3652 +/- 7.36808
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=91.9962 and stop= 95.0243 so gap is 3.0281, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (91.9962 - 95.0243), with lastBin= 0x1ec3420 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (89.3239 - 91.9962), exposure 2.67225
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0.716049 bg counts (1), with cf=1.09177 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.348 +/- 7.36545
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (95.0243 - 99.3422), exposure 4.31792
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.09216 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.1473 +/- 7.32646
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=95.0243 and stop= 99.3422 so gap is 4.31792, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (95.0243 - 99.3422), with lastBin= 0x1ec1500 and workMinC was 45
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (91.9962 - 95.0243), exposure 3.0281
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0.716049 bg counts (1), with cf=1.09216 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.3652 +/- 7.36808
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1500 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (99.3422 - 102.856), exposure 3.5138
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 32 counts and 0 bg counts (0), with cf=1.09222 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.951 +/- 6.17852
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (94.3625 - 102.856), exposure 8.49356, 31 soft counts and 56 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.98629, 7.201 and 1.80644. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=99.3422 and stop= 102.856 so gap is 3.5138, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (99.3422 - 102.856), with lastBin= 0x1ec3420 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (95.0243 - 99.3422), exposure 4.31792
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 45 counts and 0 bg counts (0), with cf=1.09216 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =49.1473 +/- 7.32646
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (94.3625 - 102.856) = 94.3625- 102.856
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (102.856 - 107.971), exposure 5.11499
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.09242 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.7725 +/- 5.98342
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=102.856 and stop= 107.971 so gap is 5.11499, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (102.856 - 107.971), with lastBin= 0x1ec1500 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (99.3422 - 102.856), exposure 3.5138
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 32 counts and 0 bg counts (0), with cf=1.09222 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =34.951 +/- 6.17852
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1500 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (107.971 - 112.504), exposure 4.53325
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.09242 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.7725 +/- 5.98342
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=107.971 and stop= 112.504 so gap is 4.53325, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (107.971 - 112.504), with lastBin= 0x1ec3420 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (102.856 - 107.971), exposure 5.11499
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.09242 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.7725 +/- 5.98342
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (112.504 - 118.333), exposure 5.8284
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.716049 bg counts (1), with cf=1.09254 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.9938 +/- 6.035
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.504 and stop= 118.333 so gap is 5.8284, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (112.504 - 118.333), with lastBin= 0x1ec1500 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (107.971 - 112.504), exposure 4.53325
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.09242 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.7725 +/- 5.98342
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1500 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (102.856 - 119.146), exposure 16.2897, 30 soft counts and 65 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.01192, 4.3112 and 2.14283. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=118.333 and stop= 119.146 so gap is 0.813064, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (102.856 - 119.146) = 102.856- 119.146
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (118.333 - 124.661), exposure 6.32836
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.09256 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.7769 +/- 5.98422
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=118.333 and stop= 124.661 so gap is 6.32836, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (118.333 - 124.661), with lastBin= 0x1ec3420 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (112.504 - 118.333), exposure 5.8284
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.716049 bg counts (1), with cf=1.09254 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.9938 +/- 6.035
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (124.661 - 130.152), exposure 5.49129
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.716049 bg counts (1), with cf=1.09253 and errBG= 0.716049
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.6982 +/- 4.43959
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (119.146 - 130.152), exposure 11.0066, 15 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.41787, 2.58085 and 1.82024. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=124.661 and stop= 130.152 so gap is 5.49129, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (130.152) and the bin is not full 16 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  492  INFO   >>  Discarding leftover counts, as skip is set and I have no bin to carry back to
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 81.2057
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (130.152) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  787  INFO   >>  I'm on the last event, so save the previous bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (118.333 - 124.661), exposure 6.32836
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0 bg counts (0), with cf=1.09256 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.7769 +/- 5.98422
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x1ec3420
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 81.2057 - 130.152
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 81.2057 - 130.152 the cf is 1.09226
++tructures/grbBin.cpp::        binData:  line  921  INFO   >>  This bin is empty, so found a emptyBin CF of 1.09226
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81.2057 - 130.152), exposure 48.9466
++taStructures/bin.cpp::        fullBin:  line  192  INFO   >>  Producing an upper limit of 6.46073 given bg=0 and numCts= 0
++tructures/grbBin.cpp::        binData:  line  929  INFO   >>  Not saving this bin as it is an incomplete WT one
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (119.146 - 130.152), exposure 11.0066, 15 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.41787, 2.58085 and 1.82024. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for WT mode.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: WT, with files: wtsourcetotal_incbad.evt, wtbacktotal_incbad.evt, and wtcorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 81.2057 - 3000
++/SourceEventList.cpp::SourceEventList:  line   67  FATAL  >>  Can't open file wtsourcetotal_incbad.evt
++/genlc_cpp/genlc.cpp::           main:  line  388  WARN   >>  Unable to open the files for this mode, skipping
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: PC, with files: pcsourcetotal.evt, pcbacktotal.evt, and pccorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 131.841 - 380606
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	131.841 - 1255.11
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	4681.62 - 7025.94
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	10320 - 11568.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	11947.3 - 12799.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	16099.5 - 18571.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	27646.2 - 30118.4
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	56480 - 58987.3
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - PC mode, suffix = 
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 20 ct/bin at rateFact=10 and binFact= 1.5 with minT 2.51 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file PCCURVE.qdp, reading from pcsourcetotal.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (131.841 - 151.899), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0628967 bg counts (3), with cf=2.11687 and errBG= 0.0363134
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.3211 +/- 9.70101
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=131.841 and stop= 151.899 so gap is 20.0585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (131.841 - 151.899), with lastBin= 0 and workMinC was 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (151.899 - 181.987), exposure 30.0879
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.11359 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2718 +/- 9.45226
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=151.899 and stop= 181.987 so gap is 30.0879, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (151.899 - 181.987), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (131.841 - 151.899), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0628967 bg counts (3), with cf=2.11687 and errBG= 0.0363134
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.3211 +/- 9.70101
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (181.987 - 204.553), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.0209656 bg counts (1), with cf=2.09925 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.2388 +/- 10.0678
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=181.987 and stop= 204.553 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (181.987 - 204.553), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (151.899 - 181.987), exposure 30.0879
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.11359 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2718 +/- 9.45226
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (131.841 - 242.163), exposure 110.322, 20 soft counts and 62 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.379524, 1.18092 and 3.11158. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=204.553 and stop= 242.163 so gap is 37.6098, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (131.841 - 242.163) = 131.841- 242.163
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (204.553 - 254.699), exposure 50.1464
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.07639 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.5278 +/- 9.28589
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=204.553 and stop= 254.699 so gap is 50.1464, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (204.553 - 254.699), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (181.987 - 204.553), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.0209656 bg counts (1), with cf=2.09925 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.2388 +/- 10.0678
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (254.699 - 329.919), exposure 75.2196
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.125793 bg counts (6), with cf=2.09308 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.6914 +/- 9.5923
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=254.699 and stop= 329.919 so gap is 75.2196, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (254.699 - 329.919), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (204.553 - 254.699), exposure 50.1464
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.07639 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.5278 +/- 9.28589
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (329.919 - 392.602), exposure 62.683
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.1033 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.8015 +/- 9.40687
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=329.919 and stop= 392.602 so gap is 62.683, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (329.919 - 392.602), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (254.699 - 329.919), exposure 75.2196
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.125793 bg counts (6), with cf=2.09308 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.6914 +/- 9.5923
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (242.163 - 472.836), exposure 230.673, 20 soft counts and 42 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.180623, 0.380145 and 2.10463. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.602 and stop= 472.836 so gap is 80.2343, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (242.163 - 472.836) = 242.163- 472.836
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (392.602 - 475.344), exposure 82.7416
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.10057 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.7471 +/- 9.39464
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.602 and stop= 475.344 so gap is 82.7416, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (392.602 - 475.344), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (329.919 - 392.602), exposure 62.683
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.1033 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.8015 +/- 9.40687
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (475.344 - 555.578), exposure 80.2342
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0209656 bg counts (1), with cf=2.07524 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.4613 +/- 9.28085
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=475.344 and stop= 555.578 so gap is 80.2342, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (475.344 - 555.578), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (392.602 - 475.344), exposure 82.7416
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.10057 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.7471 +/- 9.39464
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (555.578 - 630.797), exposure 75.2195
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0209656 bg counts (1), with cf=2.09694 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.8948 +/- 9.3779
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=555.578 and stop= 630.797 so gap is 75.2195, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (555.578 - 630.797), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (475.344 - 555.578), exposure 80.2342
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0209656 bg counts (1), with cf=2.07524 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.4613 +/- 9.28085
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (630.797 - 716.046), exposure 85.2488
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.104828 bg counts (5), with cf=2.07879 and errBG= 0.0468804
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.3579 +/- 9.29716
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=630.797 and stop= 716.046 so gap is 85.2488, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (630.797 - 716.046), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (555.578 - 630.797), exposure 75.2195
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0209656 bg counts (1), with cf=2.09694 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.8948 +/- 9.3779
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (472.836 - 783.744), exposure 310.907, 20 soft counts and 57 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.133963, 0.382551 and 2.85565. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=716.046 and stop= 783.744 so gap is 67.6976, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (472.836 - 783.744) = 472.836- 783.744
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (716.046 - 798.788), exposure 82.7415
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.13061 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.3442 +/- 9.52902
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=716.046 and stop= 798.788 so gap is 82.7415, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (716.046 - 798.788), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (630.797 - 716.046), exposure 85.2488
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.104828 bg counts (5), with cf=2.07879 and errBG= 0.0468804
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.3579 +/- 9.29716
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (798.788 - 954.241), exposure 155.454
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335449 bg counts (16), with cf=2.11302 and errBG= 0.0838622
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.5515 +/- 9.45135
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=798.788 and stop= 954.241 so gap is 155.454, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (798.788 - 954.241), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (716.046 - 798.788), exposure 82.7415
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.13061 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.3442 +/- 9.52902
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (954.241 - 1082.11), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.104828 bg counts (5), with cf=2.11687 and errBG= 0.0468804
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.1154 +/- 9.46744
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=954.241 and stop= 1082.11 so gap is 127.873, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (954.241 - 1082.11), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (798.788 - 954.241), exposure 155.454
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335449 bg counts (16), with cf=2.11302 and errBG= 0.0838622
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.5515 +/- 9.45135
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 12
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (783.744 - 1104.68), exposure 320.936, 20 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.130032, 0.216236 and 1.66295. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1082.11 and stop= 1104.68 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (783.744 - 1104.68) = 783.744- 1104.68
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1082.11 - 1199.96), exposure 117.844
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.146759 bg counts (7), with cf=2.0979 and errBG= 0.0554697
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.6502 +/- 9.38283
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1082.11 and stop= 1199.96 so gap is 117.844, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1082.11 - 1199.96), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (954.241 - 1082.11), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.104828 bg counts (5), with cf=2.11687 and errBG= 0.0468804
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.1154 +/- 9.46744
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 13
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1199.96 - 1255.11), exposure 55.1529
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 0.0838622 bg counts (4), with cf=2.14064 and errBG= 0.0419311
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.7894 +/- 8.01004
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1104.68 - 1255.11), exposure 150.431, 7 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0978286, 0.251435 and 2.57016. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1199.96 and stop= 1255.11 so gap is 55.1529, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (1255.11) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=55.1529 whereas forward=3426.5
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1082.11 - 1255.11), exposure 172.997
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 34 counts and 0.230621 bg counts (11), with cf=2.1155 and errBG= 0.0695349
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =71.4391 +/- 12.3363
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (1255.11) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (783.744 - 1255.11), exposure 471.367, 27 soft counts and 51 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.119756, 0.22747 and 1.89945. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1082.11 - 1255.11), with lastBin= 0 and workMinC was 17
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 4681.62
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (783.744 - 1255.11) = 783.744- 1255.11
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 4681.62 - 7025.94


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4681.62 - 4899.75), exposure 218.136
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0892533 bg counts (7), with cf=1.28044 and errBG= 0.0337346
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0923 +/- 4.95931
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4681.62 and stop= 4899.75 so gap is 218.136, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4681.62 - 4899.75), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1082.11 - 1255.11), exposure 172.997
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 34 counts and 0.230621 bg counts (11), with cf=2.1155 and errBG= 0.0695349
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =71.4391 +/- 12.3363
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 14
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4899.75 - 5180.57), exposure 280.819
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0637524 bg counts (5), with cf=1.28167 and errBG= 0.0285109
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1433 +/- 4.96401
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4899.75 and stop= 5180.57 so gap is 280.819, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4899.75 - 5180.57), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4681.62 - 4899.75), exposure 218.136
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0892533 bg counts (7), with cf=1.28044 and errBG= 0.0337346
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0923 +/- 4.95931
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 15
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (4681.62 - 5348.56), exposure 666.946, 17 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0323976, 0.0498253 and 1.53793. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5180.57 and stop= 5348.56 so gap is 167.99, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (4681.62 - 5348.56) = 4681.62- 5348.56
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5180.57 - 5408.74), exposure 228.166
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.102004 bg counts (8), with cf=1.28204 and errBG= 0.0360638
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.5101 +/- 5.73367
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5180.57 and stop= 5408.74 so gap is 228.166, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (5180.57 - 5408.74), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4899.75 - 5180.57), exposure 280.819
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0637524 bg counts (5), with cf=1.28167 and errBG= 0.0285109
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1433 +/- 4.96401
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 16
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5408.74 - 5734.69), exposure 325.951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0892533 bg counts (7), with cf=1.28321 and errBG= 0.0337346
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1336 +/- 4.97003
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5408.74 and stop= 5734.69 so gap is 325.951, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (5408.74 - 5734.69), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5180.57 - 5408.74), exposure 228.166
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.102004 bg counts (8), with cf=1.28204 and errBG= 0.0360638
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.5101 +/- 5.73367
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 17
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5734.69 - 6093.24), exposure 358.547
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.153006 bg counts (12), with cf=1.28225 and errBG= 0.0441689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0375 +/- 4.96645
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5734.69 and stop= 6093.24 so gap is 358.547, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (5734.69 - 6093.24), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5408.74 - 5734.69), exposure 325.951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0892533 bg counts (7), with cf=1.28321 and errBG= 0.0337346
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1336 +/- 4.97003
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 18
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (5348.56 - 6208.57), exposure 860.01, 15 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0220679, 0.0430007 and 1.94856. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6093.24 and stop= 6208.57 so gap is 115.337, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (5348.56 - 6208.57) = 5348.56- 6208.57
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6093.24 - 6396.62), exposure 303.385
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.153006 bg counts (12), with cf=1.28228 and errBG= 0.0441689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0379 +/- 4.96656
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6093.24 and stop= 6396.62 so gap is 303.385, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6093.24 - 6396.62), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5734.69 - 6093.24), exposure 358.547
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.153006 bg counts (12), with cf=1.28225 and errBG= 0.0441689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0375 +/- 4.96645
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 19
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6396.62 - 6642.34), exposure 245.717
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.204008 bg counts (16), with cf=1.2822 and errBG= 0.0510019
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9714 +/- 4.96635
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6396.62 and stop= 6642.34 so gap is 245.717, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6396.62 - 6642.34), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6093.24 - 6396.62), exposure 303.385
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.153006 bg counts (12), with cf=1.28228 and errBG= 0.0441689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0379 +/- 4.96656
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6642.34 - 6918.14), exposure 275.805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.153006 bg counts (12), with cf=1.28087 and errBG= 0.0441689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.017 +/- 4.9611
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6642.34 and stop= 6918.14 so gap is 275.805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6642.34 - 6918.14), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6396.62 - 6642.34), exposure 245.717
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.204008 bg counts (16), with cf=1.2822 and errBG= 0.0510019
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9714 +/- 4.96635
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 21
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6918.14 - 7025.94), exposure 107.799
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.0127505 bg counts (1), with cf=1.28122 and errBG= 0.0127505
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.2334 +/- 3.62387
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6208.57 - 7025.94), exposure 817.369, 14 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0216143, 0.0498084 and 2.30442. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6918.14 and stop= 7025.94 so gap is 107.799, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 1 (7025.94) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=107.799 whereas forward=3294.07
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6642.34 - 7025.94), exposure 383.603
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.165756 bg counts (13), with cf=1.28099 and errBG= 0.0459725
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.2504 +/- 6.14369
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 1 (7025.94) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (5348.56 - 7025.94), exposure 1677.38, 29 soft counts and 61 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0218468, 0.046318 and 2.12012. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6642.34 - 7025.94), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 10320
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (5348.56 - 7025.94) = 5348.56- 7025.94
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 10320 - 11568.7


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10320 - 11353), exposure 1033.01
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.190866 bg counts (28), with cf=3.24616 and errBG= 0.0360704
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.0728 +/- 12.5729
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=10320 and stop= 11353 so gap is 1033.01, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10320 - 11353), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6642.34 - 7025.94), exposure 383.603
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.165756 bg counts (13), with cf=1.28099 and errBG= 0.0459725
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.2504 +/- 6.14369
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 22
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11353 - 11568.7), exposure 215.621
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.02045 bg counts (3), with cf=3.32302 and errBG= 0.0118068
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.57808 +/- 4.69962
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (10320 - 11568.7), exposure 1248.64, 6 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0148464, 0.0289229 and 1.94814. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=11353 and stop= 11568.7 so gap is 215.621, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 2 (11568.7) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=215.621 whereas forward=378.606
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10320 - 11568.7), exposure 1248.64
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.211316 bg counts (31), with cf=3.2552 and errBG= 0.0379535
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =54.6506 +/- 13.4221
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 2 (11568.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10320 - 11568.7), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 11947.3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 11947.3 - 12799.7


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11947.3 - 12799.7), exposure 852.482
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.290022 bg counts (41), with cf=1.34371 and errBG= 0.0452938
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.0785 +/- 4.8452
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (10320 - 12799.7), exposure 2101.12, 8 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0100104, 0.0240564 and 2.40313. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=11947.3 and stop= 12799.7 so gap is 852.482, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 3 (12799.7) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 17 counts, because gotBinThisOrb=0 and gapBack=1231.09 whereas forward=3299.77
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10320 - 12799.7), exposure 2101.12
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.501338 bg counts (72), with cf=2.42689 and errBG= 0.0590833
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =71.59 +/- 13.2934
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 3 (12799.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10320 - 12799.7), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 16099.5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 16099.5 - 18571.7


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16099.5 - 16676.2), exposure 576.683
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.132353 bg counts (18), with cf=1.49397 and errBG= 0.0311959
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.2118 +/- 5.78631
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16099.5 and stop= 16676.2 so gap is 576.683, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16099.5 - 16676.2), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10320 - 12799.7), exposure 2101.12
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.501338 bg counts (72), with cf=2.42689 and errBG= 0.0590833
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =71.59 +/- 13.2934
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 23
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16676.2 - 17405.8), exposure 729.63
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.176471 bg counts (24), with cf=1.4998 and errBG= 0.0360219
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.2323 +/- 5.80894
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16676.2 and stop= 17405.8 so gap is 729.63, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16676.2 - 17405.8), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16099.5 - 16676.2), exposure 576.683
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.132353 bg counts (18), with cf=1.49397 and errBG= 0.0311959
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.2118 +/- 5.78631
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 24
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (10320 - 17466), exposure 3467.61, 15 soft counts and 48 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00902998, 0.0257475 and 2.85134. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17405.8 and stop= 17466 so gap is 60.1757, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (10320 - 17466) = 10320- 17466
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17405.8 - 18571.7), exposure 1165.88
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.272059 bg counts (37), with cf=1.489 and errBG= 0.0447262
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9519 +/- 5.36908
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17466 - 18571.7), exposure 1105.71, 3 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00392056, 0.0091782 and 2.34104. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17405.8 and stop= 18571.7 so gap is 1165.88, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 4 (18571.7) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=1165.88 whereas forward=9074.52
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16676.2 - 18571.7), exposure 1895.51
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.448529 bg counts (61), with cf=1.49478 and errBG= 0.0574283
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.1835 +/- 7.91012
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 4 (18571.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (10320 - 18571.7), exposure 4573.32, 18 soft counts and 55 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00779018, 0.0217344 and 2.78998. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16676.2 - 18571.7), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 27646.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (10320 - 18571.7) = 10320- 18571.7
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 27646.2 - 30118.4


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (27646.2 - 30118.4), exposure 2472.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.350637 bg counts (88), with cf=1.66129 and errBG= 0.037378
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.3529 +/- 5.7552
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (27646.2 - 30118.4), exposure 2472.2, 3 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00194514, 0.00588273 and 3.02433. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=27646.2 and stop= 30118.4 so gap is 2472.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 5 (30118.4) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 28 counts, because gotBinThisOrb=0 and gapBack=11546.7 whereas forward=26361.6
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16676.2 - 30118.4), exposure 4367.71
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 40 counts and 0.799166 bg counts (149), with cf=1.54474 and errBG= 0.0654703
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =60.5549 +/- 9.77029
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 5 (30118.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16676.2 - 30118.4), with lastBin= 0 and workMinC was 9
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 56480
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 56480 - 58987.3


++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (56480 - 58987.3), exposure 2507.3
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 0.562507 bg counts (140), with cf=3.24947 and errBG= 0.0475405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.4173 +/- 9.74962
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (27646.2 - 58987.3), exposure 4979.5, 5 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00211098, 0.00733715 and 3.4757. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=56480 and stop= 58987.3 so gap is 2507.3, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  787  INFO   >>  I'm on the last event, so save the previous bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16676.2 - 30118.4), exposure 4367.71
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 40 counts and 0.799166 bg counts (149), with cf=1.54474 and errBG= 0.0654703
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =60.5549 +/- 9.77029
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 25
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x1ec3420
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (56480 - 58987.3), exposure 2507.3
++taStructures/bin.cpp::   bayesian_bin:  line  273  INFO   >>  Making a Bayesian bin - I have 9 counts and 0.562507 bg counts, with cf=3.24947
++taStructures/bin.cpp::   bayesian_bin:  line  274  INFO   >>    Therefore net =27.4157 + 10.9832 -8.77031 and sigma=177.48
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 26
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (27646.2 - 58987.3), exposure 4979.5, 5 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00211098, 0.00733715 and 3.4757. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for PC mode.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: PC, with files: pcsourcetotal_incbad.evt, pcbacktotal_incbad.evt, and pccorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 131.841 - 380606
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	131.841 - 1255.11
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	4681.62 - 7025.94
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	10320 - 11568.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	11947.3 - 12799.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	16099.5 - 18571.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	21886.1 - 24345.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	27646.2 - 30118.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	33385.1 - 35067.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	39189.5 - 40947.2
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	46727.6 - 46945.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	52487.8 - 52886.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	56480 - 58987.3
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	62247.7 - 64759.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	68052.8 - 70530.4
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	73832.5 - 74547.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	75592.1 - 76304.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	79603.9 - 82076.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	85379.7 - 87848.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	91157.2 - 93623.2
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	96929.1 - 98110.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	143456 - 144926
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	160797 - 162085
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	166602 - 167786
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	178183 - 179547
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	183961 - 185365
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	189729 - 191246
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	195523 - 196406
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	212802 - 214166
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	218611 - 220105
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	230167 - 230906
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	235963 - 236667
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	241723 - 243147
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	247482 - 249027
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	253303 - 254667
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	259063 - 260485
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	264851 - 266245
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	276402 - 276926
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	294331 - 294807
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	299269 - 299344
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	299413 - 300747
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	305082 - 306747
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	310804 - 311187
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	316663 - 318325
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	351133 - 351507
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	356944 - 357267
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	374501 - 375446
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	380022 - 380606
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - PC mode, suffix = _incbad
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 20 ct/bin at rateFact=10 and binFact= 1.5 with minT 2.51 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file PCCURVE_incbad.qdp, reading from pcsourcetotal_incbad.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (131.841 - 151.899), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0628967 bg counts (3), with cf=2.11687 and errBG= 0.0363134
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.3211 +/- 9.70101
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=131.841 and stop= 151.899 so gap is 20.0585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (131.841 - 151.899), with lastBin= 0 and workMinC was 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (151.899 - 181.987), exposure 30.0879
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.11359 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2718 +/- 9.45226
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=151.899 and stop= 181.987 so gap is 30.0879, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (151.899 - 181.987), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (131.841 - 151.899), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.0628967 bg counts (3), with cf=2.11687 and errBG= 0.0363134
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.3211 +/- 9.70101
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (181.987 - 204.553), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.0209656 bg counts (1), with cf=2.09925 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.2388 +/- 10.0678
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=181.987 and stop= 204.553 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (181.987 - 204.553), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (151.899 - 181.987), exposure 30.0879
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.11359 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.2718 +/- 9.45226
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (131.841 - 242.163), exposure 110.322, 20 soft counts and 62 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.379524, 1.18092 and 3.11158. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=204.553 and stop= 242.163 so gap is 37.6098, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (131.841 - 242.163) = 131.841- 242.163
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (204.553 - 254.699), exposure 50.1464
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.07639 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.5278 +/- 9.28589
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=204.553 and stop= 254.699 so gap is 50.1464, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (204.553 - 254.699), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (181.987 - 204.553), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.0209656 bg counts (1), with cf=2.09925 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.2388 +/- 10.0678
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (254.699 - 329.919), exposure 75.2196
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.125793 bg counts (6), with cf=2.09308 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.6914 +/- 9.5923
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=254.699 and stop= 329.919 so gap is 75.2196, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (254.699 - 329.919), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (204.553 - 254.699), exposure 50.1464
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0 bg counts (0), with cf=2.07639 and errBG= 0
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.5278 +/- 9.28589
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (329.919 - 392.602), exposure 62.683
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.1033 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.8015 +/- 9.40687
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=329.919 and stop= 392.602 so gap is 62.683, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (329.919 - 392.602), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (254.699 - 329.919), exposure 75.2196
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.125793 bg counts (6), with cf=2.09308 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =43.6914 +/- 9.5923
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (242.163 - 472.836), exposure 230.673, 20 soft counts and 42 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.180623, 0.380145 and 2.10463. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.602 and stop= 472.836 so gap is 80.2343, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (242.163 - 472.836) = 242.163- 472.836
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (392.602 - 475.344), exposure 82.7416
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.10057 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.7471 +/- 9.39464
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=392.602 and stop= 475.344 so gap is 82.7416, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (392.602 - 475.344), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (329.919 - 392.602), exposure 62.683
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.1033 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.8015 +/- 9.40687
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (475.344 - 555.578), exposure 80.2342
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0209656 bg counts (1), with cf=2.07524 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.4613 +/- 9.28085
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=475.344 and stop= 555.578 so gap is 80.2342, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (475.344 - 555.578), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (392.602 - 475.344), exposure 82.7416
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.10057 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.7471 +/- 9.39464
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (555.578 - 630.797), exposure 75.2195
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0209656 bg counts (1), with cf=2.09694 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.8948 +/- 9.3779
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=555.578 and stop= 630.797 so gap is 75.2195, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (555.578 - 630.797), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (475.344 - 555.578), exposure 80.2342
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0209656 bg counts (1), with cf=2.07524 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.4613 +/- 9.28085
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (630.797 - 716.046), exposure 85.2488
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.104828 bg counts (5), with cf=2.07879 and errBG= 0.0468804
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.3579 +/- 9.29716
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=630.797 and stop= 716.046 so gap is 85.2488, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (630.797 - 716.046), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (555.578 - 630.797), exposure 75.2195
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0209656 bg counts (1), with cf=2.09694 and errBG= 0.0209656
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.8948 +/- 9.3779
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (472.836 - 783.744), exposure 310.907, 20 soft counts and 57 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.133963, 0.382551 and 2.85565. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=716.046 and stop= 783.744 so gap is 67.6976, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (472.836 - 783.744) = 472.836- 783.744
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (716.046 - 798.788), exposure 82.7415
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.13061 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.3442 +/- 9.52902
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=716.046 and stop= 798.788 so gap is 82.7415, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (716.046 - 798.788), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (630.797 - 716.046), exposure 85.2488
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.104828 bg counts (5), with cf=2.07879 and errBG= 0.0468804
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.3579 +/- 9.29716
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (798.788 - 954.241), exposure 155.454
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335449 bg counts (16), with cf=2.11302 and errBG= 0.0838622
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.5515 +/- 9.45135
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=798.788 and stop= 954.241 so gap is 155.454, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (798.788 - 954.241), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (716.046 - 798.788), exposure 82.7415
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.125793 bg counts (6), with cf=2.13061 and errBG= 0.0513549
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.3442 +/- 9.52902
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (954.241 - 1082.11), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.104828 bg counts (5), with cf=2.11687 and errBG= 0.0468804
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.1154 +/- 9.46744
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=954.241 and stop= 1082.11 so gap is 127.873, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (954.241 - 1082.11), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (798.788 - 954.241), exposure 155.454
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335449 bg counts (16), with cf=2.11302 and errBG= 0.0838622
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.5515 +/- 9.45135
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 12
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (783.744 - 1104.68), exposure 320.936, 20 soft counts and 33 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.130032, 0.216236 and 1.66295. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1082.11 and stop= 1104.68 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (783.744 - 1104.68) = 783.744- 1104.68
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1082.11 - 1199.96), exposure 117.844
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.146759 bg counts (7), with cf=2.0979 and errBG= 0.0554697
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.6502 +/- 9.38283
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1082.11 and stop= 1199.96 so gap is 117.844, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1082.11 - 1199.96), with lastBin= 0x1ec3420 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (954.241 - 1082.11), exposure 127.873
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.104828 bg counts (5), with cf=2.11687 and errBG= 0.0468804
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =42.1154 +/- 9.46744
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 13
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1199.96 - 1255.11), exposure 55.1529
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 0.0838622 bg counts (4), with cf=2.14064 and errBG= 0.0419311
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.7894 +/- 8.01004
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1104.68 - 1255.11), exposure 150.431, 7 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0978286, 0.251435 and 2.57016. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1199.96 and stop= 1255.11 so gap is 55.1529, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (1255.11) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=55.1529 whereas forward=3426.5
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1082.11 - 1255.11), exposure 172.997
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 34 counts and 0.230621 bg counts (11), with cf=2.1155 and errBG= 0.0695349
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =71.4391 +/- 12.3363
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (1255.11) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (783.744 - 1255.11), exposure 471.367, 27 soft counts and 51 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.119756, 0.22747 and 1.89945. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1082.11 - 1255.11), with lastBin= 0 and workMinC was 17
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 4681.62
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (783.744 - 1255.11) = 783.744- 1255.11
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 4681.62 - 7025.94


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4681.62 - 4899.75), exposure 218.136
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0892533 bg counts (7), with cf=1.28044 and errBG= 0.0337346
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0923 +/- 4.95931
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4681.62 and stop= 4899.75 so gap is 218.136, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4681.62 - 4899.75), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1082.11 - 1255.11), exposure 172.997
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 34 counts and 0.230621 bg counts (11), with cf=2.1155 and errBG= 0.0695349
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =71.4391 +/- 12.3363
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 14
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4899.75 - 5180.57), exposure 280.819
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0637524 bg counts (5), with cf=1.28167 and errBG= 0.0285109
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1433 +/- 4.96401
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=4899.75 and stop= 5180.57 so gap is 280.819, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (4899.75 - 5180.57), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4681.62 - 4899.75), exposure 218.136
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0892533 bg counts (7), with cf=1.28044 and errBG= 0.0337346
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0923 +/- 4.95931
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 15
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (4681.62 - 5348.56), exposure 666.946, 17 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0323976, 0.0498253 and 1.53793. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5180.57 and stop= 5348.56 so gap is 167.99, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (4681.62 - 5348.56) = 4681.62- 5348.56
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5180.57 - 5408.74), exposure 228.166
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.102004 bg counts (8), with cf=1.28204 and errBG= 0.0360638
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.5101 +/- 5.73367
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5180.57 and stop= 5408.74 so gap is 228.166, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (5180.57 - 5408.74), with lastBin= 0x1ec1950 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (4899.75 - 5180.57), exposure 280.819
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0637524 bg counts (5), with cf=1.28167 and errBG= 0.0285109
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1433 +/- 4.96401
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 16
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5408.74 - 5734.69), exposure 325.951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0892533 bg counts (7), with cf=1.28321 and errBG= 0.0337346
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1336 +/- 4.97003
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5408.74 and stop= 5734.69 so gap is 325.951, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (5408.74 - 5734.69), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5180.57 - 5408.74), exposure 228.166
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.102004 bg counts (8), with cf=1.28204 and errBG= 0.0360638
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.5101 +/- 5.73367
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 17
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5734.69 - 6093.24), exposure 358.547
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.153006 bg counts (12), with cf=1.28225 and errBG= 0.0441689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0375 +/- 4.96645
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=5734.69 and stop= 6093.24 so gap is 358.547, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (5734.69 - 6093.24), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5408.74 - 5734.69), exposure 325.951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.0892533 bg counts (7), with cf=1.28321 and errBG= 0.0337346
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.1336 +/- 4.97003
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 18
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (5348.56 - 6208.57), exposure 860.01, 15 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0220679, 0.0430007 and 1.94856. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6093.24 and stop= 6208.57 so gap is 115.337, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (5348.56 - 6208.57) = 5348.56- 6208.57
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6093.24 - 6396.62), exposure 303.385
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.153006 bg counts (12), with cf=1.28228 and errBG= 0.0441689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0379 +/- 4.96656
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6093.24 and stop= 6396.62 so gap is 303.385, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6093.24 - 6396.62), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (5734.69 - 6093.24), exposure 358.547
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.153006 bg counts (12), with cf=1.28225 and errBG= 0.0441689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0375 +/- 4.96645
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 19
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6396.62 - 6642.34), exposure 245.717
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.204008 bg counts (16), with cf=1.2822 and errBG= 0.0510019
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9714 +/- 4.96635
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6396.62 and stop= 6642.34 so gap is 245.717, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6396.62 - 6642.34), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6093.24 - 6396.62), exposure 303.385
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.153006 bg counts (12), with cf=1.28228 and errBG= 0.0441689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.0379 +/- 4.96656
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6642.34 - 6918.14), exposure 275.805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.153006 bg counts (12), with cf=1.28087 and errBG= 0.0441689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.017 +/- 4.9611
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6642.34 and stop= 6918.14 so gap is 275.805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6642.34 - 6918.14), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6396.62 - 6642.34), exposure 245.717
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.204008 bg counts (16), with cf=1.2822 and errBG= 0.0510019
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9714 +/- 4.96635
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 21
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6918.14 - 7025.94), exposure 107.799
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.0127505 bg counts (1), with cf=1.28122 and errBG= 0.0127505
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.2334 +/- 3.62387
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (6208.57 - 7025.94), exposure 817.369, 14 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0216143, 0.0498084 and 2.30442. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=6918.14 and stop= 7025.94 so gap is 107.799, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 1 (7025.94) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=107.799 whereas forward=3294.07
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6642.34 - 7025.94), exposure 383.603
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.165756 bg counts (13), with cf=1.28099 and errBG= 0.0459725
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.2504 +/- 6.14369
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 1 (7025.94) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (5348.56 - 7025.94), exposure 1677.38, 29 soft counts and 61 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0218468, 0.046318 and 2.12012. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (6642.34 - 7025.94), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 10320
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (5348.56 - 7025.94) = 5348.56- 7025.94
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 10320 - 11568.7


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10320 - 11353), exposure 1033.01
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.190866 bg counts (28), with cf=3.24616 and errBG= 0.0360704
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.0728 +/- 12.5729
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=10320 and stop= 11353 so gap is 1033.01, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10320 - 11353), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (6642.34 - 7025.94), exposure 383.603
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.165756 bg counts (13), with cf=1.28099 and errBG= 0.0459725
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.2504 +/- 6.14369
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 22
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11353 - 11568.7), exposure 215.621
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.02045 bg counts (3), with cf=3.32302 and errBG= 0.0118068
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.57808 +/- 4.69962
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (10320 - 11568.7), exposure 1248.64, 6 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0148464, 0.0289229 and 1.94814. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=11353 and stop= 11568.7 so gap is 215.621, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 2 (11568.7) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=215.621 whereas forward=378.606
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10320 - 11568.7), exposure 1248.64
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.211316 bg counts (31), with cf=3.2552 and errBG= 0.0379535
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =54.6506 +/- 13.4221
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 2 (11568.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10320 - 11568.7), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 11947.3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 11947.3 - 12799.7


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (11947.3 - 12799.7), exposure 852.482
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.290022 bg counts (41), with cf=1.34371 and errBG= 0.0452938
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.0785 +/- 4.8452
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (10320 - 12799.7), exposure 2101.12, 8 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0100104, 0.0240564 and 2.40313. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=11947.3 and stop= 12799.7 so gap is 852.482, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 3 (12799.7) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 17 counts, because gotBinThisOrb=0 and gapBack=1231.09 whereas forward=3299.77
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10320 - 12799.7), exposure 2101.12
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.501338 bg counts (72), with cf=2.42689 and errBG= 0.0590833
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =71.59 +/- 13.2934
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 3 (12799.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (10320 - 12799.7), with lastBin= 0 and workMinC was 11
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 16099.5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 16099.5 - 18571.7


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16099.5 - 16676.2), exposure 576.683
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.132353 bg counts (18), with cf=1.49397 and errBG= 0.0311959
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.2118 +/- 5.78631
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16099.5 and stop= 16676.2 so gap is 576.683, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16099.5 - 16676.2), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (10320 - 12799.7), exposure 2101.12
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.501338 bg counts (72), with cf=2.42689 and errBG= 0.0590833
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =71.59 +/- 13.2934
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 23
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16676.2 - 17405.8), exposure 729.63
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.176471 bg counts (24), with cf=1.4998 and errBG= 0.0360219
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.2323 +/- 5.80894
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16676.2 and stop= 17405.8 so gap is 729.63, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16676.2 - 17405.8), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16099.5 - 16676.2), exposure 576.683
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.132353 bg counts (18), with cf=1.49397 and errBG= 0.0311959
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.2118 +/- 5.78631
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 24
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (10320 - 17466), exposure 3467.61, 15 soft counts and 48 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00902998, 0.0257475 and 2.85134. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17405.8 and stop= 17466 so gap is 60.1757, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (10320 - 17466) = 10320- 17466
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17405.8 - 18571.7), exposure 1165.88
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.272059 bg counts (37), with cf=1.489 and errBG= 0.0447262
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9519 +/- 5.36908
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17466 - 18571.7), exposure 1105.71, 3 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00392056, 0.0091782 and 2.34104. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17405.8 and stop= 18571.7 so gap is 1165.88, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 4 (18571.7) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=1165.88 whereas forward=3314.41
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16676.2 - 18571.7), exposure 1895.51
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.448529 bg counts (61), with cf=1.49478 and errBG= 0.0574283
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.1835 +/- 7.91012
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 4 (18571.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (10320 - 18571.7), exposure 4573.32, 18 soft counts and 55 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00779018, 0.0217344 and 2.78998. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16676.2 - 18571.7), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 21886.1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (10320 - 18571.7) = 10320- 18571.7
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 21886.1 - 24345.8


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (21886.1 - 24345.8), exposure 2459.66
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.207295 bg counts (98), with cf=4.35516 and errBG= 0.0209399
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.2282 +/- 10.6683
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (21886.1 - 24345.8), exposure 2459.66, 2 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00338861, 0.00686826 and 2.02687. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=21886.1 and stop= 24345.8 so gap is 2459.66, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 5 (24345.8) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5774.07 whereas forward=3300.45
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 5 (24345.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 27646.2 - 30118.4


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (21886.1 - 29105.5), exposure 3918.92
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.374644 bg counts (140), with cf=2.74139 and errBG= 0.0316632
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =40.0938 +/- 10.6177
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=21886.1 and stop= 29105.5 so gap is 7219.37, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (21886.1 - 29105.5), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16676.2 - 18571.7), exposure 1895.51
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.448529 bg counts (61), with cf=1.49478 and errBG= 0.0574283
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =41.1835 +/- 7.91012
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 25
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29105.5 - 30118.4), exposure 1012.94
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 3 counts and 0.183287 bg counts (46), with cf=1.64853 and errBG= 0.0270243
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =4.64344 +/- 2.85569
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (21886.1 - 30118.4), exposure 4931.86, 5 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.002662, 0.00638627 and 2.39905. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29105.5 and stop= 30118.4 so gap is 1012.94, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 6 (30118.4) and the bin is not full 3 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=1012.94 whereas forward=3266.67
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (21886.1 - 30118.4), exposure 4931.86
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 18 counts and 0.557932 bg counts (186), with cf=2.55925 and errBG= 0.0409095
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6385 +/- 10.8585
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 6 (30118.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (21886.1 - 30118.4), with lastBin= 0 and workMinC was 8
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 33385.1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 7
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 33385.1 - 35067.5


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (33385.1 - 35067.5), exposure 1682.4
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.129035 bg counts (63), with cf=2.6301 and errBG= 0.0162569
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.8111 +/- 5.88123
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (21886.1 - 35067.5), exposure 6614.26, 6 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00236169, 0.00632121 and 2.67656. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=33385.1 and stop= 35067.5 so gap is 1682.4, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 7 (35067.5) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=4949.07 whereas forward=4122.05
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 7 (35067.5) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 39189.5 - 40947.2


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (33385.1 - 40947.2), exposure 3440.02
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.317399 bg counts (129), with cf=1.94695 and errBG= 0.0279455
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.7455 +/- 6.74466
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (21886.1 - 40947.2), exposure 8371.87, 9 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00238451, 0.00566687 and 2.37653. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=33385.1 and stop= 40947.2 so gap is 7562.06, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 8 (40947.2) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=10828.7 whereas forward=5780.48
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 8 (40947.2) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 46727.6 - 46945.8


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (33385.1 - 46945.8), exposure 3658.15
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.373898 bg counts (137), with cf=1.82228 and errBG= 0.0319442
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.6528 +/- 7.05788
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (21886.1 - 46945.8), exposure 8590.01, 10 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00247681, 0.00582701 and 2.35263. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=33385.1 and stop= 46945.8 so gap is 13560.7, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 9 (46945.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (33385.1 - 46945.8), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (21886.1 - 30118.4), exposure 4931.86
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 18 counts and 0.557932 bg counts (186), with cf=2.55925 and errBG= 0.0409095
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.6385 +/- 10.8585
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 26
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 52487.8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 10
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 52487.8 - 52886.5


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52487.8 - 52886.5), exposure 398.661
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 3 counts and 0.182925 bg counts (24), with cf=1.2909 and errBG= 0.0373394
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =3.63655 +/- 2.23642
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (21886.1 - 52886.5), exposure 8988.67, 11 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00248148, 0.00584964 and 2.35732. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52487.8 and stop= 52886.5 so gap is 398.661, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 10 (52886.5) and the bin is not full 3 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5940.72 whereas forward=3593.5
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 10 (52886.5) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 56480 - 58987.3


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52487.8 - 58987.3), exposure 2905.96
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.745432 bg counts (164), with cf=2.75982 and errBG= 0.0582085
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.0606 +/- 9.56166
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (21886.1 - 58987.3), exposure 11496, 13 soft counts and 32 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00243678, 0.00648633 and 2.66184. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52487.8 and stop= 58987.3 so gap is 6499.46, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 11 (58987.3) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=12041.5 whereas forward=3260.43
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 11 (58987.3) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 62247.7 - 64759.5


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 14, last was 12 so increasing dead to 27.4618
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 14, last was 12 so increasing dead to 54.5977
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52487.8 - 62693.5), exposure 3297.1
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.47076 bg counts (309), with cf=2.48316 and errBG= 0.0836689
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.5953 +/- 9.61949
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52487.8 and stop= 62693.5 so gap is 10205.6, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (52487.8 - 62693.5), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (33385.1 - 46945.8), exposure 3658.15
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.373898 bg counts (137), with cf=1.82228 and errBG= 0.0319442
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.6528 +/- 7.05788
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 27
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 14
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (21886.1 - 63535.9), exposure 12729.6, 15 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00229206, 0.00627647 and 2.73836. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=62693.5 and stop= 63535.9 so gap is 842.461, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (21886.1 - 63535.9) = 21886.1- 63535.9
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (62693.5 - 64759.5), exposure 2066.02
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 1.06049 bg counts (212), with cf=1.3644 and errBG= 0.0728345
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.8326 +/- 4.0944
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (63535.9 - 64759.5), exposure 1223.55, 3 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00244217, 0.0032522 and 1.33168. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=62693.5 and stop= 64759.5 so gap is 2066.02, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 12 (64759.5) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=2066.02 whereas forward=3293.37
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52487.8 - 64759.5), exposure 5363.11
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 2.53125 bg counts (521), with cf=2.06363 and errBG= 0.110896
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.3035 +/- 10.1122
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 12 (64759.5) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (21886.1 - 64759.5), exposure 13953.1, 18 soft counts and 39 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00228094, 0.00600967 and 2.63473. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (52487.8 - 64759.5), with lastBin= 0 and workMinC was 8
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 68052.8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 15
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (21886.1 - 64759.5) = 21886.1- 64759.5
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 68052.8 - 70530.4


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 10.6186
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 17.0625
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 23.5136
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 32.1376
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 38.7068
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 48.383
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 68.7287
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 81.5743
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 89.1148
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 95.5902
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 105.299
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 111.783
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 122.492
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 131.14
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 138.681
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 149.395
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 156.966
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 165.56
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 172.083
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 182.838
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 189.31
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 196.874
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 205.461
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 216.25
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 222.762
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 232.464
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 241.142
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 247.64
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 256.248
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 262.706
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 269.2
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 279.927
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 290.659
++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 49, last was 15 so increasing dead to 297.193
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68052.8 - 70530.4), exposure 1975.75
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 3 counts and 0.20412 bg counts (80), with cf=2.19509 and errBG= 0.0228214
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.13722 +/- 3.80235
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 70530.4), exposure 1975.75, 0 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of -5.94048e-05, 0.00323667 and -54.4849. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=68052.8 and stop= 70530.4 so gap is 2477.53, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 13 (70530.4) and the bin is not full 3 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5770.89 whereas forward=3302.17
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 13 (70530.4) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 73832.5 - 74547.1


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68052.8 - 74547.1), exposure 2690.33
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.262223 bg counts (102), with cf=1.87708 and errBG= 0.025964
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.7703 +/- 4.59815
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 74547.1), exposure 2690.33, 2 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00108795, 0.00292367 and 2.68733. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=68052.8 and stop= 74547.1 so gap is 6494.28, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 14 (74547.1) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=9787.65 whereas forward=1044.94
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 14 (74547.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 75592.1 - 76304.1


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68052.8 - 76304.1), exposure 3402.41
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.309057 bg counts (117), with cf=1.77209 and errBG= 0.0285723
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =13.6291 +/- 5.01249
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 76304.1), exposure 3402.41, 4 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00171071, 0.00229502 and 1.34156. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=68052.8 and stop= 76304.1 so gap is 8251.3, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 15 (76304.1) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=11544.7 whereas forward=3299.73
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 15 (76304.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 79603.9 - 82076.1


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68052.8 - 81474.3), exposure 5272.87
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.440191 bg counts (159), with cf=1.65994 and errBG= 0.0349094
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1684 +/- 6.42918
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=68052.8 and stop= 81474.3 so gap is 13421.5, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (68052.8 - 81474.3), with lastBin= 0x1ec1950 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52487.8 - 64759.5), exposure 5363.11
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 2.53125 bg counts (521), with cf=2.06363 and errBG= 0.110896
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =44.3035 +/- 10.1122
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 28
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 74
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (81474.3 - 82076.1), exposure 601.737
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0468336 bg counts (15), with cf=1.52438 and errBG= 0.0120924
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.45298 +/- 1.52449
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 82076.1), exposure 5874.6, 8 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00202062, 0.00233853 and 1.15733. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=81474.3 and stop= 82076.1 so gap is 601.737, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 16 (82076.1) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=601.737 whereas forward=3303.67
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68052.8 - 82076.1), exposure 5874.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.487024 bg counts (174), with cf=1.65147 and errBG= 0.0369212
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.6192 +/- 6.60615
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 16 (82076.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (68052.8 - 82076.1), with lastBin= 0 and workMinC was 7
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 85379.7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 75
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 85379.7 - 87848.7


++tructures/grbBin.cpp::        binData:  line  187  INFO   >>  This GTI bin= 76, last was 75 so increasing dead to 26.8886
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85379.7 - 87848.7), exposure 2442.11
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 5 counts and 0.21079 bg counts (68), with cf=1.45244 and errBG= 0.0255621
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.95604 +/- 3.24797
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 87848.7), exposure 8316.71, 10 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00176195, 0.0021524 and 1.2216. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=85379.7 and stop= 87848.7 so gap is 2469, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 17 (87848.7) and the bin is not full 5 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=5772.67 whereas forward=3308.43
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 17 (87848.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 91157.2 - 93623.2


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 96929.1 - 98110.1 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85379.7 - 98110.1), exposure 6082.71
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.431753 bg counts (189), with cf=1.94755 and errBG= 0.0314054
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.7395 +/- 5.50883
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 98110.1), exposure 11957.3, 10 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00121689, 0.00215988 and 1.77492. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=85379.7 and stop= 98110.1 so gap is 12730.3, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 19 (98110.1) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 16 counts, because gotBinThisOrb=0 and gapBack=16034 whereas forward=45346.3
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68052.8 - 98110.1), exposure 11957.3
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.918777 bg counts (363), with cf=1.75016 and errBG= 0.0482233
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =40.3958 +/- 8.57441
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 19 (98110.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (68052.8 - 98110.1), with lastBin= 0 and workMinC was 7
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 143456
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec1950 which has initial GTIBin: 80
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 143456 - 144926


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 144926), exposure 1469.28
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 3 counts and 0.153817 bg counts (58), with cf=1.61104 and errBG= 0.0201971
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =4.58533 +/- 2.7906
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 144926), exposure 13426.6, 12 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00131802, 0.00202944 and 1.53976. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 144926 so gap is 1469.28, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 20 (144926) and the bin is not full 3 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=46815.6 whereas forward=15870.9
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 20 (144926) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 160797 - 162085


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 166602 - 167786 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 167786), exposure 3941.48
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.285489 bg counts (140), with cf=1.68858 and errBG= 0.0241282
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.27225 +/- 3.37741
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 167786), exposure 15898.8, 12 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00110938, 0.0018235 and 1.64371. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 167786 so gap is 24329.4, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 22 (167786) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=69675.7 whereas forward=10396.8
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 22 (167786) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 178183 - 179547


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 179547), exposure 5305.45
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.329532 bg counts (181), with cf=1.68858 and errBG= 0.024494
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.19788 +/- 3.37741
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 179547), exposure 17262.8, 12 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00102021, 0.00167646 and 1.64326. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 179547 so gap is 36090.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 23 (179547) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=81436.5 whereas forward=4414.47
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 23 (179547) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 183961 - 185365


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 185365), exposure 6709.53
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.356858 bg counts (218), with cf=1.68858 and errBG= 0.0241695
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.15174 +/- 3.37741
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 185365), exposure 18666.8, 12 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000942865, 0.00154833 and 1.64215. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 185365 so gap is 41908.7, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 24 (185365) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=87255 whereas forward=4363.88
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 24 (185365) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 189729 - 191246


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 191246), exposure 8226.45
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.464908 bg counts (252), with cf=1.5884 and errBG= 0.0292865
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.3803 +/- 4.20276
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 191246), exposure 20183.8, 12 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000869843, 0.00164386 and 1.88983. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 191246 so gap is 47789.5, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 25 (191246) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=93135.8 whereas forward=4277.52
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 25 (191246) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 195523 - 196406


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 196406), exposure 9109.02
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.54608 bg counts (283), with cf=1.58548 and errBG= 0.0324611
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.8181 +/- 4.48472
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 196406), exposure 21066.3, 12 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000831127, 0.00164556 and 1.97991. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 196406 so gap is 52949.6, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 26 (196406) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=98295.9 whereas forward=16396.2
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 26 (196406) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 212802 - 214166


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 218611 - 220105 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 220105), exposure 11967.3
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.63232 bg counts (377), with cf=1.58548 and errBG= 0.0325662
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.6813 +/- 4.48472
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 220105), exposure 23924.7, 12 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000730555, 0.00144392 and 1.97647. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 220105 so gap is 76648.6, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 28 (220105) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=121995 whereas forward=10061.6
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 28 (220105) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 230167 - 230906


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 230906), exposure 12707
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.643391 bg counts (400), with cf=1.58548 and errBG= 0.0321696
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.6638 +/- 4.48472
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 230906), exposure 24664.3, 12 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000708439, 0.00140005 and 1.97625. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 230906 so gap is 87449.9, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 29 (230906) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=132796 whereas forward=5056.33
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 29 (230906) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 235963 - 236667


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 236667), exposure 13411.5
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 8 counts and 0.667033 bg counts (422), with cf=1.58548 and errBG= 0.0324707
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =11.6263 +/- 4.48472
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 236667), exposure 25368.9, 12 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000688182, 0.00136017 and 1.97647. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 236667 so gap is 93210.8, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 30 (236667) and the bin is not full 8 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=138557 whereas forward=5055.88
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 30 (236667) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 241723 - 243147


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 243147), exposure 14835.7
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.780934 bg counts (459), with cf=1.55824 and errBG= 0.0364509
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.3655 +/- 4.92791
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 243147), exposure 26793, 13 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000704938, 0.00133606 and 1.89528. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 243147 so gap is 99690.8, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 31 (243147) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=145037 whereas forward=4335.05
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 31 (243147) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 247482 - 249027


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 249027), exposure 16380.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 0.877227 bg counts (505), with cf=1.77742 and errBG= 0.0390361
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7699 +/- 6.15757
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (68052.8 - 249027), exposure 28337.5, 15 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000863179, 0.00125978 and 1.45946. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 249027 so gap is 105570, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 32 (249027) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=150917 whereas forward=4276.24
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (68052.8 - 249027) = 68052.8- 249027
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 253303 - 254667


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 254667), exposure 17744.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 0.979575 bg counts (546), with cf=1.77086 and errBG= 0.041922
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.0573 +/- 6.62636
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (253303 - 254667), exposure 1363.97, 1 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00120574, 0.00120208 and 0.996961. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 254667 so gap is 111211, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 33 (254667) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=156557 whereas forward=4396.51
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 33 (254667) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 259063 - 260485


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 264851 - 266245 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 266245), exposure 20559.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.08274 bg counts (627), with cf=1.76505 and errBG= 0.0432405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.5646 +/- 6.83642
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (253303 - 266245), exposure 4179.67, 1 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000379889, 0.000767062 and 2.01917. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=143456 and stop= 266245 so gap is 122789, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 35 (266245) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (143456 - 266245), with lastBin= 0x1ec3420 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (68052.8 - 98110.1), exposure 11957.3
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.918777 bg counts (363), with cf=1.75016 and errBG= 0.0482233
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =40.3958 +/- 8.57441
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 29
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 276402
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 96
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 276402 - 276926


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (276402 - 276926), exposure 524.026
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0510455 bg counts (24), with cf=2.79215 and errBG= 0.0104196
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.64963 +/- 2.7923
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (253303 - 276926), exposure 4703.69, 1 soft counts and 3 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000332967, 0.00124754 and 3.74673. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=276402 and stop= 276926 so gap is 524.026, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 36 (276926) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=0 and gapBack=10680.8 whereas forward=17404.6
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 276926), exposure 21083.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 1.13379 bg counts (651), with cf=1.82924 and errBG= 0.0444366
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.1939 +/- 7.31741
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 36 (276926) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (143456 - 276926), with lastBin= 0 and workMinC was 6
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 294331
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ec3420 which has initial GTIBin: 97
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 294331 - 294807


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (294331 - 294807), exposure 476.387
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0471847 bg counts (17), with cf=1.52282 and errBG= 0.011444
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.45097 +/- 1.52292
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (253303 - 294807), exposure 5180.08, 1 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000295987, 0.00142124 and 4.8017. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=294331 and stop= 294807 so gap is 476.387, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 37 (294807) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=17881 whereas forward=4461.56
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 37 (294807) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 299269 - 299344


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  346  INFO   >>  Adding an empty orbit from 299413 - 300747 to this bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (294331 - 300747), exposure 1885.49
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0705532 bg counts (53), with cf=1.52282 and errBG= 0.00969123
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.41538 +/- 1.52289
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (253303 - 300747), exposure 6589.18, 1 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00023102, 0.00111233 and 4.81489. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=294331 and stop= 300747 so gap is 6416.18, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 39 (300747) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=23820.8 whereas forward=4335.18
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 39 (300747) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 305082 - 306747


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (294331 - 306747), exposure 3550.34
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.130094 bg counts (109), with cf=1.52282 and errBG= 0.0124607
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =1.32471 +/- 1.52294
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (253303 - 306747), exposure 8254.03, 1 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000180492, 0.000878472 and 4.8671. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=294331 and stop= 306747 so gap is 12416.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 40 (306747) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=29820.8 whereas forward=4056.53
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 40 (306747) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 310804 - 311187


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (294331 - 311187), exposure 3933.95
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.158834 bg counts (121), with cf=1.53296 and errBG= 0.0144395
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.82243 +/- 2.16804
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (253303 - 311187), exposure 8637.65, 1 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000169655, 0.00101745 and 5.99719. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=294331 and stop= 311187 so gap is 16856.4, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 41 (311187) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=34261 whereas forward=5475.39
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 41 (311187) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 316663 - 318325


++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (294331 - 318325), exposure 5596.29
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 4 counts and 0.287059 bg counts (178), with cf=1.77774 and errBG= 0.021516
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.60066 +/- 3.5557
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (253303 - 318325), exposure 10300, 2 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000317562, 0.00104482 and 3.29012. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=294331 and stop= 318325 so gap is 23994.1, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 42 (318325) and the bin is not full 4 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=41398.7 whereas forward=32808.1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 42 (318325) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  787  INFO   >>  I'm on the last event, so save the previous bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (143456 - 276926), exposure 21083.9
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 1.13379 bg counts (651), with cf=1.82924 and errBG= 0.0444366
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =27.1939 +/- 7.31741
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 30
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  903  INFO   >>  I have run out of background events
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x1ec3420
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (294331 - 380606), exposure 7822.78
++taStructures/bin.cpp::   bayesian_bin:  line  273  INFO   >>  Making a Bayesian bin - I have 4 counts and 0.359257 bg counts, with cf=1.77774
++taStructures/bin.cpp::   bayesian_bin:  line  274  INFO   >>    Therefore net =6.47277 + 4.27548 -3.04172 and sigma=3.41461
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 31
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (253303 - 318325), exposure 12526.5, 2 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000256151, 0.000853334 and 3.33137. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for PC mode.
++/genlc_cpp/genlc.cpp::           main:  line  397  INFO   >>  COMPLETE

