++lUtils/createLog.cpp::      createLog:  line   51  INFO   >>  Created FileAppender: 'genlc.log', level info
++/genlc_cpp/genlc.cpp::           main:  line  151  INFO   >>  Starting to run genlc.cpp, mode=0
++/genlc_cpp/genlc.cpp::           main:  line  152  INFO   >>  Argparsing reported: Selected GRB binning.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: WT, with files: wtsourcetotal.evt, wtbacktotal.evt, and wtcorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 85.7609 - 3000
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	85.7609 - 144.313
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - WT mode, suffix = 
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 30 ct/bin at rateFact=10 and binFact= 1.5 with minT 0.5 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file WTCURVE.qdp, reading from wtsourcetotal.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85.7609 - 89.8795), exposure 4.11866
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 1.69444 bg counts (2), with cf=1.10918 and errBG= 1.19815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.3959 +/- 6.21903
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=85.7609 and stop= 89.8795 so gap is 4.11866, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (85.7609 - 89.8795), with lastBin= 0 and workMinC was 30
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 94.2509), exposure 8.48997, 30 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.58732, 1.95969 and 0.546282. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 94.2509 so gap is 4.37131, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 94.3042), exposure 8.54334, 31 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.58474, 1.94745 and 0.54326. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 94.3042 so gap is 4.42468, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 94.6209), exposure 8.86002, 32 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.5818, 2.00303 and 0.559223. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 94.6209 so gap is 4.74136, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 94.8006), exposure 9.03971, 33 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.63331, 1.96321 and 0.540338. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 94.8006 so gap is 4.92105, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 94.8718), exposure 9.11088, 34 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.72667, 1.94788 and 0.522686. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 94.8718 so gap is 4.99221, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 95.3112), exposure 9.5503, 35 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.67134, 1.85825 and 0.506151. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 95.3112 so gap is 5.43164, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 95.5514), exposure 9.79048, 36 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.69457, 1.81267 and 0.49063. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 95.5514 so gap is 5.67182, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 95.7133), exposure 9.95238, 37 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.74591, 1.78318 and 0.476033. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 95.7133 so gap is 5.83372, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 96.368), exposure 10.6071, 37 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.33751, 1.68909 and 0.506094. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 96.368 so gap is 6.48844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 96.537), exposure 10.7761, 37 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.28516, 1.76553 and 0.537427. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 96.537 so gap is 6.65746, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 96.5673), exposure 10.8064, 37 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.27597, 1.86324 and 0.56876. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 96.5673 so gap is 6.6877, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 96.6811), exposure 10.9202, 38 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.34339, 1.84381 and 0.55148. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 96.6811 so gap is 6.80157, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 96.7558), exposure 10.995, 39 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.42155, 1.83128 and 0.53522. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 96.7558 so gap is 6.87629, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 97.2042), exposure 11.4433, 39 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.28749, 1.85646 and 0.564705. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 97.2042 so gap is 7.32463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (89.8795 - 97.2238), exposure 7.3442
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 4.23611 bg counts (5), with cf=1.10919 and errBG= 1.89445
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =28.5771 +/- 6.42856
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 97.2238), exposure 11.4629, 40 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.37865, 1.8533 and 0.548532. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=89.8795 and stop= 97.2238 so gap is 7.3442, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (89.8795 - 97.2238), with lastBin= 0x1ed81d0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85.7609 - 89.8795), exposure 4.11866
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 1.69444 bg counts (2), with cf=1.10918 and errBG= 1.19815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.3959 +/- 6.21903
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 97.6934), exposure 11.9326, 41 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.33862, 1.78035 and 0.533259. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 97.6934 so gap is 0.469692, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 97.7344), exposure 11.9735, 42 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.41985, 1.77426 and 0.518813. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 97.7344 so gap is 0.510612, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 97.8411), exposure 12.0802, 43 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.48145, 1.75858 and 0.50513. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 97.8411 so gap is 0.61736, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 98.4158), exposure 12.6549, 43 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.32336, 1.76638 and 0.531504. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 98.4158 so gap is 1.192, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 98.7805), exposure 13.0196, 44 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.31546, 1.64472 and 0.496076. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 98.7805 so gap is 1.55672, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 99.3089), exposure 13.548, 44 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.18615, 1.66245 and 0.521773. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 99.3089 so gap is 2.08512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 99.332), exposure 13.5711, 45 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.26245, 1.65961 and 0.508701. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 99.332 so gap is 2.10825, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 99.3925), exposure 13.6316, 46 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.32935, 1.65225 and 0.496268. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 99.3925 so gap is 2.16874, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 99.5295), exposure 13.7686, 47 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.37678, 1.63581 and 0.484428. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 99.5295 so gap is 2.30574, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 99.558), exposure 13.7971, 47 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.36982, 1.71283 and 0.508286. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 99.558 so gap is 2.3342, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 99.8319), exposure 14.0711, 48 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.38303, 1.67948 and 0.496442. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 99.8319 so gap is 2.60819, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 99.8391), exposure 14.0782, 49 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.46011, 1.67863 and 0.485137. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 99.8391 so gap is 2.61531, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 100.01), exposure 14.249, 50 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.49648, 1.65851 and 0.474336. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 100.01 so gap is 2.7861, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 100.054), exposure 14.2934, 51 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.56321, 1.65335 and 0.464006. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 100.054 so gap is 2.83058, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 101.689), exposure 15.9285, 52 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.26709, 1.48363 and 0.454115. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 101.689 so gap is 4.46561, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 102.173), exposure 16.4124, 52 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.17076, 1.50747 and 0.47543. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 102.173 so gap is 4.94952, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 102.339), exposure 16.5778, 53 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.20602, 1.49243 and 0.465508. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 102.339 so gap is 5.11498, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 102.49), exposure 16.7291, 54 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.24335, 1.47894 and 0.455991. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 102.49 so gap is 5.2662, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 102.908), exposure 17.1472, 54 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.16427, 1.50757 and 0.476435. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 102.908 so gap is 5.68429, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 103.365), exposure 17.6044, 55 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.14509, 1.46841 and 0.46689. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 103.365 so gap is 6.14153, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 104.203), exposure 18.4424, 56 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.06233, 1.40169 and 0.45772. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 104.203 so gap is 6.97949, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 104.23), exposure 18.469, 57 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.11797, 1.39967 and 0.448903. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 104.23 so gap is 7.00617, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 104.499), exposure 18.7377, 58 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.13246, 1.3796 and 0.44042. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 104.499 so gap is 7.27482, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 104.531), exposure 18.7697, 58 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.12712, 1.43634 and 0.459318. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 104.531 so gap is 7.30685, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 104.582), exposure 18.8213, 59 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.17748, 1.4324 and 0.450799. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 104.582 so gap is 7.35844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 104.671), exposure 18.9103, 59 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.16253, 1.48432 and 0.469346. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 104.671 so gap is 7.4474, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 104.995), exposure 19.2341, 60 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.16696, 1.45934 and 0.4608. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 104.995 so gap is 7.7712, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 105.641), exposure 19.8799, 61 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.11988, 1.41193 and 0.452559. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 105.641 so gap is 8.41702, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 105.648), exposure 19.887, 62 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.17454, 1.41142 and 0.444607. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 105.648 so gap is 8.42414, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (97.2238 - 105.732), exposure 8.50776
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.847222 bg counts (1), with cf=1.10923 and errBG= 0.847222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.3372 +/- 6.14795
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 105.732), exposure 19.9706, 63 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.21679, 1.40551 and 0.43693. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=97.2238 and stop= 105.732 so gap is 8.50776, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (97.2238 - 105.732), with lastBin= 0x1ed9780 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (89.8795 - 97.2238), exposure 7.3442
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 4.23611 bg counts (5), with cf=1.10919 and errBG= 1.89445
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =28.5771 +/- 6.42856
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 106.392), exposure 20.6307, 64 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.16764, 1.36054 and 0.429514. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=105.732 and stop= 106.392 so gap is 0.660052, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 106.422), exposure 20.6609, 65 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.21669, 1.35855 and 0.422345. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=105.732 and stop= 106.422 so gap is 0.690297, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 106.44), exposure 20.6787, 66 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.26756, 1.35738 and 0.415412. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=105.732 and stop= 106.44 so gap is 0.708088, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 106.735), exposure 20.974, 67 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.27444, 1.33827 and 0.408703. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=105.732 and stop= 106.735 so gap is 1.00342, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 107.085), exposure 21.3245, 67 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.17655, 1.3684 and 0.430783. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=105.732 and stop= 107.085 so gap is 1.3539, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 107.242), exposure 21.4811, 67 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.1534, 1.41018 and 0.447193. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=105.732 and stop= 107.242 so gap is 1.51046, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (85.7609 - 107.527), exposure 21.7657, 67 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.11216, 1.44281 and 0.463604. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=105.732 and stop= 107.527 so gap is 1.79512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (85.7609 - 107.527) = 85.7609- 107.527
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (105.732 - 112.184), exposure 6.45286
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.847222 bg counts (1), with cf=1.11142 and errBG= 0.847222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.401 +/- 6.1601
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=105.732 and stop= 112.184 so gap is 6.45286, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (105.732 - 112.184), with lastBin= 0x1ed81d0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (97.2238 - 105.732), exposure 8.50776
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.847222 bg counts (1), with cf=1.10923 and errBG= 0.847222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.3372 +/- 6.14795
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 115.429), exposure 7.90286, 30 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.10115, 1.68813 and 0.411625. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 115.429 so gap is 3.24512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 115.542), exposure 8.01493, 31 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.18252, 1.66453 and 0.397973. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 115.542 so gap is 3.35719, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 115.602), exposure 8.07542, 31 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.15119, 1.78973 and 0.431138. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 115.602 so gap is 3.41768, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 115.784), exposure 8.25689, 31 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.05995, 1.88505 and 0.464302. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 115.784 so gap is 3.59915, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 115.961), exposure 8.4348, 32 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.10612, 1.84528 and 0.449398. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 115.961 so gap is 3.77707, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 115.965), exposure 8.43836, 33 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.23614, 1.84451 and 0.435421. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 115.965 so gap is 3.78062, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 116.171), exposure 8.64474, 34 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.26362, 1.80047 and 0.422287. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 116.171 so gap is 3.987, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 116.449), exposure 8.92229, 34 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.13099, 1.86907 and 0.452451. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 116.449 so gap is 4.26455, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 116.506), exposure 8.97922, 34 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.1048, 1.98103 and 0.482614. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 116.506 so gap is 4.32148, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 116.607), exposure 9.08064, 35 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.18138, 1.95891 and 0.468483. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 116.607 so gap is 4.42291, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 116.723), exposure 9.19629, 35 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.1288, 2.05516 and 0.497763. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 116.723 so gap is 4.53855, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (112.184 - 116.762), exposure 4.57769
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.847222 bg counts (1), with cf=1.11176 and errBG= 0.847222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.4108 +/- 6.16197
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 116.762), exposure 9.23543, 36 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.23168, 2.04645 and 0.483603. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=112.184 and stop= 116.762 so gap is 4.57769, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (112.184 - 116.762), with lastBin= 0x1ed9780 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (105.732 - 112.184), exposure 6.45286
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.847222 bg counts (1), with cf=1.11142 and errBG= 0.847222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.401 +/- 6.1601
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 117.006), exposure 9.47917, 36 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.12287, 2.2284 and 0.540498. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 117.006 so gap is 0.243741, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 117.554), exposure 10.0271, 37 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.00843, 2.10662 and 0.525547. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 117.554 so gap is 0.791714, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 117.577), exposure 10.0503, 38 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.10983, 2.10177 and 0.511402. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 117.577 so gap is 0.814842, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 117.666), exposure 10.1392, 38 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.07378, 2.19309 and 0.538344. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 117.666 so gap is 0.903785, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 117.755), exposure 10.2282, 39 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.14715, 2.17402 and 0.524221. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 117.755 so gap is 0.992742, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 118.872), exposure 11.3454, 40 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.83683, 1.95993 and 0.510819. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 118.872 so gap is 2.11002, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 119.038), exposure 11.5109, 40 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.78168, 2.02843 and 0.536384. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 119.038 so gap is 2.27548, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 119.05), exposure 11.5234, 41 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.87416, 2.02624 and 0.523014. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 119.05 so gap is 2.28793, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 119.217), exposure 11.6906, 42 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.91393, 1.99725 and 0.510294. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 119.217 so gap is 2.45517, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 119.23), exposure 11.7031, 43 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 4.00485, 1.99513 and 0.498178. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 119.23 so gap is 2.46762, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 120.133), exposure 12.6069, 43 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.71774, 1.94037 and 0.521921. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 120.133 so gap is 3.37142, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 120.418), exposure 12.8915, 43 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.63565, 1.98385 and 0.545665. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 120.418 so gap is 3.65608, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 120.868), exposure 13.3416, 44 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.5964, 1.91691 and 0.53301. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 120.868 so gap is 4.1062, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 121.512), exposure 13.9857, 45 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.51035, 1.82864 and 0.520928. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 121.512 so gap is 4.75025, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 121.607), exposure 14.08, 45 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.48684, 1.89543 and 0.543595. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 121.607 so gap is 4.84454, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 121.637), exposure 14.1102, 46 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.55824, 1.89137 and 0.531547. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 121.637 so gap is 4.87479, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 122.302), exposure 14.7756, 47 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.47331, 1.80619 and 0.520021. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 122.302 so gap is 5.54018, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 122.509), exposure 14.982, 47 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.42547, 1.85559 and 0.541705. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 122.509 so gap is 5.74656, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 122.747), exposure 15.2204, 48 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.44493, 1.82653 and 0.530208. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 122.747 so gap is 5.98496, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 123.179), exposure 15.6527, 49 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.42088, 1.77608 and 0.519189. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 123.179 so gap is 6.41728, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 123.331), exposure 15.8039, 50 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.45856, 1.75908 and 0.508618. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 123.331 so gap is 6.56851, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 123.352), exposure 15.8253, 51 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.52421, 1.75671 and 0.49847. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 123.352 so gap is 6.58985, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 123.398), exposure 15.8715, 52 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.58405, 1.75159 and 0.488718. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 123.398 so gap is 6.63611, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 123.452), exposure 15.9249, 53 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.64192, 1.74572 and 0.479341. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 123.452 so gap is 6.68949, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 124.145), exposure 16.6188, 54 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.50013, 1.67283 and 0.477934. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 124.145 so gap is 7.38335, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 124.224), exposure 16.6971, 55 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.55037, 1.66499 and 0.468963. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 124.224 so gap is 7.46163, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 124.692), exposure 17.165, 56 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.51842, 1.6196 and 0.460321. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 124.692 so gap is 7.92954, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 124.813), exposure 17.286, 57 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.55817, 1.60827 and 0.451993. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 124.813 so gap is 8.05052, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (116.762 - 124.827), exposure 8.06476
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.847222 bg counts (1), with cf=1.1127 and errBG= 0.847222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.4382 +/- 6.1672
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 124.827), exposure 17.3002, 57 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.55524, 1.67127 and 0.470086. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=116.762 and stop= 124.827 so gap is 8.06476, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (116.762 - 124.827), with lastBin= 0x1ed81d0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (112.184 - 116.762), exposure 4.57769
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.847222 bg counts (1), with cf=1.11176 and errBG= 0.847222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.4108 +/- 6.16197
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 125.131), exposure 17.6044, 57 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.44028, 1.7056 and 0.495774. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=124.827 and stop= 125.131 so gap is 0.304232, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 125.138), exposure 17.6115, 58 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.50208, 1.70491 and 0.486829. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=124.827 and stop= 125.138 so gap is 0.311349, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 125.142), exposure 17.6151, 59 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.56455, 1.70457 and 0.478201. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=124.827 and stop= 125.142 so gap is 0.314907, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 125.329), exposure 17.8019, 60 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.58965, 1.68668 and 0.469873. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=124.827 and stop= 125.329 so gap is 0.501716, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 125.578), exposure 18.051, 61 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.60177, 1.66341 and 0.461831. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=124.827 and stop= 125.578 so gap is 0.750794, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 125.905), exposure 18.3783, 62 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.59816, 1.63378 and 0.454059. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=124.827 and stop= 125.905 so gap is 1.07815, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 125.987), exposure 18.4602, 62 soft counts and 28 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.58221, 1.68682 and 0.470888. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=124.827 and stop= 125.987 so gap is 1.15999, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 126.008), exposure 18.4815, 62 soft counts and 29 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.57807, 1.74508 and 0.487716. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=124.827 and stop= 126.008 so gap is 1.18134, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (107.527 - 126.106), exposure 18.5794, 62 soft counts and 30 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.55923, 1.79579 and 0.504545. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=124.827 and stop= 126.106 so gap is 1.2792, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (107.527 - 126.106) = 107.527- 126.106
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (124.827 - 132.463), exposure 7.63598
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 1.69444 bg counts (2), with cf=1.11286 and errBG= 1.19815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.5001 +/- 6.23973
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=124.827 and stop= 132.463 so gap is 7.63598, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (124.827 - 132.463), with lastBin= 0x1ed9780 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (116.762 - 124.827), exposure 8.06476
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 0.847222 bg counts (1), with cf=1.1127 and errBG= 0.847222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =32.4382 +/- 6.1672
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 138.231), exposure 12.1247, 30 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.28699, 1.74392 and 0.762539. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=132.463 and stop= 138.231 so gap is 5.76793, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 138.323), exposure 12.2172, 31 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.36076, 1.73071 and 0.733116. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=132.463 and stop= 138.323 so gap is 5.86044, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (132.463 - 138.336), exposure 5.87289
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 4.23611 bg counts (5), with cf=1.11288 and errBG= 1.89445
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =28.672 +/- 6.44996
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 138.336), exposure 12.2297, 31 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.35836, 1.81995 and 0.771702. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=132.463 and stop= 138.336 so gap is 5.87289, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (132.463 - 138.336), with lastBin= 0x1ed81d0 and workMinC was 30
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (124.827 - 132.463), exposure 7.63598
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 1.69444 bg counts (2), with cf=1.11286 and errBG= 1.19815
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.5001 +/- 6.23973
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 138.603), exposure 12.4965, 31 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.30799, 1.87014 and 0.810287. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 138.603 so gap is 0.266865, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 139.27), exposure 13.1637, 31 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.19102, 1.86004 and 0.848937. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 139.27 so gap is 0.93403, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 139.366), exposure 13.2598, 31 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.17515, 1.93063 and 0.887587. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 139.366 so gap is 1.0301, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 139.391), exposure 13.2847, 32 soft counts and 23 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.25496, 1.92701 and 0.854567. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 139.391 so gap is 1.05501, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 139.771), exposure 13.6654, 32 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.19213, 1.88589 and 0.860299. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 139.771 so gap is 1.43575, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 140.225), exposure 14.1191, 32 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.12169, 1.90424 and 0.897509. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 140.225 so gap is 1.88942, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 140.284), exposure 14.1778, 33 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.19151, 1.89635 and 0.865317. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 140.284 so gap is 1.94814, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 140.565), exposure 14.4589, 34 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.22599, 1.85949 and 0.835353. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 140.565 so gap is 2.22924, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 140.57), exposure 14.4643, 35 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.30222, 1.8588 and 0.807395. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 140.57 so gap is 2.23458, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 140.907), exposure 14.8005, 36 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.32521, 1.81657 and 0.781248. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 140.907 so gap is 2.57083, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 140.919), exposure 14.813, 37 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.3985, 1.81504 and 0.75674. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 140.919 so gap is 2.58329, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 141.841), exposure 15.7346, 38 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.32885, 1.70873 and 0.733724. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 141.841 so gap is 3.50488, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 142.39), exposure 16.2843, 38 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.25023, 1.7195 and 0.764144. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 142.39 so gap is 4.05463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 142.846), exposure 16.7398, 39 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.25559, 1.67271 and 0.741588. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 142.846 so gap is 4.51008, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 143.05), exposure 16.9444, 39 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.22835, 1.7183 and 0.77111. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 143.05 so gap is 4.71467, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 143.273), exposure 17.1667, 40 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.26441, 1.69604 and 0.749. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 143.273 so gap is 4.93706, and is Full=0 and tryBin= 0, endOrb=0
++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  286  INFO   >>  This is the last event, so we must call fullbin().
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (138.336 - 144.313), exposure 5.97711
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 0.847222 bg counts (1), with cf=1.11464 and errBG= 0.847222
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.0045 +/- 4.69188
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 144.313), exposure 18.2068, 41 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.19627, 1.59916 and 0.728123. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=138.336 and stop= 144.313 so gap is 5.97711, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (144.313) and the bin is not full 17 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  492  INFO   >>  Discarding leftover counts, as skip is set and I have no bin to carry back to
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 85.7609
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (144.313) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  787  INFO   >>  I'm on the last event, so save the previous bin
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (132.463 - 138.336), exposure 5.87289
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 30 counts and 4.23611 bg counts (5), with cf=1.11288 and errBG= 1.89445
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =28.672 +/- 6.44996
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x1ed81d0
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 85.7609 - 144.313
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 85.7609 - 144.313 the cf is 1.11151
++tructures/grbBin.cpp::        binData:  line  921  INFO   >>  This bin is empty, so found a emptyBin CF of 1.11151
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85.7609 - 144.313), exposure 58.5519
++taStructures/bin.cpp::        fullBin:  line  192  INFO   >>  Producing an upper limit of 6.57457 given bg=0 and numCts= 0
++tructures/grbBin.cpp::        binData:  line  929  INFO   >>  Not saving this bin as it is an incomplete WT one
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (126.106 - 144.313), exposure 18.2068, 41 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.19627, 1.59916 and 0.728123. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for WT mode.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: WT, with files: wtsourcetotal_incbad.evt, wtbacktotal_incbad.evt, and wtcorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 85.7609 - 3000
++/SourceEventList.cpp::SourceEventList:  line   67  FATAL  >>  Can't open file wtsourcetotal_incbad.evt
++/genlc_cpp/genlc.cpp::           main:  line  388  WARN   >>  Unable to open the files for this mode, skipping
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: PC, with files: pcsourcetotal.evt, pcbacktotal.evt, and pccorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 146.018 - 385384
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	146.018 - 1384.62
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	16646.4 - 18363.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	22348.6 - 23524.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	28134.2 - 29871.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	33831.6 - 35569.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	51902.8 - 53284.3
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	57563.6 - 59163.3
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - PC mode, suffix = 
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 20 ct/bin at rateFact=10 and binFact= 1.5 with minT 2.51 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file PCCURVE.qdp, reading from pcsourcetotal.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (146.018 - 171.091), exposure 25.0731
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.305075 bg counts (10), with cf=4.03613 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =95.6357 +/- 19.7767
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=146.018 and stop= 171.091 so gap is 25.0731, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (146.018 - 171.091), with lastBin= 0 and workMinC was 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 183.628), exposure 37.6097, 20 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.1223, 1.37022 and 0.645629. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 183.628 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 186.135), exposure 40.117, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.98659, 1.38557 and 0.697465. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 186.135 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 188.642), exposure 42.6243, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.86973, 1.39574 and 0.746492. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 188.642 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 191.149), exposure 45.1316, 23 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.02831, 1.40477 and 0.692583. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 191.149 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 193.657), exposure 47.6389, 25 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.08818, 1.41544 and 0.677836. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 193.657 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (171.091 - 196.164), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.366089 bg counts (12), with cf=4.04016 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =83.3642 +/- 18.5192
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 196.164), exposure 50.1463, 26 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.06414, 1.50542 and 0.729319. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 196.164 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (171.091 - 196.164), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (146.018 - 171.091), exposure 25.0731
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.305075 bg counts (10), with cf=4.03613 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =95.6357 +/- 19.7767
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 198.671), exposure 52.6536, 27 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.04241, 1.51029 and 0.739465. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=196.164 and stop= 198.671 so gap is 2.50726, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (146.018 - 198.671) = 146.018- 198.671
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (196.164 - 211.208), exposure 15.0438
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0610149 bg counts (2), with cf=4.03267 and errBG= 0.0431441
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.4073 +/- 18.0355
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=196.164 and stop= 211.208 so gap is 15.0438, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (196.164 - 211.208), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (171.091 - 196.164), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.366089 bg counts (12), with cf=4.04016 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =83.3642 +/- 18.5192
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 226.252), exposure 27.5805, 21 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.05103, 1.88437 and 0.617617. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=211.208 and stop= 226.252 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 233.774), exposure 35.1024, 22 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.5042, 1.48057 and 0.591237. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=211.208 and stop= 233.774 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 236.281), exposure 37.6097, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.33397, 1.49152 and 0.63905. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=211.208 and stop= 236.281 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (211.208 - 238.788), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.0507 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.6547 +/- 18.1199
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 238.788), exposure 40.1171, 23 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.28938, 1.49959 and 0.65502. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=211.208 and stop= 238.788 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (211.208 - 238.788), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (196.164 - 211.208), exposure 15.0438
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0610149 bg counts (2), with cf=4.03267 and errBG= 0.0431441
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.4073 +/- 18.0355
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 241.296), exposure 42.6243, 24 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.24715, 1.60204 and 0.712921. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=238.788 and stop= 241.296 so gap is 2.50728, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 243.803), exposure 45.1317, 26 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.30237, 1.60307 and 0.69627. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=238.788 and stop= 243.803 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 246.31), exposure 47.639, 27 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.26648, 1.68929 and 0.745334. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=238.788 and stop= 246.31 so gap is 7.52192, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (198.671 - 246.31) = 198.671- 246.31
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (238.788 - 258.847), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.09765 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.078 +/- 18.3282
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=238.788 and stop= 258.847 so gap is 20.0585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (238.788 - 258.847), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (211.208 - 238.788), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.0507 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.6547 +/- 18.1199
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (258.847 - 276.398), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.152537 bg counts (5), with cf=4.08161 and errBG= 0.0682167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.0096 +/- 18.2556
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=258.847 and stop= 276.398 so gap is 17.5512, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (258.847 - 276.398), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (238.788 - 258.847), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.09765 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.078 +/- 18.3282
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (246.31 - 291.442), exposure 45.1317, 22 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.97708, 1.96 and 0.991359. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=276.398 and stop= 291.442 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (246.31 - 291.442) = 246.31- 291.442
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (276.398 - 301.471), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.24406 bg counts (8), with cf=4.05155 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.0936 +/- 18.5698
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=276.398 and stop= 301.471 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (276.398 - 301.471), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (258.847 - 276.398), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.152537 bg counts (5), with cf=4.08161 and errBG= 0.0682167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.0096 +/- 18.2556
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301.471 - 326.544), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.03845 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =87.737 +/- 18.9456
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=301.471 and stop= 326.544 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (301.471 - 326.544), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (276.398 - 301.471), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.24406 bg counts (8), with cf=4.05155 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.0936 +/- 18.5698
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (291.442 - 339.081), exposure 47.639, 20 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.69369, 1.84803 and 1.09113. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=326.544 and stop= 339.081 so gap is 12.5365, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (291.442 - 339.081) = 291.442- 339.081
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (326.544 - 344.096), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.10645 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.6279 +/- 18.3663
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=326.544 and stop= 344.096 so gap is 17.5512, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (326.544 - 344.096), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301.471 - 326.544), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.03845 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =87.737 +/- 18.9456
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (344.096 - 384.213), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.396597 bg counts (13), with cf=4.0765 and errBG= 0.109996
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.2192 +/- 19.9757
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=344.096 and stop= 384.213 so gap is 40.1171, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (344.096 - 384.213), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (326.544 - 344.096), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.10645 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.6279 +/- 18.3663
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (339.081 - 389.227), exposure 50.1463, 21 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.68178, 1.61175 and 0.958363. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=384.213 and stop= 389.227 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (339.081 - 389.227) = 339.081- 389.227
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (384.213 - 404.271), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.305075 bg counts (10), with cf=4.03627 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =83.5302 +/- 18.5006
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=384.213 and stop= 404.271 so gap is 20.0585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (384.213 - 404.271), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (344.096 - 384.213), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.396597 bg counts (13), with cf=4.0765 and errBG= 0.109996
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.2192 +/- 19.9757
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 424.33), exposure 35.1024, 20 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.27374, 1.25137 and 0.550358. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=404.271 and stop= 424.33 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (404.271 - 426.837), exposure 22.5658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.0915224 bg counts (3), with cf=4.03837 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.5514 +/- 19.7851
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 426.837), exposure 37.6097, 24 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.54866, 1.27539 and 0.500415. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=404.271 and stop= 426.837 so gap is 22.5658, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (404.271 - 426.837), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (384.213 - 404.271), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.305075 bg counts (10), with cf=4.03627 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =83.5302 +/- 18.5006
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 429.344), exposure 40.117, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.38937, 1.29282 and 0.541072. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 429.344 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 431.852), exposure 42.6244, 24 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.24594, 1.31109 and 0.583761. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 431.852 so gap is 5.01464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 436.866), exposure 47.639, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.00952, 1.25231 and 0.623185. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 436.866 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 439.374), exposure 50.1463, 26 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.0735, 1.27191 and 0.613411. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 439.374 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 441.881), exposure 52.6536, 27 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.05307, 1.36795 and 0.666294. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 441.881 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 444.388), exposure 55.1609, 28 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.0345, 1.38051 and 0.678553. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 444.388 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 446.896), exposure 57.6683, 31 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.16055, 1.31835 and 0.61019. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 446.896 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 449.403), exposure 60.1756, 32 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.13985, 1.32861 and 0.62089. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 449.403 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (389.227 - 449.403) = 389.227- 449.403
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (426.837 - 454.418), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.12292 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5779 +/- 18.4413
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 454.418 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (426.837 - 454.418), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (404.271 - 426.837), exposure 22.5658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.0915224 bg counts (3), with cf=4.03837 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.5514 +/- 19.7851
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 12
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (454.418 - 479.491), exposure 25.0731
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.335582 bg counts (11), with cf=4.13624 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =93.7456 +/- 19.8411
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=454.418 and stop= 479.491 so gap is 25.0731, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (454.418 - 479.491), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (426.837 - 454.418), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.12292 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5779 +/- 18.4413
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 13
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (479.491 - 507.071), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.03797 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =87.7267 +/- 18.9434
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (449.403 - 507.071), exposure 57.6683, 22 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.53191, 1.90431 and 1.24309. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=479.491 and stop= 507.071 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (479.491 - 507.071), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (454.418 - 479.491), exposure 25.0731
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.335582 bg counts (11), with cf=4.13624 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =93.7456 +/- 19.8411
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 14
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (449.403 - 507.071) = 449.403- 507.071
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (507.071 - 537.159), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.183045 bg counts (6), with cf=4.04062 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.1134 +/- 18.5189
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=507.071 and stop= 537.159 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (507.071 - 537.159), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (479.491 - 507.071), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.03797 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =87.7267 +/- 18.9434
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 15
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (537.159 - 552.203), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.12819 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.0601 +/- 18.4636
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (507.071 - 552.203), exposure 45.1317, 20 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.79541, 1.8865 and 1.05074. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=537.159 and stop= 552.203 so gap is 15.0439, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (537.159 - 552.203), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (507.071 - 537.159), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.183045 bg counts (6), with cf=4.04062 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.1134 +/- 18.5189
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 16
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (507.071 - 552.203) = 507.071- 552.203
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (552.203 - 572.261), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.213552 bg counts (7), with cf=4.05293 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.4048 +/- 19.8579
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=552.203 and stop= 572.261 so gap is 20.0585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (552.203 - 572.261), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (537.159 - 552.203), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.12819 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.0601 +/- 18.4636
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 17
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (572.261 - 602.349), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0915224 bg counts (3), with cf=4.09421 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5094 +/- 18.3111
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (552.203 - 602.349), exposure 50.1463, 20 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.61144, 1.93643 and 1.20168. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=572.261 and stop= 602.349 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (572.261 - 602.349), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (552.203 - 572.261), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.213552 bg counts (7), with cf=4.05293 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.4048 +/- 19.8579
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 18
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (552.203 - 602.349) = 552.203- 602.349
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (602.349 - 629.93), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.24406 bg counts (8), with cf=4.08407 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.7687 +/- 18.7189
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=602.349 and stop= 629.93 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (602.349 - 629.93), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (572.261 - 602.349), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0915224 bg counts (3), with cf=4.09421 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5094 +/- 18.3111
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 19
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (629.93 - 660.017), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.05235 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.1815 +/- 18.1256
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=629.93 and stop= 660.017 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (629.93 - 660.017), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (602.349 - 629.93), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.24406 bg counts (8), with cf=4.08407 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.7687 +/- 18.7189
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (602.349 - 670.047), exposure 67.6975, 20 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.17261, 1.49342 and 1.27359. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=660.017 and stop= 670.047 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (602.349 - 670.047) = 602.349- 670.047
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (660.017 - 692.613), exposure 32.5951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.05249 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.6899 +/- 18.1279
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=660.017 and stop= 692.613 so gap is 32.5951, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (660.017 - 692.613), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (629.93 - 660.017), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.05235 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.1815 +/- 18.1256
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 21
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (692.613 - 717.686), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.24406 bg counts (8), with cf=4.07741 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.5532 +/- 18.2381
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=692.613 and stop= 717.686 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (692.613 - 717.686), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (660.017 - 692.613), exposure 32.5951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.05249 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.6899 +/- 18.1279
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 22
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (670.047 - 720.193), exposure 50.1463, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.60112, 1.44242 and 0.900883. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 720.193 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (670.047 - 722.7), exposure 52.6536, 21 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.59882, 1.45003 and 0.906938. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 722.7 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (670.047 - 725.208), exposure 55.1609, 24 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.74016, 1.38412 and 0.795401. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 725.208 so gap is 7.52192, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (670.047 - 727.715), exposure 57.6683, 26 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.80168, 1.32394 and 0.734837. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 727.715 so gap is 10.0292, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (670.047 - 730.222), exposure 60.1756, 28 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.85638, 1.39853 and 0.753366. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 730.222 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (670.047 - 730.222) = 670.047- 730.222
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (717.686 - 750.281), exposure 32.5951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.427104 bg counts (14), with cf=4.0067 and errBG= 0.114148
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =86.436 +/- 18.7986
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 750.281 so gap is 32.5951, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (717.686 - 750.281), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (692.613 - 717.686), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.24406 bg counts (8), with cf=4.07741 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.5532 +/- 18.2381
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 23
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (750.281 - 777.861), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.366089 bg counts (12), with cf=4.03446 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.2122 +/- 18.0477
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.281 and stop= 777.861 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (750.281 - 777.861), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (717.686 - 750.281), exposure 32.5951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.427104 bg counts (14), with cf=4.0067 and errBG= 0.114148
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =86.436 +/- 18.7986
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 24
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (730.222 - 797.92), exposure 67.6976, 20 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.17889, 1.54963 and 1.31448. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=777.861 and stop= 797.92 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (730.222 - 797.92) = 730.222- 797.92
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (777.861 - 805.442), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.274567 bg counts (9), with cf=4.17603 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.3741 +/- 18.6797
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=777.861 and stop= 805.442 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (777.861 - 805.442), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (750.281 - 777.861), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.366089 bg counts (12), with cf=4.03446 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.2122 +/- 18.0477
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 25
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (805.442 - 835.53), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.152537 bg counts (5), with cf=4.12042 and errBG= 0.0682167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.7799 +/- 18.4292
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=805.442 and stop= 835.53 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (805.442 - 835.53), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (777.861 - 805.442), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.274567 bg counts (9), with cf=4.17603 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.3741 +/- 18.6797
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 26
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (797.92 - 863.11), exposure 65.1902, 20 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.2466, 1.32173 and 1.06027. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=835.53 and stop= 863.11 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (797.92 - 863.11) = 797.92- 863.11
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (835.53 - 865.617), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.10287 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5568 +/- 18.3503
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=835.53 and stop= 865.617 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (835.53 - 865.617), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (805.442 - 835.53), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.152537 bg counts (5), with cf=4.12042 and errBG= 0.0682167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.7799 +/- 18.4292
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 27
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (865.617 - 900.72), exposure 35.1024
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.305075 bg counts (10), with cf=4.14781 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.6908 +/- 18.5539
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=865.617 and stop= 900.72 so gap is 35.1024, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (865.617 - 900.72), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (835.53 - 865.617), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.10287 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5568 +/- 18.3503
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 28
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 918.271), exposure 55.161, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.48411, 1.33041 and 0.896437. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=900.72 and stop= 918.271 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 920.778), exposure 57.6683, 20 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.41959, 1.34452 and 0.947118. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=900.72 and stop= 920.778 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 923.286), exposure 60.1756, 21 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.42098, 1.2885 and 0.906768. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=900.72 and stop= 923.286 so gap is 22.5659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (900.72 - 925.793), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.396597 bg counts (13), with cf=4.14359 and errBG= 0.109996
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.2285 +/- 18.5363
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 925.793), exposure 62.6829, 23 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.49451, 1.23294 and 0.824979. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=900.72 and stop= 925.793 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (900.72 - 925.793), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (865.617 - 900.72), exposure 35.1024
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.305075 bg counts (10), with cf=4.14781 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.6908 +/- 18.5539
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 29
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 928.3), exposure 65.1902, 25 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.56044, 1.18552 and 0.759731. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=925.793 and stop= 928.3 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 930.808), exposure 67.6976, 26 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.55817, 1.31746 and 0.845522. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=925.793 and stop= 930.808 so gap is 5.01464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (863.11 - 930.808) = 863.11- 930.808
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (925.793 - 948.359), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.183045 bg counts (6), with cf=4.08604 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.9729 +/- 18.2759
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=925.793 and stop= 948.359 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (925.793 - 948.359), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (900.72 - 925.793), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.396597 bg counts (13), with cf=4.14359 and errBG= 0.109996
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.2285 +/- 18.5363
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 30
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (948.359 - 975.939), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.183045 bg counts (6), with cf=4.0862 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =85.0623 +/- 18.7278
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 975.939), exposure 45.1317, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.79952, 1.35401 and 0.752427. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=948.359 and stop= 975.939 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (948.359 - 975.939), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (925.793 - 948.359), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.183045 bg counts (6), with cf=4.08604 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.9729 +/- 18.2759
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 31
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 978.447), exposure 47.639, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.03962, 1.28274 and 0.628912. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 978.447 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 980.954), exposure 50.1463, 25 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.0176, 1.29856 and 0.643617. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 980.954 so gap is 5.01464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 983.461), exposure 52.6537, 25 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.92152, 1.31287 and 0.683245. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 983.461 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 985.969), exposure 55.161, 25 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.83193, 1.32588 and 0.723761. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 985.969 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 988.476), exposure 57.6683, 26 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.82181, 1.26823 and 0.696139. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 988.476 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 990.983), exposure 60.1756, 27 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.81306, 1.34972 and 0.744441. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 990.983 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (930.808 - 990.983) = 930.808- 990.983
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (975.939 - 1003.52), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.02932 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.7259 +/- 18.0226
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 1003.52 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (975.939 - 1003.52), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (948.359 - 975.939), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.183045 bg counts (6), with cf=4.0862 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =85.0623 +/- 18.7278
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 32
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1018.56), exposure 27.5805, 20 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.9394, 0.712915 and 0.242537. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1003.52 and stop= 1018.56 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1021.07), exposure 30.0878, 21 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.82838, 0.653505 and 0.231052. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1003.52 and stop= 1021.07 so gap is 17.5513, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1023.58), exposure 32.5951, 22 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.73445, 0.603235 and 0.220606. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1003.52 and stop= 1023.58 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1003.52 - 1026.09), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.24406 bg counts (8), with cf=4.08665 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =88.9088 +/- 19.1713
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1026.09), exposure 35.1025, 24 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.76517, 0.671437 and 0.242819. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1003.52 and stop= 1026.09 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1003.52 - 1026.09), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (975.939 - 1003.52), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.02932 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.7259 +/- 18.0226
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 33
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1028.59), exposure 37.6098, 25 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.68797, 0.626675 and 0.23314. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1028.59 so gap is 2.5073, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1031.1), exposure 40.1171, 27 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.72086, 0.684883 and 0.251715. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1031.1 so gap is 5.01462, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1036.11), exposure 45.1317, 27 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.41854, 0.78738 and 0.325559. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1036.11 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1038.62), exposure 47.639, 28 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.37584, 0.745939 and 0.313969. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1038.62 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1041.13), exposure 50.1464, 29 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.33781, 1.03171 and 0.441313. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1041.13 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1046.14), exposure 55.161, 30 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.19871, 1.08252 and 0.492342. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1046.14 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1048.65), exposure 57.6683, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.10096, 1.10568 and 0.526275. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1048.65 so gap is 22.5659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1026.09 - 1051.16), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0915224 bg counts (3), with cf=4.03453 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.3213 +/- 18.0442
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1051.16), exposure 60.1756, 31 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.08005, 1.25952 and 0.605524. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1051.16 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1026.09 - 1051.16), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1003.52 - 1026.09), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.24406 bg counts (8), with cf=4.08665 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =88.9088 +/- 19.1713
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 34
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1056.17), exposure 65.1903, 32 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.98155, 1.16263 and 0.586728. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1051.16 and stop= 1056.17 so gap is 5.01464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1058.68), exposure 67.6976, 32 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.90816, 1.1788 and 0.617769. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1051.16 and stop= 1058.68 so gap is 7.52194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (990.983 - 1058.68) = 990.983- 1058.68
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1051.16 - 1093.78), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.457612 bg counts (15), with cf=4.02174 and errBG= 0.118155
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.6162 +/- 18.4361
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1051.16 and stop= 1093.78 so gap is 42.6244, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1051.16 - 1093.78), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1026.09 - 1051.16), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0915224 bg counts (3), with cf=4.03453 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.3213 +/- 18.0442
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 35
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1093.78 - 1128.89), exposure 35.1025
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.366089 bg counts (12), with cf=4.11888 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.8696 +/- 18.4253
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1093.78 and stop= 1128.89 so gap is 35.1025, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1093.78 - 1128.89), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1051.16 - 1093.78), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.457612 bg counts (15), with cf=4.02174 and errBG= 0.118155
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.6162 +/- 18.4361
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 36
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1058.68 - 1131.39), exposure 72.7122, 21 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.13669, 1.11576 and 0.98159. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1128.89 and stop= 1131.39 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1058.68 - 1131.39) = 1058.68- 1131.39
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1128.89 - 1166.5), exposure 37.6098
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.366089 bg counts (12), with cf=4.10917 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.7883 +/- 18.8356
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1128.89 and stop= 1166.5 so gap is 37.6098, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1128.89 - 1166.5), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1093.78 - 1128.89), exposure 35.1025
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.366089 bg counts (12), with cf=4.11888 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.8696 +/- 18.4253
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 37
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1166.5 - 1201.6), exposure 35.1025
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.24406 bg counts (8), with cf=4.09715 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =89.1373 +/- 19.2206
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1166.5 and stop= 1201.6 so gap is 35.1025, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1166.5 - 1201.6), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1128.89 - 1166.5), exposure 37.6098
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.366089 bg counts (12), with cf=4.10917 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.7883 +/- 18.8356
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 38
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1131.39 - 1211.63), exposure 80.2342, 20 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.00927, 1.20586 and 1.19478. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1201.6 and stop= 1211.63 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1131.39 - 1211.63) = 1131.39- 1211.63
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1201.6 - 1251.74), exposure 50.1464
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.549134 bg counts (18), with cf=4.12213 and errBG= 0.129432
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.179 +/- 18.4424
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1201.6 and stop= 1251.74 so gap is 50.1464, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1201.6 - 1251.74), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1166.5 - 1201.6), exposure 35.1025
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.24406 bg counts (8), with cf=4.09715 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =89.1373 +/- 19.2206
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 39
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1251.74 - 1284.34), exposure 32.5952
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.06173 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =88.2429 +/- 19.0548
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1251.74 and stop= 1284.34 so gap is 32.5952, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1251.74 - 1284.34), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1201.6 - 1251.74), exposure 50.1464
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.549134 bg counts (18), with cf=4.12213 and errBG= 0.129432
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.179 +/- 18.4424
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 40
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1211.63 - 1286.85), exposure 75.2196, 21 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.12375, 1.11762 and 0.994538. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1284.34 and stop= 1286.85 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1211.63 - 1286.85) = 1211.63- 1286.85
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1284.34 - 1324.46), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.15197 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.646 +/- 18.5729
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1284.34 and stop= 1324.46 so gap is 40.1171, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1284.34 - 1324.46), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1251.74 - 1284.34), exposure 32.5952
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.06173 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =88.2429 +/- 19.0548
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 41
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1286.85 - 1372.1), exposure 85.2489, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.94478, 0.666911 and 0.70589. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1324.46 and stop= 1372.1 so gap is 47.6391, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1286.85 - 1374.6), exposure 87.7562, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.917786, 0.693544 and 0.755671. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1324.46 and stop= 1374.6 so gap is 50.1464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1286.85 - 1379.62), exposure 92.7708, 21 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.911396, 0.656056 and 0.719836. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1324.46 and stop= 1379.62 so gap is 55.161, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1324.46 - 1382.12), exposure 57.6684
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.427104 bg counts (14), with cf=4.09742 and errBG= 0.114148
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.1984 +/- 18.3302
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1286.85 - 1382.12), exposure 95.2781, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.930926, 0.638791 and 0.686189. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1324.46 and stop= 1382.12 so gap is 57.6684, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1324.46 - 1382.12), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1284.34 - 1324.46), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.15197 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.646 +/- 18.5729
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 42
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1382.12 - 1384.62), exposure 2.49908
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0305075 bg counts (1), with cf=4.14651 and errBG= 0.0305075
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =4.02001 +/- 4.14844
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1286.85 - 1384.62), exposure 97.7772, 23 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.948249, 0.622464 and 0.656435. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1382.12 and stop= 1384.62 so gap is 2.49908, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (1384.62) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=2.49908 whereas forward=15261.8
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1324.46 - 1384.62), exposure 60.1674
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.457612 bg counts (15), with cf=4.09976 and errBG= 0.118155
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.2189 +/- 18.7937
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (1384.62) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1211.63 - 1384.62), exposure 172.997, 44 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.02457, 0.837751 and 0.817662. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1324.46 - 1384.62), with lastBin= 0 and workMinC was 21
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 16646.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1211.63 - 1384.62) = 1211.63- 1384.62
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 16646.4 - 18363.9


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16646.4 - 16809.4), exposure 162.975
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.787668 bg counts (38), with cf=1.31218 and errBG= 0.127777
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.21 +/- 5.87063
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16646.4 and stop= 16809.4 so gap is 162.975, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16646.4 - 16809.4), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1324.46 - 1384.62), exposure 60.1674
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.457612 bg counts (15), with cf=4.09976 and errBG= 0.118155
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.2189 +/- 18.7937
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 43
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16949.8), exposure 303.385, 20 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.082571, 0.0538391 and 0.652034. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16949.8 so gap is 140.41, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16952.3), exposure 305.892, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0818942, 0.0575819 and 0.703125. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16952.3 so gap is 142.917, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16954.8), exposure 308.4, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0812284, 0.0613514 and 0.755295. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16954.8 so gap is 145.424, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16957.3), exposure 310.907, 21 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0846907, 0.0608566 and 0.718575. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16957.3 so gap is 147.932, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16972.3), exposure 325.951, 21 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0807819, 0.0620071 and 0.767587. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16972.3 so gap is 162.975, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16979.9), exposure 333.473, 21 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0789598, 0.0644468 and 0.816198. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16979.9 so gap is 170.497, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17012.5), exposure 366.068, 22 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0753778, 0.0585609 and 0.776899. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 17012.5 so gap is 203.092, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16809.4 - 17015), exposure 205.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.787668 bg counts (38), with cf=1.30851 and errBG= 0.127777
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.1395 +/- 5.85422
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17015), exposure 368.575, 23 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0784383, 0.0581626 and 0.741508. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 17015 so gap is 205.6, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16809.4 - 17015), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16646.4 - 16809.4), exposure 162.975
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.787668 bg counts (38), with cf=1.31218 and errBG= 0.127777
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.21 +/- 5.87063
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 44
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17022.5), exposure 376.097, 23 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0768695, 0.0605594 and 0.787821. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17015 and stop= 17022.5 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17025), exposure 378.605, 24 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0798972, 0.0600869 and 0.752053. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17015 and stop= 17025 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17027.5), exposure 381.112, 24 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0793716, 0.0632051 and 0.796319. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17015 and stop= 17027.5 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17030), exposure 383.619, 24 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0788528, 0.0661367 and 0.838736. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17015 and stop= 17030 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (16646.4 - 17030) = 16646.4- 17030
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17015 - 17145.4), exposure 130.38
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.663299 bg counts (32), with cf=1.31056 and errBG= 0.117256
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.6524 +/- 6.00769
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17015 and stop= 17145.4 so gap is 130.38, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17015 - 17145.4), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16809.4 - 17015), exposure 205.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.787668 bg counts (38), with cf=1.30851 and errBG= 0.127777
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.1395 +/- 5.85422
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 45
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17275.7), exposure 245.717, 20 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.102698, 0.0659893 and 0.642556. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17145.4 and stop= 17275.7 so gap is 130.38, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17278.2), exposure 248.224, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.101661, 0.0704425 and 0.692918. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17145.4 and stop= 17278.2 so gap is 132.888, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17283.3), exposure 253.239, 21 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.104811, 0.0690476 and 0.658783. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17145.4 and stop= 17283.3 so gap is 137.902, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17285.8), exposure 255.746, 21 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.103783, 0.0734831 and 0.708043. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17145.4 and stop= 17285.8 so gap is 140.41, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17145.4 - 17288.3), exposure 142.917
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.663299 bg counts (32), with cf=1.30649 and errBG= 0.117256
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.2632 +/- 5.84481
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17288.3), exposure 258.253, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.107839, 0.0727697 and 0.674801. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17145.4 and stop= 17288.3 so gap is 142.917, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17145.4 - 17288.3), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17015 - 17145.4), exposure 130.38
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.663299 bg counts (32), with cf=1.31056 and errBG= 0.117256
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.6524 +/- 6.00769
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 46
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17335.9), exposure 305.892, 22 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0903359, 0.0653787 and 0.723728. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17288.3 and stop= 17335.9 so gap is 47.6389, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17030 - 17335.9) = 17030- 17335.9
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17288.3 - 17488.9), exposure 200.585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.07786 bg counts (52), with cf=1.31154 and errBG= 0.149472
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.2595 +/- 5.08336
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17288.3 and stop= 17488.9 so gap is 200.585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17288.3 - 17488.9), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17145.4 - 17288.3), exposure 142.917
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.663299 bg counts (32), with cf=1.30649 and errBG= 0.117256
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.2632 +/- 5.84481
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 47
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17649.3), exposure 313.414, 20 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0798929, 0.0483778 and 0.605533. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17488.9 and stop= 17649.3 so gap is 160.468, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17661.9), exposure 325.951, 20 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0766532, 0.050529 and 0.65919. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17488.9 and stop= 17661.9 so gap is 173.005, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17488.9 - 17666.9), exposure 178.019
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.559659 bg counts (27), with cf=1.31127 and errBG= 0.107706
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.4915 +/- 5.86588
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17666.9), exposure 330.965, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0754918, 0.0537145 and 0.711528. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17488.9 and stop= 17666.9 so gap is 178.019, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17488.9 - 17666.9), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17288.3 - 17488.9), exposure 200.585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.07786 bg counts (52), with cf=1.31154 and errBG= 0.149472
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.2595 +/- 5.08336
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 48
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17671.9), exposure 335.98, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0743651, 0.0568244 and 0.764127. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17671.9 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17679.4), exposure 343.502, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0803093, 0.0555801 and 0.692075. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17679.4 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17686.9), exposure 351.024, 23 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0823161, 0.0543891 and 0.660735. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17686.9 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17694.5), exposure 358.546, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0842609, 0.0530965 and 0.630144. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17694.5 so gap is 27.5804, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17714.5), exposure 378.604, 25 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0829831, 0.0501399 and 0.604218. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17714.5 so gap is 47.6389, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17717), exposure 381.112, 26 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.085888, 0.04981 and 0.579942. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17717 so gap is 50.1463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17752.1), exposure 416.214, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0815392, 0.0483083 and 0.592455. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17752.1 so gap is 85.2486, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17767.2), exposure 431.258, 27 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0785687, 0.0495972 and 0.63126. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17767.2 so gap is 100.293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17769.7), exposure 433.765, 28 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0811343, 0.0492479 and 0.606993. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17769.7 so gap is 102.8, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17809.8), exposure 473.882, 29 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0765821, 0.0449067 and 0.586387. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17809.8 so gap is 142.917, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17814.8), exposure 478.897, 29 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0757802, 0.047232 and 0.623277. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17814.8 so gap is 147.931, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17824.8), exposure 488.926, 29 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0742257, 0.048935 and 0.659273. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17824.8 so gap is 157.961, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17827.3), exposure 491.433, 30 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0764498, 0.0486853 and 0.636827. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17827.3 so gap is 160.468, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17834.9), exposure 498.955, 30 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0751883, 0.0505865 and 0.672798. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17834.9 so gap is 167.99, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17335.9 - 17834.9) = 17335.9- 17834.9
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17666.9 - 17875), exposure 208.107
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.994949 bg counts (48), with cf=1.31443 and errBG= 0.143609
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.9808 +/- 5.88133
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17875 so gap is 208.107, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17666.9 - 17875), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17488.9 - 17666.9), exposure 178.019
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.559659 bg counts (27), with cf=1.31127 and errBG= 0.107706
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.4915 +/- 5.86588
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 49
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17875 - 18012.9), exposure 137.902
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.704756 bg counts (34), with cf=1.31079 and errBG= 0.120865
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.2919 +/- 5.86415
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17875 and stop= 18012.9 so gap is 137.902, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17875 - 18012.9), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17666.9 - 17875), exposure 208.107
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.994949 bg counts (48), with cf=1.31443 and errBG= 0.143609
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.9808 +/- 5.88133
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 50
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18103.1), exposure 268.283, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0934452, 0.0665542 and 0.712228. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18103.1 so gap is 90.2634, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18168.3), exposure 333.473, 21 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0784728, 0.0528911 and 0.674005. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18168.3 so gap is 155.454, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18170.8), exposure 335.98, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0818858, 0.0524963 and 0.641092. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18170.8 so gap is 157.961, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18173.4), exposure 338.488, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0811184, 0.0559831 and 0.690141. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18173.4 so gap is 160.468, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18178.4), exposure 343.502, 22 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0799342, 0.0589848 and 0.737918. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18178.4 so gap is 165.483, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18183.4), exposure 348.517, 23 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0825377, 0.0581361 and 0.704359. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18183.4 so gap is 170.497, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18185.9), exposure 351.024, 24 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0855198, 0.0577209 and 0.674941. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18185.9 so gap is 173.005, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18195.9), exposure 361.053, 24 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0831443, 0.059744 and 0.718559. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18195.9 so gap is 183.034, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18208.5), exposure 373.59, 24 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0802085, 0.0610939 and 0.761688. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18208.5 so gap is 195.571, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18213.5), exposure 378.605, 25 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0826013, 0.0602847 and 0.729827. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18213.5 so gap is 200.585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18012.9 - 18216), exposure 203.093
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.87058 bg counts (42), with cf=1.31343 and errBG= 0.134333
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.1252 +/- 5.8765
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18216), exposure 381.112, 26 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0854902, 0.0598881 and 0.700525. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18216 so gap is 203.093, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18012.9 - 18216), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17875 - 18012.9), exposure 137.902
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.704756 bg counts (34), with cf=1.31079 and errBG= 0.120865
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.2919 +/- 5.86415
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 51
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18218.5), exposure 383.619, 27 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0883414, 0.0594966 and 0.673486. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18216 and stop= 18218.5 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18231), exposure 396.156, 27 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0854084, 0.0606142 and 0.709698. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18216 and stop= 18231 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18246.1), exposure 411.2, 27 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0822175, 0.0614955 and 0.747961. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18216 and stop= 18246.1 so gap is 30.0878, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17834.9 - 18246.1) = 17834.9- 18246.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18216 - 18363.9), exposure 147.922
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 19 counts and 0.76694 bg counts (37), with cf=1.30693 and errBG= 0.126084
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8294 +/- 5.69918
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (18246.1 - 18363.9), exposure 117.834, 9 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0965043, 0.0744126 and 0.771081. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18216 and stop= 18363.9 so gap is 147.922, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 1 (18363.9) and the bin is not full 19 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=147.922 whereas forward=3984.7
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18012.9 - 18363.9), exposure 351.014
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 39 counts and 1.63752 bg counts (79), with cf=1.31027 and errBG= 0.184235
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.9548 +/- 8.18618
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 1 (18363.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18363.9), exposure 529.034, 36 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0854003, 0.0643724 and 0.753772. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18012.9 - 18363.9), with lastBin= 0 and workMinC was 14
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 22348.6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17834.9 - 18363.9) = 17834.9- 18363.9
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 22348.6 - 23524.5


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22348.6 - 22571.8), exposure 223.151
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.920562 bg counts (67), with cf=1.2462 and errBG= 0.112465
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.5458 +/- 4.82855
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22348.6 and stop= 22571.8 so gap is 223.151, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (22348.6 - 22571.8), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18012.9 - 18363.9), exposure 351.014
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 39 counts and 1.63752 bg counts (79), with cf=1.31027 and errBG= 0.184235
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.9548 +/- 8.18618
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 52
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22789.9), exposure 441.288, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0536446, 0.0377666 and 0.704014. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22571.8 and stop= 22789.9 so gap is 218.136, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22571.8 - 22797.4), exposure 225.658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.604548 bg counts (44), with cf=1.23801 and errBG= 0.091139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.0118 +/- 5.53771
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22797.4), exposure 448.809, 21 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0555045, 0.0370956 and 0.668334. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22571.8 and stop= 22797.4 so gap is 225.658, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (22571.8 - 22797.4), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22348.6 - 22571.8), exposure 223.151
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.920562 bg counts (67), with cf=1.2462 and errBG= 0.112465
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.5458 +/- 4.82855
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 53
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22812.5), exposure 463.853, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0563744, 0.0358925 and 0.63668. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22812.5 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22832.5), exposure 483.912, 24 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0590519, 0.0342635 and 0.580228. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22832.5 so gap is 35.1024, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22837.5), exposure 488.927, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0583765, 0.0364111 and 0.623729. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22837.5 so gap is 40.1171, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22842.5), exposure 493.941, 25 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0602568, 0.0360414 and 0.598131. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22842.5 so gap is 45.1317, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22847.6), exposure 498.956, 26 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0621335, 0.0356792 and 0.574235. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22847.6 so gap is 50.1463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22857.6), exposure 508.985, 27 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0633091, 0.0349762 and 0.552467. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22857.6 so gap is 60.1755, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22860.1), exposure 511.492, 28 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0654201, 0.0348047 and 0.532019. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22860.1 so gap is 62.6829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22862.6), exposure 514, 28 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.065101, 0.0370448 and 0.569036. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22862.6 so gap is 65.1902, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22875.1), exposure 526.536, 29 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0658058, 0.0360655 and 0.54806. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22875.1 so gap is 77.7267, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22895.2), exposure 546.595, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0655, 0.0346483 and 0.528982. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22895.2 so gap is 97.7853, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22907.7), exposure 559.131, 31 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0661536, 0.0338409 and 0.511551. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22907.7 so gap is 110.322, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22912.7), exposure 564.146, 32 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0677605, 0.0335401 and 0.49498. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22912.7 so gap is 115.336, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22915.3), exposure 566.653, 32 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0674607, 0.0355772 and 0.527376. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22915.3 so gap is 117.844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22922.8), exposure 574.175, 32 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0665769, 0.0372385 and 0.55933. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22922.8 so gap is 125.366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22927.8), exposure 579.19, 32 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0659711, 0.0390545 and 0.591993. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22927.8 so gap is 130.38, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22942.8), exposure 594.234, 32 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0642436, 0.0401212 and 0.624517. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22942.8 so gap is 145.424, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (22348.6 - 22942.8) = 22348.6- 22942.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22797.4 - 22985.5), exposure 188.049
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.645767 bg counts (47), with cf=1.23837 and errBG= 0.0941948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9677 +/- 5.53938
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22985.5 so gap is 188.049, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (22797.4 - 22985.5), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22571.8 - 22797.4), exposure 225.658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.604548 bg counts (44), with cf=1.23801 and errBG= 0.091139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.0118 +/- 5.53771
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 54
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22985.5 - 23158.5), exposure 173.005
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.48089 bg counts (35), with cf=1.2384 and errBG= 0.0812853
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1726 +/- 5.53923
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22985.5 and stop= 23158.5 so gap is 173.005, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (22985.5 - 23158.5), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22797.4 - 22985.5), exposure 188.049
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.645767 bg counts (47), with cf=1.23837 and errBG= 0.0941948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9677 +/- 5.53938
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 55
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23261.3), exposure 318.429, 15 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0559852, 0.0451202 and 0.805931. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23261.3 so gap is 102.8, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23266.3), exposure 323.443, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0588931, 0.0443681 and 0.753366. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23266.3 so gap is 107.814, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23301.4), exposure 358.546, 17 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0563917, 0.0399294 and 0.708073. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23301.4 so gap is 142.917, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23303.9), exposure 361.053, 18 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0594303, 0.0396521 and 0.667204. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23303.9 so gap is 145.424, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23311.4), exposure 368.575, 19 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0615776, 0.0387506 and 0.629296. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23311.4 so gap is 152.946, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23318.9), exposure 376.097, 20 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0635941, 0.0379756 and 0.597155. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23318.9 so gap is 160.468, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23326.5), exposure 383.619, 21 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0655757, 0.0371866 and 0.567079. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23326.5 so gap is 167.99, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23334), exposure 391.141, 22 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0674381, 0.0364715 and 0.540814. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23334 so gap is 175.512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23336.5), exposure 393.648, 23 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0701554, 0.0362392 and 0.516556. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23336.5 so gap is 178.019, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23354), exposure 411.199, 24 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0700901, 0.0346924 and 0.494968. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23354 so gap is 195.57, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23384.1), exposure 441.287, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0651955, 0.0350185 and 0.537131. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23384.1 so gap is 225.658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23158.5 - 23391.6), exposure 233.18
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.700726 bg counts (51), with cf=1.23855 and errBG= 0.0981213
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.7104 +/- 4.79844
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23391.6), exposure 448.809, 25 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0667872, 0.0343558 and 0.514407. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23391.6 so gap is 233.18, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (23158.5 - 23391.6), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22985.5 - 23158.5), exposure 173.005
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.48089 bg counts (35), with cf=1.2384 and errBG= 0.0812853
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1726 +/- 5.53923
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 56
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23411.7), exposure 468.868, 25 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0638211, 0.0354543 and 0.555526. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23411.7 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23419.2), exposure 476.39, 25 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0627777, 0.0400934 and 0.638656. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23419.2 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23429.3), exposure 486.419, 26 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0639596, 0.0392667 and 0.61393. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23429.3 so gap is 37.6097, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23431.8), exposure 488.926, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.06613, 0.0390653 and 0.590735. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23431.8 so gap is 40.117, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23451.8), exposure 508.985, 27 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0635239, 0.0398925 and 0.627993. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23451.8 so gap is 60.1755, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23391.6 - 23524.5), exposure 132.881
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.384712 bg counts (28), with cf=1.23839 and errBG= 0.0727038
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.1923 +/- 3.27771
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23524.5), exposure 581.69, 28 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0574492, 0.0346724 and 0.603531. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23524.5 so gap is 132.881, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 2 (23524.5) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=132.881 whereas forward=4609.68
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23158.5 - 23524.5), exposure 366.061
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 1.08544 bg counts (79), with cf=1.2385 and errBG= 0.122121
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.9027 +/- 5.81106
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (23158.5 - 23524.5), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 28134.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (22942.8 - 23524.5) = 22942.8- 23524.5
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 28134.2 - 29871.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28134.2 - 28400), exposure 265.775
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.957794 bg counts (67), with cf=1.2989 and errBG= 0.117013
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5383 +/- 5.19781
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28134.2 and stop= 28400 so gap is 265.775, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28134.2 - 28400), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23158.5 - 23524.5), exposure 366.061
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 1.08544 bg counts (79), with cf=1.2385 and errBG= 0.122121
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.9027 +/- 5.81106
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 57
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28475.2), exposure 340.995, 16 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0586727, 0.0172182 and 0.293461. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28475.2 so gap is 75.2195, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28482.7), exposure 348.517, 17 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0610972, 0.0168465 and 0.275733. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28482.7 so gap is 82.7414, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28500.3), exposure 366.068, 17 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0578108, 0.0194638 and 0.336681. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28500.3 so gap is 100.293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28525.3), exposure 391.141, 17 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0540572, 0.0214199 and 0.396244. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28525.3 so gap is 125.366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28552.9), exposure 418.722, 17 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0504074, 0.0231572 and 0.459401. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28552.9 so gap is 152.946, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28600.6), exposure 466.361, 17 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.045058, 0.0234578 and 0.520614. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28600.6 so gap is 200.585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28613.1), exposure 478.897, 18 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0465221, 0.0227657 and 0.489352. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28613.1 so gap is 213.122, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28618.1), exposure 483.912, 18 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.04604, 0.025305 and 0.549631. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28618.1 so gap is 218.136, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28625.6), exposure 491.434, 18 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0452974, 0.0276132 and 0.609598. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28625.6 so gap is 225.658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28668.3), exposure 534.058, 19 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0439672, 0.0253741 and 0.577114. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28668.3 so gap is 268.283, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28400 - 28705.9), exposure 305.892
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.857726 bg counts (60), with cf=1.31838 and errBG= 0.110732
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6449 +/- 5.10815
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28705.9), exposure 571.668, 20 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0431191, 0.0236719 and 0.548989. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28705.9 so gap is 305.892, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28400 - 28705.9), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28134.2 - 28400), exposure 265.775
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.957794 bg counts (67), with cf=1.2989 and errBG= 0.117013
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5383 +/- 5.19781
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 58
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28708.4), exposure 574.175, 21 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0452587, 0.0235358 and 0.520029. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28708.4 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28725.9), exposure 591.726, 22 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0460676, 0.022806 and 0.495055. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28725.9 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28763.5), exposure 629.336, 23 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0453197, 0.0214132 and 0.472492. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28763.5 so gap is 57.6682, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28791.1), exposure 656.916, 23 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0433885, 0.0223867 and 0.51596. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28791.1 so gap is 85.2487, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28821.2), exposure 687.004, 23 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.041352, 0.023275 and 0.562852. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28821.2 so gap is 115.336, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28856.3), exposure 722.106, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0411291, 0.0220655 and 0.536493. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28856.3 so gap is 150.439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28891.4), exposure 757.209, 24 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0391234, 0.0227344 and 0.581095. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28891.4 so gap is 185.541, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28896.4), exposure 762.224, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.038866, 0.0242903 and 0.624975. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28896.4 so gap is 190.556, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (28134.2 - 28896.4) = 28134.2- 28896.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28705.9 - 28964.1), exposure 258.253
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.686181 bg counts (48), with cf=1.31767 and errBG= 0.0990417
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8609 +/- 5.10499
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28964.1 so gap is 258.253, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28705.9 - 28964.1), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28400 - 28705.9), exposure 305.892
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.857726 bg counts (60), with cf=1.31838 and errBG= 0.110732
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6449 +/- 5.10815
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 59
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28964.1 - 29209.8), exposure 245.717
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.743362 bg counts (52), with cf=1.33235 and errBG= 0.103086
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9948 +/- 5.16199
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28964.1 and stop= 29209.8 so gap is 245.717, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28964.1 - 29209.8), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28705.9 - 28964.1), exposure 258.253
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.686181 bg counts (48), with cf=1.31767 and errBG= 0.0990417
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8609 +/- 5.10499
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 60
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29337.7), exposure 441.287, 17 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0487144, 0.0401831 and 0.824872. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29337.7 so gap is 127.873, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29357.8), exposure 461.346, 18 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0494616, 0.0382724 and 0.77378. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29357.8 so gap is 147.932, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29360.3), exposure 463.853, 19 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0519372, 0.0380248 and 0.73213. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29360.3 so gap is 150.439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29435.5), exposure 539.073, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0467842, 0.0325439 and 0.695618. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29435.5 so gap is 225.658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29445.5), exposure 549.102, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0458608, 0.0343811 and 0.749684. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29445.5 so gap is 235.688, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (28896.4 - 29445.5) = 28896.4- 29445.5
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29209.8 - 29463.1), exposure 253.239
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.84343 bg counts (59), with cf=1.32319 and errBG= 0.109805
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7319 +/- 5.12677
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29463.1 so gap is 253.239, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (29209.8 - 29463.1), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28964.1 - 29209.8), exposure 245.717
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.743362 bg counts (52), with cf=1.33235 and errBG= 0.103086
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9948 +/- 5.16199
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 61
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29463.1 - 29698.8), exposure 235.688
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.729067 bg counts (51), with cf=1.3148 and errBG= 0.10209
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7634 +/- 5.09395
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29463.1 and stop= 29698.8 so gap is 235.688, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (29463.1 - 29698.8), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29209.8 - 29463.1), exposure 253.239
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.84343 bg counts (59), with cf=1.32319 and errBG= 0.109805
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7319 +/- 5.12677
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 62
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29796.6), exposure 351.024, 15 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0541211, 0.0246101 and 0.454723. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29796.6 so gap is 97.7854, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29811.6), exposure 366.068, 16 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0553565, 0.0235475 and 0.42538. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29811.6 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29814.1), exposure 368.576, 17 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0585183, 0.0233874 and 0.399659. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29814.1 so gap is 115.337, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29839.2), exposure 393.649, 18 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0578812, 0.0218501 and 0.377499. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29839.2 so gap is 140.41, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29849.2), exposure 403.678, 19 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0596926, 0.0212608 and 0.356171. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29849.2 so gap is 150.439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29698.8 - 29871.8), exposure 172.994
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.471749 bg counts (33), with cf=1.31717 and errBG= 0.082121
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.5503 +/- 4.16666
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29871.8), exposure 426.233, 20 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.059406, 0.0200917 and 0.33821. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29871.8 so gap is 172.994, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 3 (29871.8) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=172.994 whereas forward=3959.81
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29463.1 - 29871.8), exposure 408.682
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 1.20082 bg counts (84), with cf=1.31575 and errBG= 0.13102
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.3137 +/- 6.58099
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 3 (29871.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29871.8), exposure 975.335, 40 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0517806, 0.0281354 and 0.543359. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (29463.1 - 29871.8), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 33831.6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (28896.4 - 29871.8) = 28896.4- 29871.8
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 33831.6 - 35569.1


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (33831.6 - 34175.1), exposure 343.502
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.587295 bg counts (77), with cf=1.37104 and errBG= 0.0669284
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7604 +/- 5.3108
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=33831.6 and stop= 34175.1 so gap is 343.502, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (33831.6 - 34175.1), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29463.1 - 29871.8), exposure 408.682
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 1.20082 bg counts (84), with cf=1.31575 and errBG= 0.13102
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.3137 +/- 6.58099
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 63
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34340.6), exposure 508.985, 15 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0386144, 0.0206009 and 0.533505. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34340.6 so gap is 165.483, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34378.2), exposure 546.595, 16 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0383465, 0.0190876 and 0.497766. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34378.2 so gap is 203.093, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34428.3), exposure 596.741, 16 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0349333, 0.0196898 and 0.56364. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34428.3 so gap is 253.239, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34445.9), exposure 614.292, 17 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0360616, 0.0190932 and 0.529462. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34445.9 so gap is 270.79, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34463.4), exposure 631.844, 18 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.037127, 0.0185298 and 0.499092. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34463.4 so gap is 288.341, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34473.4), exposure 641.873, 18 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0365469, 0.0203259 and 0.55616. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34473.4 so gap is 298.371, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34493.5), exposure 661.931, 18 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0354238, 0.0217097 and 0.612859. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34493.5 so gap is 318.429, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34175.1 - 34501), exposure 325.951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.610176 bg counts (80), with cf=1.34791 and errBG= 0.0682198
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.3962 +/- 5.22125
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34501), exposure 669.453, 19 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0370235, 0.0214658 and 0.579789. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34501 so gap is 325.951, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34175.1 - 34501), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (33831.6 - 34175.1), exposure 343.502
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.587295 bg counts (77), with cf=1.37104 and errBG= 0.0669284
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7604 +/- 5.3108
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 64
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34503.5), exposure 671.961, 20 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0388911, 0.0213857 and 0.549888. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34503.5 so gap is 2.5073, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34576.2), exposure 744.673, 21 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0367588, 0.0192276 and 0.523074. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34576.2 so gap is 75.2194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34578.8), exposure 747.18, 21 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0366217, 0.0209478 and 0.572007. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34578.8 so gap is 77.7268, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34606.3), exposure 774.761, 21 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.035278, 0.0219399 and 0.621914. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34606.3 so gap is 105.307, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34689.1), exposure 857.502, 22 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0332107, 0.019738 and 0.594328. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34689.1 so gap is 188.049, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34691.6), exposure 860.009, 23 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0346749, 0.0196805 and 0.567572. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34691.6 so gap is 190.556, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34744.2), exposure 912.663, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0341057, 0.0184767 and 0.541749. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34744.2 so gap is 243.21, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34746.7), exposure 915.17, 25 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0354792, 0.0184261 and 0.519349. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34746.7 so gap is 245.717, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34781.8), exposure 950.273, 26 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0355604, 0.0176908 and 0.497485. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34781.8 so gap is 280.819, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34817), exposure 985.375, 27 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0356194, 0.0170395 and 0.478376. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34817 so gap is 315.922, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34824.5), exposure 992.897, 27 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0353496, 0.0182682 and 0.516788. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34824.5 so gap is 323.444, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34842), exposure 1010.45, 28 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0360487, 0.0179098 and 0.496822. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34842 so gap is 340.995, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34899.7), exposure 1068.12, 28 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0340349, 0.0181468 and 0.533184. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34899.7 so gap is 398.663, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (33831.6 - 34899.7) = 33831.6- 34899.7
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34501 - 34995), exposure 493.941
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.800856 bg counts (105), with cf=1.34536 and errBG= 0.0781556
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.103 +/- 5.21162
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34995 so gap is 493.941, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34501 - 34995), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34175.1 - 34501), exposure 325.951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.610176 bg counts (80), with cf=1.34791 and errBG= 0.0682198
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.3962 +/- 5.22125
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 65
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34995 - 35280.8), exposure 285.834
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.503395 bg counts (66), with cf=1.34673 and errBG= 0.0619637
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.523 +/- 5.21654
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34995 and stop= 35280.8 so gap is 285.834, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34995 - 35280.8), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34501 - 34995), exposure 493.941
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.800856 bg counts (105), with cf=1.34536 and errBG= 0.0781556
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.103 +/- 5.21162
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 66
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35406.2), exposure 506.478, 15 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0382281, 0.0259741 and 0.67945. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35406.2 so gap is 125.366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35418.7), exposure 519.015, 15 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.037285, 0.0279181 and 0.748777. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35418.7 so gap is 137.902, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35506.5), exposure 606.771, 15 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0316556, 0.026001 and 0.82137. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35506.5 so gap is 225.659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35529), exposure 629.337, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.032612, 0.0250524 and 0.768195. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35529 so gap is 248.225, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35551.6), exposure 651.903, 17 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0334716, 0.0241536 and 0.721617. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35551.6 so gap is 270.79, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (35280.8 - 35569.1), exposure 288.33
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.480514 bg counts (63), with cf=1.34585 and errBG= 0.0605391
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.8494 +/- 4.85322
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35569.1), exposure 669.442, 18 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0345923, 0.0235055 and 0.679499. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35569.1 so gap is 288.33, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 4 (35569.1) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=288.33 whereas forward=16333.6
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34995 - 35569.1), exposure 574.164
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.983909 bg counts (129), with cf=1.34632 and errBG= 0.0866284
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.3724 +/- 7.12503
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 4 (35569.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 35569.1), exposure 1737.56, 46 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0342495, 0.0202127 and 0.590162. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34995 - 35569.1), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 51902.8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (33831.6 - 35569.1) = 33831.6- 35569.1
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 51902.8 - 53284.3


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (51902.8 - 52492), exposure 589.218
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.0854 bg counts (147), with cf=1.63412 and errBG= 0.0895226
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.7381 +/- 6.3306
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=51902.8 and stop= 52492 so gap is 589.218, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (51902.8 - 52492), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34995 - 35569.1), exposure 574.164
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.983909 bg counts (129), with cf=1.34632 and errBG= 0.0866284
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.3724 +/- 7.12503
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 67
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52655), exposure 752.193, 15 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0308481, 0.00980176 and 0.317742. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52655 so gap is 162.975, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52732.7), exposure 829.92, 16 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0297761, 0.00878268 and 0.294957. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52732.7 so gap is 240.702, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52757.8), exposure 854.993, 17 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0308226, 0.00846905 and 0.274767. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52757.8 so gap is 265.775, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52830.5), exposure 927.705, 17 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0282632, 0.00946578 and 0.334915. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52830.5 so gap is 338.487, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52903.2), exposure 1000.42, 18 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0277176, 0.00866921 and 0.312769. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52903.2 so gap is 411.199, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52918.2), exposure 1015.46, 19 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0288775, 0.00852889 and 0.295347. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52918.2 so gap is 426.243, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 53033.6), exposure 1130.8, 19 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0258144, 0.00896201 and 0.347171. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 53033.6 so gap is 541.58, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 53073.7), exposure 1170.91, 19 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.024868, 0.0100724 and 0.405034. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 53073.7 so gap is 581.697, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 53076.2), exposure 1173.42, 20 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0262517, 0.0100508 and 0.382864. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 53076.2 so gap is 584.204, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 53103.8), exposure 1201, 21 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.026984, 0.00976949 and 0.362047. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 53103.8 so gap is 611.784, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52492 - 53284.3), exposure 792.305
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.49151 bg counts (202), with cf=1.65143 and errBG= 0.104942
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.3084 +/- 6.39832
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 53284.3), exposure 1381.52, 21 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0230898, 0.0095179 and 0.412212. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 53284.3 so gap is 792.305, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 5 (53284.3) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (52492 - 53284.3), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (51902.8 - 52492), exposure 589.218
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.0854 bg counts (147), with cf=1.63412 and errBG= 0.0895226
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.7381 +/- 6.3306
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 68
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 57563.6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 57563.6 - 59163.3


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 57593.7), exposure 1411.61, 21 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0225371, 0.0107331 and 0.476242. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 57593.7 so gap is 30.0876, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 57643.9), exposure 1461.76, 21 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0217139, 0.0116863 and 0.538197. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 57643.9 so gap is 80.2338, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 57774.2), exposure 1592.14, 22 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0212434, 0.0106248 and 0.500147. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 57774.2 so gap is 210.614, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 57811.8), exposure 1629.75, 22 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.020738, 0.0116942 and 0.563904. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 57811.8 so gap is 248.224, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 57952.3), exposure 1770.16, 22 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0189809, 0.0119409 and 0.629101. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 57952.3 so gap is 388.633, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58130.3), exposure 1948.17, 23 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0182818, 0.0107947 and 0.59046. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58130.3 so gap is 566.652, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58258.2), exposure 2076.05, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0181568, 0.0100975 and 0.556128. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58258.2 so gap is 694.525, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58371), exposure 2188.88, 24 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0171624, 0.0105373 and 0.613975. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58371 so gap is 807.355, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58516.4), exposure 2334.3, 25 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0169016, 0.00979899 and 0.579767. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58516.4 so gap is 952.779, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58624.2), exposure 2442.12, 26 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0170231, 0.00931608 and 0.547261. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58624.2 so gap is 1060.59, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58664.3), exposure 2482.23, 26 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0167111, 0.0100857 and 0.603531. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58664.3 so gap is 1100.71, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (51902.8 - 58664.3) = 51902.8- 58664.3
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57563.6 - 58942.6), exposure 1379.02
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.74827 bg counts (235), with cf=2.22407 and errBG= 0.114045
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.4728 +/- 8.61753
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58942.6 so gap is 1379.02, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (57563.6 - 58942.6), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52492 - 53284.3), exposure 792.305
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.49151 bg counts (202), with cf=1.65143 and errBG= 0.104942
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.3084 +/- 6.39832
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 69
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 6
++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++tructures/grbBin.cpp::        binData:  line  385  INFO   >>  I have run out of background events
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (58942.6 - 59163.3), exposure 220.635
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.334776 bg counts (45), with cf=2.31733 and errBG= 0.0499054
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =3.85887 +/- 3.27924
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (58664.3 - 59163.3), exposure 498.947, 4 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0164666, 0.00772227 and 0.468965. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58942.6 and stop= 59163.3 so gap is 220.635, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 6 (59163.3) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=220.635 whereas forward=6.34556e+08
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57563.6 - 59163.3), exposure 1599.66
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 2.08305 bg counts (280), with cf=2.23504 and errBG= 0.124486
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.34 +/- 9.21952
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 6 (59163.3) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 59163.3), exposure 2981.18, 30 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.016674, 0.00969485 and 0.581434. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x1ed9780
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57563.6 - 59163.3), exposure 1599.66
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 2.08305 bg counts (280), with cf=2.23504 and errBG= 0.124486
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.34 +/- 9.21952
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 70
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 59163.3), exposure 2981.18, 30 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.016674, 0.00969485 and 0.581434. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  941  INFO   >>  Saving a final HR bin.
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for PC mode.
++/genlc_cpp/genlc.cpp::           main:  line  326  INFO   >>  STARTING MODE: PC, with files: pcsourcetotal_incbad.evt, pcbacktotal_incbad.evt, and pccorr.fits
++/genlc_cpp/genlc.cpp::           main:  line  327  INFO   >>  Grades: 0 -- 12
++/SourceEventList.cpp::SourceEventList:  line   29  INFO   >>  CREATING SOURCE EVENT LIST, with time ranges : 146.018 - 385384
++ctures/binMethod.cpp::    buildOrbits:  line   66  INFO   >>  Defining orbits
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	146.018 - 1384.62
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	16646.4 - 18363.9
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	22348.6 - 23524.5
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	28134.2 - 29871.8
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	33831.6 - 35569.1
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	51902.8 - 53284.3
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	57563.6 - 59163.3
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	62963.4 - 63261.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	85568.4 - 87123
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	91567.8 - 93064.7
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	97587.2 - 98763.2
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	161131 - 161344
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	213346 - 213544
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	217412 - 218164
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	223919 - 225243
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	234741 - 235563
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	257452 - 259144
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	269006 - 270664
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	280519 - 281763
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	366488 - 368105
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	372658 - 373864
++ctures/binMethod.cpp::    buildOrbits:  line   83  INFO   >>     Added an orbit:	378479 - 379264
++ctures/binMethod.cpp::    buildOrbits:  line   92  INFO   >>     Added an orbit:	385209 - 385384
++tructures/grbBin.cpp::        binData:  line   57  INFO   >>  BINNING DATA - COUNTS PER BIN BINNING - PC mode, suffix = _incbad
++tructures/grbBin.cpp::        binData:  line   85  INFO   >>  Working to 20 ct/bin at rateFact=10 and binFact= 1.5 with minT 2.51 and minSNR 1.5
++tructures/grbBin.cpp::        binData:  line   90  INFO   >>  Creating main output file PCCURVE_incbad.qdp, reading from pcsourcetotal_incbad.evt
++tructures/grbBin.cpp::        binData:  line  133  INFO   >>  SPLIT TIME IS 1e+80
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (146.018 - 171.091), exposure 25.0731
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.305075 bg counts (10), with cf=4.03613 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =95.6357 +/- 19.7767
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=146.018 and stop= 171.091 so gap is 25.0731, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (146.018 - 171.091), with lastBin= 0 and workMinC was 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 183.628), exposure 37.6097, 20 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.1223, 1.37022 and 0.645629. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 183.628 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 186.135), exposure 40.117, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.98659, 1.38557 and 0.697465. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 186.135 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 188.642), exposure 42.6243, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.86973, 1.39574 and 0.746492. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 188.642 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 191.149), exposure 45.1316, 23 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.02831, 1.40477 and 0.692583. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 191.149 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 193.657), exposure 47.6389, 25 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.08818, 1.41544 and 0.677836. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 193.657 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (171.091 - 196.164), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.366089 bg counts (12), with cf=4.04016 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =83.3642 +/- 18.5192
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 196.164), exposure 50.1463, 26 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.06414, 1.50542 and 0.729319. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=171.091 and stop= 196.164 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (171.091 - 196.164), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (146.018 - 171.091), exposure 25.0731
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.305075 bg counts (10), with cf=4.03613 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =95.6357 +/- 19.7767
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 1
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (146.018 - 198.671), exposure 52.6536, 27 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.04241, 1.51029 and 0.739465. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=196.164 and stop= 198.671 so gap is 2.50726, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (146.018 - 198.671) = 146.018- 198.671
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (196.164 - 211.208), exposure 15.0438
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0610149 bg counts (2), with cf=4.03267 and errBG= 0.0431441
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.4073 +/- 18.0355
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=196.164 and stop= 211.208 so gap is 15.0438, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (196.164 - 211.208), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (171.091 - 196.164), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.366089 bg counts (12), with cf=4.04016 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =83.3642 +/- 18.5192
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 226.252), exposure 27.5805, 21 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 3.05103, 1.88437 and 0.617617. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=211.208 and stop= 226.252 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 233.774), exposure 35.1024, 22 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.5042, 1.48057 and 0.591237. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=211.208 and stop= 233.774 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 236.281), exposure 37.6097, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.33397, 1.49152 and 0.63905. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=211.208 and stop= 236.281 so gap is 25.0732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (211.208 - 238.788), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.0507 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.6547 +/- 18.1199
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 238.788), exposure 40.1171, 23 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.28938, 1.49959 and 0.65502. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=211.208 and stop= 238.788 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (211.208 - 238.788), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (196.164 - 211.208), exposure 15.0438
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0610149 bg counts (2), with cf=4.03267 and errBG= 0.0431441
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.4073 +/- 18.0355
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 3
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 241.296), exposure 42.6243, 24 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.24715, 1.60204 and 0.712921. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=238.788 and stop= 241.296 so gap is 2.50728, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 243.803), exposure 45.1317, 26 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.30237, 1.60307 and 0.69627. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=238.788 and stop= 243.803 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (198.671 - 246.31), exposure 47.639, 27 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.26648, 1.68929 and 0.745334. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=238.788 and stop= 246.31 so gap is 7.52192, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (198.671 - 246.31) = 198.671- 246.31
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (238.788 - 258.847), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.09765 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.078 +/- 18.3282
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=238.788 and stop= 258.847 so gap is 20.0585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (238.788 - 258.847), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (211.208 - 238.788), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.0507 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.6547 +/- 18.1199
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (258.847 - 276.398), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.152537 bg counts (5), with cf=4.08161 and errBG= 0.0682167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.0096 +/- 18.2556
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=258.847 and stop= 276.398 so gap is 17.5512, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (258.847 - 276.398), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (238.788 - 258.847), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.09765 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.078 +/- 18.3282
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 5
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (246.31 - 291.442), exposure 45.1317, 22 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.97708, 1.96 and 0.991359. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=276.398 and stop= 291.442 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (246.31 - 291.442) = 246.31- 291.442
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (276.398 - 301.471), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.24406 bg counts (8), with cf=4.05155 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.0936 +/- 18.5698
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=276.398 and stop= 301.471 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (276.398 - 301.471), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (258.847 - 276.398), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.152537 bg counts (5), with cf=4.08161 and errBG= 0.0682167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.0096 +/- 18.2556
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301.471 - 326.544), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.03845 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =87.737 +/- 18.9456
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=301.471 and stop= 326.544 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (301.471 - 326.544), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (276.398 - 301.471), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.24406 bg counts (8), with cf=4.05155 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.0936 +/- 18.5698
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 7
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (291.442 - 339.081), exposure 47.639, 20 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.69369, 1.84803 and 1.09113. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=326.544 and stop= 339.081 so gap is 12.5365, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (291.442 - 339.081) = 291.442- 339.081
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (326.544 - 344.096), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.10645 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.6279 +/- 18.3663
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=326.544 and stop= 344.096 so gap is 17.5512, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (326.544 - 344.096), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (301.471 - 326.544), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.03845 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =87.737 +/- 18.9456
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (344.096 - 384.213), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.396597 bg counts (13), with cf=4.0765 and errBG= 0.109996
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.2192 +/- 19.9757
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=344.096 and stop= 384.213 so gap is 40.1171, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (344.096 - 384.213), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (326.544 - 344.096), exposure 17.5512
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.10645 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.6279 +/- 18.3663
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 9
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (339.081 - 389.227), exposure 50.1463, 21 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.68178, 1.61175 and 0.958363. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=384.213 and stop= 389.227 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (339.081 - 389.227) = 339.081- 389.227
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (384.213 - 404.271), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.305075 bg counts (10), with cf=4.03627 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =83.5302 +/- 18.5006
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=384.213 and stop= 404.271 so gap is 20.0585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (384.213 - 404.271), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (344.096 - 384.213), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.396597 bg counts (13), with cf=4.0765 and errBG= 0.109996
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.2192 +/- 19.9757
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 10
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 424.33), exposure 35.1024, 20 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.27374, 1.25137 and 0.550358. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=404.271 and stop= 424.33 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (404.271 - 426.837), exposure 22.5658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.0915224 bg counts (3), with cf=4.03837 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.5514 +/- 19.7851
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 426.837), exposure 37.6097, 24 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.54866, 1.27539 and 0.500415. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=404.271 and stop= 426.837 so gap is 22.5658, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (404.271 - 426.837), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (384.213 - 404.271), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.305075 bg counts (10), with cf=4.03627 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =83.5302 +/- 18.5006
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 11
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 429.344), exposure 40.117, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.38937, 1.29282 and 0.541072. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 429.344 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 431.852), exposure 42.6244, 24 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.24594, 1.31109 and 0.583761. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 431.852 so gap is 5.01464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 436.866), exposure 47.639, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.00952, 1.25231 and 0.623185. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 436.866 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 439.374), exposure 50.1463, 26 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.0735, 1.27191 and 0.613411. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 439.374 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 441.881), exposure 52.6536, 27 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.05307, 1.36795 and 0.666294. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 441.881 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 444.388), exposure 55.1609, 28 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.0345, 1.38051 and 0.678553. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 444.388 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 446.896), exposure 57.6683, 31 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.16055, 1.31835 and 0.61019. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 446.896 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (389.227 - 449.403), exposure 60.1756, 32 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.13985, 1.32861 and 0.62089. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 449.403 so gap is 22.5658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (389.227 - 449.403) = 389.227- 449.403
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (426.837 - 454.418), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.12292 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5779 +/- 18.4413
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=426.837 and stop= 454.418 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (426.837 - 454.418), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (404.271 - 426.837), exposure 22.5658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.0915224 bg counts (3), with cf=4.03837 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.5514 +/- 19.7851
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 12
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (454.418 - 479.491), exposure 25.0731
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.335582 bg counts (11), with cf=4.13624 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =93.7456 +/- 19.8411
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=454.418 and stop= 479.491 so gap is 25.0731, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (454.418 - 479.491), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (426.837 - 454.418), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.12292 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5779 +/- 18.4413
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 13
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (479.491 - 507.071), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.03797 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =87.7267 +/- 18.9434
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (449.403 - 507.071), exposure 57.6683, 22 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.53191, 1.90431 and 1.24309. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=479.491 and stop= 507.071 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (479.491 - 507.071), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (454.418 - 479.491), exposure 25.0731
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 0.335582 bg counts (11), with cf=4.13624 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =93.7456 +/- 19.8411
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 14
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (449.403 - 507.071) = 449.403- 507.071
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (507.071 - 537.159), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.183045 bg counts (6), with cf=4.04062 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.1134 +/- 18.5189
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=507.071 and stop= 537.159 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (507.071 - 537.159), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (479.491 - 507.071), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.03797 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =87.7267 +/- 18.9434
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 15
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (537.159 - 552.203), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.12819 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.0601 +/- 18.4636
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (507.071 - 552.203), exposure 45.1317, 20 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.79541, 1.8865 and 1.05074. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=537.159 and stop= 552.203 so gap is 15.0439, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (537.159 - 552.203), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (507.071 - 537.159), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.183045 bg counts (6), with cf=4.04062 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.1134 +/- 18.5189
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 16
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (507.071 - 552.203) = 507.071- 552.203
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (552.203 - 572.261), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.213552 bg counts (7), with cf=4.05293 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.4048 +/- 19.8579
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=552.203 and stop= 572.261 so gap is 20.0585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (552.203 - 572.261), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (537.159 - 552.203), exposure 15.0439
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.12819 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.0601 +/- 18.4636
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 17
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (572.261 - 602.349), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0915224 bg counts (3), with cf=4.09421 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5094 +/- 18.3111
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (552.203 - 602.349), exposure 50.1463, 20 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.61144, 1.93643 and 1.20168. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=572.261 and stop= 602.349 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (572.261 - 602.349), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (552.203 - 572.261), exposure 20.0585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 24 counts and 0.213552 bg counts (7), with cf=4.05293 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =96.4048 +/- 19.8579
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 18
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (552.203 - 602.349) = 552.203- 602.349
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (602.349 - 629.93), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.24406 bg counts (8), with cf=4.08407 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.7687 +/- 18.7189
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=602.349 and stop= 629.93 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (602.349 - 629.93), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (572.261 - 602.349), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0915224 bg counts (3), with cf=4.09421 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5094 +/- 18.3111
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 19
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (629.93 - 660.017), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.05235 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.1815 +/- 18.1256
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=629.93 and stop= 660.017 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (629.93 - 660.017), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (602.349 - 629.93), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.24406 bg counts (8), with cf=4.08407 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.7687 +/- 18.7189
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 20
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (602.349 - 670.047), exposure 67.6975, 20 soft counts and 25 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.17261, 1.49342 and 1.27359. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=660.017 and stop= 670.047 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (602.349 - 670.047) = 602.349- 670.047
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (660.017 - 692.613), exposure 32.5951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.05249 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.6899 +/- 18.1279
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=660.017 and stop= 692.613 so gap is 32.5951, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (660.017 - 692.613), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (629.93 - 660.017), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.05235 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.1815 +/- 18.1256
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 21
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (692.613 - 717.686), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.24406 bg counts (8), with cf=4.07741 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.5532 +/- 18.2381
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=692.613 and stop= 717.686 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (692.613 - 717.686), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (660.017 - 692.613), exposure 32.5951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.05249 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.6899 +/- 18.1279
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 22
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (670.047 - 720.193), exposure 50.1463, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.60112, 1.44242 and 0.900883. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 720.193 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (670.047 - 722.7), exposure 52.6536, 21 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.59882, 1.45003 and 0.906938. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 722.7 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (670.047 - 725.208), exposure 55.1609, 24 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.74016, 1.38412 and 0.795401. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 725.208 so gap is 7.52192, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (670.047 - 727.715), exposure 57.6683, 26 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.80168, 1.32394 and 0.734837. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 727.715 so gap is 10.0292, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (670.047 - 730.222), exposure 60.1756, 28 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.85638, 1.39853 and 0.753366. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 730.222 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (670.047 - 730.222) = 670.047- 730.222
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (717.686 - 750.281), exposure 32.5951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.427104 bg counts (14), with cf=4.0067 and errBG= 0.114148
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =86.436 +/- 18.7986
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=717.686 and stop= 750.281 so gap is 32.5951, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (717.686 - 750.281), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (692.613 - 717.686), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.24406 bg counts (8), with cf=4.07741 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.5532 +/- 18.2381
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 23
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (750.281 - 777.861), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.366089 bg counts (12), with cf=4.03446 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.2122 +/- 18.0477
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=750.281 and stop= 777.861 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (750.281 - 777.861), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (717.686 - 750.281), exposure 32.5951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.427104 bg counts (14), with cf=4.0067 and errBG= 0.114148
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =86.436 +/- 18.7986
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 24
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (730.222 - 797.92), exposure 67.6976, 20 soft counts and 26 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.17889, 1.54963 and 1.31448. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=777.861 and stop= 797.92 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (730.222 - 797.92) = 730.222- 797.92
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (777.861 - 805.442), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.274567 bg counts (9), with cf=4.17603 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.3741 +/- 18.6797
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=777.861 and stop= 805.442 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (777.861 - 805.442), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (750.281 - 777.861), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.366089 bg counts (12), with cf=4.03446 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.2122 +/- 18.0477
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 25
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (805.442 - 835.53), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.152537 bg counts (5), with cf=4.12042 and errBG= 0.0682167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.7799 +/- 18.4292
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=805.442 and stop= 835.53 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (805.442 - 835.53), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (777.861 - 805.442), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.274567 bg counts (9), with cf=4.17603 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.3741 +/- 18.6797
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 26
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (797.92 - 863.11), exposure 65.1902, 20 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.2466, 1.32173 and 1.06027. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=835.53 and stop= 863.11 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (797.92 - 863.11) = 797.92- 863.11
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (835.53 - 865.617), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.10287 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5568 +/- 18.3503
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=835.53 and stop= 865.617 so gap is 30.0878, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (835.53 - 865.617), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (805.442 - 835.53), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.152537 bg counts (5), with cf=4.12042 and errBG= 0.0682167
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.7799 +/- 18.4292
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 27
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (865.617 - 900.72), exposure 35.1024
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.305075 bg counts (10), with cf=4.14781 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.6908 +/- 18.5539
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=865.617 and stop= 900.72 so gap is 35.1024, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (865.617 - 900.72), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (835.53 - 865.617), exposure 30.0878
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.12203 bg counts (4), with cf=4.10287 and errBG= 0.0610149
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.5568 +/- 18.3503
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 28
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 918.271), exposure 55.161, 20 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.48411, 1.33041 and 0.896437. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=900.72 and stop= 918.271 so gap is 17.5512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 920.778), exposure 57.6683, 20 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.41959, 1.34452 and 0.947118. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=900.72 and stop= 920.778 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 923.286), exposure 60.1756, 21 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.42098, 1.2885 and 0.906768. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=900.72 and stop= 923.286 so gap is 22.5659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (900.72 - 925.793), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.396597 bg counts (13), with cf=4.14359 and errBG= 0.109996
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.2285 +/- 18.5363
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 925.793), exposure 62.6829, 23 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.49451, 1.23294 and 0.824979. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=900.72 and stop= 925.793 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (900.72 - 925.793), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (865.617 - 900.72), exposure 35.1024
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.305075 bg counts (10), with cf=4.14781 and errBG= 0.096473
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.6908 +/- 18.5539
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 29
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 928.3), exposure 65.1902, 25 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.56044, 1.18552 and 0.759731. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=925.793 and stop= 928.3 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (863.11 - 930.808), exposure 67.6976, 26 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.55817, 1.31746 and 0.845522. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=925.793 and stop= 930.808 so gap is 5.01464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (863.11 - 930.808) = 863.11- 930.808
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (925.793 - 948.359), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.183045 bg counts (6), with cf=4.08604 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.9729 +/- 18.2759
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=925.793 and stop= 948.359 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (925.793 - 948.359), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (900.72 - 925.793), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.396597 bg counts (13), with cf=4.14359 and errBG= 0.109996
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.2285 +/- 18.5363
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 30
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (948.359 - 975.939), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.183045 bg counts (6), with cf=4.0862 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =85.0623 +/- 18.7278
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 975.939), exposure 45.1317, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.79952, 1.35401 and 0.752427. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=948.359 and stop= 975.939 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (948.359 - 975.939), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (925.793 - 948.359), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.183045 bg counts (6), with cf=4.08604 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.9729 +/- 18.2759
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 31
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 978.447), exposure 47.639, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.03962, 1.28274 and 0.628912. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 978.447 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 980.954), exposure 50.1463, 25 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.0176, 1.29856 and 0.643617. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 980.954 so gap is 5.01464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 983.461), exposure 52.6537, 25 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.92152, 1.31287 and 0.683245. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 983.461 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 985.969), exposure 55.161, 25 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.83193, 1.32588 and 0.723761. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 985.969 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 988.476), exposure 57.6683, 26 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.82181, 1.26823 and 0.696139. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 988.476 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (930.808 - 990.983), exposure 60.1756, 27 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.81306, 1.34972 and 0.744441. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 990.983 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (930.808 - 990.983) = 930.808- 990.983
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (975.939 - 1003.52), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.02932 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.7259 +/- 18.0226
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=975.939 and stop= 1003.52 so gap is 27.5805, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (975.939 - 1003.52), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (948.359 - 975.939), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.183045 bg counts (6), with cf=4.0862 and errBG= 0.0747277
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =85.0623 +/- 18.7278
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 32
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1018.56), exposure 27.5805, 20 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.9394, 0.712915 and 0.242537. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1003.52 and stop= 1018.56 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1021.07), exposure 30.0878, 21 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.82838, 0.653505 and 0.231052. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1003.52 and stop= 1021.07 so gap is 17.5513, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1023.58), exposure 32.5951, 22 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.73445, 0.603235 and 0.220606. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1003.52 and stop= 1023.58 so gap is 20.0586, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1003.52 - 1026.09), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.24406 bg counts (8), with cf=4.08665 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =88.9088 +/- 19.1713
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1026.09), exposure 35.1025, 24 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.76517, 0.671437 and 0.242819. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1003.52 and stop= 1026.09 so gap is 22.5659, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1003.52 - 1026.09), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (975.939 - 1003.52), exposure 27.5805
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.213552 bg counts (7), with cf=4.02932 and errBG= 0.0807151
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =79.7259 +/- 18.0226
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 33
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1028.59), exposure 37.6098, 25 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.68797, 0.626675 and 0.23314. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1028.59 so gap is 2.5073, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1031.1), exposure 40.1171, 27 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.72086, 0.684883 and 0.251715. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1031.1 so gap is 5.01462, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1036.11), exposure 45.1317, 27 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.41854, 0.78738 and 0.325559. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1036.11 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1038.62), exposure 47.639, 28 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.37584, 0.745939 and 0.313969. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1038.62 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1041.13), exposure 50.1464, 29 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.33781, 1.03171 and 0.441313. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1041.13 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1046.14), exposure 55.161, 30 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.19871, 1.08252 and 0.492342. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1046.14 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1048.65), exposure 57.6683, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.10096, 1.10568 and 0.526275. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1048.65 so gap is 22.5659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1026.09 - 1051.16), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0915224 bg counts (3), with cf=4.03453 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.3213 +/- 18.0442
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1051.16), exposure 60.1756, 31 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 2.08005, 1.25952 and 0.605524. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1026.09 and stop= 1051.16 so gap is 25.0732, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1026.09 - 1051.16), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1003.52 - 1026.09), exposure 22.5659
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.24406 bg counts (8), with cf=4.08665 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =88.9088 +/- 19.1713
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 34
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1056.17), exposure 65.1903, 32 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.98155, 1.16263 and 0.586728. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1051.16 and stop= 1056.17 so gap is 5.01464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (990.983 - 1058.68), exposure 67.6976, 32 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.90816, 1.1788 and 0.617769. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1051.16 and stop= 1058.68 so gap is 7.52194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (990.983 - 1058.68) = 990.983- 1058.68
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1051.16 - 1093.78), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.457612 bg counts (15), with cf=4.02174 and errBG= 0.118155
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.6162 +/- 18.4361
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1051.16 and stop= 1093.78 so gap is 42.6244, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1051.16 - 1093.78), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1026.09 - 1051.16), exposure 25.0732
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.0915224 bg counts (3), with cf=4.03453 and errBG= 0.0528405
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.3213 +/- 18.0442
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 35
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1093.78 - 1128.89), exposure 35.1025
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.366089 bg counts (12), with cf=4.11888 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.8696 +/- 18.4253
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1093.78 and stop= 1128.89 so gap is 35.1025, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1093.78 - 1128.89), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1051.16 - 1093.78), exposure 42.6244
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.457612 bg counts (15), with cf=4.02174 and errBG= 0.118155
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =82.6162 +/- 18.4361
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 36
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1058.68 - 1131.39), exposure 72.7122, 21 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.13669, 1.11576 and 0.98159. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1128.89 and stop= 1131.39 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1058.68 - 1131.39) = 1058.68- 1131.39
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1128.89 - 1166.5), exposure 37.6098
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.366089 bg counts (12), with cf=4.10917 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.7883 +/- 18.8356
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1128.89 and stop= 1166.5 so gap is 37.6098, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1128.89 - 1166.5), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1093.78 - 1128.89), exposure 35.1025
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.366089 bg counts (12), with cf=4.11888 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.8696 +/- 18.4253
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 37
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1166.5 - 1201.6), exposure 35.1025
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.24406 bg counts (8), with cf=4.09715 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =89.1373 +/- 19.2206
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1166.5 and stop= 1201.6 so gap is 35.1025, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1166.5 - 1201.6), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1128.89 - 1166.5), exposure 37.6098
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.366089 bg counts (12), with cf=4.10917 and errBG= 0.105681
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.7883 +/- 18.8356
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 38
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1131.39 - 1211.63), exposure 80.2342, 20 soft counts and 24 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.00927, 1.20586 and 1.19478. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1201.6 and stop= 1211.63 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1131.39 - 1211.63) = 1131.39- 1211.63
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1201.6 - 1251.74), exposure 50.1464
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.549134 bg counts (18), with cf=4.12213 and errBG= 0.129432
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.179 +/- 18.4424
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1201.6 and stop= 1251.74 so gap is 50.1464, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1201.6 - 1251.74), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1166.5 - 1201.6), exposure 35.1025
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.24406 bg counts (8), with cf=4.09715 and errBG= 0.0862881
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =89.1373 +/- 19.2206
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 39
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1251.74 - 1284.34), exposure 32.5952
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.06173 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =88.2429 +/- 19.0548
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1251.74 and stop= 1284.34 so gap is 32.5952, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1251.74 - 1284.34), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1201.6 - 1251.74), exposure 50.1464
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.549134 bg counts (18), with cf=4.12213 and errBG= 0.129432
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.179 +/- 18.4424
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 40
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1211.63 - 1286.85), exposure 75.2196, 21 soft counts and 21 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.12375, 1.11762 and 0.994538. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1284.34 and stop= 1286.85 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1211.63 - 1286.85) = 1211.63- 1286.85
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1284.34 - 1324.46), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.15197 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.646 +/- 18.5729
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1284.34 and stop= 1324.46 so gap is 40.1171, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1284.34 - 1324.46), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1251.74 - 1284.34), exposure 32.5952
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 0.274567 bg counts (9), with cf=4.06173 and errBG= 0.0915224
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =88.2429 +/- 19.0548
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 41
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1286.85 - 1372.1), exposure 85.2489, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.94478, 0.666911 and 0.70589. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1324.46 and stop= 1372.1 so gap is 47.6391, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1286.85 - 1374.6), exposure 87.7562, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.917786, 0.693544 and 0.755671. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1324.46 and stop= 1374.6 so gap is 50.1464, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1286.85 - 1379.62), exposure 92.7708, 21 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.911396, 0.656056 and 0.719836. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1324.46 and stop= 1379.62 so gap is 55.161, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1324.46 - 1382.12), exposure 57.6684
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.427104 bg counts (14), with cf=4.09742 and errBG= 0.114148
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =80.1984 +/- 18.3302
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1286.85 - 1382.12), exposure 95.2781, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.930926, 0.638791 and 0.686189. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1324.46 and stop= 1382.12 so gap is 57.6684, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1324.46 - 1382.12), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1284.34 - 1324.46), exposure 40.1171
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.335582 bg counts (11), with cf=4.15197 and errBG= 0.101182
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =81.646 +/- 18.5729
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 42
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1382.12 - 1384.62), exposure 2.49908
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.0305075 bg counts (1), with cf=4.14651 and errBG= 0.0305075
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =4.02001 +/- 4.14844
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1286.85 - 1384.62), exposure 97.7772, 23 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.948249, 0.622464 and 0.656435. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=1382.12 and stop= 1384.62 so gap is 2.49908, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 0 (1384.62) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=2.49908 whereas forward=15261.8
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1324.46 - 1384.62), exposure 60.1674
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.457612 bg counts (15), with cf=4.09976 and errBG= 0.118155
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.2189 +/- 18.7937
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 0 (1384.62) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (1211.63 - 1384.62), exposure 172.997, 44 soft counts and 36 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 1.02457, 0.837751 and 0.817662. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (1324.46 - 1384.62), with lastBin= 0 and workMinC was 21
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 16646.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (1211.63 - 1384.62) = 1211.63- 1384.62
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 16646.4 - 18363.9


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16646.4 - 16809.4), exposure 162.975
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.787668 bg counts (38), with cf=1.31218 and errBG= 0.127777
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.21 +/- 5.87063
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16646.4 and stop= 16809.4 so gap is 162.975, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16646.4 - 16809.4), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (1324.46 - 1384.62), exposure 60.1674
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.457612 bg counts (15), with cf=4.09976 and errBG= 0.118155
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =84.2189 +/- 18.7937
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 43
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16949.8), exposure 303.385, 20 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.082571, 0.0538391 and 0.652034. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16949.8 so gap is 140.41, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16952.3), exposure 305.892, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0818942, 0.0575819 and 0.703125. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16952.3 so gap is 142.917, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16954.8), exposure 308.4, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0812284, 0.0613514 and 0.755295. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16954.8 so gap is 145.424, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16957.3), exposure 310.907, 21 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0846907, 0.0608566 and 0.718575. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16957.3 so gap is 147.932, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16972.3), exposure 325.951, 21 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0807819, 0.0620071 and 0.767587. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16972.3 so gap is 162.975, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 16979.9), exposure 333.473, 21 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0789598, 0.0644468 and 0.816198. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 16979.9 so gap is 170.497, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17012.5), exposure 366.068, 22 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0753778, 0.0585609 and 0.776899. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 17012.5 so gap is 203.092, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16809.4 - 17015), exposure 205.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.787668 bg counts (38), with cf=1.30851 and errBG= 0.127777
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.1395 +/- 5.85422
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17015), exposure 368.575, 23 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0784383, 0.0581626 and 0.741508. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=16809.4 and stop= 17015 so gap is 205.6, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (16809.4 - 17015), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16646.4 - 16809.4), exposure 162.975
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.787668 bg counts (38), with cf=1.31218 and errBG= 0.127777
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.21 +/- 5.87063
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 44
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17022.5), exposure 376.097, 23 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0768695, 0.0605594 and 0.787821. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17015 and stop= 17022.5 so gap is 7.52196, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17025), exposure 378.605, 24 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0798972, 0.0600869 and 0.752053. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17015 and stop= 17025 so gap is 10.0293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17027.5), exposure 381.112, 24 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0793716, 0.0632051 and 0.796319. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17015 and stop= 17027.5 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (16646.4 - 17030), exposure 383.619, 24 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0788528, 0.0661367 and 0.838736. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17015 and stop= 17030 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (16646.4 - 17030) = 16646.4- 17030
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17015 - 17145.4), exposure 130.38
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.663299 bg counts (32), with cf=1.31056 and errBG= 0.117256
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.6524 +/- 6.00769
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17015 and stop= 17145.4 so gap is 130.38, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17015 - 17145.4), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (16809.4 - 17015), exposure 205.6
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.787668 bg counts (38), with cf=1.30851 and errBG= 0.127777
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.1395 +/- 5.85422
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 45
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17275.7), exposure 245.717, 20 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.102698, 0.0659893 and 0.642556. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17145.4 and stop= 17275.7 so gap is 130.38, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17278.2), exposure 248.224, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.101661, 0.0704425 and 0.692918. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17145.4 and stop= 17278.2 so gap is 132.888, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17283.3), exposure 253.239, 21 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.104811, 0.0690476 and 0.658783. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17145.4 and stop= 17283.3 so gap is 137.902, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17285.8), exposure 255.746, 21 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.103783, 0.0734831 and 0.708043. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17145.4 and stop= 17285.8 so gap is 140.41, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17145.4 - 17288.3), exposure 142.917
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.663299 bg counts (32), with cf=1.30649 and errBG= 0.117256
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.2632 +/- 5.84481
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17288.3), exposure 258.253, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.107839, 0.0727697 and 0.674801. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17145.4 and stop= 17288.3 so gap is 142.917, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17145.4 - 17288.3), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17015 - 17145.4), exposure 130.38
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 21 counts and 0.663299 bg counts (32), with cf=1.31056 and errBG= 0.117256
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =26.6524 +/- 6.00769
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 46
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17030 - 17335.9), exposure 305.892, 22 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0903359, 0.0653787 and 0.723728. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17288.3 and stop= 17335.9 so gap is 47.6389, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17030 - 17335.9) = 17030- 17335.9
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17288.3 - 17488.9), exposure 200.585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.07786 bg counts (52), with cf=1.31154 and errBG= 0.149472
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.2595 +/- 5.08336
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17288.3 and stop= 17488.9 so gap is 200.585, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17288.3 - 17488.9), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17145.4 - 17288.3), exposure 142.917
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.663299 bg counts (32), with cf=1.30649 and errBG= 0.117256
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.2632 +/- 5.84481
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 47
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17649.3), exposure 313.414, 20 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0798929, 0.0483778 and 0.605533. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17488.9 and stop= 17649.3 so gap is 160.468, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17661.9), exposure 325.951, 20 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0766532, 0.050529 and 0.65919. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17488.9 and stop= 17661.9 so gap is 173.005, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17488.9 - 17666.9), exposure 178.019
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.559659 bg counts (27), with cf=1.31127 and errBG= 0.107706
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.4915 +/- 5.86588
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17666.9), exposure 330.965, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0754918, 0.0537145 and 0.711528. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17488.9 and stop= 17666.9 so gap is 178.019, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17488.9 - 17666.9), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17288.3 - 17488.9), exposure 200.585
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.07786 bg counts (52), with cf=1.31154 and errBG= 0.149472
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.2595 +/- 5.08336
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 48
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17671.9), exposure 335.98, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0743651, 0.0568244 and 0.764127. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17671.9 so gap is 5.0146, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17679.4), exposure 343.502, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0803093, 0.0555801 and 0.692075. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17679.4 so gap is 12.5366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17686.9), exposure 351.024, 23 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0823161, 0.0543891 and 0.660735. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17686.9 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17694.5), exposure 358.546, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0842609, 0.0530965 and 0.630144. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17694.5 so gap is 27.5804, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17714.5), exposure 378.604, 25 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0829831, 0.0501399 and 0.604218. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17714.5 so gap is 47.6389, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17717), exposure 381.112, 26 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.085888, 0.04981 and 0.579942. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17717 so gap is 50.1463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17752.1), exposure 416.214, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0815392, 0.0483083 and 0.592455. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17752.1 so gap is 85.2486, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17767.2), exposure 431.258, 27 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0785687, 0.0495972 and 0.63126. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17767.2 so gap is 100.293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17769.7), exposure 433.765, 28 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0811343, 0.0492479 and 0.606993. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17769.7 so gap is 102.8, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17809.8), exposure 473.882, 29 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0765821, 0.0449067 and 0.586387. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17809.8 so gap is 142.917, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17814.8), exposure 478.897, 29 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0757802, 0.047232 and 0.623277. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17814.8 so gap is 147.931, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17824.8), exposure 488.926, 29 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0742257, 0.048935 and 0.659273. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17824.8 so gap is 157.961, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17827.3), exposure 491.433, 30 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0764498, 0.0486853 and 0.636827. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17827.3 so gap is 160.468, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17335.9 - 17834.9), exposure 498.955, 30 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0751883, 0.0505865 and 0.672798. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17834.9 so gap is 167.99, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17335.9 - 17834.9) = 17335.9- 17834.9
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17666.9 - 17875), exposure 208.107
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.994949 bg counts (48), with cf=1.31443 and errBG= 0.143609
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.9808 +/- 5.88133
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17666.9 and stop= 17875 so gap is 208.107, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17666.9 - 17875), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17488.9 - 17666.9), exposure 178.019
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.559659 bg counts (27), with cf=1.31127 and errBG= 0.107706
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.4915 +/- 5.86588
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 49
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17875 - 18012.9), exposure 137.902
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.704756 bg counts (34), with cf=1.31079 and errBG= 0.120865
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.2919 +/- 5.86415
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=17875 and stop= 18012.9 so gap is 137.902, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (17875 - 18012.9), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17666.9 - 17875), exposure 208.107
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.994949 bg counts (48), with cf=1.31443 and errBG= 0.143609
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.9808 +/- 5.88133
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 50
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18103.1), exposure 268.283, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0934452, 0.0665542 and 0.712228. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18103.1 so gap is 90.2634, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18168.3), exposure 333.473, 21 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0784728, 0.0528911 and 0.674005. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18168.3 so gap is 155.454, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18170.8), exposure 335.98, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0818858, 0.0524963 and 0.641092. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18170.8 so gap is 157.961, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18173.4), exposure 338.488, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0811184, 0.0559831 and 0.690141. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18173.4 so gap is 160.468, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18178.4), exposure 343.502, 22 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0799342, 0.0589848 and 0.737918. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18178.4 so gap is 165.483, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18183.4), exposure 348.517, 23 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0825377, 0.0581361 and 0.704359. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18183.4 so gap is 170.497, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18185.9), exposure 351.024, 24 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0855198, 0.0577209 and 0.674941. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18185.9 so gap is 173.005, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18195.9), exposure 361.053, 24 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0831443, 0.059744 and 0.718559. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18195.9 so gap is 183.034, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18208.5), exposure 373.59, 24 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0802085, 0.0610939 and 0.761688. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18208.5 so gap is 195.571, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18213.5), exposure 378.605, 25 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0826013, 0.0602847 and 0.729827. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18213.5 so gap is 200.585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18012.9 - 18216), exposure 203.093
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.87058 bg counts (42), with cf=1.31343 and errBG= 0.134333
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.1252 +/- 5.8765
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18216), exposure 381.112, 26 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0854902, 0.0598881 and 0.700525. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18012.9 and stop= 18216 so gap is 203.093, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18012.9 - 18216), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (17875 - 18012.9), exposure 137.902
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.704756 bg counts (34), with cf=1.31079 and errBG= 0.120865
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.2919 +/- 5.86415
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 51
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 1
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18218.5), exposure 383.619, 27 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0883414, 0.0594966 and 0.673486. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18216 and stop= 18218.5 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18231), exposure 396.156, 27 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0854084, 0.0606142 and 0.709698. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18216 and stop= 18231 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18246.1), exposure 411.2, 27 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0822175, 0.0614955 and 0.747961. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18216 and stop= 18246.1 so gap is 30.0878, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17834.9 - 18246.1) = 17834.9- 18246.1
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18216 - 18363.9), exposure 147.922
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 19 counts and 0.76694 bg counts (37), with cf=1.30693 and errBG= 0.126084
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.8294 +/- 5.69918
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (18246.1 - 18363.9), exposure 117.834, 9 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0965043, 0.0744126 and 0.771081. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=18216 and stop= 18363.9 so gap is 147.922, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 1 (18363.9) and the bin is not full 19 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 20 counts, because gotBinThisOrb=1 and gapBack=147.922 whereas forward=3984.7
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18012.9 - 18363.9), exposure 351.014
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 39 counts and 1.63752 bg counts (79), with cf=1.31027 and errBG= 0.184235
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.9548 +/- 8.18618
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 1 (18363.9) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (17834.9 - 18363.9), exposure 529.034, 36 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0854003, 0.0643724 and 0.753772. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (18012.9 - 18363.9), with lastBin= 0 and workMinC was 14
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 22348.6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (17834.9 - 18363.9) = 17834.9- 18363.9
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 22348.6 - 23524.5


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22348.6 - 22571.8), exposure 223.151
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.920562 bg counts (67), with cf=1.2462 and errBG= 0.112465
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.5458 +/- 4.82855
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22348.6 and stop= 22571.8 so gap is 223.151, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (22348.6 - 22571.8), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (18012.9 - 18363.9), exposure 351.014
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 39 counts and 1.63752 bg counts (79), with cf=1.31027 and errBG= 0.184235
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =48.9548 +/- 8.18618
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 52
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22789.9), exposure 441.288, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0536446, 0.0377666 and 0.704014. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22571.8 and stop= 22789.9 so gap is 218.136, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22571.8 - 22797.4), exposure 225.658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.604548 bg counts (44), with cf=1.23801 and errBG= 0.091139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.0118 +/- 5.53771
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22797.4), exposure 448.809, 21 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0555045, 0.0370956 and 0.668334. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22571.8 and stop= 22797.4 so gap is 225.658, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (22571.8 - 22797.4), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22348.6 - 22571.8), exposure 223.151
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.920562 bg counts (67), with cf=1.2462 and errBG= 0.112465
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.5458 +/- 4.82855
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 53
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22812.5), exposure 463.853, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0563744, 0.0358925 and 0.63668. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22812.5 so gap is 15.0439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22832.5), exposure 483.912, 24 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0590519, 0.0342635 and 0.580228. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22832.5 so gap is 35.1024, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22837.5), exposure 488.927, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0583765, 0.0364111 and 0.623729. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22837.5 so gap is 40.1171, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22842.5), exposure 493.941, 25 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0602568, 0.0360414 and 0.598131. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22842.5 so gap is 45.1317, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22847.6), exposure 498.956, 26 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0621335, 0.0356792 and 0.574235. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22847.6 so gap is 50.1463, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22857.6), exposure 508.985, 27 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0633091, 0.0349762 and 0.552467. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22857.6 so gap is 60.1755, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22860.1), exposure 511.492, 28 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0654201, 0.0348047 and 0.532019. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22860.1 so gap is 62.6829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22862.6), exposure 514, 28 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.065101, 0.0370448 and 0.569036. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22862.6 so gap is 65.1902, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22875.1), exposure 526.536, 29 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0658058, 0.0360655 and 0.54806. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22875.1 so gap is 77.7267, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22895.2), exposure 546.595, 30 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0655, 0.0346483 and 0.528982. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22895.2 so gap is 97.7853, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22907.7), exposure 559.131, 31 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0661536, 0.0338409 and 0.511551. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22907.7 so gap is 110.322, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22912.7), exposure 564.146, 32 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0677605, 0.0335401 and 0.49498. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22912.7 so gap is 115.336, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22915.3), exposure 566.653, 32 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0674607, 0.0355772 and 0.527376. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22915.3 so gap is 117.844, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22922.8), exposure 574.175, 32 soft counts and 18 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0665769, 0.0372385 and 0.55933. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22922.8 so gap is 125.366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22927.8), exposure 579.19, 32 soft counts and 19 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0659711, 0.0390545 and 0.591993. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22927.8 so gap is 130.38, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22348.6 - 22942.8), exposure 594.234, 32 soft counts and 20 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0642436, 0.0401212 and 0.624517. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22942.8 so gap is 145.424, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (22348.6 - 22942.8) = 22348.6- 22942.8
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22797.4 - 22985.5), exposure 188.049
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.645767 bg counts (47), with cf=1.23837 and errBG= 0.0941948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9677 +/- 5.53938
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22797.4 and stop= 22985.5 so gap is 188.049, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (22797.4 - 22985.5), with lastBin= 0x1ed81d0 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22571.8 - 22797.4), exposure 225.658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.604548 bg counts (44), with cf=1.23801 and errBG= 0.091139
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.0118 +/- 5.53771
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 54
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22985.5 - 23158.5), exposure 173.005
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.48089 bg counts (35), with cf=1.2384 and errBG= 0.0812853
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1726 +/- 5.53923
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=22985.5 and stop= 23158.5 so gap is 173.005, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (22985.5 - 23158.5), with lastBin= 0x1ed9780 and workMinC was 20
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22797.4 - 22985.5), exposure 188.049
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.645767 bg counts (47), with cf=1.23837 and errBG= 0.0941948
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =23.9677 +/- 5.53938
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 55
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23261.3), exposure 318.429, 15 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0559852, 0.0451202 and 0.805931. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23261.3 so gap is 102.8, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23266.3), exposure 323.443, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0588931, 0.0443681 and 0.753366. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23266.3 so gap is 107.814, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23301.4), exposure 358.546, 17 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0563917, 0.0399294 and 0.708073. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23301.4 so gap is 142.917, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23303.9), exposure 361.053, 18 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0594303, 0.0396521 and 0.667204. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23303.9 so gap is 145.424, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23311.4), exposure 368.575, 19 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0615776, 0.0387506 and 0.629296. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23311.4 so gap is 152.946, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23318.9), exposure 376.097, 20 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0635941, 0.0379756 and 0.597155. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23318.9 so gap is 160.468, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23326.5), exposure 383.619, 21 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0655757, 0.0371866 and 0.567079. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23326.5 so gap is 167.99, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23334), exposure 391.141, 22 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0674381, 0.0364715 and 0.540814. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23334 so gap is 175.512, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23336.5), exposure 393.648, 23 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0701554, 0.0362392 and 0.516556. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23336.5 so gap is 178.019, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23354), exposure 411.199, 24 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0700901, 0.0346924 and 0.494968. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23354 so gap is 195.57, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23384.1), exposure 441.287, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0651955, 0.0350185 and 0.537131. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23384.1 so gap is 225.658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23158.5 - 23391.6), exposure 233.18
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.700726 bg counts (51), with cf=1.23855 and errBG= 0.0981213
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.7104 +/- 4.79844
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23391.6), exposure 448.809, 25 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0667872, 0.0343558 and 0.514407. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23158.5 and stop= 23391.6 so gap is 233.18, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (23158.5 - 23391.6), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (22985.5 - 23158.5), exposure 173.005
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 20 counts and 0.48089 bg counts (35), with cf=1.2384 and errBG= 0.0812853
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =24.1726 +/- 5.53923
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 56
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 2
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23411.7), exposure 468.868, 25 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0638211, 0.0354543 and 0.555526. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23411.7 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23419.2), exposure 476.39, 25 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0627777, 0.0400934 and 0.638656. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23419.2 so gap is 27.5805, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23429.3), exposure 486.419, 26 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0639596, 0.0392667 and 0.61393. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23429.3 so gap is 37.6097, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23431.8), exposure 488.926, 27 soft counts and 16 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.06613, 0.0390653 and 0.590735. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23431.8 so gap is 40.117, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23451.8), exposure 508.985, 27 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0635239, 0.0398925 and 0.627993. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23451.8 so gap is 60.1755, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23391.6 - 23524.5), exposure 132.881
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 0.384712 bg counts (28), with cf=1.23839 and errBG= 0.0727038
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.1923 +/- 3.27771
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (22942.8 - 23524.5), exposure 581.69, 28 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0574492, 0.0346724 and 0.603531. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=23391.6 and stop= 23524.5 so gap is 132.881, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 2 (23524.5) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=132.881 whereas forward=4609.68
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23158.5 - 23524.5), exposure 366.061
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 1.08544 bg counts (79), with cf=1.2385 and errBG= 0.122121
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.9027 +/- 5.81106
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (23158.5 - 23524.5), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 28134.2
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (22942.8 - 23524.5) = 22942.8- 23524.5
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 28134.2 - 29871.8


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28134.2 - 28400), exposure 265.775
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.957794 bg counts (67), with cf=1.2989 and errBG= 0.117013
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5383 +/- 5.19781
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28134.2 and stop= 28400 so gap is 265.775, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28134.2 - 28400), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (23158.5 - 23524.5), exposure 366.061
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 22 counts and 1.08544 bg counts (79), with cf=1.2385 and errBG= 0.122121
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =25.9027 +/- 5.81106
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 57
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28475.2), exposure 340.995, 16 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0586727, 0.0172182 and 0.293461. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28475.2 so gap is 75.2195, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28482.7), exposure 348.517, 17 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0610972, 0.0168465 and 0.275733. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28482.7 so gap is 82.7414, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28500.3), exposure 366.068, 17 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0578108, 0.0194638 and 0.336681. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28500.3 so gap is 100.293, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28525.3), exposure 391.141, 17 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0540572, 0.0214199 and 0.396244. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28525.3 so gap is 125.366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28552.9), exposure 418.722, 17 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0504074, 0.0231572 and 0.459401. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28552.9 so gap is 152.946, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28600.6), exposure 466.361, 17 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.045058, 0.0234578 and 0.520614. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28600.6 so gap is 200.585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28613.1), exposure 478.897, 18 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0465221, 0.0227657 and 0.489352. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28613.1 so gap is 213.122, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28618.1), exposure 483.912, 18 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.04604, 0.025305 and 0.549631. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28618.1 so gap is 218.136, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28625.6), exposure 491.434, 18 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0452974, 0.0276132 and 0.609598. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28625.6 so gap is 225.658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28668.3), exposure 534.058, 19 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0439672, 0.0253741 and 0.577114. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28668.3 so gap is 268.283, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28400 - 28705.9), exposure 305.892
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.857726 bg counts (60), with cf=1.31838 and errBG= 0.110732
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6449 +/- 5.10815
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28705.9), exposure 571.668, 20 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0431191, 0.0236719 and 0.548989. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28400 and stop= 28705.9 so gap is 305.892, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28400 - 28705.9), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28134.2 - 28400), exposure 265.775
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 0.957794 bg counts (67), with cf=1.2989 and errBG= 0.117013
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.5383 +/- 5.19781
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 58
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28708.4), exposure 574.175, 21 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0452587, 0.0235358 and 0.520029. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28708.4 so gap is 2.50732, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28725.9), exposure 591.726, 22 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0460676, 0.022806 and 0.495055. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28725.9 so gap is 20.0585, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28763.5), exposure 629.336, 23 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0453197, 0.0214132 and 0.472492. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28763.5 so gap is 57.6682, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28791.1), exposure 656.916, 23 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0433885, 0.0223867 and 0.51596. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28791.1 so gap is 85.2487, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28821.2), exposure 687.004, 23 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.041352, 0.023275 and 0.562852. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28821.2 so gap is 115.336, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28856.3), exposure 722.106, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0411291, 0.0220655 and 0.536493. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28856.3 so gap is 150.439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28891.4), exposure 757.209, 24 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0391234, 0.0227344 and 0.581095. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28891.4 so gap is 185.541, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28134.2 - 28896.4), exposure 762.224, 24 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.038866, 0.0242903 and 0.624975. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28896.4 so gap is 190.556, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (28134.2 - 28896.4) = 28134.2- 28896.4
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28705.9 - 28964.1), exposure 258.253
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.686181 bg counts (48), with cf=1.31767 and errBG= 0.0990417
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8609 +/- 5.10499
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28705.9 and stop= 28964.1 so gap is 258.253, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28705.9 - 28964.1), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28400 - 28705.9), exposure 305.892
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.857726 bg counts (60), with cf=1.31838 and errBG= 0.110732
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.6449 +/- 5.10815
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 59
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28964.1 - 29209.8), exposure 245.717
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.743362 bg counts (52), with cf=1.33235 and errBG= 0.103086
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9948 +/- 5.16199
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=28964.1 and stop= 29209.8 so gap is 245.717, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (28964.1 - 29209.8), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28705.9 - 28964.1), exposure 258.253
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.686181 bg counts (48), with cf=1.31767 and errBG= 0.0990417
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.8609 +/- 5.10499
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 60
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29337.7), exposure 441.287, 17 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0487144, 0.0401831 and 0.824872. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29337.7 so gap is 127.873, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29357.8), exposure 461.346, 18 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0494616, 0.0382724 and 0.77378. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29357.8 so gap is 147.932, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29360.3), exposure 463.853, 19 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0519372, 0.0380248 and 0.73213. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29360.3 so gap is 150.439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29435.5), exposure 539.073, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0467842, 0.0325439 and 0.695618. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29435.5 so gap is 225.658, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29445.5), exposure 549.102, 20 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0458608, 0.0343811 and 0.749684. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29445.5 so gap is 235.688, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (28896.4 - 29445.5) = 28896.4- 29445.5
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29209.8 - 29463.1), exposure 253.239
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.84343 bg counts (59), with cf=1.32319 and errBG= 0.109805
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7319 +/- 5.12677
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29209.8 and stop= 29463.1 so gap is 253.239, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (29209.8 - 29463.1), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (28964.1 - 29209.8), exposure 245.717
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.743362 bg counts (52), with cf=1.33235 and errBG= 0.103086
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.9948 +/- 5.16199
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 61
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29463.1 - 29698.8), exposure 235.688
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.729067 bg counts (51), with cf=1.3148 and errBG= 0.10209
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7634 +/- 5.09395
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29463.1 and stop= 29698.8 so gap is 235.688, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (29463.1 - 29698.8), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29209.8 - 29463.1), exposure 253.239
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.84343 bg counts (59), with cf=1.32319 and errBG= 0.109805
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.7319 +/- 5.12677
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 62
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 3
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29796.6), exposure 351.024, 15 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0541211, 0.0246101 and 0.454723. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29796.6 so gap is 97.7854, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29811.6), exposure 366.068, 16 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0553565, 0.0235475 and 0.42538. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29811.6 so gap is 112.829, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29814.1), exposure 368.576, 17 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0585183, 0.0233874 and 0.399659. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29814.1 so gap is 115.337, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29839.2), exposure 393.649, 18 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0578812, 0.0218501 and 0.377499. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29839.2 so gap is 140.41, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29849.2), exposure 403.678, 19 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0596926, 0.0212608 and 0.356171. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29849.2 so gap is 150.439, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29698.8 - 29871.8), exposure 172.994
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 0.471749 bg counts (33), with cf=1.31717 and errBG= 0.082121
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.5503 +/- 4.16666
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (29445.5 - 29871.8), exposure 426.233, 20 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.059406, 0.0200917 and 0.33821. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=29698.8 and stop= 29871.8 so gap is 172.994, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 3 (29871.8) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=172.994 whereas forward=3959.81
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29463.1 - 29871.8), exposure 408.682
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 1.20082 bg counts (84), with cf=1.31575 and errBG= 0.13102
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.3137 +/- 6.58099
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 3 (29871.8) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (28896.4 - 29871.8), exposure 975.335, 40 soft counts and 22 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0517806, 0.0281354 and 0.543359. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (29463.1 - 29871.8), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 33831.6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (28896.4 - 29871.8) = 28896.4- 29871.8
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 33831.6 - 35569.1


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (33831.6 - 34175.1), exposure 343.502
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.587295 bg counts (77), with cf=1.37104 and errBG= 0.0669284
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7604 +/- 5.3108
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=33831.6 and stop= 34175.1 so gap is 343.502, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (33831.6 - 34175.1), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (29463.1 - 29871.8), exposure 408.682
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 25 counts and 1.20082 bg counts (84), with cf=1.31575 and errBG= 0.13102
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =31.3137 +/- 6.58099
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 63
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34340.6), exposure 508.985, 15 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0386144, 0.0206009 and 0.533505. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34340.6 so gap is 165.483, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34378.2), exposure 546.595, 16 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0383465, 0.0190876 and 0.497766. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34378.2 so gap is 203.093, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34428.3), exposure 596.741, 16 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0349333, 0.0196898 and 0.56364. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34428.3 so gap is 253.239, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34445.9), exposure 614.292, 17 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0360616, 0.0190932 and 0.529462. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34445.9 so gap is 270.79, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34463.4), exposure 631.844, 18 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.037127, 0.0185298 and 0.499092. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34463.4 so gap is 288.341, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34473.4), exposure 641.873, 18 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0365469, 0.0203259 and 0.55616. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34473.4 so gap is 298.371, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34493.5), exposure 661.931, 18 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0354238, 0.0217097 and 0.612859. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34493.5 so gap is 318.429, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34175.1 - 34501), exposure 325.951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.610176 bg counts (80), with cf=1.34791 and errBG= 0.0682198
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.3962 +/- 5.22125
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34501), exposure 669.453, 19 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0370235, 0.0214658 and 0.579789. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34175.1 and stop= 34501 so gap is 325.951, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34175.1 - 34501), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (33831.6 - 34175.1), exposure 343.502
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.587295 bg counts (77), with cf=1.37104 and errBG= 0.0669284
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.7604 +/- 5.3108
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 64
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34503.5), exposure 671.961, 20 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0388911, 0.0213857 and 0.549888. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34503.5 so gap is 2.5073, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34576.2), exposure 744.673, 21 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0367588, 0.0192276 and 0.523074. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34576.2 so gap is 75.2194, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34578.8), exposure 747.18, 21 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0366217, 0.0209478 and 0.572007. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34578.8 so gap is 77.7268, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34606.3), exposure 774.761, 21 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.035278, 0.0219399 and 0.621914. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34606.3 so gap is 105.307, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34689.1), exposure 857.502, 22 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0332107, 0.019738 and 0.594328. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34689.1 so gap is 188.049, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34691.6), exposure 860.009, 23 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0346749, 0.0196805 and 0.567572. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34691.6 so gap is 190.556, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34744.2), exposure 912.663, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0341057, 0.0184767 and 0.541749. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34744.2 so gap is 243.21, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34746.7), exposure 915.17, 25 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0354792, 0.0184261 and 0.519349. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34746.7 so gap is 245.717, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34781.8), exposure 950.273, 26 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0355604, 0.0176908 and 0.497485. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34781.8 so gap is 280.819, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34817), exposure 985.375, 27 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0356194, 0.0170395 and 0.478376. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34817 so gap is 315.922, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34824.5), exposure 992.897, 27 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0353496, 0.0182682 and 0.516788. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34824.5 so gap is 323.444, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34842), exposure 1010.45, 28 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0360487, 0.0179098 and 0.496822. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34842 so gap is 340.995, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 34899.7), exposure 1068.12, 28 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0340349, 0.0181468 and 0.533184. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34899.7 so gap is 398.663, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (33831.6 - 34899.7) = 33831.6- 34899.7
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34501 - 34995), exposure 493.941
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.800856 bg counts (105), with cf=1.34536 and errBG= 0.0781556
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.103 +/- 5.21162
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34501 and stop= 34995 so gap is 493.941, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34501 - 34995), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34175.1 - 34501), exposure 325.951
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.610176 bg counts (80), with cf=1.34791 and errBG= 0.0682198
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.3962 +/- 5.22125
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 65
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34995 - 35280.8), exposure 285.834
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.503395 bg counts (66), with cf=1.34673 and errBG= 0.0619637
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.523 +/- 5.21654
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=34995 and stop= 35280.8 so gap is 285.834, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34995 - 35280.8), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34501 - 34995), exposure 493.941
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 0.800856 bg counts (105), with cf=1.34536 and errBG= 0.0781556
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =19.103 +/- 5.21162
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 66
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 4
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35406.2), exposure 506.478, 15 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0382281, 0.0259741 and 0.67945. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35406.2 so gap is 125.366, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35418.7), exposure 519.015, 15 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.037285, 0.0279181 and 0.748777. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35418.7 so gap is 137.902, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35506.5), exposure 606.771, 15 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0316556, 0.026001 and 0.82137. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35506.5 so gap is 225.659, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35529), exposure 629.337, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.032612, 0.0250524 and 0.768195. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35529 so gap is 248.225, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35551.6), exposure 651.903, 17 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0334716, 0.0241536 and 0.721617. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35551.6 so gap is 270.79, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (35280.8 - 35569.1), exposure 288.33
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 0.480514 bg counts (63), with cf=1.34585 and errBG= 0.0605391
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.8494 +/- 4.85322
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (34899.7 - 35569.1), exposure 669.442, 18 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0345923, 0.0235055 and 0.679499. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=35280.8 and stop= 35569.1 so gap is 288.33, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 4 (35569.1) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=288.33 whereas forward=16333.6
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34995 - 35569.1), exposure 574.164
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.983909 bg counts (129), with cf=1.34632 and errBG= 0.0866284
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.3724 +/- 7.12503
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 4 (35569.1) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (33831.6 - 35569.1), exposure 1737.56, 46 soft counts and 27 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0342495, 0.0202127 and 0.590162. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (34995 - 35569.1), with lastBin= 0 and workMinC was 12
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 51902.8
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (33831.6 - 35569.1) = 33831.6- 35569.1
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 51902.8 - 53284.3


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (51902.8 - 52492), exposure 589.218
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.0854 bg counts (147), with cf=1.63412 and errBG= 0.0895226
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.7381 +/- 6.3306
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=51902.8 and stop= 52492 so gap is 589.218, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (51902.8 - 52492), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (34995 - 35569.1), exposure 574.164
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 28 counts and 0.983909 bg counts (129), with cf=1.34632 and errBG= 0.0866284
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =36.3724 +/- 7.12503
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 67
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 5
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52655), exposure 752.193, 15 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0308481, 0.00980176 and 0.317742. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52655 so gap is 162.975, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52732.7), exposure 829.92, 16 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0297761, 0.00878268 and 0.294957. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52732.7 so gap is 240.702, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52757.8), exposure 854.993, 17 soft counts and 5 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0308226, 0.00846905 and 0.274767. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52757.8 so gap is 265.775, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52830.5), exposure 927.705, 17 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0282632, 0.00946578 and 0.334915. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52830.5 so gap is 338.487, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52903.2), exposure 1000.42, 18 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0277176, 0.00866921 and 0.312769. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52903.2 so gap is 411.199, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 52918.2), exposure 1015.46, 19 soft counts and 6 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0288775, 0.00852889 and 0.295347. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 52918.2 so gap is 426.243, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 53033.6), exposure 1130.8, 19 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0258144, 0.00896201 and 0.347171. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 53033.6 so gap is 541.58, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 53073.7), exposure 1170.91, 19 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.024868, 0.0100724 and 0.405034. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 53073.7 so gap is 581.697, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 53076.2), exposure 1173.42, 20 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0262517, 0.0100508 and 0.382864. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 53076.2 so gap is 584.204, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 53103.8), exposure 1201, 21 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.026984, 0.00976949 and 0.362047. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 53103.8 so gap is 611.784, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52492 - 53284.3), exposure 792.305
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.49151 bg counts (202), with cf=1.65143 and errBG= 0.104942
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.3084 +/- 6.39832
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 53284.3), exposure 1381.52, 21 soft counts and 9 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0230898, 0.0095179 and 0.412212. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=52492 and stop= 53284.3 so gap is 792.305, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 5 (53284.3) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (52492 - 53284.3), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (51902.8 - 52492), exposure 589.218
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.0854 bg counts (147), with cf=1.63412 and errBG= 0.0895226
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.7381 +/- 6.3306
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 68
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 57563.6
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 57563.6 - 59163.3


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 57593.7), exposure 1411.61, 21 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0225371, 0.0107331 and 0.476242. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 57593.7 so gap is 30.0876, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 57643.9), exposure 1461.76, 21 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0217139, 0.0116863 and 0.538197. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 57643.9 so gap is 80.2338, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 57774.2), exposure 1592.14, 22 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0212434, 0.0106248 and 0.500147. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 57774.2 so gap is 210.614, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 57811.8), exposure 1629.75, 22 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.020738, 0.0116942 and 0.563904. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 57811.8 so gap is 248.224, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 57952.3), exposure 1770.16, 22 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0189809, 0.0119409 and 0.629101. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 57952.3 so gap is 388.633, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58130.3), exposure 1948.17, 23 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0182818, 0.0107947 and 0.59046. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58130.3 so gap is 566.652, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58258.2), exposure 2076.05, 24 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0181568, 0.0100975 and 0.556128. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58258.2 so gap is 694.525, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58371), exposure 2188.88, 24 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0171624, 0.0105373 and 0.613975. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58371 so gap is 807.355, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58516.4), exposure 2334.3, 25 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0169016, 0.00979899 and 0.579767. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58516.4 so gap is 952.779, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58624.2), exposure 2442.12, 26 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0170231, 0.00931608 and 0.547261. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58624.2 so gap is 1060.59, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 58664.3), exposure 2482.23, 26 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0167111, 0.0100857 and 0.603531. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58664.3 so gap is 1100.71, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (51902.8 - 58664.3) = 51902.8- 58664.3
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57563.6 - 58942.6), exposure 1379.02
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.74827 bg counts (235), with cf=2.22407 and errBG= 0.114045
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =29.4728 +/- 8.61753
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=57563.6 and stop= 58942.6 so gap is 1379.02, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (57563.6 - 58942.6), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (52492 - 53284.3), exposure 792.305
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 1.49151 bg counts (202), with cf=1.65143 and errBG= 0.104942
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =22.3084 +/- 6.39832
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 69
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 6
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (58942.6 - 59163.3), exposure 220.635
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.334776 bg counts (45), with cf=2.31733 and errBG= 0.0499054
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =3.85887 +/- 3.27924
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (58664.3 - 59163.3), exposure 498.947, 4 soft counts and 2 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.0164666, 0.00772227 and 0.468965. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=58942.6 and stop= 59163.3 so gap is 220.635, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 6 (59163.3) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=220.635 whereas forward=3800.09
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57563.6 - 59163.3), exposure 1599.66
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 2.08305 bg counts (280), with cf=2.23504 and errBG= 0.124486
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =33.34 +/- 9.21952
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 6 (59163.3) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  703  INFO   >>  Adding the HR counts to the previous bin.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (51902.8 - 59163.3), exposure 2981.18, 30 soft counts and 17 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.016674, 0.00969485 and 0.581434. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (57563.6 - 59163.3), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 62963.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 7
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (51902.8 - 59163.3) = 51902.8- 59163.3
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 62963.4 - 63261.7


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (62963.4 - 63261.7), exposure 298.369
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 0.490427 bg counts (61), with cf=1.32357 and errBG= 0.0627927
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =7.29228 +/- 3.24313
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 63261.7), exposure 298.369, 2 soft counts and 4 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00737978, 0.0170598 and 2.3117. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=62963.4 and stop= 63261.7 so gap is 298.369, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 7 (63261.7) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 17 counts, because gotBinThisOrb=0 and gapBack=4098.46 whereas forward=22306.7
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57563.6 - 63261.7), exposure 1898.03
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 2.57348 bg counts (341), with cf=1.99727 and errBG= 0.139362
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =40.7972 +/- 9.5826
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 7 (63261.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (57563.6 - 63261.7), with lastBin= 0 and workMinC was 10
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 85568.4
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 8
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 85568.4 - 87123


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85568.4 - 87123), exposure 1554.53
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 9 counts and 1.852 bg counts (361), with cf=1.34443 and errBG= 0.0974739
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =9.60995 +/- 4.03541
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 87123), exposure 1852.89, 8 soft counts and 7 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00464123, 0.00448461 and 0.966255. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=85568.4 and stop= 87123 so gap is 1554.53, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 8 (87123) and the bin is not full 9 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=23861.2 whereas forward=4444.87
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 8 (87123) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 91567.8 - 93064.7


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85568.4 - 93064.7), exposure 3051.38
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 2.69577 bg counts (753), with cf=1.51245 and errBG= 0.0982392
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =14.0722 +/- 5.24139
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 93064.7), exposure 3349.75, 10 soft counts and 8 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00344797, 0.0029561 and 0.857344. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=85568.4 and stop= 93064.7 so gap is 7496.25, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 9 (93064.7) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=29802.9 whereas forward=4522.56
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 9 (93064.7) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 97587.2 - 98763.2


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85568.4 - 98364.5), exposure 3828.65
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 3.14981 bg counts (930), with cf=1.55778 and errBG= 0.103286
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.46 +/- 6.03542
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=85568.4 and stop= 98364.5 so gap is 12796.1, and is Full=1 and tryBin= 1, endOrb=0
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (85568.4 - 98364.5), with lastBin= 0x1ed81d0 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (57563.6 - 63261.7), exposure 1898.03
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 23 counts and 2.57348 bg counts (341), with cf=1.99727 and errBG= 0.139362
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =40.7972 +/- 9.5826
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 70
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 10
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (98364.5 - 98763.2), exposure 398.658
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.246258 bg counts (96), with cf=1.68607 and errBG= 0.0251336
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.95692 +/- 2.38483
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 98763.2), exposure 4525.68, 13 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00350572, 0.00285752 and 0.815103. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=98364.5 and stop= 98763.2 so gap is 398.658, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 10 (98763.2) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=1 and gapBack=398.658 whereas forward=62367.8
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85568.4 - 98763.2), exposure 4227.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 3.39606 bg counts (1026), with cf=1.57288 and errBG= 0.106024
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.3973 +/- 6.48728
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 10 (98763.2) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (85568.4 - 98763.2), with lastBin= 0 and workMinC was 8
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 161131
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 11
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 161131 - 161344


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 161131 - 161344
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 161131 - 161344 the cf is 2.02462
++tructures/grbBin.cpp::        binData:  line  405  INFO   >>  This bin is empty, so found a emptyBin CF of 2.02462
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 161344), exposure 213.12
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 0 counts and 0.0460411 bg counts (43), with cf=2.02462 and errBG= 0.0070212
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =-0.093216 +/- 0.0142153
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 161344), exposure 4738.8, 13 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00334011, 0.00272233 and 0.815042. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 161344 so gap is 213.12, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 11 (161344) and the bin is not full 0 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=62580.9 whereas forward=52001.9
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 11 (161344) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 213346 - 213544


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 161131 - 213544
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 161131 - 213544 the cf is 2.0147
++tructures/grbBin.cpp::        binData:  line  405  INFO   >>  This bin is empty, so found a emptyBin CF of 2.0147
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 213544), exposure 411.197
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 0 counts and 0.107072 bg counts (100), with cf=2.0147 and errBG= 0.0107072
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =-0.215718 +/- 0.0215718
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 213544), exposure 4936.87, 13 soft counts and 10 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00319448, 0.00260605 and 0.815796. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 213544 so gap is 52413.1, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 12 (213544) and the bin is not full 0 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=114781 whereas forward=3867.7
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 12 (213544) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 217412 - 218164


++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 218164), exposure 1163.39
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 2 counts and 0.614116 bg counts (269), with cf=1.45387 and errBG= 0.0374433
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =2.0149 +/- 2.0568
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 218164), exposure 5689.06, 14 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00293701, 0.00247625 and 0.84312. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 218164 so gap is 57033, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 13 (218164) and the bin is not full 2 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=119401 whereas forward=5754.82
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 13 (218164) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 223919 - 225243


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 224433), exposure 6203.06, 15 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00288306, 0.00224995 and 0.780405. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 224433 so gap is 63301.8, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 224493), exposure 6263.24, 16 soft counts and 11 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00308321, 0.00222609 and 0.722006. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 224493 so gap is 63362, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 224704), exposure 6473.85, 16 soft counts and 12 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00296586, 0.00236818 and 0.798478. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 224704 so gap is 63572.6, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 225243), exposure 2487.24
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 6 counts and 1.29512 bg counts (484), with cf=1.44537 and errBG= 0.058869
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =6.80032 +/- 3.54145
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 225243), exposure 7012.92, 16 soft counts and 13 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00270027, 0.00237312 and 0.878846. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 225243 so gap is 64111.7, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 14 (225243) and the bin is not full 6 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=126479 whereas forward=9498.19
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 14 (225243) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 234741 - 235563


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 235563), exposure 3309.64
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 7 counts and 1.66966 bg counts (658), with cf=1.51937 and errBG= 0.06509
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =8.09875 +/- 4.02108
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 235563), exposure 7835.31, 16 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00236901, 0.00234262 and 0.988859. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 235563 so gap is 74432.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 15 (235563) and the bin is not full 7 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=136800 whereas forward=21888.6
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 15 (235563) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 257452 - 259144


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 257535), exposure 7918.05, 17 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00252293, 0.00231573 and 0.917875. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 257535 so gap is 96403.5, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 257881), exposure 8264.06, 18 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00256969, 0.00220492 and 0.858049. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 257881 so gap is 96749.5, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 259144), exposure 5002.06
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 10 counts and 2.72443 bg counts (991), with cf=1.50863 and errBG= 0.0865444
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =10.9761 +/- 4.77249
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 259144), exposure 9527.74, 19 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00231186, 0.0018649 and 0.806666. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 259144 so gap is 98013.2, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 16 (259144) and the bin is not full 10 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=160381 whereas forward=9861.97
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 16 (259144) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 269006 - 270664


++tructures/grbBin.cpp::        binData:  line  275  INFO   >>  I have enough counts and exposure to try for a full bin, and we have all events this frame
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 269154), exposure 9675.67, 20 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00242604, 0.00183047 and 0.75451. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 269154 so gap is 108023, and is Full=0 and tryBin= 0, endOrb=0
++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 270664), exposure 6659.39
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 12 counts and 3.5163 bg counts (1241), with cf=1.50704 and errBG= 0.099816
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =12.7853 +/- 5.22271
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 270664), exposure 11185.1, 21 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00217495, 0.00154463 and 0.710192. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 270664 so gap is 109533, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 17 (270664) and the bin is not full 12 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=171900 whereas forward=9855.95
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 17 (270664) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 280519 - 281763


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 281763), exposure 7903.01
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 13 counts and 3.71117 bg counts (1423), with cf=1.78893 and errBG= 0.0983803
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.6171 +/- 6.45248
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 281763), exposure 12428.7, 22 soft counts and 14 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00229113, 0.00138177 and 0.603094. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 281763 so gap is 120632, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 18 (281763) and the bin is not full 13 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=183000 whereas forward=84724.5
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 18 (281763) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 366488 - 368105


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 368105), exposure 9520.22
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 14 counts and 4.61381 bg counts (1708), with cf=1.76631 and errBG= 0.111639
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =16.5789 +/- 6.61187
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (62963.4 - 368105), exposure 14045.9, 22 soft counts and 15 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00195785, 0.00129366 and 0.660755. ISFULL=1
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 368105 so gap is 206974, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 19 (368105) and the bin is not full 14 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  659  INFO   >>    -> Continue accumulating counts in this bin for now, because gotBinThisOrb=0 and gapBack=269342 whereas forward=4553.61
++tructures/grbBin.cpp::        binData:  line  982  INFO   >>  GOT A FULL HR BIN (62963.4 - 368105) = 62963.4- 368105
++tructures/grbBin.cpp::        binData:  line  985  INFO   >>  Writing the previous HR bin to disk
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 372658 - 373864


++tructures/grbBin.cpp::        binData:  line  272  INFO   >>  The next event is in the next orbit; so try for a full bin.
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 373864), exposure 10726.2
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 15 counts and 4.96675 bg counts (1892), with cf=1.75488 and errBG= 0.114186
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =17.6072 +/- 6.79959
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (372658 - 373864), exposure 1206.01, 1 soft counts and 0 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00102567, -0.000106563 and -0.103895. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=161131 and stop= 373864 so gap is 212733, and is Full=1 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 20 (373864) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  953  INFO   >>  FULL BIN (161131 - 373864), with lastBin= 0x1ed9780 and workMinC was 15
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (85568.4 - 98763.2), exposure 4227.31
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 17 counts and 3.39606 bg counts (1026), with cf=1.57288 and errBG= 0.106024
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =21.3973 +/- 6.48728
++tructures/grbBin.cpp::        binData:  line  958  INFO   >>  Writing the previous bin to disk
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 71
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 378479
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed9780 which has initial GTIBin: 22
++tructures/grbBin.cpp::        binData:  line 1050  INFO   >>  Previous orbit completed, now starting new orbit: 378479 - 379264


++/SourceEventList.cpp::   getNextEvent:  line  163  INFO   >>  Need to read more source events from the FITS file
++tructures/grbBin.cpp::        binData:  line  198  INFO   >>  No more source events, setting the relevant flag
++tructures/grbBin.cpp::        binData:  line  244  INFO   >>  This was the last event in the orbit, or we have run out of events, or hit the split, so call fullBin().
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (378479 - 379264), exposure 784.785
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 1 counts and 0.385636 bg counts (130), with cf=1.57436 and errBG= 0.0338225
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =0.967227 +/- 1.57526
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (372658 - 379264), exposure 1990.8, 1 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.000438354, 0.000564852 and 1.28858. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  468  INFO   >>  AT THIS POINT, start=378479 and stop= 379264 so gap is 784.785, and is Full=0 and tryBin= 1, endOrb=1
++tructures/grbBin.cpp::        binData:  line  483  INFO   >>  End of orbit 21 (379264) and the bin is not full 1 There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  605  INFO   >>    -> Adding these counts to the previous bin, which had 15 counts, because gotBinThisOrb=0 and gapBack=5399.14 whereas forward=5945.4
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 379264), exposure 11511
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 5.35239 bg counts (2022), with cf=1.7436 and errBG= 0.11903
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.5652 +/- 6.97749
++tructures/grbBin.cpp::        binData:  line  670  INFO   >>  HR: End of orbit 21 (379264) and the HR bin is not full. There are future events. Deciding what to do.
++tructures/grbBin.cpp::        binData:  line  801  INFO   >>  I'm on the last event, so save the previous HR bin
++tructures/grbBin.cpp::        binData:  line  810  INFO   >>  The current bin is full, and there are orbits left, so writing this bin, which ends at the end of orbit 21 with stop = 379264 = 379264
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (161131 - 379264), exposure 11511
++taStructures/bin.cpp::frequentist_bin:  line  242  INFO   >>  Making a frequentist bin - I have 16 counts and 5.35239 bg counts (2022), with cf=1.7436 and errBG= 0.11903
++taStructures/bin.cpp::frequentist_bin:  line  243  INFO   >>    Therefore net =18.5652 +/- 6.97749
++ctures/binMethod.cpp::        saveBin:  line  408  INFO   >>  Saving a bin, bin number: 72
++tructures/grbBin.cpp::        binData:  line  825  INFO   >>  ON THE LAST EVENT, handling any leftover empty orbits
++tructures/grbBin.cpp::         newBin:  line 1121  INFO   >>     newBin:: We were at the end of an orbit, and the new time is 385209
++tructures/grbBin.cpp::         newBin:  line 1133  INFO   >>     newBin:: Made new bin: 0x1ed81d0 which has initial GTIBin: 23
++tructures/grbBin.cpp::        binData:  line  903  INFO   >>  I have run out of background events
++tructures/grbBin.cpp::        binData:  line  912  INFO   >>  Now setting the bayesian and UL permissions to 1, 1, Bin=0x1ed81d0
++ctures/binMethod.cpp::        emptyCF:  line  272  INFO   >>  Searching for the correction factor for an empty bin from 385209 - 385384
++ctures/binMethod.cpp::        emptyCF:  line  326  INFO   >>  EMPTYCF: For an empty bin at 385209 - 385384 the cf is 2.03946
++tructures/grbBin.cpp::        binData:  line  921  INFO   >>  This bin is empty, so found a emptyBin CF of 2.03946
++taStructures/bin.cpp::        fullBin:  line   97  INFO   >>  IN NORMAL FULLBIN, with (385209 - 385384), exposure 175.511
++taStructures/bin.cpp::        fullBin:  line  192  INFO   >>  Producing an upper limit of 12.0634 given bg=0.0546057 and numCts= 0
++ctures/binMethod.cpp::        saveBin:  line  378  INFO   >>  Saving an upper limit, bin number: 73 with rate=0.068733
++tructures/grbBin.cpp::        binData:  line  933  INFO   >>  I have now saved the final bin, so setting complete flag.
++Structures/hrbin.cpp::        fullBin:  line   95  INFO   >>  IN HR FULLBIN, with (372658 - 379264), exposure 2166.31, 1 soft counts and 1 hard ones
++Structures/hrbin.cpp::        fullBin:  line  231  INFO   >>  At the end of the HRBin::fullBin() call I have rates of 0.00037919, 0.000502748 and 1.32584. ISFULL=0
++tructures/grbBin.cpp::        binData:  line  944  INFO   >>  Discarding the final HR bin as it is not full
++tructures/grbBin.cpp::        binData:  line 1074  INFO   >>  Completed binning for PC mode.
++/genlc_cpp/genlc.cpp::           main:  line  397  INFO   >>  COMPLETE

